{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Directions","EUI Table for Medians","Categories from RECS & CBECS"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Directions","index":0,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":false,"merged":[[1,1,1,9],[3,2,3,9],[7,2,7,9],[2,1,2,9],[4,2,4,9],[5,2,5,9],[6,2,6,9]]}
[]
[null,"Directions for Preliminary EUI Targets for Topic 1, Phase 2:"]
[null,"This table contains BTO’s preliminary EUI targets for Topic 1, Phase 2 by end use, building type, and major climate region. Use this table to find the 75% reduction targets for heating, cooling, water heating, and ventilation end uses."]
[null,"1)","Select your building category by type and climate zone"]
[null,"2)","Record the median site EUI values for your selected building category"]
[null,"3)","Compare the 75% reduction EUI values to your intended retrofit measures"]
[null,"4)","Use the \"Energy Saved with Reductions\" columns for rough estimates of the overall technical potential of measures that reduce median EUI by 75%"]
[null,"Note:","All energy data in this table is given in site energy consumption for 2012 and 2015. Data is publically available from the EIA 2012 Commercial Buildings Energy Consumption Survey microdata (CBECS) and the EIA 2015 Residential Buildings Energy Consumption Survey microdata (RECS). "]

{"sheet":"EUI Table for Medians","index":1,"n_rows":43,"n_cols":22,"rows_kept":43,"cut":false,"hidden":false,"merged":[[0,10,0,12],[0,13,0,15],[0,16,0,18],[0,19,0,21],[0,0,2,0],[0,1,2,1],[0,2,2,2],[0,3,2,3],[0,4,0,6],[0,7,0,9]]}
["Ordering","Building Type","Climate Region","Number of Unweighted Samples in RECS 2015/ \nCBECS 2012","Total of \nHeating, Cooling, Water Heating, and Ventilation",null,null,"Heating",null,null,"Cooling",null,null,"Hot Water",null,null,"Ventilation",null,null,"Other"]
[{"$nulls":4},"Median Site EUI","75% Reduction in Site EUI","Energy Saved with Reduction","Median Site EUI","75% Reduction in Site EUI","Energy Saved with Reduction","Median Site EUI","75% Reduction in Site EUI","Energy Saved with Reduction","Median Site EUI","75% Reduction in Site EUI","Energy Saved with Reduction","Median Site EUI","75% Reduction in Site EUI","Energy Saved with Reduction","Median Site EUI","75% Reduction in Site EUI","Energy Saved with Reduction"]
[{"$nulls":4},"kBTU/sqft","kBTU/sqft","Quads","kBTU/sqft","kBTU/sqft","Quads","kBTU/sqft","kBTU/sqft","Quads","kBTU/sqft","kBTU/sqft","Quads","kBTU/sqft","kBTU/sqft","Quads","kBTU/sqft","kBTU/sqft","Quads"]
[1,"Single-family detached house","Cold/Very Cold",1360,32.338695370370402,8.0846738425925899,1.8472030978019101,23.6836765601218,5.9209191400304402,1.4026419080771999,1.10759558232932,0.276898895582329,7.2292704721969803E-2,6.2465193846153797,1.56162984615385,0.37226848500274301,null,null,null,8.2362584312239502,2.0590646078059902,0.51571512861268698]
[2,"Single-family detached house","Hot-Dry/Mixed-Dry",434,19.513024534686998,4.8782561336717398,0.224592215247121,5.7569800000000004,1.4392450000000001,8.6584969703137296E-2,3.6027976095617502,0.900699402390438,5.1196137588400303E-2,7.1807977900552498,1.79519944751381,8.6811107955583305E-2,null,null,null,11.388546846846801,2.8471367117117099,0.13257804396218101]
[3,"Single-family detached house","Hot-Humid",695,22.6025598802395,5.6506399700598804,0.51232333701127397,6.0269094228094602,1.5067273557023599,0.17918293528333601,8.7521896551724101,2.1880474137930999,0.20304987069833499,5.0567794476035699,1.26419486190089,0.130090531029603,null,null,null,10.954261229314399,2.7385653073285998,0.27795019557130701]
[4,"Single-family detached house","Mixed-Humid",960,27.1834392857143,6.7958598214285697,1.0687180138199299,16.4642848151062,4.1160712037765501,0.69292125863783005,3.40262204450626,0.85065551112656501,0.13668630131904699,5.8568796561604604,1.46421991404011,0.23911045386305399,null,null,null,9.9165564556962007,2.4791391139240502,0.42557200644029503]
[5,"Single-family detached house","Marine",303,19.823255159474702,4.95581378986867,0.15122342801062799,10.5860668973472,2.6465167243367902,8.6610325577627198E-2,0.42835875000000001,0.1070896875,3.9196459942710702E-3,7.9549401315789501,1.98873503289474,6.0693456438730101E-2,null,null,null,11.218814878892699,2.8047037197231801,8.6883025267883496E-2]
[6,"Single-family attached house","Cold/Very Cold",153,33.179950268817201,8.2949875672043003,0.11600132034911299,24.131260649087199,6.0328151622718096,8.8431610904275398E-2,1.01596556671449,0.253991391678623,3.8484585044892099E-3,6.3383607666290898,1.58459019165727,2.37212509403486E-2,null,null,null,9.8566983024691393,2.4641745756172799,3.5961275103429099E-2]
[7,"Single-family attached house","Hot-Dry/Mixed-Dry",89,21.915196054254,5.4787990135635001,2.0226402920556798E-2,3.7572296918767498,0.93930742296918801,6.57190467840556E-3,2.3312039018250501,0.58280097545626197,3.2793504632168701E-3,9.8844544117647093,2.47111360294118,1.0375147778934401E-2,null,null,null,12.2549171339564,3.0637292834891001,1.20028845541019E-2]
[8,"Single-family attached house","Hot-Humid",75,18.0966061403509,4.5241515350877197,2.0557746285453499E-2,2.6225059808612401,0.65562649521531102,4.68990124441831E-3,8.7852801235839308,2.19632003089598,8.9796144421813804E-3,5.5534822761194,1.38837056902985,6.8882305988538298E-3,null,null,null,12.243957182320401,3.0609892955801099,1.3277648796524599E-2]
[9,"Single-family attached house","Mixed-Humid",132,30.592458947368399,7.6481147368421096,0.10683874144779,18.757988029465899,4.6894970073664801,7.1192964260881203E-2,2.78389973958333,0.69597493489583295,9.6012146405780908E-3,7.5009070175438604,1.87522675438596,2.60445625463302E-2,null,null,null,8.7141175438596505,2.17852938596491,3.1858014754421397E-2]
[10,"Single-family attached house","Marine",30,18.3516377079482,4.5879094269870597,6.6116044822767603E-3,7.4928285714285696,1.87320714285714,2.5812452444372099E-3,0,0,1.12410239660063E-4,9.9203140822784803,2.4800785205696201,3.9179489981794801E-3,null,null,null,10.589890928725699,2.6474727321814302,4.66851073750658E-3]
[11,"Apartment in a building with 2-4 units","Cold/Very Cold",126,43.973278900565901,10.9933197251415,0.15151182095975099,26.095286786786801,6.5238216966967002,9.5852999229848301E-2,1.04914321295143,0.262285803237858,3.9680906259226597E-3,12.623012605042,3.1557531512604999,5.1690731103979697E-2,null,null,null,11.823320158102799,2.95583003952569,5.2858927280396803E-2]
[12,"Apartment in a building with 2-4 units","Hot-Dry/Mixed-Dry",45,22.087818497109801,5.52195462427746,1.8874026807511199E-2,4.3522752992382996,1.08806882480958,3.9134532657432502E-3,2.7859858989424202,0.69649647473560505,2.34806198002044E-3,14.671487394958,3.6678718487394999,1.26125115617476E-2,null,null,null,13.145750303030299,3.2864375757575801,1.25977813261958E-2]
[13,"Apartment in a building with 2-4 units","Hot-Humid",44,25.195525388600998,6.2988813471502603,2.0850690361732899E-2,4.7412488114104603,1.18531220285261,4.8027315640816401E-3,7.8640364321608001,1.9660091080402,7.2157178687838599E-3,9.1260958429561203,2.2815239607390301,8.8322409288674394E-3,null,null,null,13.693515434986001,3.4233788587464899,1.5380601495307599E-2]
[14,"Apartment in a building with 2-4 units","Mixed-Humid",83,42.482717121588102,10.620679280397001,7.3736916191223495E-2,21.314446428571401,5.32861160714286,4.26536705730605E-2,3.2917460770328102,0.82293651925820299,6.02823998014508E-3,12.3850200210748,3.0962550052686999,2.50550056380178E-2,null,null,null,9.9266044479745794,2.4816511119936502,2.2595765848070999E-2]
[15,"Apartment in a building with 2-4 units","Marine",13,24.050458930899602,6.0126147327249004,5.6851582826528196E-3,6.1230825082508202,1.5307706270627099,1.8655659480799199E-3,0,0,2.0269413641385499E-5,16.772490712074301,4.1931226780185797,3.7993229209315098E-3,null,null,null,9.6178659695817501,2.4044664923954402,3.1324537852867899E-3]
[16,"Apartment in a building with 5 or more units","Cold/Very Cold",301,31.047559718969602,7.7618899297423898,0.128606130986713,14.9422676727562,3.7355669181890399,6.6521357507273601E-2,0.86369884853852996,0.21592471213463199,4.5619095928919901E-3,12.178114055299501,3.0445285138248801,5.75228638865476E-2,null,null,null,11.927457286432199,2.98186432160804,5.7024940363593402E-2]
[17,"Apartment in a building with 5 or more units","Hot-Dry/Mixed-Dry",164,17.3534358552632,4.3383589638157902,3.3988258466319803E-2,1.81839653179191,0.45459913294797699,5.04181001550925E-3,1.9315947521865899,0.48289868804664698,4.8101065656175101E-3,11.3515669144981,2.8378917286245402,2.4136341885193102E-2,null,null,null,13.7380597758406,3.4345149439601501,2.8064998469486398E-2]
[18,"Apartment in a building with 5 or more units","Hot-Humid",145,18.776898876404498,4.6942247191011202,5.4960023264140297E-2,1.4097874818049501,0.35244687045123702,9.2832312009365307E-3,6.34141666666667,1.58535416666667,2.0430198966349698E-2,6.8970812500000003,1.7242703125000001,2.5246593096854099E-2,null,null,null,12.510960698690001,3.12774017467249,3.8404877508511799E-2]
[19,"Apartment in a building with 5 or more units","Mixed-Humid",198,30.2147610810811,7.5536902702702697,0.128462522265788,13.791358490565999,3.44783962264151,5.5927525724195799E-2,2.5118064211520301,0.62795160528800797,1.11941360478395E-2,12.379488306828801,3.0948720767072002,6.1340860493752501E-2,null,null,null,12.4109385194479,3.1027346298619798,5.8908856524224097E-2]
[20,"Apartment in a building with 5 or more units","Marine",50,18.1983142857143,4.5495785714285697,9.2274721916869706E-3,4.5862154605263203,1.1465538651315801,2.2025475028935402E-3,0,0,6.4000977618648101E-5,12.757245852186999,3.1893114630467601,6.96092371117479E-3,null,null,null,9.0024444444444391,2.2506111111111098,5.0860841493523996E-3]
[21,"Mobile Home","Cold/Very Cold",68,45.468144176136398,11.3670360440341,7.1868663287192297E-2,31.660538095238099,7.9151345238095203,4.8617846519870798E-2,1.22215740740741,0.30553935185185199,2.0130095590567901E-3,12.200198958333299,3.0500497395833301,2.1237807208264702E-2,null,null,null,14.766857248520701,3.6917143121301801,2.6639210230265501E-2]
[22,"Mobile Home","Hot-Dry/Mixed-Dry",18,29.682966872110899,7.42074171802774,7.8565566904536793E-3,8.4639414483821298,2.1159853620955298,2.5595062626456999E-3,5.0773081597222198,1.2693270399305601,1.5741055401697001E-3,12.612996918335901,3.15324922958398,3.7229448876382799E-3,null,null,null,10.758953775038499,2.6897384437596301,3.9231964295562303E-3]
[23,"Mobile Home","Hot-Humid",77,25.470157828282801,6.36753945707071,4.0492241824400199E-2,4.6397195652173897,1.1599298913043501,9.8031795129388793E-3,10.137001736111101,2.5342504340277801,1.6118763125124599E-2,8.2858843750000002,2.07147109375,1.45702991863367E-2,null,null,null,13.635909763313601,3.4089774408284002,2.7797644214934199E-2]
[24,"Mobile Home","Mixed-Humid",95,32.813079365079403,8.2032698412698402,7.3785951020057194E-2,15.253380859375,3.8133452148437499,3.8219513350075299E-2,3.8288744588744601,0.95721861471861502,8.5239972657903396E-3,10.3831343984962,2.5957835996240601,2.7042440404191501E-2,null,null,null,14.494399019607799,3.6235997549019601,3.8060252842010298E-2]
[25,"Mobile Home","Marine",28,31.4735883520847,7.8683970880211804,9.3565451569890996E-3,8.8310716981132096,2.2077679245283002,3.8060956129503699E-3,0.58537346938775503,0.14634336734693901,2.37865850252302E-4,15.0299706439394,3.75749266098485,5.3125836937864303E-3,null,null,null,14.5642634408602,3.6410658602150501,4.8877094442987797E-3]
[26,"Education","Cold/Very Cold",94,61.7603333333333,15.4400833333333,4.96389831706322E-2,38.880555555555603,9.72013888888889,3.4867739228763503E-2,3.58575,0.8964375,4.0915211004732702E-3,2.2646029411764701,0.56615073529411797,6.2175006260652803E-3,2.7074193548387102,0.676854838709677,4.4622222153302103E-3,18.944575,4.7361437500000001,2.2682340201421101E-2]
[27,"Education","Hot-Dry/Mixed-Dry",30,22.453600000000002,5.6134000000000004,8.0380575906959795E-3,6.62,1.655,3.7505693582134902E-3,3.8588607594936701,0.96471518987341798,1.3782001997235001E-3,0.91096363636363598,0.22774090909090899,1.72241345932371E-3,3.1589610389610399,0.78974025974025996,1.18687457343528E-3,16.5075,4.1268750000000001,5.4975702562881203E-3]
[28,"Education","Hot-Humid",44,21.151228070175399,5.2878070175438596,1.7573303741499801E-2,0.44624657534246598,0.111561643835616,4.10545169482965E-3,15.533740740740701,3.8834351851851898,7.7531801817343803E-3,1.5780487804878001,0.39451219512195101,2.3519018728092801E-3,4.8351641791044804,1.2087910447761201,3.3627699921264498E-3,21.937938144329902,5.4844845360824701,1.45385416210522E-2]
[29,"Education","Mixed-Humid",69,33.483809523809498,8.3709523809523798,6.4877493776457407E-2,11.6734920634921,2.9183730158730201,3.9274469248618597E-2,6.3891372549019598,1.59728431372549,8.1497079685088694E-3,2.8405714285714301,0.71014285714285696,8.4285498528957406E-3,3.4718367346938801,0.86795918367346903,9.0247667064342306E-3,21.670204081632701,5.4175510204081601,4.04055933715049E-2]
[30,"Education","Marine",6,87.095692307692303,21.773923076923101,1.26824079926295E-3,43.425538461538501,10.8563846153846,7.0195344438032405E-4,3.36830769230769,0.84207692307692295,4.64206750430565E-5,37.502153846153803,9.3755384615384596,4.5083966076481702E-4,2.7996923076923101,0.69992307692307698,6.9027019074752698E-5,13.648,3.4119999999999999,1.0138270162283901E-3]
[31,"Mercantile","Cold/Very Cold",92,31.574909090909099,7.8937272727272703,4.8537777811477799E-2,18.024117647058802,4.5060294117647102,2.9150187567461398E-2,1.5637333333333301,0.39093333333333302,3.7438989574393902E-3,0.341052631578947,8.5263157894736805E-2,4.9684895253903003E-3,6.1729670329670299,1.5432417582417599,1.0675201761186699E-2,34.697263157894703,8.6743157894736793,4.50734890060474E-2]
[32,"Mercantile","Hot-Dry/Mixed-Dry",24,16.1364615384615,4.0341153846153803,1.1650360065062201E-2,0.73483870967741904,0.18370967741935501,2.1268764306497001E-3,5.0740824742267998,1.2685206185567,2.3507822226253501E-3,0.155846153846154,3.8961538461538499E-2,3.53558695475369E-3,5.71608870967742,1.4290221774193499,3.63711445703348E-3,25.967666666666702,6.4919166666666701,1.8197897229302401E-2]
[33,"Mercantile","Hot-Humid",40,20.6068888888889,5.1517222222222196,9.9839503753285999E-3,0.06,1.4999999999999999E-2,4.6579497474165399E-4,10.925555555555601,2.73138888888889,5.11115837835907E-3,0.10666666666666701,2.66666666666667E-2,1.51772883515393E-3,4.5834999999999999,1.145875,2.8892681870739401E-3,26.195,6.5487500000000001,1.9599287393187899E-2]
[34,"Mercantile","Mixed-Humid",69,17.912500000000001,4.4781250000000004,1.6906656031416601E-2,4.1346999999999996,1.0336749999999999,4.8940218283906704E-3,4.07308641975309,1.0182716049382701,3.7638919497107398E-3,0.25766666666666699,6.4416666666666705E-2,3.7517445632324E-3,4.3613999999999997,1.0903499999999999,4.49699769008276E-3,27.0992,6.7747999999999999,2.2317425381583999E-2]
[35,"Mercantile","Marine",9,27.348815789473701,6.8372039473684199,5.1410745977769302E-3,22.1453947368421,5.5363486842105303,3.11727837327094E-3,1.79111111111111,0.447777777777778,1.5556102858809901E-4,3.0263157894736801E-2,7.5657894736842098E-3,3.6425606933894098E-4,3.2428947368421102,0.81072368421052599,1.5039791265789499E-3,16.885555555555602,4.2213888888888897,5.1966663669228801E-3]
[36,"Office","Cold/Very Cold",156,33.982466666666703,8.4956166666666704,7.3743353669313505E-2,23.744822222222201,5.93620555555556,4.5841349577591901E-2,1.899,0.47475000000000001,6.7385754333646004E-3,0.16520000000000001,4.1300000000000003E-2,1.92771718458376E-3,6.3,1.575,1.9235711473773301E-2,17.401250000000001,4.3503125000000002,4.9276270932273797E-2]
[37,"Office","Hot-Dry/Mixed-Dry",57,19.7690612244898,4.94226530612245,1.6036122720513499E-2,2.3007317073170701,0.57518292682926797,4.1383270561301203E-3,5.5963768115942001,1.39909420289855,5.5425671407488102E-3,0.41485106382978698,0.103712765957447,1.4880223009089001E-3,6.13791666666667,1.5344791666666699,4.8672062227256398E-3,22.818965517241399,5.7047413793103496,1.6021270124139401E-2]
[38,"Office","Hot-Humid",59,15.5352,3.8837999999999999,1.38789856668708E-2,0.2421875,6.0546875E-2,2.3938263491271698E-3,7.8718181818181803,1.96795454545455,5.51977387987093E-3,7.1142857142857105E-2,1.7785714285714301E-2,1.9317241734499201E-4,6.1684999999999999,1.542125,5.7722130205277097E-3,16.958666666666701,4.23966666666667,1.3446770929184899E-2]
[39,"Office","Mixed-Humid",139,25.867699999999999,6.4669249999999998,4.3175499695262999E-2,11.048999999999999,2.7622499999999999,1.67129921704635E-2,4.0568674698795197,1.0142168674698799,9.2821092152964406E-3,0.15021276595744701,3.7553191489361697E-2,2.0069982992078198E-3,5.3544444444444403,1.3386111111111101,1.5173400010295201E-2,24.204186046511602,6.0510465116279102,4.0935692018016903E-2]
[40,"Office","Marine",24,24.677,6.1692499999999999,7.9908786951327204E-3,10.157435897435899,2.53935897435897,4.03724201936277E-3,1.242,0.3105,6.4607839996113595E-4,1.24897435897436,0.31224358974359001,4.51812901377956E-4,8.8913333333333302,2.2228333333333299,2.8557453744308598E-3,27.086666666666702,6.7716666666666701,7.6988995411114902E-3]

{"sheet":"Categories from RECS & CBECS","index":2,"n_rows":64,"n_cols":4,"rows_kept":64,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Fields Included"]
["RECS/CBECS","Category","Description","Field Name"]
["RECS 2015","Other","Microwave","BTUELMICRO"]
["RECS 2015","Other","TVs & Related Peripherals","BTUELTVREL"]
["RECS 2015","Other","Swimming pool pumps","BTUELPLPMP"]
["RECS 2015","Other","Hot tub pumps","BTUELHTBPMP"]
["RECS 2015","Other","Hot Tub Heaters","BTUELHTBHEAT"]
["RECS 2015","Other","Other devices and uses","BTUELNEC"]
["RECS 2015","Other","Swimming Pool Heater, Natural Gas","BTUNGPLHEAT"]
["RECS 2015","Other","Hot Tub Heaters, Natural Gas","BTUNGHTBHEAT"]
["RECS 2015","Other","Other devices and uses, Natural Gas","BTUNGNEC"]
["RECS 2015","Other","Other devices and uses, Propane","BTULPNEC"]
["RECS 2015","Other","Other devices and uses, Fuel Oil","BTUFONEC"]
["RECS 2015","Heating","Space Heating, Electric","BTUELSPH"]
["RECS 2015","Cooling","Air Conditioning","BTUELCOL"]
["RECS 2015","Water Heating","Water Heating, Electric","BTUELWTH"]
["RECS 2015","Other","Refrigerators (all)","BTUELRFG"]
["RECS 2015","Other","Freezers","BTUELFRZ"]
["RECS 2015","Other","Stoves, Cooktop, Oven, Electric","BTUELCOK"]
["RECS 2015","Other","Clothes Washers","BTUELCW"]
["RECS 2015","Other","Clothes Dryers","BTUELCDR"]
["RECS 2015","Other","Dishwashers","BTUELDWH"]
["RECS 2015","Other","Lighting (indoor and outdoor)","BTUELLGT"]
["RECS 2015","Heating","Air handlers and boiler pumps for heating","BTUELAHUHEAT"]
["RECS 2015","Cooling","Air handlers for cooling","BTUELAHUCOL"]
["RECS 2015","Cooling","Evaporative Coolers","BTUELEVAPCOL"]
["RECS 2015","Other","Ceiling fans","BTUELCFAN"]
["RECS 2015","Other","Dehumidifiers","BTUELDHUM"]
["RECS 2015","Other","Humidifiers","BTUELHUM"]
["RECS 2015","Heating","Space Heating, Natural Gas","BTUNGSPH"]
["RECS 2015","Water Heating","Water Heating, Natural Gas","BTUNGWTH"]
["RECS 2015","Other","Stove, Cooktop, Oven, Natural Gas","BTUNGCOK"]
["RECS 2015","Other","Clothes Dryer, Natural Gas","BTUNGCDR"]
["RECS 2015","Heating","Space Heating, Propane","BTULPSPH"]
["RECS 2015","Water Heating","Water Heating, Propane","BTULPWTH"]
["RECS 2015","Other","Stove, Cooktop, Oven, Propane","BTULPCOK"]
["RECS 2015","Other","Clothes Dryers, Propane","BTULPCDR"]
["RECS 2015","Heating","Space Heating, Fuel Oil","BTUFOSPH"]
["RECS 2015","Water Heating","Water Heating, Fuel Oil","BTUFOWTH"]
["CBECS 2012","Other","Office Equipment, Electric","ELOFBTU"]
["CBECS 2012","Other","Computing, Electric","ELPCBTU"]
["CBECS 2012","Other","Misc, Electric","ELOTBTU"]
["CBECS 2012","Other","Misc, Natural Gas","NGOTBTU"]
["CBECS 2012","Other","Misc, Fuel Oil","FKOTBTU"]
["CBECS 2012","Other","Misc, District","DHOTBTU"]
["CBECS 2012","Heating","Heating, Electric","ELHTBTU"]
["CBECS 2012","Cooling","Cooling, Electric","ELCLBTU"]
["CBECS 2012","Ventilation","Ventilation, Electric","ELVNBTU"]
["CBECS 2012","Water Heating","Water Heating, Electric","ELWTBTU"]
["CBECS 2012","Other","Lighting, Electric","ELLTBTU"]
["CBECS 2012","Other","Cooking, Electric","ELCKBTU"]
["CBECS 2012","Other","Refrigeration, Electric","ELRFBTU"]
["CBECS 2012","Heating","Heating, Natural Gas","NGHTBTU"]
["CBECS 2012","Cooling","Cooling, Natural Gas","NGCLBTU"]
["CBECS 2012","Water Heating","Water Heating, Natural Gas","NGWTBTU"]
["CBECS 2012","Other","Cooking, Natural Gas","NGCKBTU"]
["CBECS 2012","Heating","Heating, Fuel Oil","FKHTBTU"]
["CBECS 2012","Cooling","Cooling, Fuel Oil","FKCLBTU"]
["CBECS 2012","Water Heating","Water Heating, Fuel Oil","FKWTBTU"]
["CBECS 2012","Other","Cooking, Fuel Oil","FKCKBTU"]
["CBECS 2012","Heating","Heating, District","DHHTBTU"]
["CBECS 2012","Cooling","Cooling, District","DHCLBTU"]
["CBECS 2012","Water Heating","Water Heating, District","DHWTBTU"]
["CBECS 2012","Other","Cooking, District","DHCKBTU"]