{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Directions","Residential Buildings Data","RECS_2015_Cut"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":1},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Directions","index":0,"n_rows":18,"n_cols":4,"rows_kept":18,"cut":false,"hidden":false,"merged":[[10,2,10,9],[2,1,2,9],[3,2,3,9],[4,3,4,9],[5,3,5,9],[6,3,6,9],[17,2,17,9],[11,2,11,9],[12,3,12,9],[13,2,13,9],[14,2,14,9],[15,3,15,9],[16,3,16,9]]}
[]
[]
[null,"Directions for Residential Buildings Data Pivot Table"]
[null,"1)","Select building characteristics in the white cells of the next tab:"]
[null,null,"A)"," Select type(s) of residential building."]
[null,null,"B)","Select the geographic region(s) (census division), climate zone(s), and/or the location type(s) (large city, small city, rural)."]
[null,null,"C)","Select the construction year range(s)."]
[null,null,"D)","Select the building façade type(s)."]
[null,null,"E)","Select the heating equipment type(s)."]
[null,null,"F)","Select the cooling equipment type(s)."]
[null,"2)","Record the results in the YELLOW highlighted cells: the number of homes/buildings, square feet, EUI, and other energy consumption data for your applicable building market."]
[null,"3)","Next, calculate your retrofit prototype solution's estimated potential site energy reductions at the building level."]
[null,null,"A)","Enter the estimated percentage reductions achievable by your retrofit prototype solution into the WHITE cells."]
[null,"4)","Record the resulting technical potential energy reductions in the YELLOW highlighted cells if your retrofit prototype solution was applied to the building market(s) (per the above selections)."]
[null,"5)","Repeat the above analysis using the building characteristics and percentage reductions you anticipate to achieve through your multi-system retrofit for Phase 2."]
[null,null,"A)","Select the appropriate building characteristics and market applicable to your multi-system retrofit for Phase 2 and record the results."]
[null,null,"B)","Enter the estimated percentage reductions achievable by your  multi-system retrofit to estimate the technical potential of energy reductions for the applicable market in Phase 2 and record the results."]
[null,"Note:","All energy data in this table is given in site energy consumption for 2015. Data is publically available from the EIA 2015 Residential Buildings Energy Consumption Survey microdata. "]

{"sheet":"Residential Buildings Data","index":1,"n_rows":24,"n_cols":11,"rows_kept":24,"cut":false,"hidden":false,"merged":[[1,7,1,12],[2,1,4,2],[11,3,11,5],[11,7,11,10],[18,4,18,5]]}
[]
[{"$nulls":6},"Source:","EIA 2015 Residential Energy Consumption Survey (RECS) Microdata. "]
[null,"Select Building Characteristics:",null,"Characteristic","Filter"]
[null,null,null,"Housing Type","(All)"]
[null,null,null,"Census Division","(All)"]
[null,null,null,"BA Climate Zone","(All)"]
[null,null,null,"Location Type","(All)"]
[null,null,null,"Year Built","(All)"]
[null,null,null,"Façade Type","(All)"]
[null,null,null,"Heating Equipment","(All)"]
[null,null,null,"Cooling Equipment","(All)"]
[null,null,null,"Summary",null,null,"Total Site Energy","Site Energy by End Use"]
[null,null,null,"Total Homes/Units","Total Buildings","Total Square Feet (Millions)","Total Site Energy (TBtu)","Site Heating (TBtu)","Site Cooling (TBtu)","Site Water Heating (TBtu)","Site All Other (TBtu)"]
[null,"Results:","Total",118208250.00058906,92481089.003122658,237420.53637304189,9113.851351215073,4013.7233179869822,774.03110649047869,1745.3395277648403,2575.7728374629964]
[null,null,"% of Total Residential",{"$f":"GETPIVOTDATA(\"Total Homes/Units\",$D$13)/D16","v":1},{"$f":"GETPIVOTDATA(\"Total Buildings\",$D$13)/E16","v":1},{"$f":"GETPIVOTDATA(\"Total Square Feet (Millions)\",$D$13)/F16","v":1},{"$f":"GETPIVOTDATA(\"Total Site Energy (TBtu)\",$D$13)/G16","v":1},{"$f":"GETPIVOTDATA(\"Site Heating (TBtu)\",$D$13)/H16","v":1},{"$f":"GETPIVOTDATA(\"Site Cooling (TBtu)\",$D$13)/I16","v":1},{"$f":"GETPIVOTDATA(\"Site Water Heating (TBtu)\",$D$13)/J16","v":1},{"$f":"GETPIVOTDATA(\"Site All Other (TBtu)\",$D$13)/K16","v":1}]
[null,null,"All Residential",118208250.00058906,92481089.003122658,237420.53637304189,9113.851351215073,4013.7233179869822,774.03110649047869,1745.3395277648403,2575.7728374629964]
[]
[]
[null,null,"Provide below inputs:",null,"Technical Potential Energy Savings"]
[null,null,"% Total Site Energy Savings",0.2,"Annual Site Energy Savings (TBtu)",{"$f":"D20*GETPIVOTDATA(\"Total Site Energy (TBtu)\",$D$13)","v":1822.7702702430147}]
[null,null,"% Total Site Heating Savings",0.2,"Annual Site Heating Savings (TBtu)",{"$f":"D21*GETPIVOTDATA(\"Site Heating (TBtu)\",$D$13)","v":802.74466359739654}]
[null,null,"% Total Site Cooling Savings",0.2,"Annual Site Cooling Savings (TBtu)",{"$f":"D22*GETPIVOTDATA(\"Site Cooling (TBtu)\",$D$13)","v":154.80622129809575}]
[null,null,"% Total Site Water Heating",0.2,"Annual Site Water Heating Savings (TBtu)",{"$f":"D23*GETPIVOTDATA(\"Site Water Heating (TBtu)\",$D$13)","v":349.06790555296811}]
[null,null,"% Total Site Other",0.2,"Annual Site Other Savings (TBtu)",{"$f":"D24*GETPIVOTDATA(\"Site All Other (TBtu)\",$D$13)","v":515.15456749259931}]

{"sheet":"RECS_2015_Cut","index":2,"n_rows":5687,"n_cols":25,"rows_kept":2250,"cut":true,"hidden":true,"merged":[],"bounds":{"rows_first":1000,"rows_last":250,"rows_between":1000,"halvings":1}}
["Housing Type","DOEID","Census Division","Year Built","Façade Type","Heating Equipment","Cooling Equipment","Total Sq Ft (Millions)","Number of Homes/ Units","Number of Buildings","BA Climate Zone","Weighted Total Site Electricity Use (GWh)","Location Type","Wtd Site Space Heating (TBtu)","Wtd Site Water Heating (TBtu)","Wtd Site Total Cooling (TBtu)","Wtd Site Ventilation (TBtu)","Wtd Other Energy (Tbtu)","Wtd Total Site Energy (Tbtu)","Air Handlers Heat","Air Handlers Cool","Wtd Air Handlers Heat (Tbtu)","Wtd Air Handlers Cool (Tbtu)","New Wtd Site Heating (Tbtu)","New Wtd Site Cooling (Tbtu)"]
["Single Family Detached",10001,"Pacific","2000s","Stucco","central furnace","central AC",21.849973391409897,12085.162270000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12085.162270000001},"Hot-Dry/Mixed-Dry",63.697772374439488,"Metropolitan Area",0.15618706610638491,0.21192087363086876,8.6318779090290343E-2,9.6882999518286307E-3,0.13743890672592984,0.591865625553474,454.14299999999997,347.52600000000001,{"$f":"T2*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4883918487846099E-3},{"$f":"U2*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.19990810304402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16167545795516952},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0518687193334363E-2}]
["Single Family Detached",10002,"West South Central","1980s","Siding","fireplace","window/wall unit",10.937338966048609,14410.19627,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14410.19627},"Hot-Humid",175.41531914849764,"Rural",0.1667262590478254,0.10274448325215595,0.10933479918368894,0,0.21970755039450973,0.59851309187818003,0,0,{"$f":"T3*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1667262590478254},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10933479918368894}]
["Single Family Detached",10003,"East South Central","1970s","Wood","central furnace","both central and individual units",53.369782398709681,23325.953850000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23325.953850000002},"Mixed-Humid",458.48081326088464,"Metropolitan Area",0.56410812670773725,0.43023420288100173,0.5651852726046227,3.6973759514050353E-2,0.69255032226905466,2.2520779244624163,684.19399999999996,900.89700000000005,{"$f":"T4*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5959477668446902E-2},{"$f":"U4*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1014281845603451E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5800676043761841},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.5861995544502262}]
["Single Family Detached",10004,"West North Central","1950s","Siding","central furnace","central AC",31.301402285567459,12165.333189999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12165.333189999999},"Mixed-Humid",119.85937099402773,"Micropolitan Area",0.65829696936920379,9.8269602890176402E-2,0.15488362076714363,2.8888469286299453E-2,0.17472361254938673,1.0861738055759105,1704.3420000000001,670.31299999999999,{"$f":"T5*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0733888299710981E-2},{"$f":"U5*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1545809865884705E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6790308576689148},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1630382017537321}]
["Single Family Detached",10005,"Middle Atlantic","1970s","Brick","central furnace","central AC",17.118895023781889,16717.67092,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16717.67092},"Cold/Very Cold",52.086494995430819,"Metropolitan Area",9.523274736124944E-2,0.28973413860890013,1.988889606982756E-2,6.8744400236713599E-3,0.20671249633541716,0.61156827837539429,356.69099999999997,54.517000000000003,{"$f":"T6*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9630427581257193E-3},{"$f":"U6*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1139726554564004E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10119579011937516},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0800293335373199E-2}]
["Multi-Family (5+ units)",10006,"New England","1980s","Siding","central furnace","window/wall unit",16.234691153470575,26058.89431,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2072.7617818139915},"Cold/Very Cold",72.365549491473189,"Rural",0.26546725080774664,0.27751786925844268,1.3977391553314868E-2,5.7978433950319E-3,0.22713278863890327,0.78943197488460359,222.49,0,{"$f":"T7*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6116876883579497E-4},{"$f":"U7*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26592841957658242},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3977391553314868E-2}]
["Multi-Family (2-4 units)",10007,"South Atlantic","1960s","Brick","central furnace","central AC",38.232692485446954,45952.755389999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15317.585129999999},"Hot-Humid",110.18358686120229,"Metropolitan Area",0.63230295998275099,0.47541787885559583,0.14892903550512238,1.0934090523007379E-2,1.1560118695511965,2.4199511375766707,83.980999999999995,153.96100000000001,{"$f":"T8*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2863861168025299E-3},{"$f":"U8*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3583107241999302E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63358934609955353},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1512873462293223}]
["Single Family Detached",10008,"East North Central","1970s","Siding","central furnace","window/wall unit",40.983597867968925,15280.983550000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15280.983550000001},"Cold/Very Cold",212.26659904570158,"Metropolitan Area",1.0389082133328664,0.26499016406972059,3.527968043237506E-2,2.4278869812762949E-2,0.66469506472084017,2.0038731225558024,1588.829,0,{"$f":"T9*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4278869812762949E-2},{"$f":"U9*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0631870831456294},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.527968043237506E-2}]
["Single Family Detached",10009,"Middle Atlantic","1980s","Siding","central furnace","central AC",26.66595848763366,14034.71499,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14034.71499},"Cold/Very Cold",146.27575038132463,"Metropolitan Area",0.82654707339881472,0.15971573025251956,4.0509997833145864E-2,1.2786467438789402E-2,0.28804701680968581,1.3148198182941659,770.95500000000004,140.10499999999999,{"$f":"T10*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.082013369511545E-2},{"$f":"U10*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9663337436739499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.8373672070939302},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.2476331576819813E-2}]
["Single Family Detached",10010,"West South Central","1950s","Brick","central furnace","central AC",53.331761991720043,43359.156089999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":43359.156089999997},"Hot-Humid",802.39595750398109,"Metropolitan Area",0.38584957459411057,0.46818150110742185,0.48120706854757478,2.7820145089621891E-2,1.4025369310361426,2.7377750752852497,129.24799999999999,512.37300000000005,{"$f":"T11*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.604084206320319E-3},{"$f":"U11*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.221606088330157E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39145365880043087},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.5034231294308763}]
["Single Family Detached",10011,"New England","1960s","Siding","central furnace","window/wall unit",26.988394411658337,12617.295190000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12617.295190000001},"Cold/Very Cold",31.154688369910623,"Metropolitan Area",0.91351413846692597,1.6477064578868092E-2,3.3952384318578603E-3,1.6170451688455902E-3,8.4810430116334434E-2,1.0181968715939862,128.161,0,{"$f":"T12*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6170451688455902E-3},{"$f":"U12*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.91513118363577162},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3952384318578603E-3}]
["Single Family Detached",10012,"West North Central","Before 1950","Stucco","central furnace","N/A",27.993834028563363,46656.390050000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":46656.390050000002},"Mixed-Humid",516.27763710709121,"Metropolitan Area",1.4118442914163236,0.29623411096554364,0,1.8923365240379502E-2,0.41322804168127181,2.1213064440631388,405.59,0,{"$f":"T13*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8923365240379502E-2},{"$f":"U13*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4307676566567031},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10013,"East South Central","2010s","Brick","central furnace","central AC",37.25418310527823,19773.982540000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19773.982540000001},"Hot-Humid",291.99761486376445,"Metropolitan Area",0.27791134156628072,8.9769451359511046E-2,0.21829523618201568,1.5699454567720299E-2,0.4257023441320138,1.0116783732398213,234.50299999999999,559.44200000000001,{"$f":"T14*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6370582275776203E-3},{"$f":"U14*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.106239634014268E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28254839979385832},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22935763252215835}]
["Multi-Family (5+ units)",10014,"East North Central","1970s","Brick","built-in electric unit","window/wall unit",10.419215608897508,13323.805130000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1059.7945458953436},"Cold/Very Cold",89.943399086823163,"Metropolitan Area",0.19929220090770852,0.15811816554286959,1.1417155292091872E-2,0,9.6177500940556354E-2,0.4650050226832263,0,0,{"$f":"T15*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U15*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19929220090770852},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1417155292091872E-2}]
["Single Family Detached",10015,"Mountain North","2000s","Brick","central furnace","central AC",38.511144248735377,8939.4485260000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8939.4485260000001},"Cold/Very Cold",148.2675567191387,"Metropolitan Area",0.61291670550817434,0.31452827453113585,5.2674055580926221E-2,2.3606589451027248E-2,0.37799185114720879,1.3581108867674454,2309.732,330.98899999999998,{"$f":"T16*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0647730322855034E-2},{"$f":"U16*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9588591281722136E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63356443583102939},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5632914709098438E-2}]
["Multi-Family (5+ units)",10016,"West South Central","2010s","Stucco","central furnace","central AC",83.770257748457496,52454.763769999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4172.3270497633484},"Hot-Humid",1078.1559489952433,"Metropolitan Area",0.35380223589073778,1.4056993352138112,0.43957809853801733,2.8063351071713767E-2,1.4537573406846103,3.6786681622549402,114.92,420.08100000000002,{"$f":"T17*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.79483824558804E-4},{"$f":"U17*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7527153193916374E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35428171971529659},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.44133081385740897}]
["Mobile Home",10017,"South Atlantic","1990s","Siding","central furnace","central AC",27.059889715197016,29285.594929999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29285.594929999999},"Mixed-Humid",349.20143394373292,"Metropolitan Area",0.34476697987542443,0.42082849345225315,0.13345972750309743,1.0317812948952811E-2,0.68719913640945962,1.5862543372402347,198.44900000000001,153.86799999999999,{"$f":"T18*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8116970282635697E-3},{"$f":"U18*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5061159206892399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35057867690368799},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13796584342378668}]
["Multi-Family (2-4 units)",10018,"Middle Atlantic","Before 1950","Siding","central furnace","N/A",53.465292539020979,43752.285219999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14584.095073333332},"Cold/Very Cold",100.51514374392642,"Metropolitan Area",0.8357033140959893,1.1965884238565558,0,9.7831422320476605E-3,0.4334921729241078,2.4723060056980182,223.60300000000001,0,{"$f":"T19*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2610474106825531E-3},{"$f":"U19*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83896436150667186},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10019,"Pacific","1990s","Wood","central furnace","central AC",21.530537456946252,12939.02491,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12939.02491},"Marine",61.228345746885061,"Metropolitan Area",0.37849728643581071,0.25242085100551082,1.1828235499526319E-2,3.1338577112518199E-3,0.28488525267544795,0.92763162561629597,197.999,44.203000000000003,{"$f":"T20*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5619139931550901E-3},{"$f":"U20*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7194371809673008E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38105920042896579},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2400179217623049E-2}]
["Single Family Detached",10020,"South Atlantic","1970s","Siding","heater burning gas/oil/kerosene","window/wall unit",71.965886920459283,25702.102470000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25702.102470000002},"Mixed-Humid",230.63665993422495,"Metropolitan Area",1.8159157642955801,0.62287523771578779,0.16842299885043338,0,0.61850924727131129,3.2257232481331126,0,0,{"$f":"T21*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U21*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8159157642955801},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16842299885043338}]
["Single Family Detached",10021,"Pacific","Before 1950","Stucco","heater burning gas/oil/kerosene","N/A",78.047703272709285,25946.709859999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25946.709859999999},"Marine",95.414199439022482,"Metropolitan Area",0.9948147852089132,0.41417534211522467,0,0,0.403983033388149,1.812973160712287,0,0,{"$f":"T22*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U22*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.9948147852089132},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10022,"South Atlantic","1970s","Brick","central furnace","window/wall unit",57.314686677486428,28387.66056,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28387.66056},"Mixed-Humid",462.03841495956885,"Metropolitan Area",1.5239472724131264,0.87529797201657888,0.21078053712020256,2.6718040304163599E-2,1.4044851553504514,4.0145109369003595,941.18499999999995,0,{"$f":"T23*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6718040304163599E-2},{"$f":"U23*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.55066531271729},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21078053712020256}]
["Single Family Detached",10023,"East North Central","1970s","Brick","central furnace","central AC",48.614779303067564,16319.16056,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16319.16056},"Cold/Very Cold",90.146080093375744,"Metropolitan Area",1.2288556696311053,0.26319813049233298,3.9237397990610559E-2,2.8797623001364563E-2,0.32623230792230179,1.8575235060363502,1652.7260000000001,111.925,{"$f":"T24*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6971100955686562E-2},{"$f":"U24*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8265220456779999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2558267705867918},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1063920036288559E-2}]
["Multi-Family (5+ units)",10024,"South Atlantic","2000s","Siding","central furnace","central AC",58.821052015074081,34846.594799999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2771.7480668426019},"Mixed-Humid",271.59435983737404,"Metropolitan Area",0.34630674979230636,0.19765176742171919,0.10519119429193323,1.149850511913E-2,0.26697673305446767,0.92671034211119996,179.69300000000001,150.28200000000001,{"$f":"T25*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9806372537514773E-4},{"$f":"U25*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1654384298123995E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3468048135176815},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10560773813491448}]
["Single Family Detached",10025,"East North Central","2000s","Siding","central furnace","central AC",55.992420689624744,16565.804940000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16565.804940000002},"Cold/Very Cold",173.87036495162761,"Metropolitan Area",0.95563175523182942,0.59414259991928386,4.1287021915181764E-2,2.4766309096228442E-2,0.52941632241000747,2.1204776994763024,1360.777,134.249,{"$f":"T26*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2542366348838383E-2},{"$f":"U26*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.22394274739006E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.97817412158066785},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.3510964662571823E-2}]
["Single Family Attached",10026,"Middle Atlantic","1980s","Siding","central furnace","central AC",26.982703805763485,17241.344280000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17241.344280000001},"Mixed-Humid",204.23403337772803,"Metropolitan Area",0.35549912253722155,9.9736590462221539E-2,6.3155578579312685E-2,9.1470676222126807E-3,0.17845524086931897,0.69684653244807471,358.32499999999999,172.20599999999999,{"$f":"T27*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1780046891310005E-3},{"$f":"U27*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9690629330816798E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36167712722635253},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6124641512394361E-2}]
["Single Family Detached",10027,"South Atlantic","1970s","Siding","central furnace","both central and individual units",62.76087250472677,19686.597399999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19686.597399999999},"Mixed-Humid",209.62456245435803,"Metropolitan Area",1.0328799328048153,0.28116453529152718,0.25351553608031796,5.5027721126713801E-2,0.41804300587564919,1.9856030100523097,2218.7910000000002,576.39599999999996,{"$f":"T28*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3680445131743399E-2},{"$f":"U28*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1347275994970398E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0765603779365587},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26486281207528833}]
["Single Family Detached",10028,"South Atlantic","1970s","Siding","built-in electric unit","window/wall unit",23.225782235878849,20302.2572,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20302.2572},"Mixed-Humid",289.57474883841127,"Metropolitan Area",0.444636791109906,0.18126778980862598,0.10129210283126878,0,0.26083235607768324,0.98802903982748402,0,0,{"$f":"T29*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U29*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.444636791109906},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10129210283126878}]
["Single Family Detached",10029,"South Atlantic","1960s","Concrete","central furnace","central AC",47.114961919556762,21533.346399999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21533.346399999999},"Hot-Humid",273.78080164530382,"Metropolitan Area",0.3556503047457712,0.21502047681007599,0.55279418497480237,3.6353047592754401E-2,0.3892038665731008,1.5126688331037506,330.536,1357.6849999999999,{"$f":"T30*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.117546185670399E-3},{"$f":"U30*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9235501407083996E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36276785093144159},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.58202968638188635}]
["Single Family Detached",10030,"Middle Atlantic","1950s","Siding","central furnace","central AC",48.95815963673509,16004.628839999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16004.628839999999},"Cold/Very Cold",197.51266044142471,"Metropolitan Area",1.7947056706711608,7.1456714627276513E-2,2.89680581078232E-2,1.50630765253428E-2,0.56006607765473337,2.4551965210609938,838.65300000000002,102.517,{"$f":"T31*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.342232999055252E-2},{"$f":"U31*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6407465347902798E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8081280006617133},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.060880464261348E-2}]
["Single Family Detached",10031,"Mountain South","2000s","Stucco","central furnace","central AC",31.576592448696488,10172.871279999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10172.871279999999},"Hot-Dry/Mixed-Dry",133.88399918999849,"Metropolitan Area",9.5938212738711198E-2,8.2203931125167287E-2,0.34580172372737994,2.3846695519526877E-2,0.1001515820468477,0.62409544963810615,318.57799999999997,2025.568,{"$f":"T32*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2408529866398395E-3},{"$f":"U32*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0605842532887039E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.917906572535104E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36640756626026699}]
["Single Family Detached",10032,"West South Central","1950s","Brick","central furnace","central AC",56.947020152188543,31602.11995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31602.11995},"Hot-Humid",291.12321649213231,"Metropolitan Area",1.1700405864768344,0.50917787573755291,0.58830054588604719,4.1460590881122202E-2,0.49940593141085388,2.7669249395112883,372.33600000000001,939.62,{"$f":"T33*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.17666069337032E-2},{"$f":"U33*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9693983947418998E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1818071934105376},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.61799452983346614}]
["Multi-Family (5+ units)",10033,"Middle Atlantic","Before 1950","Brick","portable electric heaters","N/A",27.722226608732665,27889.563989999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2218.375870527399},"Cold/Very Cold",119.03176665474803,"Metropolitan Area",0.18417690745021406,0.19464949450758703,0,0,0.2219594575787468,0.60078585953654795,0,0,{"$f":"T34*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U34*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18417690745021406},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10034,"Middle Atlantic","1970s","Wood","heat pump","central AC",14.68064539492299,13072.702929999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1039.8215172127843},"Mixed-Humid",107.24845487083546,"Metropolitan Area",0.11002857273637327,8.5862061897763062E-2,2.3310594104482094E-2,2.9289260187635702E-3,0.14404698933321797,0.36594417311948996,142.352,81.697000000000003,{"$f":"T35*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4802067261827429E-4},{"$f":"U35*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4950298491732841E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11017659340899155},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3395544402973825E-2}]
["Single Family Attached",10035,"South Atlantic","1970s","Shingle","built-in electric unit","central AC",25.967152492152405,17712.928029999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17712.928029999999},"Mixed-Humid",250.31589288164849,"Metropolitan Area",0.44123383743079614,9.2761452752788048E-2,0.12881486013996293,6.0431550818511601E-3,0.19126765088890577,0.85407780121245291,0,341.17200000000003,{"$f":"T36*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U36*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0431550818511601E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44123383743079614},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13485801522181409}]
["Single Family Attached",10036,"Middle Atlantic","Before 1950","Brick","radiator","window/wall unit",77.926269548602974,33033.603029999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33033.603029999998},"Mixed-Humid",98.53451403430995,"Metropolitan Area",2.2508194626607216,6.6723881054633366E-2,8.0838511990894799E-2,2.3907079184871602E-3,0.231353778811275,2.6297356345175249,72.372,0,{"$f":"T37*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3907079184871602E-3},{"$f":"U37*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2532101705792087},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.0838511990894799E-2}]
["Single Family Detached",10037,"East South Central","1980s","Brick","central furnace","N/A",54.923210153546243,16653.490040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16653.490040000001},"Hot-Humid",300.37621872753726,"Metropolitan Area",0.27384854136412656,0.28738528078267039,0,4.9963800818007996E-3,0.4636498495106201,1.024883671657417,300.02,0,{"$f":"T38*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9963800818007996E-3},{"$f":"U38*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27884492144592737},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10038,"East South Central","1970s","Brick","central furnace","central AC",56.92068629962575,33841.073900000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33841.073900000003},"Mixed-Humid",293.02471505597015,"Rural",1.5803612305930503,0.54394233550292037,0.34663960221167184,3.650040701028371E-2,0.63346459868898586,3.1044077669966277,582.01700000000005,496.56599999999997,{"$f":"T39*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9696080308056304E-2},{"$f":"U39*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6804326702227403E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6000573109011067},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36344392891389926}]
["Single Family Detached",10039,"Mountain North","2000s","Siding","wood-burning stove","N/A",24.5153267778336,12257.66339,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12257.66339},"Cold/Very Cold",67.135222381097321,"Metropolitan Area",0.14494829147570323,0.12833799310423119,0,0,0.29556001568281487,0.56884630026274929,0,0,{"$f":"T40*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U40*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14494829147570323},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10040,"South Atlantic","1970s","Siding","central furnace","window/wall unit",50.1366143568655,47749.15653,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":47749.15653},"Mixed-Humid",1051.1976810156134,"Metropolitan Area",1.6885528493805115,0.6906268490993519,0.19589158315251642,2.347305560773923E-2,1.0115588619620399,3.5866301435944199,491.59100000000001,0,{"$f":"T41*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.347305560773923E-2},{"$f":"U41*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7120259049882507},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19589158315251642}]
["Single Family Detached",10041,"West North Central","1950s","Brick","central furnace","central AC",28.931280633820371,11489.7858,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11489.7858},"Mixed-Humid",217.58005141273424,"Metropolitan Area",1.2438091938965117,0.38047681138580153,0.1785722172115134,2.7986670884424598E-2,0.30168689211831118,2.1045451146121379,1618.8589999999999,816.928,{"$f":"T42*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8600343150402199E-2},{"$f":"U42*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.3863277340224E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2624095370469139},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18795854494553579}]
["Single Family Detached",10042,"West North Central","Before 1950","Stone","central furnace","central AC",25.834065475873956,11663.234979999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11663.234979999999},"Mixed-Humid",185.48894001382433,"Metropolitan Area",0.70737013969301865,0.10441034089534318,0.13502880532365893,2.2135187139142795E-2,0.51557176274388261,1.4623810486559032,1402.684,495.17599999999999,{"$f":"T43*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6359833094686319E-2},{"$f":"U43*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7753540444564792E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.72372997278770501},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14080415936811541}]
["Single Family Detached",10043,"Pacific","1960s","Wood","central furnace","central AC",26.672752207161388,17399.05558,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17399.05558},"Hot-Dry/Mixed-Dry",168.54736567522289,"Metropolitan Area",0.45813408010153495,0.24513835630040207,0.19063245667832515,2.1279932326174578E-2,0.40436694437938475,1.2982718374596469,721.77200000000005,501.279,{"$f":"T44*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2558151144087761E-2},{"$f":"U44*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7217811820868192E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.47069223124562271},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19935423786041198}]
["Multi-Family (5+ units)",10044,"New England","1980s","Brick","central furnace","central AC",19.549981465166859,24106.019069999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1917.4272878032659},"Cold/Very Cold",138.14790706499025,"Metropolitan Area",7.887391409843425E-2,0.17258330709870914,1.5401392604261261E-2,2.2110522811385402E-3,0.20246681575921602,0.47136061157606735,63.908000000000001,27.814,{"$f":"T45*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2253894310893112E-4},{"$f":"U45*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.333132258296004E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.899645304154318E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5454723926844221E-2}]
["Single Family Detached",10045,"Pacific","1980s","Wood","central furnace","N/A",22.307798766604606,9464.4882340000004,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9464.4882340000004},"Marine",84.562041228181613,"Metropolitan Area",0.21235138154191144,0.12266569228227449,0,6.4422310641897166E-3,0.2695570293698718,0.60457410319405769,680.67399999999998,0,{"$f":"T46*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4422310641897166E-3},{"$f":"U46*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21879361260610117},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10046,"New England","1980s","Siding","radiator","window/wall unit",45.538376890985212,15510.34635,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15510.34635},"Cold/Very Cold",48.144673450676493,"Metropolitan Area",0.42085274352937535,0.18548139193690966,3.1756255365302397E-2,1.4559562118745002E-3,0.38481995995810447,1.0229103507896919,93.87,0,{"$f":"T47*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4559562118745002E-3},{"$f":"U47*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42230869974124985},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.1756255365302397E-2}]
["Single Family Attached",10047,"Pacific","2010s","Siding","built-in electric unit","N/A",11.376262381103295,7624.8407379999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7624.8407379999999},"Marine",58.862489524153766,"Metropolitan Area",5.4546151055582338E-2,6.2380987532347588E-2,0,0,8.3911684940160242E-2,0.20083882352809018,0,0,{"$f":"T48*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U48*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.4546151055582338E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10048,"South Atlantic","1970s","Brick","central furnace","central AC",38.02296703031805,24218.450339999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24218.450339999999},"Mixed-Humid",637.58318208401943,"Metropolitan Area",1.0357175285983173,0.57701797215353801,0.23739237441277389,2.875061848127658E-2,0.32530593038978217,2.1754338055544116,721.548,465.589,{"$f":"T49*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7474774405926322E-2},{"$f":"U49*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1275844075350261E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0531923030042436},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24866821848812415}]
["Single Family Detached",10049,"West South Central","1960s","Brick","central furnace","central AC",39.948802039607308,24478.43262,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24478.43262},"Hot-Humid",569.79128115374158,"Metropolitan Area",0.53758273080764063,0.43273658581749358,0.68086089623476198,4.2189827020633619E-2,0.29294760065445974,1.9441278135143558,371.13900000000001,1352.412,{"$f":"T50*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0849010041541799E-3},{"$f":"U50*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3104926016479443E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54666763181179479},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.71396582225124139}]
["Single Family Detached",10050,"West South Central","1960s","Brick","central furnace","central AC",111.56553974649421,45315.003960000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":45315.003960000002},"Hot-Humid",561.41809712613235,"Metropolitan Area",1.3549311706600971,0.56416232846617231,1.0121531642353183,7.866856884471049E-2,1.0523992771673569,3.9836459405289446,489.96800000000002,1246.07,{"$f":"T51*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2202901860273284E-2},{"$f":"U51*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6465666984437196E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3771340725203702},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0686188312197555}]
["Single Family Detached",10051,"East North Central","1970s","Siding","built-in electric unit","window/wall unit",40.528092173903651,27570.130730000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27570.130730000001},"Cold/Very Cold",652.0970582183711,"Metropolitan Area",1.4296794285778225,0.29662549259674914,4.2138187807732E-2,0,0.45651201435479305,2.2249551233370966,0,0,{"$f":"T52*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U52*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4296794285778225},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.2138187807732E-2}]
["Single Family Detached",10052,"Middle Atlantic","2010s","Siding","central furnace","central AC",68.642327178273717,22329.969799999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22329.969799999999},"Cold/Very Cold",284.84413169894464,"Metropolitan Area",2.0466766275175621,0.91483898903287797,3.2416707448267398E-2,2.7424865029447198E-2,0.64811893271641541,3.6420512567151229,1155.547,72.617000000000004,{"$f":"T53*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5803329612480601E-2},{"$f":"U53*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6215354169666E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0724799571300427},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4038242865233999E-2}]
["Single Family Detached",10053,"West South Central","Before 1950","Siding","portable electric heaters","window/wall unit",16.212740474505715,14411.32487,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14411.32487},"Hot-Humid",78.610361661276627,"Metropolitan Area",6.6575766920741075E-2,0.20564234258716552,9.4202939617475098E-2,0,0.16612509189511324,0.53254614102049491,0,0,{"$f":"T54*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U54*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.6575766920741075E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.4202939617475098E-2}]
["Single Family Detached",10054,"East North Central","Before 1950","Siding","central furnace","central AC",18.744854554555417,18596.085869999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18596.085869999999},"Cold/Very Cold",153.70552002879271,"Metropolitan Area",0.76178250236012701,0.20857211845062107,8.6183652944944344E-2,2.1255233168980647E-2,0.21211078622690915,1.2686490599826017,945.18200000000002,197.81299999999999,{"$f":"T55*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7576685634778339E-2},{"$f":"U55*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6785475342023099E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.77935918799490533},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.9862200479146656E-2}]
["Single Family Detached",10055,"New England","1980s","Wood","radiator","N/A",47.733319574000333,18302.65321,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18302.65321},"Cold/Very Cold",49.716009391029594,"Micropolitan Area",1.5400352256353165,0.1134151543163997,0,2.0673761933355499E-3,0.17898872886738229,1.8324391088190985,112.955,0,{"$f":"T56*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0673761933355499E-3},{"$f":"U56*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5421026018286521},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10056,"West North Central","2010s","Siding","built-in furnace","central AC",56.63988440512658,18509.766149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18509.766149999999},"Cold/Very Cold",423.43448201960865,"Rural",1.1137758865689926,0.21317769863042987,1.6720852780900949E-2,8.6318443463910001E-4,0.31196574582497333,1.6556401838052968,0,46.634,{"$f":"T57*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U57*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6318443463910001E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1137758865689926},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7584037215540048E-2}]
["Single Family Attached",10057,"Pacific","1980s","Shingle","portable electric heaters","central AC",7.3088014795697145,5894.1947419999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5894.1947419999997},"Hot-Dry/Mixed-Dry",18.096704453114704,"Metropolitan Area",5.5295385958966849E-3,5.7132488576153419E-2,6.7311291360008059E-3,3.6179746165344401E-4,5.9995422740432382E-2,0.1293885790484833,3.15,58.231999999999999,{"$f":"T58*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8566713437299999E-5},{"$f":"U58*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4323074821614397E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.5481053093339849E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0743598842169502E-3}]
["Single Family Attached",10058,"West South Central","1970s","Brick","central furnace","central AC",13.664552429775553,8540.3452689999995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8540.3452689999995},"Hot-Humid",81.59234923101593,"Metropolitan Area",0.24314478275504128,0.23191460450149814,9.5759347258010358E-2,9.2444113329763593E-3,0.17795671163230145,0.74877544614685121,547.63900000000001,534.80100000000004,{"$f":"T59*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6770261427698905E-3},{"$f":"U59*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5673851902064688E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24782180889781116},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10032673244821683}]
["Single Family Detached",10059,"East South Central","1970s","Brick","central furnace","central AC",13.703918793359282,10773.521059999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10773.521059999999},"Mixed-Humid",24.156550532430884,"Rural",0.41151436320376078,0.2109586214093668,9.4245577145563395E-3,1.1243569783847801E-3,0.12852325816132307,0.76042080048900695,62.39,41.972999999999999,{"$f":"T60*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7215997893340003E-4},{"$f":"U60*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5219699945137993E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.41218652318269416},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.876754714007719E-3}]
["Single Family Detached",10060,"South Atlantic","Before 1950","Siding","built-in furnace","central AC",41.187415292627342,24342.444029999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24342.444029999999},"Mixed-Humid",285.0463681822531,"Metropolitan Area",1.4452553757063427,0.15187620835466256,0.41860929342915243,1.938065063603301E-2,0.30099176447432685,2.3167326419644847,0,796.16700000000003,{"$f":"T61*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U61*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.938065063603301E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4452553757063427},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.43798994406518543}]
["Single Family Detached",10061,"Pacific","1980s","Stucco","central furnace","central AC",46.706994198803791,10215.878000000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10215.878000000001},"Hot-Dry/Mixed-Dry",93.651640367434098,"Metropolitan Area",0.21264689224149599,0.377674951644346,0.104152541398114,7.7367602381059998E-3,0.22616795411434792,0.92064233939830398,250.18799999999999,507.13900000000001,{"$f":"T62*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.555890085064E-3},{"$f":"U62*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1808701530420007E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21520278232655998},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.109333411551156}]
["Multi-Family (5+ units)",10062,"South Atlantic","2000s","Wood","heat pump","central AC",16.51660128539126,20093.188910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1598.2410286469571},"Hot-Humid",244.06483262796999,"Metropolitan Area",1.4007068405569043E-3,8.8503926675776418E-2,0.15480057674849718,6.8782401481044704E-3,0.58171286874299366,0.83274921408172531,1.113,341.20400000000001,{"$f":"T63*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7788422648840633E-6},{"$f":"U63*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4532623193845645E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4024856828217885E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15534590298043563}]
["Single Family Attached",10063,"West North Central","Before 1950","Wood","radiator","window/wall unit",14.207015621418199,6632.5936609999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6632.5936609999999},"Cold/Very Cold",21.472046985548587,"Metropolitan Area",0.49721736487470442,6.5107602113004565E-2,5.5066445611086402E-3,8.3739148007589402E-4,8.1107062906564595E-2,0.64893867445538211,126.254,0,{"$f":"T64*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3739148007589402E-4},{"$f":"U64*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4980547563547803},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5066445611086402E-3}]
["Single Family Detached",10064,"Mountain South","1960s","Wood","wood-burning stove","window/wall unit",24.519370136939184,13576.616910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13576.616910000001},"Cold/Very Cold",161.88758001819647,"Metropolitan Area",0,0.2963306263572591,4.973471839157733E-2,0,0.32372680016024663,0.66979214490908301,0,0,{"$f":"T65*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U65*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.973471839157733E-2}]
["Multi-Family (5+ units)",10065,"Pacific","1960s","Stucco","built-in electric unit","N/A",11.957361369633992,16050.14949,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1276.6518816766072},"Hot-Dry/Mixed-Dry",130.02168320858476,"Metropolitan Area",0.1250287545593107,9.1026207911905382E-2,0,0,0.31860522586738993,0.53466018833860596,0,0,{"$f":"T66*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U66*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1250287545593107},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10066,"East North Central","Before 1950","Siding","central furnace","central AC",126.21047676342815,25404.68534,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25404.68534},"Cold/Very Cold",71.644896334943255,"Metropolitan Area",1.9735621930926546,0.24837652763211196,3.5559776425014226E-2,1.3179391851314521E-2,0.26686816621144771,2.5243666633612278,435.17,83.608000000000004,{"$f":"T67*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.10553569194078E-2},{"$f":"U67*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1240349319067201E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9846175500120624},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7683811356920949E-2}]
["Single Family Detached",10067,"East North Central","1950s","Siding","central furnace","both central and individual units",68.458623143174407,28079.829020000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28079.829020000001},"Cold/Very Cold",215.92290592672774,"Metropolitan Area",1.0981126506369423,0.80497917234674654,6.7768701751738603E-2,4.6744126331816738E-2,0.62527666248762348,2.596137187223051,1555.692,108.995,{"$f":"T68*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.368356536778184E-2},{"$f":"U68*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0605609640349E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1417962160047241},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.08292627157735E-2}]
["Single Family Detached",10068,"Middle Atlantic","Before 1950","Brick","central furnace","central AC",100.08214455339487,26688.57188,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26688.57188},"Cold/Very Cold",209.87999681431452,"Metropolitan Area",2.4545026652971198,0.60426575064095989,0.18477747337687983,7.7915043763622086E-2,0.56256149431840274,3.8061073836333623,2506.0970000000002,413.31900000000002,{"$f":"T69*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6884149922752364E-2},{"$f":"U69*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1030893840869721E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5213868152198722},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19580836721774955}]
["Single Family Detached",10069,"Pacific","1950s","Shingle","central furnace","window/wall unit",21.278147528483103,18109.061730000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18109.061730000001},"Cold/Very Cold",374.72022050263553,"Micropolitan Area",0.82505432135544243,0.19120420231309387,3.7540990419376509E-2,1.5948958519660411E-2,0.22474589699470854,1.2785454110826213,880.71699999999998,0,{"$f":"T70*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5948958519660411E-2},{"$f":"U70*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84100327987510282},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7540990419376509E-2}]
["Single Family Attached",10070,"East South Central","1970s","Concrete","built-in electric unit","central AC",14.113595857275628,10212.442730000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10212.442730000001},"Mixed-Humid",97.459771564251312,"Micropolitan Area",3.881240902025046E-2,7.0347952185682142E-2,4.7040533278040544E-2,2.2438677041928703E-3,0.17633183520487555,0.33253272968884873,0,219.71899999999999,{"$f":"T71*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U71*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2438677041928703E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.881240902025046E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.9284400982233412E-2}]
["Single Family Attached",10071,"New England","2000s","Wood","central furnace","central AC",34.030008020261555,6979.0828590000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6979.0828590000001},"Cold/Very Cold",40.951234282315205,"Metropolitan Area",0.36296706655211175,0.20070077990337246,2.3631760803534154E-2,1.2885878490294662E-2,0.11641579203180111,0.7037153992908195,1624.875,221.482,{"$f":"T72*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1340137260517625E-2},{"$f":"U72*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5457412297770381E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37430720381262939},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5177502033311192E-2}]
["Multi-Family (2-4 units)",10072,"Pacific","1980s","Wood","central furnace","central AC",16.239078167035533,19565.154419999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6521.7181399999999},"Hot-Dry/Mixed-Dry",48.596947931744026,"Metropolitan Area",0.13647310858142414,0.28559604166622676,3.5297345089604783E-2,4.0542717337579796E-3,0.12696484135811062,0.58703418451787159,129.989,77.23,{"$f":"T73*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4775161930045998E-4},{"$f":"U73*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0367229195219998E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13732086020072459},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5801017381556985E-2}]
["Single Family Detached",10073,"Mountain North","2000s","Concrete","central furnace","central AC",109.84306755179179,20966.418699999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20966.418699999998},"Cold/Very Cold",288.33635404353896,"Metropolitan Area",1.5773105557863334,0.79179520875767873,6.0947701847404001E-2,2.8462269814367894E-2,0.66828838902084498,3.098341855412261,1188.1469999999999,169.37,{"$f":"T74*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4911187479148899E-2},{"$f":"U74*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5510823352189998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6022217432654824},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4498784182623004E-2}]
["Single Family Detached",10074,"East South Central","2000s","Brick","heat pump","central AC",88.390204216418454,24745.297930000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24745.297930000001},"Mixed-Humid",562.52580113020645,"Metropolitan Area",0.19329824121436603,0.34494336580090923,0.1849470001065662,1.386592871388378E-2,1.1961494457056006,1.919338052827442,155.625,404.721,{"$f":"T75*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8509869903562504E-3},{"$f":"U75*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0014941723527531E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19714922820472228},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19496194183009374}]
["Single Family Detached",10075,"New England","1980s","Siding","central furnace","window/wall unit",14.414196260003125,11531.35701,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11531.35701},"Cold/Very Cold",148.47740689432993,"Rural",0.80615527742655024,0.30240484450966465,8.5078928587630481E-3,7.5614913262383298E-3,0.1881306763364749,1.305198691131453,655.73299999999995,0,{"$f":"T76*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5614913262383298E-3},{"$f":"U76*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.81371676875278853},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5078928587630481E-3}]
["Single Family Detached",10076,"West North Central","Before 1950","Siding","central furnace","central AC",28.32326107839236,12792.80085,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12792.80085},"Mixed-Humid",166.94623017103675,"Metropolitan Area",1.2588616874553278,0.19640835757648228,0.15482303012380261,2.9365119575924848E-2,0.3932756824690597,2.0033687576246724,1682.3389999999999,613.10199999999998,{"$f":"T77*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1521827789188149E-2},{"$f":"U77*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8432917867367006E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.280383515244516},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16266632191053931}]
["Single Family Detached",10077,"West South Central","2000s","Brick","central furnace","central AC",46.312332678703818,22657.69701,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22657.69701},"Hot-Humid",289.99998767087948,"Micropolitan Area",0.20803384289392496,0.22270787378548138,0.20426507486176662,1.5382605050150129E-2,0.354473144304711,0.98947993584588401,209.429,469.48399999999998,{"$f":"T78*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7451788271072898E-3},{"$f":"U78*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.063742622304284E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21277902172103225},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21490250108480946}]
["Single Family Detached",10078,"Pacific","1990s","Siding","built-in electric unit","N/A",37.207917643147702,19982.769950000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19982.769950000002},"Marine",571.4672749552393,"Metropolitan Area",0.7254059221338216,0.51661413187918104,0,0,0.70782630008077863,1.9498463540937812,0,0,{"$f":"T79*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U79*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.7254059221338216},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10079,"West South Central","1980s","Brick","central furnace","central AC",50.653255557710168,19071.255860000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19071.255860000001},"Hot-Humid",305.40423061477298,"Metropolitan Area",0.50052716974133293,0.21565192546058684,0.52190133696019547,3.7824803668628268E-2,0.46570427710134793,1.7037847092634633,432.35300000000001,1550.9880000000001,{"$f":"T80*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2455146848385806E-3},{"$f":"U80*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9579288983789684E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.50877268442617152},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.55148062594398517}]
["Single Family Detached",10080,"West South Central","1990s","Brick","central furnace","central AC",77.867557996872748,18066.718789999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18066.718789999999},"Mixed-Humid",194.22047903174513,"Metropolitan Area",1.0602621581061873,0.24872047063692101,0.16289965397316239,3.2274657447237849E-2,0.68425495084104493,2.1561372335573155,1171.0740000000001,615.34100000000001,{"$f":"T81*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1157464640280458E-2},{"$f":"U81*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1117192806957389E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0814196227464679},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17401684678011978}]
["Multi-Family (5+ units)",10081,"East North Central","1980s","Brick","built-in electric unit","window/wall unit",7.2246720788015129,10687.38473,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":850.08989070520727},"Cold/Very Cold",85.499858034724639,"Metropolitan Area",0.11943546800271537,7.8970977437067214E-2,6.9053650839017901E-3,0,8.6413714912578099E-2,0.29172552543626251,0,0,{"$f":"T82*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U82*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11943546800271537},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9053650839017901E-3}]
["Single Family Detached",10082,"East South Central","1980s","Brick","heat pump","central AC",45.676487716251749,15296.88135,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15296.88135},"Mixed-Humid",366.93660308186583,"Metropolitan Area",1.1616650250709923,0.1776767339754351,0.30159638736975131,3.1238128529987398E-2,0.28790599979600978,1.9288441462121886,964.40499999999997,1077.7190000000001,{"$f":"T83*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.475238885834675E-2},{"$f":"U83*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6485739671640652E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1764174139293391},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31808212704139194}]
["Single Family Detached",10083,"East North Central","1990s","Brick","central furnace","central AC",103.64149293721145,13155.812760000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13155.812760000001},"Cold/Very Cold",290.63563699368621,"Metropolitan Area",3.5929324126301427,0.48978385753916065,0.12906094384514785,5.9868933319884847E-2,0.8133674250466213,5.0251446390610726,3741.3440000000001,809.41499999999996,{"$f":"T84*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9220421134749441E-2},{"$f":"U84*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0648512185135401E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.6421528337648921},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13970945603028326}]
["Single Family Detached",10084,"Mountain North","1970s","Wood","central furnace","N/A",35.091987841387343,16009.118539999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16009.118539999999},"Cold/Very Cold",138.4680372044854,"Metropolitan Area",0.34077675703575255,0.50142616439012389,6.9525312515268778E-2,2.2854665655059621E-2,0.38007293151345922,1.2918011654546044,1427.6030000000001,0,{"$f":"T85*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2854665655059621E-2},{"$f":"U85*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36363142269081217},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9525312515268778E-2}]
["Multi-Family (2-4 units)",10085,"Pacific","1950s","Wood","built-in electric unit","N/A",10.321812766371357,27378.813699999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9126.2712333333329},"Hot-Dry/Mixed-Dry",210.13173808592509,"Metropolitan Area",9.4634185083707495E-2,0.20469526391363069,0,0,0.4176400655620221,0.71696951455936031,0,0,{"$f":"T86*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U86*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.4634185083707495E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10086,"Pacific","1960s","Stucco","central furnace","N/A",18.20164284677119,13664.89703,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13664.89703},"Marine",40.995347011389036,"Metropolitan Area",0.39166337432813919,2.4736100949426788E-2,0,3.73744499198421E-3,0.111402594765679,0.52780207004324498,273.50700000000001,0,{"$f":"T87*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.73744499198421E-3},{"$f":"U87*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39540081932012339},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10087,"South Atlantic","1970s","Brick","heat pump","central AC",20.626510105325888,16620.878410000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16620.878410000001},"Mixed-Humid",117.15219498094206,"Metropolitan Area",0.11685883648543488,8.7027999711856652E-2,4.2942382916090815E-2,4.3397944572430508E-3,0.15289408096068199,0.39972330007406431,144.54599999999999,116.559,{"$f":"T88*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.40248149065186E-3},{"$f":"U88*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9373129665911902E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11926131797608674},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.4879695882682008E-2}]
["Single Family Detached",10088,"West South Central","Before 1950","Wood","central furnace","central AC",107.75230177734723,29537.363430000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29537.363430000001},"Hot-Humid",662.50176520184107,"Metropolitan Area",1.3194442738832102,0.67923471121632539,1.3182475971412071,0.10323405992084318,0.63898494357907776,3.9559115258198205,828.16499999999996,2666.8679999999999,{"$f":"T89*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.446181058500595E-2},{"$f":"U89*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8772249335837249E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.343906084468216},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3970198464770442}]
["Single Family Detached",10089,"East North Central","1990s","Siding","central furnace","central AC",30.812151775286701,20165.020799999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20165.020799999998},"Cold/Very Cold",97.83676888497817,"Metropolitan Area",1.6858556289917759,0.21679262624423995,8.1825702062323188E-2,2.17234542675072E-2,0.25298488623616289,2.237458843534502,894.90300000000002,182.381,{"$f":"T90*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8045737608982398E-2},{"$f":"U90*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6777166585247995E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7039013666007583},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.550341872084799E-2}]
["Single Family Detached",10090,"Pacific","1990s","Siding","built-in electric unit","window/wall unit",20.453842974756231,12487.083619999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12487.083619999999},"Marine",130.97780680972252,"Metropolitan Area",8.4744804234241133E-2,0.12563624447757152,6.5903955317127404E-3,0,0.22992480805297977,0.44689625229650515,0,0,{"$f":"T91*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U91*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.4744804234241133E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5903955317127404E-3}]
["Single Family Detached",10091,"East North Central","1950s","Brick","central furnace","central AC",47.591700568131152,21151.86692,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21151.86692},"Cold/Very Cold",155.27739913990766,"Metropolitan Area",2.5178544441261694,0.20573989454998834,6.6057407302361523E-2,2.2165633597741756E-2,0.23874926539480448,3.0284010113733233,910.55499999999995,137.37299999999999,{"$f":"T92*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9259938183340597E-2},{"$f":"U92*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9056954144011595E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5371143823095101},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.8963102716762689E-2}]
["Single Family Attached",10092,"East North Central","2010s","Siding","central furnace","central AC",46.530510092268216,14255.670980000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14255.670980000001},"Cold/Very Cold",178.31834351563884,"Metropolitan Area",0.20415794459133055,0.37271343434110554,2.7161543753258702E-2,2.3355065766534001E-2,0.55939174519329604,1.1634246678789908,1534.05,104.25,{"$f":"T93*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1868912066869001E-2},{"$f":"U93*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4861536996650002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22602685665819955},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8647697452923702E-2}]
["Single Family Detached",10093,"East North Central","Before 1950","Siding","central furnace","window/wall unit",52.476319997966478,33595.595390000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33595.595390000002},"Mixed-Humid",523.53628883605029,"Micropolitan Area",0.69652568716688812,0.58411939399292123,0.25842148559370837,5.7279381485302136E-2,0.88648559813651939,2.4255521648900369,1704.9670000000001,0,{"$f":"T94*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7279381485302136E-2},{"$f":"U94*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.75380506865219021},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25842148559370837}]
["Single Family Detached",10094,"East North Central","Before 1950","Siding","central furnace","window/wall unit",51.140528862162178,39922.348839999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39922.348839999999},"Cold/Very Cold",168.10730206318317,"Metropolitan Area",1.3191920590291693,0.36054551917334277,5.668298847584604E-2,2.3350062845981075E-2,0.74434345112740374,2.4807640178057619,584.88699999999994,0,{"$f":"T95*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3350062845981075E-2},{"$f":"U95*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3425421218751503},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.668298847584604E-2}]
["Single Family Detached",10095,"East South Central","1960s","Other","central furnace","both central and individual units",41.252344126547698,38196.614930000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38196.614930000003},"Hot-Humid",861.60868234385339,"Micropolitan Area",1.3286772716291855,1.8120526452154457,0.61684469743432624,4.0328711778777671E-2,2.0337307869994974,5.7913054012784544,477.91500000000002,577.904,{"$f":"T96*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.825473522427095E-2},{"$f":"U96*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2073976554506724E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3469320068534565},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.63891867398883295}]
["Mobile Home",10096,"Mountain North","1970s","Siding","central furnace","N/A",10.898067907827071,15199.536829999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15199.536829999999},"Cold/Very Cold",87.801401265365868,"Metropolitan Area",0.34069003347557186,0.44476109495567667,5.9823066633281838E-2,3.0311372332490895E-3,0.25223243781195831,1.0975066328764886,199.423,0,{"$f":"T97*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0311372332490895E-3},{"$f":"U97*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34372117070882097},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9823066633281838E-2}]
["Single Family Detached",10097,"East South Central","1970s","Siding","central furnace","central AC",28.743667377271873,16084.87262,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16084.87262},"Hot-Humid",137.48836010689794,"Metropolitan Area",3.7180054382149039E-2,0.13193821044437273,0.13172288225460879,8.0699414421801993E-3,0.16826914440091198,0.46911029148204253,57.133000000000003,444.577,{"$f":"T98*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1897702739846009E-4},{"$f":"U98*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1509644147817403E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.8099031409547499E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13887384666939054}]
["Single Family Detached",10098,"Pacific","1990s","Wood","radiator","window/wall unit",105.15159331698609,15836.083329999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15836.083329999999},"Marine",229.06848613463822,"Micropolitan Area",1.384909780733574,0.27926725499763377,1.2770138416895348E-2,9.2473224997201991E-4,0.81136956827379847,2.4883167424219015,58.393999999999998,0,{"$f":"T99*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.2473224997201991E-4},{"$f":"U99*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3858345129835459},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2770138416895348E-2}]
["Mobile Home",10099,"East South Central","2000s","Siding","central furnace","central AC",50.70471179307976,39003.624459999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39003.624459999999},"Mixed-Humid",571.93304052903932,"Micropolitan Area",0.61067740795275238,0.27087397029841087,0.26241201696094046,1.7476041982796519E-2,1.274286556652922,2.4182499518650253,202.78700000000001,245.27500000000001,{"$f":"T100*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.90942799337002E-3},{"$f":"U100*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5666139894264989E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6185868359461224},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27197863095036695}]
["Single Family Detached",10100,"Pacific","2000s","Siding","central furnace","N/A",25.365985864923992,15373.324769999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15373.324769999999},"Marine",194.80562137881944,"Rural",0.33191318719590351,9.0015935845498399E-2,0,3.8451759914724E-3,0.38380364657159632,0.80573276961299822,250.12,0,{"$f":"T101*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8451759914724E-3},{"$f":"U101*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3357583631873759},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10101,"East North Central","1950s","Wood","central furnace","N/A",20.393289588968756,22046.799559999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22046.799559999999},"Cold/Very Cold",104.67383902387573,"Metropolitan Area",1.4741578195374285,0.19985906626050362,0,2.1545763993199438E-2,0.33560132138542176,2.0096182071833537,977.274,0,{"$f":"T102*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1545763993199438E-2},{"$f":"U102*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.495703583530628},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10102,"Pacific","2010s","Siding","built-in electric unit","N/A",17.844487576576125,8833.9047410000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":702.66143733902072},"Marine",82.626452731722537,"Metropolitan Area",3.4647254604867062E-2,0.10579534671078625,0,0,0.14147886251129627,0.2819214638269496,0,0,{"$f":"T103*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U103*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.4647254604867062E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10103,"Pacific","2000s","Brick","central furnace","central AC",53.511707135107919,15789.822109999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15789.822109999999},"Hot-Dry/Mixed-Dry",427.38311508585605,"Metropolitan Area",0.28550684223620909,0.47909779831764299,0.21876620108415154,1.8433401497122529E-2,1.2847637765296176,2.268134618167621,339.88299999999998,827.54,{"$f":"T104*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3666921082131296E-3},{"$f":"U104*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3066709388909399E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2908735343444222},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23183291047306093}]
["Single Family Detached",10104,"South Atlantic","1990s","Stucco","heat pump","central AC",62.319413977581419,32627.96543,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32627.96543},"Hot-Humid",507.81848909105832,"Metropolitan Area",4.6948085805538137E-2,0.20493200923032409,0.47392331868850296,2.566372197675908E-2,1.0631019561136268,1.788905369837992,25.366,761.19,{"$f":"T105*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2764097109738006E-4},{"$f":"U105*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4836081005661703E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.7775726776635517E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.49875939969416466}]
["Single Family Attached",10105,"South Atlantic","1950s","Brick","central furnace","window/wall unit",32.880926084038485,20823.892390000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20823.892390000001},"Mixed-Humid",207.05675153045848,"Metropolitan Area",1.4331991044730832,0.34709378367060151,9.5819454097301415E-2,1.2232100157132731E-2,0.31324839901074886,2.1893607412517349,587.40700000000004,0,{"$f":"T106*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2232100157132731E-2},{"$f":"U106*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.445431204630216},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.5819454097301415E-2}]
["Single Family Detached",10106,"East North Central","2000s","Siding","central furnace","central AC",100.40994315330869,19391.64603,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19391.64603},"Cold/Very Cold",222.87183347437033,"Metropolitan Area",2.7450002579681643,0.35924005487864119,0.10562420162763876,8.6083608364482325E-2,0.6114357221493445,3.8213002366237889,4078.0239999999999,361.18700000000001,{"$f":"T107*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.9079597909844715E-2},{"$f":"U107*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0040104546376103E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8240798558780091},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11262821208227637}]
["Single Family Detached",10107,"Middle Atlantic","Before 1950","Shingle","radiator","window/wall unit",127.55928962981373,36156.261229999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":36156.261229999996},"Mixed-Humid",1043.3973505039328,"Metropolitan Area",4.8519450035585372,1.0596461549971468,0.69176729695409445,5.9417391892320499E-3,1.8005582353716794,8.4039166908814558,164.33500000000001,0,{"$f":"T108*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9417391892320499E-3},{"$f":"U108*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.8578867427477697},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.69176729695409445}]
["Single Family Attached",10108,"East North Central","1990s","Brick","central furnace","central AC",23.596063306370404,10303.957780000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10303.957780000001},"Cold/Very Cold",92.673796234714146,"Metropolitan Area",0.56770646629648447,9.961761281334644E-2,1.7814698077082039E-2,7.5692152574835404E-3,0.29642254695804848,0.98156132414496133,646.83299999999997,87.76,{"$f":"T109*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6649399227107402E-3},{"$f":"U109*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0427533477280004E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.57437140621919525},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8718973411854838E-2}]
["Single Family Detached",10109,"South Atlantic","1990s","Wood","central furnace","central AC",109.7816664205221,16168.139380000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16168.139380000001},"Mixed-Humid",289.99174799977681,"Metropolitan Area",1.1780115406426055,0.28545354521338662,0.26203376896750519,4.9218775042226541E-2,0.459428545472363,2.1849274002958601,1901.2560000000001,1142.9269999999999,{"$f":"T110*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0739772005061283E-2},{"$f":"U110*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8479003037165258E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2087513126476668},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28051277200467045}]
["Single Family Detached",10110,"East South Central","1960s","Siding","central furnace","central AC",47.485636698337139,18658.403419999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18658.403419999999},"Mixed-Humid",345.9507940730706,"Metropolitan Area",0.53537010332209101,0.16422669559400208,0.26754715673057006,2.2762860345928181E-2,0.2132401570035454,1.1803841126502084,532.13300000000004,687.846,{"$f":"T111*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9287521870948595E-3},{"$f":"U111*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.283410815883332E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54529885550918589},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2803812648894034}]
["Single Family Detached",10111,"East South Central","1970s","Brick","heat pump","central AC",26.006976611392375,11114.092570000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11114.092570000001},"Mixed-Humid",216.10339395122014,"Micropolitan Area",0.19240302501531137,0.18499122561995207,0.12670565663965652,1.1771624514626341E-2,0.23324485899560343,0.73734476627052348,452.04300000000001,607.11900000000003,{"$f":"T112*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.02404774762051E-3},{"$f":"U112*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7475767670058312E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19742707276293187},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13345323340666235}]
["Single Family Attached",10112,"South Atlantic","1970s","Concrete","heat pump","central AC",29.067748221399299,11534.82072,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11534.82072},"Mixed-Humid",189.2464168373329,"Metropolitan Area",0.58938218444489665,0.17625660532096368,0.19380742332230039,2.697114459587064E-2,0.34534095139679732,1.304787164484958,1473.202,865.03499999999997,{"$f":"T113*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.699312095434544E-2},{"$f":"U113*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9780236415252001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60637530539924211},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20378544696382558}]
["Single Family Detached",10113,"East North Central","1980s","Wood","central furnace","central AC",44.140491753260385,23342.407060000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23342.407060000001},"Cold/Very Cold",159.48968062438033,"Metropolitan Area",1.3040242239942978,0.1825952789546382,4.6984063778509208E-2,2.4186468499289602E-2,0.29268266910378909,1.8262862358312342,938.92600000000004,97.233999999999995,{"$f":"T114*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1916792891217562E-2},{"$f":"U114*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2696756080720403E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3259410168855155},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.9253739386581251E-2}]
["Multi-Family (2-4 units)",10114,"South Atlantic","Before 1950","Brick","central furnace","central AC",40.634471512303193,31646.784670000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10548.928223333334},"Mixed-Humid",303.87242637160068,"Metropolitan Area",0.57521286536974736,0.18112746055455539,0.1147763793093762,1.352596235509668E-2,0.24592960047298931,1.1260636139433995,258.87200000000001,168.53200000000001,{"$f":"T115*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7308221470307469E-3},{"$f":"U115*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7778319713348137E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.57794368751677816},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11655421128071101}]
["Single Family Detached",10115,"East North Central","1950s","Brick","central furnace","central AC",17.654788118980374,21322.207869999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21322.207869999998},"Cold/Very Cold",33.209296118038282,"Metropolitan Area",2.4337646106718442,0.21452034529278857,1.385137532092514E-2,5.573987614751791E-3,0.1279110294793992,2.7900473607649574,228.155,33.262,{"$f":"T116*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8647683365798501E-3},{"$f":"U116*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0921927817193999E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4386293790084239},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4560594599097081E-2}]
["Single Family Detached",10116,"West South Central","1980s","Wood","portable electric heaters","N/A",21.196215168930227,23815.972099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23815.972099999999},"Mixed-Humid",181.04282775085801,"Metropolitan Area",0.43509635207613784,0.63236840730333221,0,0,0.21578878300716733,1.2832535423866374,0,0,{"$f":"T117*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U117*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43509635207613784},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10117,"East North Central","1960s","Brick","radiator","both central and individual units",11.303149396970211,14853.021549999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1181.4306104877717},"Cold/Very Cold",23.694579682660535,"Metropolitan Area",0.25816822900869435,0.15657248798939835,5.8850526088683785E-3,5.7840636520010004E-4,7.0476176217702746E-2,0.49163434491903024,22.934999999999999,16.007000000000001,{"$f":"T118*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7096111051537042E-5},{"$f":"U118*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8911159782077766E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25819532511974591},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9039637686504566E-3}]
["Mobile Home",10118,"West South Central","2000s","Siding","central furnace","central AC",52.407420602824743,38762.885060000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38762.885060000001},"Hot-Humid",683.97110690594866,"Rural",0.66912178211203011,0.56351629434322126,0.38644824940972766,2.4753048090074562E-2,0.71459440628726056,2.3336807321522399,256.76,381.81599999999997,{"$f":"T119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.952758368005599E-3},{"$f":"U119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.480028972206896E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.67907454048003568},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.40124853913179664}]
["Single Family Detached",10119,"Mountain South","1960s","Concrete","central furnace","central AC",36.663185925996146,23233.958129999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23233.958129999999},"Hot-Dry/Mixed-Dry",315.21510992268043,"Metropolitan Area",0.24338358772355609,0.23898611970224909,0.57512412920072609,3.3078279125513518E-2,0.51947057465819801,1.5769644112847292,241.911,1181.7929999999999,{"$f":"T120*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6205500451864303E-3},{"$f":"U120*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7457729080327085E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24900413776874253},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.60258185828105315}]
["Single Family Detached",10120,"Middle Atlantic","1950s","Siding","central furnace","central AC",34.473890365004756,27469.235349999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27469.235349999999},"Mixed-Humid",190.35171977029404,"Metropolitan Area",1.271718631502547,0.24219534159618344,0.23900855319552389,4.1069858094962698E-2,0.45709332284795168,2.2100158491422062,1134.664,360.45800000000003,{"$f":"T121*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1168352459172398E-2},{"$f":"U121*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9015056357903003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3028869839617194},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24891005883131417}]
["Multi-Family (5+ units)",10121,"Middle Atlantic","2000s","Wood","radiator","window/wall unit",12.950571064836506,21161.063829999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1683.1813294748504},"Mixed-Humid",112.11910345041775,"Metropolitan Area",0.16986447474920419,0.34868991484542083,4.339349116064907E-2,1.8261151642736801E-3,0.34821461619073513,0.9118433602942746,86.296000000000006,0,{"$f":"T122*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4525181600836171E-4},{"$f":"U122*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17000972656521254},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.339349116064907E-2}]
["Multi-Family (5+ units)",10122,"South Atlantic","2010s","Brick","built-in electric unit","window/wall unit",15.138653707906617,12238.20025,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":973.44397865154235},"Mixed-Humid",91.970074870588704,"Metropolitan Area",6.5807201431498999E-2,0.15803743597116349,1.8394590171161747E-2,0,7.1560465036425769E-2,0.31379969261024998,0,0,{"$f":"T123*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U123*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.5807201431498999E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8394590171161747E-2}]
["Single Family Detached",10123,"West South Central","1950s","Shingle","portable electric heaters","N/A",50.310213920644514,26340.42614,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26340.42614},"Hot-Humid",329.78200352638731,"Metropolitan Area",0.86798468352732749,0.290717597519907,0,0,0.30993960251685049,1.4686418835640851,0,0,{"$f":"T124*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U124*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.86798468352732749},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10124,"East North Central","1990s","Siding","central furnace","central AC",18.903790714229956,17986.480220000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17986.480220000001},"Cold/Very Cold",242.04260745418142,"Metropolitan Area",0.52289070416281025,0.10124654467166794,4.416711519326607E-2,1.0696254016670261E-2,0.15754503715187787,0.82584940117962202,488.93900000000002,105.744,{"$f":"T125*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7942916522865816E-3},{"$f":"U125*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.90196236438368E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53168499581509687},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.6069077557649753E-2}]
["Single Family Detached",10125,"Pacific","1950s","Wood","central furnace","N/A",14.767931517036034,18646.37818,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18646.37818},"Marine",172.81463295440651,"Metropolitan Area",0.36463814836267738,0.73141906392028777,0,4.9594144972909598E-3,0.26023519364866116,1.3562924059316261,265.97199999999998,0,{"$f":"T126*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9594144972909598E-3},{"$f":"U126*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36959756285996836},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10126,"Pacific","1950s","Concrete","central furnace","N/A",48.864482580862912,10414.4251,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10414.4251},"Marine",40.037153377445406,"Metropolitan Area",0.38731419826356661,9.0563632381098005E-2,0,4.3671537781587002E-3,0.12709698781161874,0.60497481845628331,419.33699999999999,0,{"$f":"T127*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3671537781587002E-3},{"$f":"U127*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39168135204172533},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",10127,"South Atlantic","1990s","Siding","central furnace","central AC",70.247054984385016,52034.855539999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":52034.855539999997},"Cold/Very Cold",438.45453873909292,"Micropolitan Area",1.6608118345525642,0.76784282339744603,0.10956292670964669,2.1751246068842017E-2,0.65417517914338208,3.1923927638030389,342.34399999999999,75.668999999999997,{"$f":"T128*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7813820584985759E-2},{"$f":"U128*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9374254838562594E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.67862565513755},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11350035219350295}]
["Mobile Home",10128,"South Atlantic","1970s","Siding","central furnace","window/wall unit",19.659740027893893,26424.38176,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26424.38176},"Mixed-Humid",317.89440253512515,"Rural",0.53485279312711231,0.15459357299004864,0.10912616984650526,6.5384490226943993E-3,0.28608311991015006,1.0846556558738163,247.44,0,{"$f":"T129*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5384490226943993E-3},{"$f":"U129*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54139124214980672},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10912616984650526}]
["Single Family Detached",10129,"South Atlantic","1970s","Stucco","central furnace","central AC",43.696872686583433,15988.610570000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15988.610570000001},"Hot-Humid",234.45930374043141,"Metropolitan Area",8.0716070193838363E-2,9.2885737174751584E-2,0.25590209305214617,1.720396881386798E-2,0.37047121614388867,0.79997511656462483,97.287999999999997,978.726,{"$f":"T130*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5554999451341601E-3},{"$f":"U130*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.564846886873382E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.2271570138972516E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27155056192088001}]
["Single Family Attached",10130,"West South Central","2000s","Concrete","central furnace","central AC",67.749776822278889,15136.232529999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15136.232529999999},"Hot-Humid",332.1300518039875,"Metropolitan Area",0.32649469611873971,0.21627193943235079,0.30541708364243636,2.6943492894746977E-2,0.28504400224547444,1.1332277214390014,456.23200000000003,1323.8340000000001,{"$f":"T131*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9056336396269603E-3},{"$f":"U131*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.003785925512002E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3334003297583667},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32545494289755639}]
["Single Family Detached",10131,"Pacific","Before 1950","Stucco","central furnace","N/A",28.176234971771567,15954.83294,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15954.83294},"Hot-Dry/Mixed-Dry",65.183118969424328,"Metropolitan Area",0.11470157554677043,0.1772289647094539,0,2.1853813322906201E-3,0.28639019260814347,0.5783207328643678,136.97300000000001,0,{"$f":"T132*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1853813322906201E-3},{"$f":"U132*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11688695687906106},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",10132,"New England","Before 1950","Siding","central furnace","window/wall unit",32.402094926123922,24602.957419999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8200.9858066666657},"Cold/Very Cold",304.28937740797323,"Rural",0.98329591014429341,0.25970431618431211,1.762430394485958E-2,1.30842218003173E-2,0.68305087352724836,1.9523982183342581,531.81500000000005,0,{"$f":"T133*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3614072667724334E-3},{"$f":"U133*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.98765731741106588},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.762430394485958E-2}]
["Single Family Detached",10133,"South Atlantic","1990s","Siding","heat pump","central AC",126.47032371047342,22087.02824,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22087.02824},"Mixed-Humid",454.94860771713786,"Metropolitan Area",0.52673723626891888,0.2866401516119424,0.12068330143307759,1.79003216019668E-2,0.962287558012207,1.8963482473261459,472.76299999999998,337.68200000000002,{"$f":"T134*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0441929731827119E-2},{"$f":"U134*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4583918701396799E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.537179166000746},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12814169330321729}]
["Single Family Detached",10134,"South Atlantic","1970s","Siding","central furnace","central AC",90.000009923072881,30991.738949999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30991.738949999999},"Mixed-Humid",434.32250656450162,"Metropolitan Area",1.261044560353815,0.35140572051497548,0.38971795613887705,5.0741503521538049E-2,1.7289509238631291,3.7311191608707968,921.32299999999998,715.93600000000004,{"$f":"T135*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8553401904630848E-2},{"$f":"U135*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2188101616907201E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2895979622584459},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.41190605775578426}]
["Single Family Detached",10135,"Pacific","2000s","Stucco","central furnace","central AC",51.760955313403642,13170.72654,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13170.72654},"Marine",234.85320449542309,"Metropolitan Area",0.20524999459550505,0.29865408721824438,2.542882709659032E-2,1.77579588866166E-2,0.76754405593993469,1.2968769648502745,1225.653,122.637,{"$f":"T136*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6142740495930619E-2},{"$f":"U136*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.61521839068598E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22139273509143567},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7044045487276298E-2}]
["Single Family Detached",10136,"Mountain South","1990s","Stucco","radiator","central AC",41.241856521865564,15621.915349999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15621.915349999999},"Hot-Dry/Mixed-Dry",47.774660326421156,"Metropolitan Area",1.0722226575795297,0.26838948910399663,5.1688137587052894E-2,1.7937239424023498E-3,0.17792699214439178,1.5702272764149712,39.384999999999998,75.436000000000007,{"$f":"T137*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1526913605974994E-4},{"$f":"U137*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1784548063426001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0728379267155894},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2866592393395494E-2}]
["Multi-Family (5+ units)",10137,"West South Central","1980s","Siding","heat pump","central AC",62.522875187882157,40311.33152,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3206.4210535834409},"Hot-Humid",246.74005696026794,"Micropolitan Area",4.8452535254873259E-2,0.17057651247758657,0.13591988519520679,8.4923882113184003E-3,0.47911126073136806,0.84187708514699455,22.254999999999999,188.41499999999999,{"$f":"T138*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1358900547499477E-5},{"$f":"U138*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0413782281092403E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.8523894155420758E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13652402301801772}]
["Single Family Detached",10138,"West North Central","1980s","Siding","central furnace","central AC",57.098293173178043,9368.0546630000008,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9368.0546630000008},"Cold/Very Cold",247.8949799673415,"Metropolitan Area",0.80209669988458121,8.7234575577482973E-2,0.14162368354825633,4.6864040069680035E-2,0.68579497113901544,1.7167499301493359,3929.4319999999998,1073.105,{"$f":"T139*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6811133770541411E-2},{"$f":"U139*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0052906299138617E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83890783365512267},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15167658984739496}]
["Single Family Detached",10139,"South Atlantic","2000s","Siding","heat pump","central AC",34.45659311826234,12341.18665,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12341.18665},"Hot-Humid",227.5924247633522,"Metropolitan Area",0.16389652458717915,0.11287767639929298,0.23552274794916855,1.4700846219853299E-2,0.29698168468955538,0.80927863362519614,225.59200000000001,965.61,{"$f":"T140*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7840729787468E-3},{"$f":"U140*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.19167732411065E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16668059756592596},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24743952119027504}]
["Single Family Attached",10140,"East North Central","1990s","Siding","central furnace","central AC",19.505376644559473,12832.484630000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12832.484630000001},"Cold/Very Cold",37.650509917853618,"Metropolitan Area",0.18319542131923258,0.27289439905554014,2.0637355771781558E-2,9.7879648190478709E-3,0.195641006537638,0.67236818268419229,690.572,72.177000000000007,{"$f":"T141*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8617545759083604E-3},{"$f":"U141*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.2621024313951016E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19205717589514093},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1563566014921067E-2}]
["Single Family Detached",10141,"South Atlantic","1980s","Stucco","heat pump","central AC",58.487434657651853,18415.439119999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18415.439119999999},"Hot-Humid",322.28692430321513,"Metropolitan Area",3.6301434365299999E-2,0.16000066441932972,0.38995826727649791,2.4988406558784235E-2,0.51338261007078334,1.0996429761319111,38.585999999999999,1318.3409999999999,{"$f":"T142*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1057813388431988E-4},{"$f":"U142*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4277828424899919E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.7012012499184316E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4142360957013978}]
["Single Family Detached",10142,"South Atlantic","Before 1950","Siding","central furnace","central AC",47.812757387338003,23906.378690000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23906.378690000001},"Cold/Very Cold",330.07176076030515,"Micropolitan Area",1.0224653455774337,0.49323815029772444,0.16545226970565699,6.6566618177322998E-2,0.69031499695982645,2.3714707625406417,2474.4490000000001,310.02199999999999,{"$f":"T143*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9155114843091813E-2},{"$f":"U143*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4115033342311799E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0816204604205255},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17286377303988817}]
["Single Family Detached",10143,"South Atlantic","Before 1950","Siding","built-in electric unit","window/wall unit",53.048380029974943,15380.80024,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15380.80024},"Mixed-Humid",196.56662707540733,"Metropolitan Area",0.31780464677978226,8.4377455132614812E-2,8.9282100093946229E-2,0,0.17922112954694319,0.67068533155328647,0,0,{"$f":"T144*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U144*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31780464677978226},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.9282100093946229E-2}]
["Multi-Family (2-4 units)",10144,"Middle Atlantic","1980s","Brick","radiator","window/wall unit",31.759318651541601,22116.517169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7372.1723899999997},"Cold/Very Cold",94.149305850568069,"Metropolitan Area",0.54749132309180815,0.47246940600824583,6.5956784281577974E-2,2.4511957144682699E-3,0.25282943356532311,1.3403810774232674,110.831,0,{"$f":"T145*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1706523815609008E-4},{"$f":"U145*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5483083883299642},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5956784281577974E-2}]
["Single Family Detached",10145,"Pacific","1970s","Wood","built-in electric unit","window/wall unit",12.751861375996162,8788.3262410000007,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8788.3262410000007},"Marine",224.35818248104954,"Metropolitan Area",0.23555025655681386,0.23173456743447521,1.2382751673569002E-2,0,0.28584255201171649,0.76551012767657456,0,0,{"$f":"T146*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U146*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23555025655681386},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2382751673569002E-2}]
["Single Family Detached",10146,"East North Central","1990s","Brick","central furnace","window/wall unit",41.003751112438522,24349.020850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24349.020850000001},"Cold/Very Cold",307.75299655084439,"Metropolitan Area",2.9063475588584708,0.75200039497088278,3.9660829564459953E-2,3.5887510501377153E-2,0.45324567647903347,4.1512544598728471,1473.8789999999999,0,{"$f":"T147*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5887510501377153E-2},{"$f":"U147*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9422350693598478},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9660829564459953E-2}]
["Single Family Detached",10147,"West South Central","2010s","Stone","heat pump","central AC",50.902504393542763,13926.81379,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13926.81379},"Hot-Humid",307.07390485874839,"Rural",0.27342902072011738,0.11288442980827935,0.37537882660799204,2.885053676471578E-2,0.4455281319609668,1.2072204090973555,384.84,1686.742,{"$f":"T148*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3595950189435993E-3},{"$f":"U148*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3490941745772178E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.278788615739061},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3988697683537642}]
["Single Family Detached",10148,"Mountain North","Before 1950","Wood","heater burning gas/oil/kerosene","window/wall unit",27.903369900467506,15441.82064,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15441.82064},"Cold/Very Cold",293.63069763954661,"Metropolitan Area",1.7012625483710806,0.22509872401889697,2.956941880897088E-2,0,0.33859372768251822,2.2945244188814669,0,0,{"$f":"T149*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U149*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7012625483710806},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.956941880897088E-2}]
["Single Family Detached",10149,"East South Central","2010s","Siding","central furnace","central AC",25.587089953049702,13661.01973,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13661.01973},"Mixed-Humid",296.50628576639872,"Metropolitan Area",0.4333025734915335,0.23487792855769066,0.14070153609893771,1.4349043327681721E-2,0.2027973870781988,1.0116794252263608,543.96400000000006,506.4,{"$f":"T150*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4311029364097208E-3},{"$f":"U150*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9179403912720001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4407336764279432},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14761947649020971}]
["Single Family Attached",10150,"West North Central","1970s","Brick","built-in electric unit","window/wall unit",7.2917996072411935,7564.1074760000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7564.1074760000001},null,45.656135803890315,"Metropolitan Area",3.6594357737603021E-2,4.2698085675534132E-2,2.6588669829962362E-3,0,7.3827428710479467E-2,0.15577873910661286,0,0,{"$f":"T151*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U151*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.6594357737603021E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6588669829962362E-3}]
["Multi-Family (2-4 units)",10151,"Pacific","1960s","Brick","built-in furnace","N/A",14.678145802898605,22721.587930000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7573.8626433333338},"Marine",28.379785921321709,"Metropolitan Area",0.32952541846545574,0.2461890641476,0,0,0.12160432536861705,0.69731880798167278,0,0,{"$f":"T152*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U152*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.32952541846545574},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10152,"West South Central","1970s","Siding","central furnace","central AC",45.703400407942951,20312.6224,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20312.6224},"Mixed-Humid",218.93452242084939,"Micropolitan Area",2.0494253197597647,0.4473829692822,0.18904267038518399,3.2129876421025598E-2,0.66919861371359401,3.3550495731407426,1086.4469999999999,495.322,{"$f":"T153*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2068587668612798E-2},{"$f":"U153*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.00612887524128E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0714939074283776},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19910395913759679}]
["Single Family Detached",10153,"South Atlantic","2000s","Concrete","heat pump","central AC",31.953079275815146,14952.306629999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14952.306629999999},"Hot-Humid",208.23749992976889,"Rural",9.1516355296553123E-2,0.12350186611794359,0.18510602733503531,1.1377748397805679E-2,0.31038211920538805,0.71050636795492006,109.062,651.87400000000002,{"$f":"T154*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.63072846568106E-3},{"$f":"U154*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7470199321246197E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.3147083762234184E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19485304726715993}]
["Single Family Detached",10154,"South Atlantic","1970s","Wood","central furnace","central AC",85.974969376817924,20031.44673,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20031.44673},"Mixed-Humid",200.93520179851538,"Metropolitan Area",1.1300858858265206,0.2865841793723452,0.30895213411182587,3.8086550862724736E-2,0.26828020454544688,1.9939024038561388,1169.1389999999999,732.19899999999996,{"$f":"T155*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3419545598465468E-2},{"$f":"U155*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4667005264259269E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.153505431424986},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32361913937608516}]
["Single Family Detached",10155,"South Atlantic","1990s","Brick","central furnace","central AC",87.976553352852619,26675.728729999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26675.728729999999},"Mixed-Humid",608.39225144930924,"Metropolitan Area",0.48488640169611996,0.3296115196326741,0.65776465049995025,5.6425728493217579E-2,1.4671508619865874,2.9394134338153313,813.61500000000001,1301.6310000000001,{"$f":"T156*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.170377303065895E-2},{"$f":"U156*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4721955462558629E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.50659017472677892},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.69248660596250888}]
["Single Family Detached",10156,"New England","1970s","Shingle","central furnace","N/A",16.363357391731892,15902.19377,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15902.19377},"Cold/Very Cold",144.81105357405195,"Metropolitan Area",1.1472711322523659,0.28654962834509629,0,1.8063254196761691E-2,0.47603205918959357,1.9098528197870555,1135.8969999999999,0,{"$f":"T157*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8063254196761691E-2},{"$f":"U157*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1653343864491275},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10157,"East North Central","1960s","Siding","central furnace","window/wall unit",44.110675200366103,26831.310949999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26831.310949999999},"Cold/Very Cold",232.54359125091105,"Metropolitan Area",1.140831441299949,0.59170709033419511,0.11645183372570965,9.6513835365807002E-2,0.5804731155838504,2.4294634809437041,3597.06,0,{"$f":"T158*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6513835365807002E-2},{"$f":"U158*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.237345276665756},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11645183372570965}]
["Single Family Detached",10158,"South Atlantic","1990s","Siding","central furnace","central AC",69.544396173653695,27144.573059999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27144.573059999999},"Mixed-Humid",386.66806423130208,"Metropolitan Area",1.0559690063144258,0.71568433984396207,0.20044402372640777,3.022382628335334E-2,1.0995849605963792,3.0716823304811749,710.36,403.07900000000001,{"$f":"T159*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.92824189189016E-2},{"$f":"U159*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.094140736445174E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0752514252333274},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2113854310908595}]
["Multi-Family (5+ units)",10159,"West North Central","1970s","Wood","central furnace","central AC",16.497368010742203,17042.735550000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1355.6035987316095},"Cold/Very Cold",38.289879870866201,"Metropolitan Area",0.35142692140300474,0.17710717048514477,1.7677338377165664E-2,5.0266525940592006E-3,0.10800404177876627,0.65884229749031642,248.47800000000001,46.466000000000001,{"$f":"T160*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3683767100563288E-4},{"$f":"U160*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2989476818662966E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35176375907401036},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7740327853984328E-2}]
["Multi-Family (5+ units)",10160,"Middle Atlantic","Before 1950","Brick","central furnace","window/wall unit",12.877578332973767,34710.453730000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2760.9192111177845},"Cold/Very Cold",240.12691888817395,"Metropolitan Area",0.45446092708389046,0.65524738862851084,1.8642880567021809E-2,6.9944688206785696E-3,0.99860795225783205,2.1333972672886206,201.50899999999999,0,{"$f":"T161*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5635006931313363E-4},{"$f":"U161*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45501727715320361},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8642880567021809E-2}]
["Single Family Detached",10161,"South Atlantic","1960s","Siding","central furnace","central AC",95.192216029816905,48198.590389999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":48198.590389999998},"Mixed-Humid",688.41665892091578,"Metropolitan Area",2.0091376114104631,0.94055553482941656,0.39327032526481587,8.8595178556389931E-2,0.94397898430763816,4.2869424558123335,1474.5820000000001,363.54599999999999,{"$f":"T162*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1072773814466986E-2},{"$f":"U162*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7522404741922938E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0802103852249303},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.41079273000673883}]
["Single Family Detached",10162,"West South Central","2000s","Brick","central furnace","both central and individual units",32.512261631508622,11058.59239,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11058.59239},"Hot-Humid",257.27945690609539,"Rural",0.23267802565839288,8.6925291380127695E-2,0.13371903944568453,9.2418536563936299E-3,0.42451513247617351,0.87783748896037861,325.27199999999999,510.44499999999999,{"$f":"T163*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5970504638800798E-3},{"$f":"U163*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6448031925135497E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23627507612227297},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13936384263819807}]
["Mobile Home",10163,"Middle Atlantic","1960s","Siding","central furnace","window/wall unit",79.290843784569461,42906.300750000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":42906.300750000002},"Cold/Very Cold",408.59670203487826,"Micropolitan Area",2.4063218310026859,0.52150433212176983,9.1868782944561744E-2,4.1080122777478502E-2,0.73961537982443948,3.7593103258934573,957.43799999999999,0,{"$f":"T164*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1080122777478502E-2},{"$f":"U164*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4474019537801643},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.1868782944561744E-2}]
["Single Family Attached",10164,"South Atlantic","2000s","Siding","heat pump","central AC",51.164766258579633,9900.3030689999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9900.3030689999996},"Hot-Humid",148.39564269540443,"Metropolitan Area",7.5095848141100277E-2,8.404895951457983E-2,0.17654057077640162,1.2245120548771167E-2,0.1706458214257853,0.50633119985786701,148.24799999999999,1088.595,{"$f":"T165*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4677001293731118E-3},{"$f":"U165*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0777420419398054E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.6563548270473389E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18731799119579967}]
["Single Family Detached",10165,"Pacific","Before 1950","Wood","built-in electric unit","window/wall unit",26.872645961377021,38389.494229999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38389.494229999997},"Marine",529.22866109954361,"Metropolitan Area",0.82692778716598236,0.24601508126555505,1.5159243481542399E-2,0,0.71762610215269351,1.8057282140657733,0,0,{"$f":"T166*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U166*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.82692778716598236},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5159243481542399E-2}]
["Single Family Detached",10166,"West South Central","2010s","Concrete","heat pump","central AC",37.833676135243593,12939.013730000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12939.013730000001},"Mixed-Humid",306.42172306253036,"Micropolitan Area",0.28802622382180915,0.13225326931916068,0.21502042665303017,1.9798230749533872E-2,0.41021099960697022,1.0455109194009704,597.80799999999999,932.31100000000004,{"$f":"T167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.73504591990384E-3},{"$f":"U167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2063184829630031E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29576126974171296},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22708361148266021}]
["Multi-Family (2-4 units)",10167,"West South Central","1980s","Wood","portable electric heaters","window/wall unit",21.03938439272731,26168.38855,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8722.7961833333338},"Hot-Humid",582.40844434313794,"Metropolitan Area",0.1731626121221562,0.69299356839929238,0.18223281110908315,0,0.93878866258144589,1.9871776542119777,0,0,{"$f":"T168*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U168*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1731626121221562},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18223281110908315}]
["Single Family Detached",10168,"East North Central","1990s","Siding","central furnace","central AC",46.603528656481323,22744.523499999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22744.523499999999},"Cold/Very Cold",256.75915022804332,"Metropolitan Area",0.16151991521192099,0.275732085835735,7.7633336193985991E-2,4.0477382224868998E-2,0.76131733654706601,1.276202673788708,1631.671,147.983,{"$f":"T169*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7111579403768503E-2},{"$f":"U169*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3658028211004999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19863149461568949},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.0999139015086485E-2}]
["Single Family Attached",10169,"West North Central","1990s","Brick","heat pump","central AC",11.627561055242381,7094.3020470000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7094.3020470000001},"Mixed-Humid",64.535368824989206,"Micropolitan Area",0.10130515052203219,3.9959848122471393E-2,3.4265606584446849E-2,3.3888132961130074E-3,4.4664065621232985E-2,0.22019467085018343,249.976,227.70500000000001,{"$f":"T170*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.773405248500872E-3},{"$f":"U170*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.615408047612135E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10307855577053307},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5881014632058984E-2}]
["Single Family Detached",10170,"West South Central","1990s","Wood","central furnace","window/wall unit",8.3109548967586342,10273.121010000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10273.121010000001},"Hot-Humid",146.64880241190298,"Metropolitan Area",0.1493648204234948,0.19631770907485943,9.5429311967875241E-2,2.9174225431458601E-3,0.41645247807560881,0.85756431954183832,283.98599999999999,0,{"$f":"T171*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9174225431458601E-3},{"$f":"U171*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15228224296664067},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.5429311967875241E-2}]
["Single Family Detached",10171,"West North Central","1990s","Siding","central furnace","central AC",17.247644726862912,14843.06775,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14843.06775},"Mixed-Humid",141.90643676783645,"Metropolitan Area",0.54044372611432345,0.40424686832761869,0.10240410557538002,1.6381091587187254E-2,0.32747332685090613,1.3745680268682285,803.84900000000005,299.77,{"$f":"T172*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1931585167769751E-2},{"$f":"U172*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4495064194174996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55237531128209316},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10685361199479751}]
["Single Family Detached",10172,"West South Central","1990s","Brick","central furnace","central AC",36.477914305006131,23640.903630000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23640.903630000001},"Hot-Humid",322.39750408541965,"Micropolitan Area",0.95220893107263449,0.21327135294466817,0.40597696372171949,2.9447866070444164E-2,0.68386280703627633,2.2553200547752987,430.63400000000001,814.99800000000005,{"$f":"T173*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.018057689380142E-2},{"$f":"U173*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9267289176642742E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.96238950796643596},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.42524425289836221}]
["Single Family Detached",10173,"West South Central","Before 1950","Wood","portable electric heaters","N/A",32.824317451032798,20362.479810000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20362.479810000001},"Hot-Humid",156.3660073956853,"Metropolitan Area",0.45340895551913224,0.53089440175252423,0,0,0.13903122472143531,1.1233345819930918,0,0,{"$f":"T174*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U174*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45340895551913224},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10174,"Pacific","1980s","Concrete","N/A","N/A",17.888583624916638,30789.30056,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2449.0250710699524},"Hot-Humid",67.930033562937098,"Metropolitan Area",0,5.7556748734349995E-2,0,0,0.23482103568465706,0.29237778441900708,0,0,{"$f":"T175*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U175*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10175,"New England","Before 1950","Wood","radiator","both central and individual units",43.903857084405544,14595.697169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14595.697169999999},"Cold/Very Cold",89.466909235893525,"Metropolitan Area",1.0762021272506999,0.22223666854881907,9.7116791446957312E-2,7.7719752118702778E-3,0.22140944281601213,1.6169650300624883,259.98399999999998,272.5,{"$f":"T176*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7946477330452794E-3},{"$f":"U176*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9773274788249997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0799967749837451},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10109411892578231}]
["Single Family Detached",10176,"West South Central","1990s","Brick","heat pump","central AC",42.397530488344827,20403.046429999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20403.046429999999},"Hot-Humid",301.11982980482787,"Metropolitan Area",0.1769431146199284,0.17767258473894018,0.32399941836521773,1.9869200720159051E-2,0.34880570745441541,1.0274208251785018,152.38900000000001,821.44600000000003,{"$f":"T177*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1091998424212699E-3},{"$f":"U177*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6760000877737779E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18005231446234968},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3407594192429555}]
["Single Family Detached",10177,"East South Central","1950s","Brick","central furnace","both central and individual units",14.697688313902241,10101.504000000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10101.504000000001},"Hot-Humid",138.86481984766795,"Metropolitan Area",0.32037174493900805,0.11759668912051201,0.27276619510963207,1.3285689989376001E-2,0.267293008313856,0.97802763748300803,229.99700000000001,1085.222,{"$f":"T178*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3233156154880003E-3},{"$f":"U178*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0962374373888001E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.32269506055449604},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2837285694835201}]
["Single Family Detached",10178,"Middle Atlantic","Before 1950","Brick","central furnace","central AC",37.83280451682171,33539.72032,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33539.72032},"Cold/Very Cold",156.14265864526615,"Metropolitan Area",1.8535329324559413,0.80213182578752062,0.12314185456844737,3.11765116262528E-2,0.4578636013409233,3.2366702141528321,767.95600000000002,161.584,{"$f":"T179*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5757029458065919E-2},{"$f":"U179*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.41948216818688E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8792899619140073},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12856133673663425}]
["Multi-Family (5+ units)",10179,"Pacific","1980s","Stucco","built-in furnace","N/A",6.1910005559274808,8423.1300080000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":669.98782665667841},"Marine",24.719359634667182,"Metropolitan Area",4.2065835649132688E-2,7.6516622690712868E-2,0,0,8.3225628895824813E-2,0.2018080872356704,0,0,{"$f":"T180*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U180*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.2065835649132688E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10180,"West South Central","2000s","Brick","central furnace","central AC",16.925028133452081,15057.85421,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15057.85421},"Hot-Humid",298.82311682238128,"Rural",0.28815959618155423,0.12711296935545016,0.10341005471284236,9.3715416668234894E-3,0.50089974616346322,1.0195823664133099,311.32100000000003,311.048,{"$f":"T181*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6878262305114103E-3},{"$f":"U181*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6837154363120791E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29284742241206563},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10809377014915443}]
["Single Family Detached",10181,"Mountain South","1980s","Stucco","central furnace","N/A",19.10672637852355,9728.4757530000006,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9728.4757530000006},"Cold/Very Cold",23.830047283650263,"Metropolitan Area",0.13273949669003005,5.0776757702829446E-2,2.3150863477889853E-2,2.0503930066537862E-3,5.1844467645196915E-2,0.25851158551594627,210.762,0,{"$f":"T182*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0503930066537862E-3},{"$f":"U182*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13478988969668382},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3150863477889853E-2}]
["Single Family Detached",10182,"East South Central","1960s","Siding","portable electric heaters","window/wall unit",56.444308379963601,17250.7055,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17250.7055},"Mixed-Humid",133.08651903533629,"Micropolitan Area",0.11856282234929301,0.120157443064302,6.7864792958164999E-2,0,0.475594222318936,0.78217928069069598,0,0,{"$f":"T183*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U183*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11856282234929301},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7864792958164999E-2}]
["Single Family Detached",10183,"West South Central","1950s","Siding","built-in electric unit","central AC",88.420840327386514,46269.408860000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":46269.408860000003},"Hot-Humid",1425.185889776812,"Metropolitan Area",1.7663417624500557,0.74164194399994643,1.1994392485214751,6.090821697394453E-2,1.1553113729811506,4.8627343279526283,0,1316.3820000000001,{"$f":"T184*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U184*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.090821697394453E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7663417624500557},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2603474654954196}]
["Single Family Attached",10184,"New England","1980s","Shingle","heater burning gas/oil/kerosene","window/wall unit",22.535053159628827,7862.8936359999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7862.8936359999998},"Cold/Very Cold",98.362008054111982,"Metropolitan Area",0.41943961343963848,5.890516646405216E-2,8.8065745415118121E-3,0,0.31029518002300416,0.79744653446820668,0,0,{"$f":"T185*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U185*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.41943961343963848},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.8065745415118121E-3}]
["Multi-Family (5+ units)",10185,"West South Central","2000s","Brick","fireplace","central AC",43.404768924598116,41655.248489999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3313.3181344883005},"Hot-Humid",232.26966556963444,"Micropolitan Area",0.12005259222110148,0.17405287346409484,0.12669673786511321,5.8785552879027595E-3,0.36627793239244916,0.79249110252224997,0,141.124,{"$f":"T186*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U186*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6758870841152693E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12005259222110148},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12716432657352472}]
["Single Family Detached",10186,"West South Central","1970s","Brick","central furnace","window/wall unit",13.972353986666484,14707.741040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14707.741040000001},"Hot-Humid",145.1301201801939,"Metropolitan Area",0.24201595235190521,6.8076809071903527E-2,9.1894010141143109E-2,3.9563088010548001E-3,9.3197218951474425E-2,0.49518399051642625,268.995,0,{"$f":"T187*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9563088010548001E-3},{"$f":"U187*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24597226115296},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.1894010141143109E-2}]
["Single Family Detached",10187,"East North Central","1970s","Siding","central furnace","central AC",35.614525450490682,20053.22379,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20053.22379},"Cold/Very Cold",166.53881505757491,"Metropolitan Area",9.1561916897831552E-2,0.17013578186457967,2.6932742903068768E-2,3.2234755113473394E-3,0.27960001376869581,0.56823045543417583,96.07,64.676000000000002,{"$f":"T188*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9265132095052998E-3},{"$f":"U188*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2969623018420401E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.3488430107336845E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8229705204910808E-2}]
["Single Family Detached",10188,"West South Central","1960s","Brick","central furnace","N/A",49.962337732630964,19216.283739999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19216.283739999999},"Hot-Humid",189.26117858795473,"Metropolitan Area",0.34596801239401848,0.20208770205860266,0,8.3818739394156388E-3,0.68167810349965263,1.2297338179522739,436.18599999999998,0,{"$f":"T189*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3818739394156388E-3},{"$f":"U189*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35434988633343412},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10189,"East North Central","2000s","Siding","central furnace","central AC",54.036311907877277,15991.805829999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15991.805829999999},"Cold/Very Cold",95.520783352304534,"Metropolitan Area",0.94689733965690859,0.4654195039573279,3.1898551244790227E-2,1.4752057074835078E-2,0.37471945048716188,1.8189348453461887,804.24800000000005,118.22799999999999,{"$f":"T190*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2861377855165841E-2},{"$f":"U190*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8906792196692398E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95975871751207442},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3789230464459467E-2}]
["Single Family Attached",10190,"Pacific","1960s","Wood","built-in electric unit","N/A",6.4544538894716164,8037.9251430000004,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8037.9251430000004},"Marine",92.906349722296127,"Metropolitan Area",0.14208869356147677,9.5103556754905116E-2,0,0,7.9804218265269816E-2,0.3169964685816517,0,0,{"$f":"T191*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U191*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14208869356147677},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10191,"South Atlantic","1980s","Stucco","heat pump","central AC",40.746928376694825,24399.35831,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24399.35831},"Hot-Humid",406.65058769823474,"Metropolitan Area",1.5632668869216999E-2,0.17049969034984955,0.29930253650427419,1.273922216530903E-2,1.3043510954677535,1.7897859911910941,15.263,506.85,{"$f":"T192*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7240740588552999E-4},{"$f":"U192*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.23668147594235E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6005076275102531E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31166935126369766}]
["Single Family Detached",10192,"West North Central","1970s","Siding","central furnace","central AC",101.11670557014811,15244.49051,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15244.49051},"Mixed-Humid",239.7512456286201,"Metropolitan Area",1.2318334490455602,0.15077810299661762,0.23435960467296246,6.6584687471201373E-2,0.41808675310114096,2.0350579098162811,3264.491,1103.296,{"$f":"T193*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9765502069480411E-2},{"$f":"U193*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6819185401720959E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2815989511150407},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25117879007468341}]
["Single Family Detached",10193,"East North Central","2000s","Siding","heat pump","central AC",39.129539288817718,18985.705620000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18985.705620000001},"Cold/Very Cold",494.04447489150562,"Metropolitan Area",0.62984816391612441,0.24037591144149617,8.2288111098082692E-2,1.5618097099946878E-2,0.73316753852911709,1.6856797249848203,610.60799999999995,212.01599999999999,{"$f":"T194*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1592823737216958E-2},{"$f":"U194*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0252733627299201E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.64144098765334134},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.6313384460812617E-2}]
["Multi-Family (2-4 units)",10194,"East North Central","1970s","Siding","central furnace","central AC",65.828444111292328,47805.696519999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15935.232173333332},"Cold/Very Cold",174.97157419654633,"Metropolitan Area",2.4116615575149547,0.46929528055890396,0.17172655537858839,4.8471868901006195E-2,0.4012832156509199,3.4862811883707043,849.55399999999997,164.381,{"$f":"T195*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3537840233784026E-2},{"$f":"U195*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6194493998847063E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4251993977487389},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17434600477847309}]
["Multi-Family (5+ units)",10195,"Pacific","1950s","Stucco","portable electric heaters","N/A",13.29520895209928,17609.548279999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1400.6886952139571},"Cold/Very Cold",116.59776745107931,"Metropolitan Area",0.10439366371452376,0.14588577443921158,0,0,0.14755213077385146,0.39783156892758681,0,0,{"$f":"T196*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U196*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10439366371452376},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10196,"Pacific","1990s","Wood","N/A","N/A",16.911008684272076,13976.040230000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13976.040230000001},"Hot-Dry/Mixed-Dry",117.03281728802796,"Metropolitan Area",0,0.33967844757963844,0.12285687080322306,0,0.44728576739106368,0.90982108577392518,0,0,{"$f":"T197*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U197*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12285687080322306}]
["Single Family Detached",10197,"West North Central","2000s","Stucco","central furnace","central AC",84.047969275662311,19527.873899999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19527.873899999999},"Cold/Very Cold",585.62084414886806,"Metropolitan Area",2.4780043801967899,0.653063051439005,4.9039646721609598E-2,5.8053986704084203E-2,1.9144633516350327,5.0945704299924373,2829.8560000000002,143.02199999999999,{"$f":"T198*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5261071123158402E-2},{"$f":"U198*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7929155809257996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5332654513199482},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.1832562302535398E-2}]
["Single Family Detached",10198,"South Atlantic","1980s","Concrete","central furnace","central AC",37.687264566696314,18330.381600000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18330.381600000001},"Hot-Humid",437.05891389387159,"Metropolitan Area",2.7325778075239199E-2,0.15945862911335043,0.90910513719730068,4.5964201738027198E-2,0.39535548107976748,1.4912450254656577,26.399000000000001,2481.143,{"$f":"T199*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8390374385840005E-4},{"$f":"U199*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5480297994168806E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.7809681819097598E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.95458543519146954}]
["Multi-Family (5+ units)",10199,"West North Central","1970s","Brick","radiator","N/A",6.601165159179688,11980.33604,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":952.93309000725526},"Cold/Very Cold",32.095320256701243,"Metropolitan Area",0.16128750196219768,0.12993710734447461,0,1.3654947411671199E-3,0.10815873733651286,0.40064022797661941,113.97799999999999,0,{"$f":"T200*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0861340773284693E-4},{"$f":"U200*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16139611536993054},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10200,"West South Central","1990s","Stone","heat pump","central AC",18.235049988982308,9497.4218689999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9497.4218689999998},"Hot-Humid",237.17798614786801,"Metropolitan Area",0.11694771985393074,0.13604486032288174,0.21508146487193469,1.2754220791786267E-2,0.38148220341321726,0.84955624846196431,178.99,1163.924,{"$f":"T201*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6999435403323101E-3},{"$f":"U201*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1054277251453954E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11864766339426305},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22613574212338863}]
["Single Family Detached",10201,"Pacific","2000s","Stucco","central furnace","central AC",51.828168036905282,28793.42669,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28793.42669},"Hot-Dry/Mixed-Dry",324.26523679703291,"Metropolitan Area",1.0809222548577739,0.46067968169756107,0.13268563852544452,1.7008133178649552E-2,0.58631323415809056,2.2606008092388703,362.79500000000002,227.9,{"$f":"T202*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.044611123599855E-2},{"$f":"U202*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5620219426510001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0913683660937725},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1392476604680955}]
["Single Family Detached",10202,"Mountain North","2000s","Stucco","central furnace","central AC",33.157161991305124,8932.4251050000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8932.4251050000003},"Cold/Very Cold",68.878224757893193,"Metropolitan Area",0.52652592459462344,0.41968221341615858,5.5706926248530825E-2,1.225678789147764E-2,0.16988049614390779,1.1717955604032206,1055.154,317.01400000000001,{"$f":"T203*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4250840792411694E-3},{"$f":"U203*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.83170381223647E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53595100867386458},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8538630060767295E-2}]
["Single Family Detached",10203,"South Atlantic","1960s","Brick","central furnace","central AC",63.130808455515648,21213.309290000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21213.309290000001},"Mixed-Humid",118.42204754207567,"Metropolitan Area",1.4243999601470987,0.32200617678230692,2.7165085050876725E-2,1.097614806621322E-2,0.47331602380652382,2.2468872457868061,412.077,105.34099999999999,{"$f":"T204*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7415168522953293E-3},{"$f":"U204*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2346312139178903E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.433141476999394},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.9399716264794616E-2}]
["Single Family Detached",10204,"Pacific","1960s","Siding","central furnace","central AC",20.969070553360382,16668.577550000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16668.577550000002},"Hot-Dry/Mixed-Dry",177.53701944661481,"Metropolitan Area",0.20278133015586175,0.31970891805105678,9.7447938084275307E-2,7.9346596282387511E-3,0.20138061957860268,0.82131880586979655,210.87200000000001,265.15300000000002,{"$f":"T205*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5149362851236007E-3},{"$f":"U205*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4197233431151513E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20629626644098534},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10186766142739045}]
["Single Family Detached",10205,"West North Central","2000s","Siding","heater burning gas/oil/kerosene","central AC",101.92929671305821,14499.18872,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14499.18872},"Cold/Very Cold",290.39560938904714,"Metropolitan Area",1.0222942120859078,0.3917719939953544,0.1960334537469596,1.4911009177214161E-2,0.84560093618878174,2.4557005960170035,0,1028.403,{"$f":"T206*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U206*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4911009177214161E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0222942120859078},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21094446292417376}]
["Multi-Family (5+ units)",10206,"Pacific","2010s","Siding","built-in electric unit","central AC",9.7938451341434867,17032.774150000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1354.8112547062747},"Marine",114.34101284435691,"Metropolitan Area",5.8120356117723905E-2,0.14417548380789683,6.2744658945856112E-3,2.6296900010185E-4,0.18132333401640321,0.39013569190575004,0,15.439,{"$f":"T207*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U207*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0916930961410173E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.8120356117723905E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2953828255470218E-3}]
["Single Family Detached",10207,"Middle Atlantic","Before 1950","Siding","central furnace","window/wall unit",71.564691037360973,43163.263590000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":43163.263590000002},"Cold/Very Cold",398.5457498971885,"Metropolitan Area",1.7351663903995058,1.2869220272007857,3.4948949222714285E-2,3.0918967954370342E-2,1.1467582634878235,4.2037956303108288,716.32600000000002,0,{"$f":"T208*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0918967954370342E-2},{"$f":"U208*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7660853583538763},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4948949222714285E-2}]
["Mobile Home",10208,"Pacific","1970s","Siding","heat pump","central AC",17.508859357075281,11587.59719,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11587.59719},"Marine",218.19942620409779,"Rural",0.12732423982138744,0.42206548128884103,1.6769107149480402E-3,1.7910717224639203E-3,0.19342982476393927,0.7444964565891159,149.09100000000001,5.4770000000000003,{"$f":"T209*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7276064526542902E-3},{"$f":"U209*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3465269809630004E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12905184627404173},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7403759847576701E-3}]
["Single Family Detached",10209,"West North Central","1990s","Siding","central furnace","central AC",185.60657932846732,24557.631560000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24557.631560000002},"Mixed-Humid",245.7603259306141,"Metropolitan Area",1.7407150124532724,0.51504568413472329,0.25528989030250554,7.6617403819307137E-2,0.54724169685751389,3.0582922837480155,2386.8690000000001,733.03300000000002,{"$f":"T210*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8615849483985648E-2},{"$f":"U210*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8001554335321482E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7993308619372581},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27329144463782701}]
["Single Family Detached",10210,"Pacific","1970s","Stucco","central furnace","central AC",19.810286042400648,11085.778420000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11085.778420000001},"Hot-Dry/Mixed-Dry",103.98532218596017,"Metropolitan Area",0.12702709042961047,0.23232797299568758,9.8372980543396008E-2,8.0838161385345213E-3,0.30233943060270824,0.76006747457140234,290.52300000000002,438.68299999999999,{"$f":"T211*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2206736039136607E-3},{"$f":"U211*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8631425346208606E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13024776403352412},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10323612307801687}]
["Single Family Detached",10211,"East South Central","1970s","Siding","built-in electric unit","window/wall unit",31.13547947107444,12865.900610000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12865.900610000001},"Mixed-Humid",186.73170585951152,"Micropolitan Area",0.25943163521811141,0.1569380111886684,3.3864761570301133E-2,0,0.18689416361725408,0.637128571594335,0,0,{"$f":"T212*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U212*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25943163521811141},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3864761570301133E-2}]
["Single Family Detached",10212,"New England","Before 1950","Wood","radiator","window/wall unit",24.584123281997694,11256.466700000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11256.466700000001},"Cold/Very Cold",64.454528348314469,"Metropolitan Area",1.0156565370377573,0.2528457379790755,2.3725682609324599E-2,1.3658258999779001E-3,0.19179383692188479,1.4840217945480423,121.337,0,{"$f":"T213*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3658258999779001E-3},{"$f":"U213*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0170223629377351},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3725682609324599E-2}]
["Mobile Home",10213,"New England","1960s","Siding","central furnace","N/A",5.6700960174033952,5400.091445,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5400.091445},"Cold/Very Cold",20.83191116757429,"Micropolitan Area",0.21798930382487516,2.3368863327688828E-2,0,1.639937570657715E-3,8.4645617986566876E-2,0.32600378513913081,303.68700000000001,0,{"$f":"T214*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.639937570657715E-3},{"$f":"U214*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21962924139553289},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10214,"Pacific","Before 1950","Siding","built-in electric unit","window/wall unit",45.120869478267338,26510.499110000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26510.499110000001},"Marine",404.14791953233072,"Metropolitan Area",0.30479778287144932,0.47322237706116538,2.7482533070367257E-2,0,0.57345001130486295,1.3789527043078449,0,0,{"$f":"T215*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U215*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30479778287144932},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7482533070367257E-2}]
["Single Family Detached",10215,"Pacific","Before 1950","Stucco","heater burning gas/oil/kerosene","window/wall unit",15.690300456804193,14461.10641,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14461.10641},"Hot-Dry/Mixed-Dry",117.40652705289612,"Metropolitan Area",4.3253371727799743E-2,0.15998348051374539,0.20227508743753522,0,0.24390690638136889,0.6494188460604492,0,0,{"$f":"T216*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U216*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.3253371727799743E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20227508743753522}]
["Single Family Detached",10216,"Mountain North","1990s","Wood","central furnace","N/A",67.106134636273922,47059.00045,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":47059.00045},"Cold/Very Cold",223.92107711813142,"Rural",2.9367900527689494,1.0867740151912375,0,2.3392370297688699E-2,0.740626313832212,4.7641903817923987,497.08600000000001,0,{"$f":"T217*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3392370297688699E-2},{"$f":"U217*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9601824230666383},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10217,"New England","1980s","Siding","central furnace","window/wall unit",46.259005001536622,12097.020140000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12097.020140000001},"Cold/Very Cold",188.02477028614246,"Metropolitan Area",1.6530623385135526,0.23073692905264112,3.8980796557068584E-2,1.9231104700343459E-2,0.7257960586951292,2.6485761228183913,1589.739,0,{"$f":"T218*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9231104700343459E-2},{"$f":"U218*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6722934432138961},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8980796557068584E-2}]
["Single Family Detached",10218,"South Atlantic","1960s","Brick","central furnace","central AC",21.858973149545143,14759.60375,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14759.60375},"Mixed-Humid",186.38151607324585,"Metropolitan Area",0.89154878721506015,0.2713564809524463,0.25268816513935255,2.5034546179373753E-2,0.45682297542706368,1.8724164087339226,971.69,724.46299999999997,{"$f":"T219*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4341759367837501E-2},{"$f":"U219*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0692786811536249E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.90589054658289769},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26338095195088879}]
["Single Family Detached",10219,"South Atlantic","1980s","Shingle","central furnace","central AC",123.52188317345588,32167.157080000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32167.157080000001},"Mixed-Humid",415.37778037784364,"Metropolitan Area",1.0665761417829982,0.58926169058620803,0.4770085093658023,5.1998305921291239E-2,0.91212772443005941,3.0449740661650679,874.57899999999995,741.92399999999998,{"$f":"T220*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8132720071869316E-2},{"$f":"U220*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.386558584942192E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0947088618548675},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.50087409521522419}]
["Single Family Detached",10220,"East North Central","1950s","Shingle","central furnace","N/A",65.000524163828672,29438.643189999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29438.643189999999},"Cold/Very Cold",117.64841701321554,"Metropolitan Area",2.519502479831178,0.49950438805230118,0,5.7653404228018935E-2,0.43433859534591296,3.4533454632293918,1958.4259999999999,0,{"$f":"T221*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7653404228018935E-2},{"$f":"U221*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5771558840591968},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10221,"Pacific","Before 1950","Siding","portable electric heaters","window/wall unit",191.78206573915472,54359.99596,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":54359.99596},"Cold/Very Cold",1215.0090759723632,"Metropolitan Area",2.4662945886665697,0.61038001871694891,0.11628021707812894,0,0.95265615683920579,4.1456109813008535,0,0,{"$f":"T222*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U222*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4662945886665697},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11628021707812894}]
["Single Family Detached",10222,"West North Central","1970s","Siding","central furnace","central AC",54.031554417932476,23451.195489999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23451.195489999998},"Mixed-Humid",149.27626324803026,"Metropolitan Area",0.93785833394044082,0.5543991595411194,0.27383142526950399,4.7893063282279554E-2,0.24461693432946802,2.0107058530805322,1547.35,494.89400000000001,{"$f":"T223*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6287207341451494E-2},{"$f":"U223*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.160585594082806E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.97414554128189235},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28543728121033207}]
["Single Family Detached",10223,"Pacific","1970s","Wood","wood-burning stove","N/A",10.968944562148915,11079.741980000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11079.741980000001},"Hot-Dry/Mixed-Dry",134.7367202963807,"Metropolitan Area",1.903794393300668E-2,0.16085143944471969,6.0945206575704049E-2,0,0.21888709469673379,0.45972168465016416,0,0,{"$f":"T224*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U224*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.903794393300668E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0945206575704049E-2}]
["Single Family Detached",10224,"New England","Before 1950","Siding","central furnace","central AC",67.303286633375606,18264.121200000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18264.121200000001},"Cold/Very Cold",73.642142122846181,"Metropolitan Area",1.364020441162751,0.18847416959528041,6.5396695009932004E-2,3.0824357349240005E-2,0.31569929825630022,1.9335906040242636,1501.585,186.11500000000001,{"$f":"T225*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7425130432102002E-2},{"$f":"U225*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3992269171380005E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.391445571594853},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.879592192707E-2}]
["Single Family Detached",10225,"Mountain North","Before 1950","Brick","central furnace","central AC",31.323146949217026,17797.242579999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17797.242579999998},"Cold/Very Cold",235.48565683719772,"Metropolitan Area",0.40998411421403064,0.37369171018625597,6.7919634655296574E-2,1.6277749603004758E-2,0.80682190365700746,1.6584173627125907,742.48199999999997,172.14,{"$f":"T226*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3214132265283559E-2},{"$f":"U226*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0636173377211993E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4231982464793142},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0983251993017776E-2}]
["Single Family Detached",10226,"West South Central","1990s","Brick","heat pump","central AC",19.266557026781733,14831.837589999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14831.837589999999},"Mixed-Humid",317.81841048751289,"Rural",0.29667254102410462,0.47856025989667933,0.11488001288518258,1.004010098796111E-2,0.21283578669235598,1.1029486004983224,327.70699999999999,349.22199999999998,{"$f":"T227*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.86049700110613E-3},{"$f":"U227*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1796039868549802E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30153303802521075},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12005961687203756}]
["Single Family Detached",10227,"New England","1980s","Wood","central furnace","window/wall unit",14.073658301970259,14360.875819999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14360.875819999999},"Cold/Very Cold",109.17272789332479,"Rural",0.28991866789385956,0.17769929454355535,9.3442485133026793E-3,1.0104010648559779E-2,0.22376206223197007,0.70072427318268771,703.57899999999995,0,{"$f":"T228*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0104010648559779E-2},{"$f":"U228*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30002267854241932},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.3442485133026793E-3}]
["Multi-Family (5+ units)",10228,"Pacific","1970s","Concrete","N/A","N/A",12.793426479978827,15697.4558,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1248.5981203534179},"Hot-Dry/Mixed-Dry",49.185780116940428,"Metropolitan Area",0,0.20104314018670177,0,0,0.17819185146005617,0.37923499164675795,0,0,{"$f":"T229*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U229*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",10229,"South Atlantic","1970s","Wood","heat pump","central AC",24.855743766442945,18050.649069999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6016.8830233333329},"Mixed-Humid",153.23195993706182,"Micropolitan Area",9.9514401615099543E-2,0.15654410965438242,8.4051283004868929E-2,5.7400703029618595E-3,0.17890054250289111,0.52283705031255001,94.908000000000001,223.09,{"$f":"T230*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7105033397852E-4},{"$f":"U230*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3423064336754334E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10008545194907806},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5393589438544359E-2}]
["Single Family Detached",10230,"East North Central","1960s","Siding","central furnace","central AC",22.087302265231479,14531.119909999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14531.119909999999},"Cold/Very Cold",74.422961547018716,"Metropolitan Area",1.2620015355120622,0.14473390676821554,7.4965945897850633E-2,3.5401353694018041E-2,0.17522938000717855,1.6569307681853072,2215.5740000000001,220.67,{"$f":"T231*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2194771463478336E-2},{"$f":"U231*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2065822305396997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2941963069755404},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.8172528128390331E-2}]
["Single Family Detached",10231,"West South Central","Before 1950","Siding","portable electric heaters","window/wall unit",15.041397782652876,12033.11823,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12033.11823},"Hot-Humid",165.32301130869428,"Rural",0.2460322639413198,9.3279035849289579E-2,0.11667488322645982,0,0.10810233336887079,0.56408851638593993,0,0,{"$f":"T232*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U232*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2460322639413198},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11667488322645982}]
["Single Family Detached",10232,"Middle Atlantic","1970s","Siding","built-in electric unit","window/wall unit",45.044961300299654,21287.78889,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21287.78889},"Cold/Very Cold",447.44803476890286,"Metropolitan Area",0.55863000493254644,0.30290086138642097,3.1982326984769306E-2,0,0.63316187473150309,1.5266750680352399,0,0,{"$f":"T233*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U233*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55863000493254644},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.1982326984769306E-2}]
["Single Family Detached",10233,"West North Central","1950s","Brick","central furnace","central AC",72.130799973892536,13694.85475,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13694.85475},"Mixed-Humid",146.08044099698435,"Metropolitan Area",1.6422251767405132,0.21054121843339352,0.155488751419388,3.9897507935124747E-2,0.31484101309171775,2.3230961596850124,2051.627,861.69399999999996,{"$f":"T234*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8096733766178252E-2},{"$f":"U234*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1800774168946499E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6703219105066913},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16728952558833451}]
["Single Family Attached",10234,"Pacific","1950s","Wood","central furnace","central AC",22.841846903535419,19050.748039999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19050.748039999999},"Hot-Dry/Mixed-Dry",58.143454549622355,"Metropolitan Area",0.37528554358071015,0.14090085656368317,4.9303202572283711E-2,8.268443765816879E-3,0.15255665668624843,0.71804625940292555,313.86500000000001,120.157,{"$f":"T235*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9793630335745994E-3},{"$f":"U235*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2890807322422796E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38126490661428475},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.159228330452599E-2}]
["Single Family Detached",10235,"West North Central","1970s","Wood","central furnace","central AC",40.386140178913031,13849.84231,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13849.84231},"Mixed-Humid",242.62891957027225,"Metropolitan Area",1.0463478167589642,0.21090273952695651,0.17208960904119702,2.8183875107157599E-2,0.59081556180763917,2.0201557271347568,1439.28,595.67999999999995,{"$f":"T236*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9933801039936798E-2},{"$f":"U236*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2500740672207997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.066281617798901},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18033968310841783}]
["Single Family Attached",10236,"Pacific","Before 1950","Siding","built-in electric unit","window/wall unit",7.4049669947780803,14240.32114,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14240.32114},"Marine",89.348303278350031,"Metropolitan Area",0.11101385536426474,0.11516663205543268,5.9490223191252601E-3,0,7.2726900737626582E-2,0.30485641047644924,0,0,{"$f":"T237*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U237*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11101385536426474},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9490223191252601E-3}]
["Single Family Attached",10237,"Pacific","1980s","Stucco","central furnace","central AC",24.370724032969001,15346.803550000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15346.803550000001},"Hot-Dry/Mixed-Dry",125.0074803746179,"Metropolitan Area",0.23319518638676717,0.25291117886704151,6.9752710774694346E-2,6.5608812920533999E-3,0.1758494147804277,0.73170849080893063,217.18199999999999,210.32599999999999,{"$f":"T238*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3330494885961E-3},{"$f":"U238*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2278318034573003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23652823587536329},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.2980542578151647E-2}]
["Multi-Family (5+ units)",10238,"Mountain South","2000s","Stucco","central furnace","central AC",13.929694374879718,17790.15884,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1415.054717874265},"Hot-Dry/Mixed-Dry",124.47507290788909,"Metropolitan Area",5.5502050223410863E-2,0.1394608444505929,0.11554031481111118,5.8283762588431202E-3,0.10884097455010897,0.42470896289750654,48.988,278.63,{"$f":"T239*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9320700519224504E-5},{"$f":"U239*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.942766960413064E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.5571370923930087E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11593459150715249}]
["Single Family Detached",10239,"Pacific","2000s","Stucco","central furnace","central AC",34.112827316716192,16804.348429999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16804.348429999998},"Hot-Dry/Mixed-Dry",117.68017989451766,"Metropolitan Area",0.18683992101898275,0.25018965951303085,0.18629379649935618,1.3659683490900378E-2,0.24812637119975017,0.87144974823111998,275.34399999999999,537.52200000000005,{"$f":"T240*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6269765141099201E-3},{"$f":"U240*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.032706976790459E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19146689753309268},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19532650347614663}]
["Single Family Detached",10240,"East North Central","1950s","Siding","central furnace","central AC",44.646168294019041,30125.619630000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30125.619630000001},"Cold/Very Cold",178.3111928010606,"Metropolitan Area",2.0233786867729751,0.50545077921658155,0.17176179270721798,0.10826451793208547,0.42513521451937009,3.1257264732161447,3340.9989999999998,252.77,{"$f":"T241*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.10064966505821037},{"$f":"U241*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6148528738751E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1240283518311855},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17937664558109306}]
["Multi-Family (5+ units)",10241,"West North Central","Before 1950","Siding","radiator","window/wall unit",9.1855372670467883,15058.257809999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1197.7553966014782},"Cold/Very Cold",63.330273959708862,"Metropolitan Area",0.28216119613722918,0.15619909744752067,2.3490174445482927E-2,2.4159920578098303E-3,0.1901767160108406,0.65425100462978625,160.44300000000001,0,{"$f":"T242*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9217146909693099E-4},{"$f":"U242*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28235336760632612},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3490174445482927E-2}]
["Single Family Detached",10242,"South Atlantic","1990s","Stucco","central furnace","central AC",93.194590563225134,17897.94326,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17897.94326},"Mixed-Humid",614.50374213170903,"Metropolitan Area",1.1610367871970515,0.15575635007773869,0.1935266124125791,2.9421874088872944E-2,2.1821516600040889,3.6924714096914584,1004.826,639.04300000000001,{"$f":"T243*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.798431873417276E-2},{"$f":"U243*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1437555354700179E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1790211059312243},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20496416776727927}]
["Single Family Detached",10243,"West South Central","2000s","Brick","central furnace","central AC",61.208257130453539,39286.429479999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39286.429479999999},"Hot-Humid",682.53956109040439,"Metropolitan Area",0.28732318775059501,0.41574388631413295,0.33669192934662429,2.1954592532026321E-2,1.2890660098063245,2.3288250132176764,133.31800000000001,425.51600000000002,{"$f":"T244*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2375882054146406E-3},{"$f":"U244*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6717004326611679E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29256077595600966},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35340893367323595}]
["Single Family Detached",10244,"Middle Atlantic","1970s","Siding","radiator","central AC",53.079854710408021,30488.14171,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30488.14171},"Mixed-Humid",178.07108315443693,"Metropolitan Area",3.1814067334390899,0.2959674771556805,0.18645504775389518,1.4440708320941499E-2,0.49972366117389105,4.163552919522556,179.386,294.26400000000001,{"$f":"T245*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4691457887900601E-3},{"$f":"U245*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9715625321514399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.18687587922788},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19542661028604663}]
["Single Family Detached",10245,"West South Central","1970s","Brick","central furnace","central AC",111.78852265446366,44115.43909,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":44115.43909},"Mixed-Humid",845.82531367562422,"Rural",1.9459733985417662,0.76657144207755501,0.66840819336363699,8.8388679105624923E-2,1.4541860859269267,4.8351391199098854,1187.164,816.41300000000001,{"$f":"T246*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2372261131840757E-2},{"$f":"U246*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6016417973784173E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9983456596736069},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.70442461133742118}]
["Single Family Detached",10246,"Mountain North","2000s","Siding","central furnace","central AC",36.75736712609767,21395.440699999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21395.440699999999},"Cold/Very Cold",181.43787298669326,"Metropolitan Area",0.91627087360666393,0.84209020626967646,4.9405987941948094E-2,2.3785097471783E-2,0.61185267075229721,2.4196197385705855,1004.696,106.994,{"$f":"T247*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1495913689527198E-2},{"$f":"U247*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2891837822557998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.93776678729619112},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.1695171724203896E-2}]
["Single Family Detached",10247,"South Atlantic","2000s","Siding","fireplace","central AC",23.851561901142595,11925.78095,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11925.78095},"Mixed-Humid",198.82879050005772,"Micropolitan Area",0.30205074174548685,0.12170822356335839,0.11397492705476901,5.7277975551326497E-3,0.14066995290667736,0.67840384527029174,0,480.28699999999998,{"$f":"T248*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U248*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7277975551326497E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30205074174548685},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11970272460990167}]
["Single Family Detached",10248,"Pacific","1990s","Wood","central furnace","central AC",71.133826937725942,22748.265729999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22748.265729999999},"Hot-Dry/Mixed-Dry",310.79251621802791,"Metropolitan Area",0.45546097656199092,1.411487667765305,0.32439547866265211,2.4725135518468461E-2,0.89020540325112629,3.0815495262410741,385.71800000000002,701.18399999999997,{"$f":"T249*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7744155608441409E-3},{"$f":"U249*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5950719957624319E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.46423539212283504},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.34034619862027643}]
["Single Family Detached",10249,"West North Central","Before 1950","Siding","central furnace","central AC",22.934730199001073,10215.91546,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10215.91546},"Cold/Very Cold",111.21484849902507,"Micropolitan Area",0.39488227759761257,0.30973896632201325,5.1855946011298157E-2,2.7709138297931001E-2,0.3084540186913699,1.0649312086222937,2464.2190000000001,248.131,{"$f":"T250*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5174252978925744E-2},{"$f":"U250*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5348853190052603E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4200565305765383},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.4390831330303417E-2}]
["Multi-Family (5+ units)",10250,"West North Central","1990s","Brick","heat pump","central AC",23.899728528665324,31323.36635,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2491.5054290359271},null,275.36371362450438,"Metropolitan Area",0.18925408691232976,0.38523552676419009,1.6528130585522459E-2,4.0751699621349993E-3,0.34477560430039023,0.93954437366824994,107.717,22.382999999999999,{"$f":"T251*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6837749029946296E-4},{"$f":"U251*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5767366018111155E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18952246440262921},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6583897951540569E-2}]
["Single Family Detached",10251,"West North Central","2000s","Wood","central furnace","central AC",130.67240119728709,25289.800889999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25289.800889999999},"Mixed-Humid",265.93712675854033,"Metropolitan Area",2.840885905173606,0.45892617691255405,0.15284194645482177,3.4086099435559791E-2,0.62230296927511886,4.0749569978161002,1017.016,330.80399999999997,{"$f":"T252*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5720132141944237E-2},{"$f":"U252*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3659672936155591E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8666060373155502},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16120791374843732}]
["Single Family Attached",10252,"Pacific","1990s","Wood","N/A","central AC",27.420068731764125,12241.10211,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12241.10211},"Hot-Dry/Mixed-Dry",29.485032488206098,"Metropolitan Area",0,9.1948793677222793E-2,4.9370935441073105E-3,4.0552323070008E-4,9.5665853297332751E-2,0.19255174051866283,0,33.128,{"$f":"T253*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U253*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0552323070008E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.3426167748073907E-3}]
["Single Family Detached",10253,"West South Central","Before 1950","Wood","heater burning gas/oil/kerosene","window/wall unit",17.316040096428825,15031.284809999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15031.284809999999},"Hot-Humid",112.56287355298117,"Micropolitan Area",0.45353778413191481,0.19255293795239745,0.13237126605022703,0,0.32187061352475799,1.1003326016592971,0,0,{"$f":"T254*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U254*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45353778413191481},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13237126605022703}]
["Single Family Detached",10254,"South Atlantic","1990s","Brick","central furnace","central AC",150.04143861580667,28831.944390000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28831.944390000001},"Mixed-Humid",545.83576107322085,"Metropolitan Area",1.7897482530870179,0.41337393738746603,0.52667929820822956,6.9431502723056551E-2,0.73546412242369508,3.4652656111064086,1365.259,1042.886,{"$f":"T255*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9363071565947011E-2},{"$f":"U255*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.006843115710954E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8291113246529649},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.55674772936533912}]
["Multi-Family (2-4 units)",10255,"East North Central","1960s","Siding","heater burning gas/oil/kerosene","window/wall unit",30.575953499824095,33599.948900000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11199.982966666668},"Cold/Very Cold",172.52505282239974,"Metropolitan Area",1.5964370936815611,1.0204834016124666,6.3826093331002101E-2,0,0.52482942102070851,3.2055760096457382,0,0,{"$f":"T256*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U256*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5964370936815611},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.3826093331002101E-2}]
["Single Family Detached",10256,"East North Central","Before 1950","Brick","central furnace","window/wall unit",103.77249028349061,32028.54638,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32028.54638},"Mixed-Humid",589.52690518983093,"Micropolitan Area",4.6424446587681274,0.49433617559441201,0.27044023778246551,5.4237845067912363E-2,0.60218288913642593,6.0094039612814312,1693.422,0,{"$f":"T257*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4237845067912363E-2},{"$f":"U257*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.6966825038360396},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27044023778246551}]
["Multi-Family (5+ units)",10257,"Pacific","1970s","Concrete","N/A","central AC",29.260784938251327,13062.850420000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1039.0378344540302},"Hot-Humid",129.42672195008666,"Metropolitan Area",0,5.0717117646769325E-2,0.2387011301107777,1.385000472345878E-2,0.1394230551824146,0.44158965844810005,0,1060.259,{"$f":"T258*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U258*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1016492153203955E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23980277932609809}]
["Multi-Family (5+ units)",10258,"East North Central","1980s","Stucco","central furnace","central AC",21.697172966373465,26109.714759999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2076.8041132053954},"Cold/Very Cold",156.86716628396124,"Metropolitan Area",0.1365075147251128,0.20518750154439538,2.6342279752708926E-2,3.59705707334092E-3,0.16387480484194594,0.53522304286524003,93.762,44.005000000000003,{"$f":"T259*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9472530726236429E-4},{"$f":"U259*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1389765001603435E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13670224003237516},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6433669517710531E-2}]
["Single Family Detached",10259,"Pacific","2000s","Wood","central furnace","central AC",14.010802956738173,9797.7643050000006,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9797.7643050000006},"Marine",101.59599660315872,"Metropolitan Area",0.15660215426286672,0.14736494944704867,1.089231174656877E-2,3.7321545812962951E-3,0.3429345269596536,0.65779394241613787,330.15199999999999,50.767000000000003,{"$f":"T260*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.23475148082436E-3},{"$f":"U260*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9740310047193502E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15983690574369108},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1389714847040705E-2}]
["Multi-Family (5+ units)",10260,"West North Central","2000s","Brick","central furnace","central AC",18.967452924989708,18397.141540000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1463.3349913124002},"Mixed-Humid",167.87080741123836,"Metropolitan Area",0.10194272667612958,0.19117428265288236,2.728657200557523E-2,3.0272864346900801E-3,0.24958511505667461,0.57277518812646133,97.224999999999994,67.326999999999998,{"$f":"T261*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4227274453034811E-4},{"$f":"U261*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8521954960089969E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10208499942065993},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7385093960535321E-2}]
["Single Family Detached",10261,"West South Central","1980s","Wood","heat pump","central AC",33.325641422741853,14364.500609999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14364.500609999999},"Mixed-Humid",268.1660642055744,"Rural",0.26545608618880484,0.123078503071127,0.1553790075357937,1.3655009195870878E-2,0.37106903716474321,0.91498263396046875,377.57,573.03800000000001,{"$f":"T262*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4236044953176995E-3},{"$f":"U262*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2314047005531792E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27087969068412254},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16361041223634687}]
["Single Family Detached",10262,"South Atlantic","1980s","Concrete","central furnace","central AC",113.16010008371011,20649.653300000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20649.653300000002},"Mixed-Humid",502.15826894811357,"Metropolitan Area",2.3544595926989826,0.21480184420691328,0.26944192127033822,5.0101716910804207E-2,1.4521710713377256,4.29087442951396,1668.345,757.92899999999997,{"$f":"T263*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.44507458347885E-2},{"$f":"U263*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.56509710760157E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3889103385337713},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28509289234635393}]
["Single Family Detached",10263,"Mountain South","1990s","Stucco","heat pump","central AC",21.455962561018836,10902.42,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10902.42},"Hot-Dry/Mixed-Dry",232.95437397620182,"Metropolitan Area",7.6219559584560004E-2,0.17255716945398,0.36551837057184,2.004575633784E-2,0.48838406495544007,1.10267916456582,144.297,1694.355,{"$f":"T264*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5731864987399999E-3},{"$f":"U264*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8472569839099999E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.7792746083300002E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.38399094041094001}]
["Single Family Detached",10264,"Pacific","1970s","Wood","heat pump","central AC",28.170870458777483,9884.5159500000009,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9884.5159500000009},"Marine",215.90763017338017,"Metropolitan Area",0.36545265644916419,0.15988363689831797,1.3475471633991452E-2,6.8850200469086995E-3,0.30705504494623959,0.84586680992771324,621.45799999999997,75.087999999999994,{"$f":"T265*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1428115132551005E-3},{"$f":"U265*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4220853365359999E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37159546796241927},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4217680167645052E-2}]
["Single Family Detached",10265,"West South Central","1970s","Brick","built-in electric unit","central AC",32.517557906559816,16971.58555,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16971.58555},"Hot-Humid",248.74563888723233,"Micropolitan Area",0.2465674377667875,0.11776922644856,0.20851755028174071,1.084964612516065E-2,0.27586589321980559,0.84872010771689388,0,639.28300000000002,{"$f":"T266*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U266*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.084964612516065E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2465674377667875},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21936719640690136}]
["Single Family Detached",10266,"Mountain North","2000s","Siding","central furnace","central AC",63.573923531430708,20782.583699999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20782.583699999999},"Cold/Very Cold",117.01301229681449,"Metropolitan Area",0.78847056768980217,0.20535175354084978,8.10667489340922E-2,2.7574061879571898E-2,0.2944801082573395,1.3693691784220836,1140.451,186.33600000000001,{"$f":"T267*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.37015183632487E-2},{"$f":"U267*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8725435163231999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.81217208605305091},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.4939292450415399E-2}]
["Single Family Detached",10267,"Mountain North","1950s","Brick","central furnace","central AC",29.853268660989972,10757.934649999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10757.934649999999},"Cold/Very Cold",112.78726269141801,"Metropolitan Area",1.1381866781490564,0.19688308134277602,8.8300611226336784E-2,2.2821516796731896E-2,0.27286072586003468,1.6962310965782039,1707.2750000000001,414.09100000000001,{"$f":"T268*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.836675287957875E-2},{"$f":"U268*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4547639171531499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1565534310286352},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2755375143489929E-2}]
["Single Family Detached",10268,"South Atlantic","2010s","Brick","heat pump","central AC",34.190802752971194,7659.2300070000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7659.2300070000001},"Mixed-Humid",119.49759090771502,"Metropolitan Area",0.14220393738123446,4.7450599605506523E-2,9.3571526244877828E-2,9.529568019329358E-3,0.31926413439441498,0.60249019762603373,417.29,826.904,{"$f":"T269*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1961200896210304E-3},{"$f":"U269*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3334479297083284E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14540005747085549},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.9904974174586159E-2}]
["Single Family Detached",10269,"Pacific","1970s","Wood","central furnace","N/A",18.956258928473485,13019.408600000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13019.408600000001},"Marine",177.83210213188141,"Metropolitan Area",0.29976023064430296,0.13548400190826601,0,5.6479366253574005E-3,0.171525305250431,0.60676953780300003,433.80900000000003,0,{"$f":"T270*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6479366253574005E-3},{"$f":"U270*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30540816726966036},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10270,"East North Central","1950s","Siding","central furnace","central AC",36.097421809019785,20336.575669999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20336.575669999998},"Cold/Very Cold",208.0939291668212,"Metropolitan Area",1.9597891858864642,0.60665565038963876,0.10464689358075115,5.57096696686116E-2,0.37392406145134022,3.0450157913081943,2519.5259999999998,219.857,{"$f":"T271*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1238531151532409E-2},{"$f":"U271*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4711385170791897E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0110277170379964},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10911803209783033}]
["Single Family Detached",10271,"West South Central","1970s","Siding","central furnace","central AC",37.038172286817407,14045.57159,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14045.57159},"Hot-Humid",219.06827447223694,"Metropolitan Area",0.17731545324135062,8.9297586680029351E-2,0.23710552725667278,1.675876869961189E-2,0.24374239692666591,0.74746096410471874,247.929,945.24199999999996,{"$f":"T272*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.48230451873711E-3},{"$f":"U272*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.327646418087478E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18079775776008772},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25038199143754758}]
["Single Family Detached",10272,"Pacific","1970s","Stucco","central furnace","central AC",30.937528128790902,11319.98834,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11319.98834},"Hot-Dry/Mixed-Dry",100.00419561772181,"Metropolitan Area",0.12461769907923428,0.11691649593175384,0.1368144318361556,1.6988755500963501E-2,0.2104885157091676,0.58883714255631137,848.81,651.96500000000003,{"$f":"T273*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6085193028753995E-3},{"$f":"U273*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3802361980880998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13422621838210969},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14419466803424369}]
["Multi-Family (5+ units)",10273,"Pacific","1970s","Concrete","N/A","central AC",9.9205127661376196,14653.63776,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1165.5713382213103},"Hot-Humid",94.838343607743994,"Metropolitan Area",0,6.2294167403362556E-2,4.6856388811879784E-2,2.3673684483167998E-3,0.27475469689899457,0.38608431768500734,0,161.55500000000001,{"$f":"T274*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U274*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8830387754634377E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7044692689426126E-2}]
["Single Family Detached",10274,"East North Central","1970s","Siding","central furnace","central AC",32.945911953797697,14103.558199999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14103.558199999999},"Cold/Very Cold",114.97894794232566,"Metropolitan Area",0.83072263729765694,0.43688930721536801,5.7033830318842398E-2,3.8227793226007403E-2,0.33283599090605853,1.6574817657379259,2514.7559999999999,195.751,{"$f":"T275*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5467007604799199E-2},{"$f":"U275*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7607856212081999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.86618964490245609},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9794615940050595E-2}]
["Single Family Detached",10275,"West South Central","1970s","Brick","central furnace","central AC",42.186515682842554,22729.80371,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22729.80371},"Mixed-Humid",158.66496292041188,"Micropolitan Area",0.52625530351534999,0.26932251201511137,0.1553640953770109,1.4072089666272132E-2,0.37231666231840432,1.3232585732258768,263.42099999999999,355.68200000000002,{"$f":"T276*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9875076230919101E-3},{"$f":"U276*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0845820431802214E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53224281113844185},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16344867742019112}]
["Single Family Detached",10276,"Middle Atlantic","1990s","Siding","central furnace","central AC",49.659721807993769,16255.228090000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16255.228090000001},"Mixed-Humid",242.9868719025155,"Metropolitan Area",0.84639454426326399,0.16752067511048041,8.1785595553568693E-2,2.029869982215941E-2,0.45632261482459258,1.5520234297519055,976.79200000000003,271.95699999999999,{"$f":"T277*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5877976756487281E-2},{"$f":"U277*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4207230656721306E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.86227252101975127},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.6206318619240829E-2}]
["Single Family Detached",10277,"East North Central","1980s","Brick","central furnace","central AC",89.653476118167504,21834.748200000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21834.748200000002},"Cold/Very Cold",210.605142326324,"Metropolitan Area",1.7439764490091056,0.35880273133923363,0.16257092340957482,6.9654702711597016E-2,0.55896710842820163,2.8243172121861155,2742.7260000000001,447.35899999999998,{"$f":"T278*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9886731591593204E-2},{"$f":"U278*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7679711200038006E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8038631806006988},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17233889452957862}]
["Multi-Family (5+ units)",10278,"Pacific","1970s","Wood","built-in electric unit","N/A",12.176950612692501,13381.26441,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1064.3649393348244},"Marine",74.965442782437592,"Metropolitan Area",8.5227802086263488E-2,8.9621848024368414E-2,0,0,8.0932456354446708E-2,0.2557821064650786,0,0,{"$f":"T279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.5227802086263488E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10279,"New England","2010s","Siding","central furnace","central AC",15.105649604600329,13169.703229999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13169.703229999999},"Cold/Very Cold",32.505619548273572,"Micropolitan Area",0.62543426355874032,1.651453128665217E-2,5.50832056387011E-3,3.2044521899235998E-3,8.5934591934408666E-2,0.73339170734367132,224.13,19.190000000000001,{"$f":"T280*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9517255849399E-3},{"$f":"U280*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5272660498370001E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62838598914368027},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7610471688538103E-3}]
["Single Family Detached",10280,"East North Central","Before 1950","Wood","wood-burning stove","window/wall unit",17.816736617500741,16558.305410000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16558.305410000001},"Cold/Very Cold",81.963611762666048,"Micropolitan Area",0.62973583441937142,6.1559341888530121E-2,3.0656708968290404E-2,0,0.18743716921266948,0.90938905448886143,0,0,{"$f":"T281*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U281*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62973583441937142},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0656708968290404E-2}]
["Single Family Detached",10281,"East South Central","Before 1950","Siding","central furnace","central AC",20.899406729406049,12293.76866,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12293.76866},"Mixed-Humid",80.043104996161475,"Metropolitan Area",0.85968249051230194,7.7635825245176301E-2,6.9132102525367709E-2,9.505283758770142E-3,0.1413037901768458,1.1477542084596917,487.822,285.35700000000003,{"$f":"T282*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.99717081525852E-3},{"$f":"U282*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5081129435116203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.86567966132756047},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.2640215468879332E-2}]
["Single Family Detached",10282,"West North Central","Before 1950","Brick","central furnace","central AC",28.69155804544015,11663.234979999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11663.234979999999},"Mixed-Humid",120.7132340543068,"Metropolitan Area",0.35903903121113845,0.1558716010579029,0.15578966683216841,3.1512544695412599E-2,0.24795572204404295,0.91865602114525269,2004.5360000000001,697.33399999999995,{"$f":"T283*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3379374393869282E-2},{"$f":"U283*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1331703015433184E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38241840560500773},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16392283713371172}]
["Multi-Family (5+ units)",10283,"Middle Atlantic","Before 1950","Brick","radiator","N/A",44.890906254730375,50439.220509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4012.007851672216},"Mixed-Humid",181.14993850399031,"Metropolitan Area",1.047603171890652,0.55040704850452438,0,4.5819492303489093E-3,0.61350157031892438,2.2157292851391959,90.840999999999994,0,{"$f":"T284*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6445480525375577E-4},{"$f":"U284*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0479676266959057},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10284,"Middle Atlantic","Before 1950","Siding","wood-burning stove","N/A",71.658416913961901,22386.259580000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22386.259580000002},"Cold/Very Cold",376.85029376121042,"Micropolitan Area",9.5538847391247114E-2,0.4803429568034816,0,0,0.80545663469297846,1.3813384388877072,0,0,{"$f":"T285*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U285*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.5538847391247114E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",10285,"East North Central","1990s","Siding","central furnace","central AC",49.686710153921887,26886.747920000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26886.747920000002},"Cold/Very Cold",648.44907452202722,"Metropolitan Area",1.3462458980276055,0.29567238385933153,7.1631216733749364E-2,1.9161244206406802E-2,0.49895872922928808,2.2125082278499746,608.17399999999998,104.491,{"$f":"T286*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.635182102949808E-2},{"$f":"U286*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8094231769087204E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3625977190571037},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.444063991065808E-2}]
["Single Family Detached",10286,"East North Central","1970s","Siding","central furnace","window/wall unit",47.952736918637633,20353.453699999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20353.453699999998},"Cold/Very Cold",107.18279334298715,"Metropolitan Area",1.4160579172719874,5.0003673032734203E-2,1.6551225014302999E-2,1.5347196107225798E-2,0.30497478655940197,1.7875876018784265,754.03399999999999,0,{"$f":"T287*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5347196107225798E-2},{"$f":"U287*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4314051133792132},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6551225014302999E-2}]
["Single Family Attached",10287,"West North Central","1980s","Wood","central furnace","central AC",17.295490014921576,13981.80276,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13981.80276},"Mixed-Humid",163.07552610017498,"Metropolitan Area",0.23290708070532673,7.4201035756842712E-2,5.2940362407197766E-2,5.7612577544690399E-3,0.19636520575618119,0.55641368462554841,242.54499999999999,169.50899999999999,{"$f":"T288*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3912163504241999E-3},{"$f":"U288*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3700414040448399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23629829705575092},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5310403811242609E-2}]
["Single Family Detached",10288,"South Atlantic","Before 1950","Wood","heat pump","central AC",55.447523728291323,14119.562959999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14119.562959999999},"Mixed-Humid",422.77204870241411,"Metropolitan Area",0.82450391561569047,0.15525069439639871,0.17616745732403161,2.6840286697989841E-2,0.2865761847048402,1.442498252040961,1189.1320000000001,711.79700000000003,{"$f":"T289*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6790024141750719E-2},{"$f":"U289*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0050262556239122E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84129393975744116},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18621771988027072}]
["Single Family Detached",10289,"Pacific","Before 1950","Wood","N/A","N/A",35.590789923899052,18158.566289999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18158.566289999999},"Hot-Dry/Mixed-Dry",97.639010417440588,"Metropolitan Area",0,0.48057976709394057,0,0,0.46182592668382172,0.94240569377776229,0,0,{"$f":"T290*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U290*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",10290,"Middle Atlantic","Before 1950","Concrete","central furnace","window/wall unit",46.600740187921701,46600.740189999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15533.580063333333},"Mixed-Humid",137.23917985342942,"Metropolitan Area",1.1999465206678281,0.35443148266678393,0.11707569198969965,1.9698738687935473E-2,0.40573158129976417,2.0903177690826995,422.71300000000002,0,{"$f":"T291*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5662462293118243E-3},{"$f":"U291*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.20651276689714},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11707569198969965}]
["Single Family Attached",10291,"South Atlantic","1970s","Siding","central furnace","central AC",40.369390396343192,17521.436799999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17521.436799999999},"Mixed-Humid",72.339757410646513,"Metropolitan Area",0.42318965617062398,0.12860885295556479,8.3241963321395204E-2,1.2977882937644798E-2,0.17898724146470726,0.81402771391229112,460.81299999999999,279.87299999999999,{"$f":"T292*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0741058561184E-3},{"$f":"U292*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9037770815264E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43126376202674238},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.8145740402921599E-2}]
["Multi-Family (2-4 units)",10292,"Middle Atlantic","1960s","Wood","built-in electric unit","window/wall unit",24.899950823867307,39461.094810000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13153.698270000001},"Cold/Very Cold",434.61431725318857,"Metropolitan Area",0.59557150605677633,0.41949835029696048,1.9590578901708931E-2,0,0.44824358750583099,1.4829040227612766,0,0,{"$f":"T293*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U293*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59557150605677633},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9590578901708931E-2}]
["Single Family Detached",10293,"South Atlantic","1970s","Brick","central furnace","central AC",64.713697530131412,44846.637239999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":44846.637239999996},"Hot-Humid",738.73116418383131,"Metropolitan Area",0.13680865825133437,0.268899495111658,0.51494729652439941,2.7812404477219076E-2,1.5998953075225613,2.520550757409953,52.137,568.03,{"$f":"T294*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3381691257818799E-3},{"$f":"U294*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5474235351437197E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13914682737711626},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.54042153187583664}]
["Single Family Detached",10294,"West South Central","2000s","Brick","heat pump","central AC",119.5135102520878,31793.963889999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31793.963889999999},"Mixed-Humid",705.2061749704668,"Rural",0.58645502043560893,0.45361697784643878,0.44005767889041492,4.4315348894834815E-2,2.4585380455449886,3.9386677227174509,524.46,869.36900000000003,{"$f":"T295*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.66746623017494E-2},{"$f":"U295*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7640686593085412E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60312968273735834},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4676983654835003}]
["Single Family Detached",10295,"Pacific","2000s","Stucco","central furnace","central AC",36.496952919767757,11671.55514,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11671.55514},"Hot-Dry/Mixed-Dry",110.86810226570961,"Metropolitan Area",0.29303149061798012,0.22391139726649636,7.4586466201302715E-2,7.7819627033744402E-3,0.67913365429781558,1.2706630083835948,331.851,334.89499999999998,{"$f":"T296*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8732172447641404E-3},{"$f":"U296*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9087454586102998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29690470786274425},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.8495211659913008E-2}]
["Single Family Detached",10296,"West North Central","Before 1950","Siding","radiator","N/A",17.921494475176321,12445.48227,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12445.48227},"Cold/Very Cold",57.147538872186729,"Metropolitan Area",1.1230970094365242,0.13157091299782289,0,4.3554956481028197E-3,0.19639318251015306,1.4510611049445001,349.96600000000001,0,{"$f":"T297*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3554956481028197E-3},{"$f":"U297*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1274525050846271},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10297,"Pacific","1970s","Wood","central furnace","central AC",12.379238842168359,10974.50252,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10974.50252},"Hot-Dry/Mixed-Dry",66.752751785366272,"Metropolitan Area",0.12007337096062744,0.15625605335550949,4.0874260273176997E-2,6.0426598580346803E-3,0.18264275213250677,0.49984643672182066,386.65600000000001,163.953,{"$f":"T298*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2433572463731195E-3},{"$f":"U298*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7993026116615602E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12431672820700056},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.2673562884838555E-2}]
["Single Family Detached",10298,"East North Central","1970s","Brick","central furnace","central AC",39.700241461736859,21482.814640000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21482.814640000001},"Cold/Very Cold",86.462593029773032,"Metropolitan Area",1.4403131592573359,0.36449251411811734,0.1029173334051845,2.8165065616586639E-2,0.26764882355076813,2.175371830331406,1110.8889999999999,200.16200000000001,{"$f":"T299*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3865022472614957E-2},{"$f":"U299*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3000431439716809E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4641781817299508},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10721737654915618}]
["Single Family Detached",10299,"West North Central","1970s","Siding","central furnace","central AC",80.738392641188895,29000.85943,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29000.85943},"Cold/Very Cold",529.1832060750811,"Metropolitan Area",1.5622252849823626,0.7653893480370263,0.38353192883025722,0.1214443759602406,1.0498656513895803,3.7610122132392267,3515.6770000000001,671.93600000000004,{"$f":"T300*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.10195765447828412},{"$f":"U300*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9486721481956484E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6641829394606467},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.40301865031221368}]
["Single Family Detached",10300,"South Atlantic","2000s","Brick","heat pump","central AC",31.771927175622331,22249.24872,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22249.24872},"Hot-Humid",308.60540099905137,"Rural",0.14632467612293665,0.18464675986901594,0.30781897902016414,1.6947230500775276E-2,0.41417125562246432,1.052961670634581,109.717,651.98199999999997,{"$f":"T301*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.44112082181224E-3},{"$f":"U301*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4506109678963038E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1487657969447489},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32232508869912718}]
["Multi-Family (5+ units)",10301,"East North Central","1980s","Brick","radiator","window/wall unit",10.11608437965964,14725.013650000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1171.2486787552175},"Cold/Very Cold",71.563566353924102,"Metropolitan Area",0.15876009894932569,0.1566603331731963,9.2035900066731492E-3,1.1032569227126001E-3,0.2338780544285643,0.55951757884446507,74.924000000000007,0,{"$f":"T302*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7754636007055913E-5},{"$f":"U302*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15884785358533274},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2035900066731492E-3}]
["Single Family Detached",10302,"West South Central","1960s","Brick","central furnace","central AC",57.442001130214678,22281.614089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22281.614089999999},"Hot-Humid",241.38757660906359,"Metropolitan Area",0.68957838928414417,0.14510524616834378,0.42773978917990463,4.2413319799684081E-2,0.44745981978766203,1.7098832444200545,830.625,1072.8869999999999,{"$f":"T303*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8507665703506249E-2},{"$f":"U303*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3905654096177828E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.70808605498765043},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.45164544327608247}]
["Single Family Attached",10303,"West North Central","1950s","Siding","central furnace","window/wall unit",34.783248238676123,13398.78592,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13398.78592},"Cold/Very Cold",86.043881237264415,"Rural",0.67311261086214913,0.11803529148121984,2.1817752267400962E-2,1.1714799708002559E-2,0.13071969433232308,0.94368534894309308,874.31799999999998,0,{"$f":"T304*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1714799708002559E-2},{"$f":"U304*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.68482741057015173},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1817752267400962E-2}]
["Multi-Family (5+ units)",10304,"South Atlantic","2000s","Brick","portable electric heaters","window/wall unit",42.875989251422254,38978.172050000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3100.3796396382995},"Cold/Very Cold",254.60222359924683,"Micropolitan Area",0.36630434893267194,1.0686141053402172,3.2057168842629949E-2,0,0.63094719376055575,2.0979228168760748,0,0,{"$f":"T305*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U305*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36630434893267194},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2057168842629949E-2}]
["Single Family Detached",10305,"West North Central","2010s","Siding","central furnace","central AC",60.640894575686659,12667.82841,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12667.82841},"Mixed-Humid",190.29481351657063,"Metropolitan Area",0.57907434384708723,0.22258874387253746,0.11014517187857034,2.8342416564427146E-2,0.29481168197252944,1.2066199415707244,1716.183,521.17100000000005,{"$f":"T306*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1740311764159033E-2},{"$f":"U306*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6021048002681106E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60081465561124625},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11674727667883845}]
["Multi-Family (2-4 units)",10306,"East North Central","1990s","Siding","built-in electric unit","central AC",11.784448789907049,23711.164570000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7903.7215233333336},"Mixed-Humid",235.88245890100947,"Metropolitan Area",0.1384307581042197,0.27959304236690341,2.9398919689836364E-2,1.2083920799809101E-3,0.35660261316947628,0.804830928050423,0,50.963000000000001,{"$f":"T307*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U307*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0279735999363667E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1384307581042197},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.980171704983E-2}]
["Single Family Detached",10307,"West South Central","2010s","Wood","central furnace","central AC",130.89266579553134,42305.32185,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":42305.32185},"Hot-Humid",733.72459164062218,"Metropolitan Area",1.1772255798398683,0.9763558926904925,0.89982793456186627,7.4098998074608652E-2,2.0821430984522209,5.1355525055444478,479.887,1271.6420000000001,{"$f":"T308*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0301773986630949E-2},{"$f":"U308*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3797224087977699E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1975273538264992},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.95362515864984398}]
["Single Family Detached",10308,"West North Central","2000s","Wood","central furnace","central AC",69.66322651230891,16892.149979999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16892.149979999998},"Mixed-Humid",268.79485002744485,"Metropolitan Area",1.07293865649536,0.50275183674085089,0.21524018045675949,5.1980996898655436E-2,0.66329062400542593,2.4542212976983961,2284.92,792.30799999999999,{"$f":"T309*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8597211332301595E-2},{"$f":"U309*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3383785566353839E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1115358678276617},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22862396602311333}]
["Single Family Detached",10309,"East North Central","1970s","Brick","central furnace","central AC",66.469220608522576,19322.44785,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19322.44785},"Cold/Very Cold",132.27154625190485,"Metropolitan Area",2.6860368751128463,0.76210174745563464,0.11085002359316821,6.8925374240004902E-2,0.3563576452244468,3.9153462913860961,3277.17,289.94400000000002,{"$f":"T310*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3322946420584503E-2},{"$f":"U310*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6024278194203997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.7493598215334307},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11645245141258861}]
["Multi-Family (5+ units)",10310,"East North Central","1980s","Brick","central furnace","central AC",19.955215769831991,20961.361099999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1667.2966882639193},"Cold/Very Cold",50.049630557321194,"Metropolitan Area",0.38950395522208325,4.6371792054836103E-2,1.0963732462133609E-2,2.5668025121393999E-3,0.14663706713618785,0.59583918223871557,96.62,25.834,{"$f":"T311*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.610942060200599E-4},{"$f":"U311*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3072942644610091E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38966504942810332},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1006805404778219E-2}]
["Multi-Family (5+ units)",10311,"Pacific","1970s","Stucco","central furnace","central AC",30.726665157135262,26397.478660000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2099.6932660224766},"Hot-Dry/Mixed-Dry",81.06744888102844,"Metropolitan Area",0.13097181189538412,0.29035669074759063,8.3074812992493155E-2,9.017299517820019E-3,0.22776201264228821,0.74046537887498265,199.72399999999999,141.87299999999999,{"$f":"T312*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1935913786307307E-4},{"$f":"U312*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9788978273040677E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13139117103324718},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.3372702775223559E-2}]
["Single Family Attached",10312,"Pacific","1980s","Wood","built-in furnace","window/wall unit",10.155343021143517,12089.69407,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12089.69407},"Cold/Very Cold",219.18313111616268,"Micropolitan Area",0.1707185578727759,0.28897770867211292,1.1934728371410741E-2,0,0.2762218724588561,0.74785286737515566,0,0,{"$f":"T313*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U313*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1707185578727759},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1934728371410741E-2}]
["Single Family Detached",10313,"Pacific","1950s","Siding","central furnace","window/wall unit",11.690732412340957,14988.118479999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14988.118479999999},"Cold/Very Cold",79.325171601812528,"Metropolitan Area",0.59816528687762693,9.1371946784676167E-2,1.3384959351142239E-2,7.3368638533817592E-3,0.11078520232906676,0.81370739534251224,489.512,0,{"$f":"T314*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3368638533817592E-3},{"$f":"U314*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60550215073100866},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3384959351142239E-2}]
["Single Family Detached",10314,"South Atlantic","1950s","Concrete","central furnace","central AC",34.042690836321597,23806.077509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23806.077509999999},"Hot-Humid",599.46733678602277,"Rural",0.87034069514067358,0.68685480519256581,0.81205377593480188,4.9059540726530487E-2,1.2372194408859802,3.6064687171540211,492.23700000000002,1568.5619999999999,{"$f":"T315*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.171823217528987E-2},{"$f":"U315*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7341308551240612E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88205892731596347},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.84939508448604251}]
["Single Family Detached",10315,"East North Central","1980s","Brick","heat pump","central AC",22.78589957761147,15736.118490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15736.118490000001},"Mixed-Humid",172.70390045876098,"Micropolitan Area",0.22135461278242491,0.16199185248805231,7.9133745454156537E-2,7.5147361765440313E-3,0.12675874613341623,0.58923895685804994,245.565,231.982,{"$f":"T316*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8642399369968501E-3},{"$f":"U316*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6504962395471799E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22521885271942177},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.2784241693703714E-2}]
["Single Family Detached",10316,"South Atlantic","1970s","Brick","heat pump","central AC",38.327059114242239,8706.7376449999992,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8706.7376449999992},"Mixed-Humid",190.12032322094356,"Metropolitan Area",0.21965399523146695,8.1938028341627014E-2,0.12126886111779614,1.2997217701490163E-2,0.22582589681218981,0.6486867815030799,588.33100000000002,904.44600000000003,{"$f":"T317*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1224436654204947E-3},{"$f":"U317*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8747740360696691E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22477643889688745},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12914363515386582}]
["Single Family Detached",10317,"Pacific","1950s","Siding","central furnace","central AC",13.683251958737511,16022.54328,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16022.54328},"Marine",107.37406435199769,"Metropolitan Area",0.53403731188595704,0.12877986174190775,2.4276300089999519E-2,6.2519162751396001E-3,0.99687002484946852,1.6839634985673329,328.44400000000002,61.750999999999998,{"$f":"T318*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.26250820505632E-3},{"$f":"U318*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8940807008327989E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5392998200910134},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5265708160082799E-2}]
["Single Family Detached",10318,"South Atlantic","1990s","Brick","heat pump","central AC",99.972835424023941,22976.978950000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22976.978950000001},"Mixed-Humid",475.0246612763296,"Micropolitan Area",0.19232062249646878,0.33566579138403368,0.15893670344762426,1.4068551464316551E-2,0.93386100679884043,1.6207841241269672,228.255,384.03399999999999,{"$f":"T319*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2446103302322498E-3},{"$f":"U319*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8239411340842993E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19756523282670102},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16776064458170856}]
["Single Family Detached",10319,"Pacific","1970s","Stucco","central furnace","both central and individual units",31.093853434310425,10948.539940000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10948.539940000001},"Hot-Dry/Mixed-Dry",263.96929799338886,"Metropolitan Area",0.45331076382033419,0.35669492422966664,8.7006426519268876E-2,1.3007172007838319E-2,0.4264960486894237,1.3235081632586934,783.47400000000005,404.55399999999997,{"$f":"T320*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.5778963809515617E-3},{"$f":"U320*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4292756268867603E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.46188866020128577},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.1435702146155637E-2}]
["Single Family Detached",10320,"Middle Atlantic","1950s","Shingle","central furnace","window/wall unit",67.513124479758517,26517.330900000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26517.330900000001},"Mixed-Humid",176.26069851412211,"Metropolitan Area",2.6221576213966267,0.44959357583154624,5.9931713497766402E-2,2.02586309089893E-2,0.5212111588489714,3.652894069574911,763.97699999999998,0,{"$f":"T321*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.02586309089893E-2},{"$f":"U321*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6424162523056158},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9931713497766402E-2}]
["Single Family Attached",10321,"East South Central","1990s","Wood","central furnace","both central and individual units",21.425054704410964,11876.41613,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11876.41613},"Mixed-Humid",227.40667076856676,"Metropolitan Area",0.46772988219032874,0.29411914854904669,0.18731557154016004,1.3800692453463251E-2,0.21945309420585954,1.1686176964853949,573.25,588.77499999999998,{"$f":"T322*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8081555465224998E-3},{"$f":"U322*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9925369069407496E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.47453803773685121},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19430810844710078}]
["Single Family Detached",10322,"Pacific","1950s","Stucco","central furnace","central AC",32.799418761482741,12238.589089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12238.589089999999},"Hot-Dry/Mixed-Dry",180.65381355904731,"Metropolitan Area",0.58417612840649791,0.23774526512293645,0.14011976559306819,1.9573542689309699E-2,0.54455170133760122,1.5065928604601038,974.07799999999997,625.25199999999995,{"$f":"T323*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1921340383609019E-2},{"$f":"U323*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6522023057006795E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59609746879010694},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14777196789876887}]
["Single Family Detached",10323,"Pacific","1950s","Wood","central furnace","N/A",16.983983132187362,13718.88783,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13718.88783},"Marine",57.401665007117636,"Metropolitan Area",0.62236516617401316,5.7208118942183576E-2,0,4.6510596654535802E-3,0.13399529955871772,0.81356858467491444,339.02600000000001,0,{"$f":"T324*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6510596654535802E-3},{"$f":"U324*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6270162258394667},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10324,"South Atlantic","2010s","Wood","central furnace","central AC",12.278601752415478,10232.16813,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10232.16813},"Hot-Humid",222.91725763466161,"Rural",0.22162056572912783,0.20431927913881853,0.11971058594600655,8.9394974014645814E-3,0.21494324721868432,0.76059367803263722,345.721,527.94500000000005,{"$f":"T325*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5374753980717301E-3},{"$f":"U325*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4020220033928514E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22515804112719956},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12511260794939941}]
["Multi-Family (2-4 units)",10325,"Pacific","1950s","Wood","heater burning gas/oil/kerosene","N/A",14.498098053112958,20305.459459999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6768.4864866666658},"Hot-Dry/Mixed-Dry",17.861636495975706,"Metropolitan Area",3.5220794095424078E-2,0.27735393581181567,0,0,0.12478161711007851,0.43735634701731824,0,0,{"$f":"T326*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U326*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.5220794095424078E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10326,"South Atlantic","1980s","Siding","heat pump","central AC",33.848725986156929,13737.30762,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13737.30762},"Mixed-Humid",233.94206280103279,"Metropolitan Area",0.24105022649697727,0.15643247780083278,4.7248851380147103E-2,1.1162812536243421E-2,0.35347874235058313,0.79821029802854027,659.02800000000002,153.56299999999999,{"$f":"T327*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.053270366193359E-3},{"$f":"U327*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1095421700500598E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25010349686317063},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.9358393550197166E-2}]
["Mobile Home",10327,"South Atlantic","1980s","Siding","central furnace","central AC",26.45222016527028,22043.516800000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22043.516800000001},"Mixed-Humid",574.92998949377659,"Metropolitan Area",0.66168859827846715,0.72195290594413453,0.19557947158775682,1.5351347578204801E-2,0.3824401150626433,1.9616610908730019,377.88499999999999,318.52600000000001,{"$f":"T328*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3299143459679998E-3},{"$f":"U328*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0214332322368006E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.67001851262443513},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20260090481999363}]
["Single Family Detached",10328,"West South Central","1970s","Brick","central furnace","central AC",19.832347087215084,14045.57159,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14045.57159},"Hot-Humid",232.20006926714842,"Metropolitan Area",0.23829792605680586,0.14254589359059427,0.22525286266787631,1.4818920761745399E-2,0.18616993607297408,0.79226661838825063,288.40600000000001,766.654,{"$f":"T329*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0508271199855396E-3},{"$f":"U329*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.076809364175986E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24234875317679139},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23602095630963615}]
["Single Family Detached",10329,"Pacific","Before 1950","Stucco","central furnace","N/A",34.802762274749306,18853.067319999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18853.067319999998},"Marine",155.55539531087982,"Metropolitan Area",0.35490976527476009,0.45730392235192252,0,1.1066354602426279E-2,0.51968866555460058,1.3319023531812832,586.97900000000004,0,{"$f":"T330*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1066354602426279E-2},{"$f":"U330*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36597611987718637},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10330,"Pacific","1970s","Stucco","central furnace","central AC",19.297347851146178,14358.14572,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14358.14572},"Hot-Dry/Mixed-Dry",85.482699448383514,"Metropolitan Area",0.28121638784304204,0.34683256817390462,0.12508454725991855,8.0820997187679607E-3,0.23120466899696673,0.9843381722738318,163.59,399.303,{"$f":"T331*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3488490583347997E-3},{"$f":"U331*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.73325066043316E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28356523690137686},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1308177979203517}]
["Multi-Family (5+ units)",10331,"South Atlantic","2010s","Wood","N/A","central AC",23.727051425100605,22814.472519999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1814.6958251238846},"Hot-Humid",194.66044865054681,"Metropolitan Area",0,0.23442267486121848,0.26594623475404078,1.217291277224372E-2,0.15260785465855409,0.66418142612690823,0,533.56100000000004,{"$f":"T332*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U332*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6825091914892498E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26691448567318971}]
["Single Family Detached",10332,"Pacific","1950s","Stucco","N/A","central AC",20.124415510136952,12346.267180000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12346.267180000001},"Hot-Dry/Mixed-Dry",21.329472918644264,"Metropolitan Area",0,0.21957515176683323,2.6213458667637021E-2,1.4628474668223002E-3,5.1286554367193309E-2,0.29707516480166357,0,118.485,{"$f":"T333*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U333*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4628474668223002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.767630613445932E-2}]
["Single Family Detached",10333,"West South Central","2000s","Stucco","central furnace","central AC",68.970194488651117,16740.338469999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16740.338469999999},"Hot-Humid",559.95985208821628,"Metropolitan Area",0.90829443884771999,0.19832093167651982,0.45979182719120543,4.77945535697889E-2,1.2447298757774663,2.8111370734929118,1026.8889999999999,1828.164,{"$f":"T334*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7190469431119827E-2},{"$f":"U334*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0604084138669076E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.92548490827883978},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.49039591132987448}]
["Mobile Home",10334,"West South Central","1980s","Wood","central furnace","both central and individual units",26.638036018420561,22198.36335,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22198.36335},"Hot-Humid",391.19536416521021,"Metropolitan Area",0.48623499306782819,0.29134623790557124,0.39676961740758709,1.7353503953772453E-2,0.45175396449918603,1.6261048128801727,223.17699999999999,558.57000000000005,{"$f":"T335*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9541641373629496E-3},{"$f":"U335*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.23993398164095E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49118915720519113},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4091689572239966}]
["Single Family Detached",10335,"Pacific","1970s","Wood","heat pump","central AC",47.363411522083929,13578.95973,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13578.95973},"Marine",197.03547182995473,"Micropolitan Area",9.1308564385727653E-2,0.20641494822522652,1.4395095946652191E-2,2.8749373540355996E-3,0.36016639966623826,0.67228500822384463,149.06299999999999,62.656999999999996,{"$f":"T336*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.02412047423299E-3},{"$f":"U336*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.5081687980261E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.3332684859960643E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5245912826454801E-2}]
["Multi-Family (2-4 units)",10336,"Middle Atlantic","Before 1950","Brick","radiator","window/wall unit",89.708942697969675,66648.545840000006,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22216.181946666667},"Mixed-Humid",159.86653447435734,"Metropolitan Area",3.1721813495655993,0.71243989735086344,0.12901532250105507,4.4498568115534411E-3,0.56011604545300486,4.5767191860782255,66.766000000000005,0,{"$f":"T337*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4832856038511468E-3},{"$f":"U337*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.1736646351694504},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12901532250105507}]
["Single Family Detached",10337,"West North Central","Before 1950","Siding","wood-burning stove","both central and individual units",27.454018103103966,17288.424500000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17288.424500000001},"Cold/Very Cold",289.62239510215466,"Metropolitan Area",0.21452198046901649,0.19067446602111252,9.3211301382428002E-2,3.8961366337445002E-3,0.70430586456721023,1.202713612439767,0,225.36099999999999,{"$f":"T338*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U338*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8961366337445002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21452198046901649},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.7107438016172498E-2}]
["Single Family Detached",10338,"Mountain South","1980s","Stucco","N/A","central AC",20.154072746059558,14395.766250000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14395.766250000001},"Hot-Dry/Mixed-Dry",68.108687833799934,"Metropolitan Area",0,5.4026216658015006E-2,8.9327140366342497E-2,4.6886722760924992E-3,8.9033495526374989E-2,0.23238685255073249,0,325.69799999999998,{"$f":"T339*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U339*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6886722760924992E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.4015812642434998E-2}]
["Multi-Family (5+ units)",10339,"West North Central","1990s","Wood","radiator","central AC",13.331581223929716,12636.569879999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1005.1308696714161},"Cold/Very Cold",26.353200025260595,"Metropolitan Area",0.2238414227125041,0.13879025231055334,4.7308908139721559E-3,7.7706059163084001E-4,8.4426035386429482E-2,0.45250385330252119,44.685000000000002,16.808,{"$f":"T340*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4914272911267231E-5},{"$f":"U340*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6894239657437163E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22388633698541535},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.747785053629593E-3}]
["Multi-Family (2-4 units)",10340,"West North Central","1980s","Wood","built-in electric unit","window/wall unit",8.2197712839102319,10619.859539999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3539.95318},null,132.63079922254411,"Metropolitan Area",0.14129833564509217,0.11527857530669999,4.2488252643418196E-3,0,0.19171055400484316,0.45253629022097713,0,0,{"$f":"T341*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U341*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14129833564509217},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.2488252643418196E-3}]
["Mobile Home",10341,"East South Central","1990s","Siding","heat pump","central AC",46.557631975542066,39826.887920000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39826.887920000001},"Mixed-Humid",499.1921248483996,"Metropolitan Area",0.79311949626360223,0.29712252329397204,0.1685073636550804,1.3499602448699442E-2,0.44449407614501191,1.7032434593576664,188.21299999999999,150.744,{"$f":"T342*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4959380560869603E-3},{"$f":"U342*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0036643926124804E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80061543431968918},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17451102804769289}]
["Single Family Attached",10342,"Pacific","Before 1950","Wood","N/A","N/A",6.1023042906348595,11623.436739999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11623.436739999999},"Marine",41.100472327018792,"Metropolitan Area",0,0.42970885531905267,0,0,0.15896380625456738,0.58867266157362008,0,0,{"$f":"T343*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U343*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",10343,"West South Central","2000s","Siding","heat pump","central AC",36.015213863651567,16490.482540000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16490.482540000001},"Mixed-Humid",463.89816724381126,"Metropolitan Area",0.30125120227047247,0.54836644253919797,0.18225975552522936,1.2139237855065441E-2,1.1372340049111125,2.1691114052460123,262.68900000000002,473.447,{"$f":"T344*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3318683679500602E-3},{"$f":"U344*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8073694871153808E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30558307063842255},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19006712501234474}]
["Single Family Detached",10344,"East North Central","1950s","Siding","built-in electric unit","window/wall unit",25.246838171234039,21039.03181,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21039.03181},"Cold/Very Cold",383.81097572601448,"Metropolitan Area",0.72296056825646315,0.20054118990459383,4.7946291411477007E-2,0,0.33811504020761146,1.3095630897801454,0,0,{"$f":"T345*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U345*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.72296056825646315},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7946291411477007E-2}]
["Mobile Home",10345,"Pacific","1970s","Siding","portable electric heaters","window/wall unit",5.9217748918034507,7959.374855,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7959.374855},"Marine",89.625298887459181,"Metropolitan Area",0.11899509761033049,9.5014559769071208E-2,5.5455750395984249E-3,0,8.6246281606932373E-2,0.30580151402593247,0,0,{"$f":"T346*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U346*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11899509761033049},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5455750395984249E-3}]
["Single Family Detached",10346,"West South Central","1950s","Shingle","central furnace","central AC",29.910905513615592,21138.449130000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21138.449130000001},"Hot-Humid",147.53140887910473,"Metropolitan Area",0.21226835327347274,0.17480294652754502,0.37605518728296039,2.611731488428368E-2,0.11897165191640652,0.88209813900038458,395.03199999999998,840.50400000000002,{"$f":"T347*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3503638367221598E-3},{"$f":"U347*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7766951047561524E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2206187171101949},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.39382213833052193}]
["Mobile Home",10347,"South Atlantic","1990s","Concrete","heat pump","central AC",21.257648845889797,19719.525829999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19719.525829999999},"Hot-Humid",225.38562197488056,"Metropolitan Area",6.4606313415321637E-2,0.37425960202213449,0.20313533162671923,8.4619048874887901E-3,0.12701449128637313,0.76901573835054848,59.009,370.10399999999998,{"$f":"T348*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1636294997024699E-3},{"$f":"U348*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.2982753877863194E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.576994291502411E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21043360701450556}]
["Single Family Detached",10348,"Mountain South","1990s","Stucco","heat pump","central AC",33.429096470649995,17809.85427,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17809.85427},"Hot-Dry/Mixed-Dry",187.48935831206029,"Metropolitan Area",7.5242644883393522E-2,0.14180368039447858,0.17295872561680362,1.0102746693783119E-2,0.48206322588417505,0.87206827677885079,71.28,495.976,{"$f":"T349*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2694864123656E-3},{"$f":"U349*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8332602814175203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.6512131295759123E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18179198589822113}]
["Multi-Family (2-4 units)",10349,"Pacific","Before 1950","Siding","N/A","N/A",21.148410212978735,33252.217320000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11084.072440000002},"Marine",114.85206128630745,"Metropolitan Area",0,0.65974161530397968,0,0,0.49909034402695035,1.15883195933093,0,0,{"$f":"T350*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U350*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10350,"West North Central","Before 1950","Wood","central furnace","central AC",36.816319014617164,21759.053790000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21759.053790000002},"Cold/Very Cold",252.90752756553351,"Metropolitan Area",1.1197156641014367,0.76464946604137563,6.549940834541107E-2,2.052507609051531E-2,0.71449645722540567,2.6643609957136292,812.72299999999996,130.566,{"$f":"T351*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7684083473370173E-2},{"$f":"U351*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8409926171451402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.137399747574807},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.8340400962556211E-2}]
["Single Family Detached",10351,"East North Central","1950s","Siding","central furnace","central AC",36.494188886911282,19370.58858,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19370.58858},"Cold/Very Cold",208.12448027496265,"Metropolitan Area",0.5024256679349447,0.25228105413059937,0.14503054102792418,3.6475999902043379E-2,0.5355530160773978,1.4352902791708659,1524.845,358.21600000000001,{"$f":"T352*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9537145143270101E-2},{"$f":"U352*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9388547587732807E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5319628130782148},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15196939578669746}]
["Single Family Detached",10352,"West North Central","1990s","Siding","central furnace","central AC",60.247087616356453,14730.33927,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14730.33927},"Mixed-Humid",320.07523267163066,"Metropolitan Area",1.2411742182041865,0.43112021931506433,0.1993593805564311,4.5519561839100567E-2,0.89032341799888393,2.761977236074566,2315.8609999999999,774.33,{"$f":"T353*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.411341823216147E-2},{"$f":"U353*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1406143606939102E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2752876364363479},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21076552416337019}]
["Single Family Detached",10353,"East North Central","1970s","Brick","central furnace","central AC",18.037633047378325,14338.341060000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14338.341060000001},"Cold/Very Cold",51.275628214141939,"Metropolitan Area",0.8190281223924325,0.13553719794348787,6.5905381735190643E-2,2.4353256478519263E-2,0.10691663609039688,1.1273873381615078,1517.8989999999999,180.572,{"$f":"T354*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1764153556632939E-2},{"$f":"U354*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5891029218863201E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84079227594906547},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.8494484657076971E-2}]
["Single Family Detached",10354,"South Atlantic","1980s","Wood","central furnace","central AC",82.167063938824569,32906.313150000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32906.313150000002},"Mixed-Humid",657.29393074137863,"Metropolitan Area",0.76474590951837562,0.52154077856839542,0.41080616468429915,5.7426485300035655E-2,1.9241545084591047,3.621247361230175,1084.788,660.36300000000006,{"$f":"T355*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5696373629362205E-2},{"$f":"U355*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1730111670673451E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.8004422831477378},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4325362763549726}]
["Single Family Attached",10355,"East North Central","2010s","Brick","central furnace","central AC",7.9746962363865199,9968.3702950000006,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9968.3702950000006},"Cold/Very Cold",139.57007323955617,"Metropolitan Area",0.28655109148791946,6.9515058259511084E-2,1.490504618967403E-2,5.120741852171205E-3,0.10524190673256731,0.47621310266967187,451.678,62.021000000000001,{"$f":"T356*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5024935581050108E-3},{"$f":"U356*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1824829406619507E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29105358504602447},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5523294483740225E-2}]
["Single Family Detached",10356,"South Atlantic","1970s","Brick","central furnace","central AC",30.701994427100018,17685.480660000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17685.480660000001},"Mixed-Humid",89.178240385312577,"Metropolitan Area",0.34081263559802094,0.21619621138461198,3.7463560448133176E-2,9.2260554378248393E-3,0.27488625711597087,0.86935866454673705,400.67,121.004,{"$f":"T357*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0860415360422006E-3},{"$f":"U357*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1400139017826404E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34789867713406314},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9603574349915814E-2}]
["Single Family Detached",10357,"South Atlantic","2000s","Stucco","heat pump","central AC",23.227135946987403,16242.752409999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16242.752409999999},"Hot-Humid",262.80667822267105,"Metropolitan Area",1.5463814975426038E-2,0.16118251712777348,0.30246456018758672,1.4564063948426497E-2,0.41758549020502422,0.89669638249581052,16.021000000000001,880.62900000000002,{"$f":"T358*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6022513636060997E-4},{"$f":"U358*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.430383881206589E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5724040111786648E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31676839899965259}]
["Single Family Detached",10358,"Mountain South","1970s","Stucco","central furnace","central AC",14.312334392489634,7946.88195,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7946.88195},"Cold/Very Cold",18.989869108435997,"Metropolitan Area",7.0527091239325365E-2,6.4358943982429945E-2,1.5403600221324001E-2,8.1593021045234997E-4,6.1592888675857368E-2,0.21188252411893665,75.103999999999999,27.568999999999999,{"$f":"T359*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9684262197279997E-4},{"$f":"U359*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1908758847955E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.1123933861298172E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.562268780980355E-2}]
["Multi-Family (5+ units)",10359,"Mountain South","1970s","Stucco","central furnace","central AC",29.792308402473669,28292.790509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2250.4490855351874},"Hot-Dry/Mixed-Dry",357.3846837765654,"Metropolitan Area",5.5738404068156236E-2,0.57163837560280539,0.21421882480411333,1.073620862924868E-2,0.36791874047227707,1.2193965801630109,32.295000000000002,347.173,{"$f":"T360*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.267825321735889E-5},{"$f":"U360*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8129516037250769E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.5811082321373592E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21500011996448584}]
["Mobile Home",10360,"South Atlantic","1980s","Siding","central furnace","window/wall unit",11.396698352761176,14611.15173,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14611.15173},"Mixed-Humid",326.24251532566603,"Metropolitan Area",0.39161963147732665,0.54073540612913895,3.4906304483701141E-2,4.7085459230546108E-3,0.14587810415111316,1.1131394462412798,322.25700000000001,0,{"$f":"T361*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7085459230546108E-3},{"$f":"U361*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39632817740038123},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4906304483701141E-2}]
["Single Family Attached",10361,"Pacific","1950s","Stucco","N/A","N/A",11.561461917396043,11084.81488,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11084.81488},"Hot-Dry/Mixed-Dry",64.086435992207441,"Metropolitan Area",0,0.32598614893069261,0,0,0.21866292692327316,0.54464907585396571,0,0,{"$f":"T362*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U362*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10362,"South Atlantic","2000s","Brick","central furnace","central AC",52.36212607040374,13012.45678,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13012.45678},"Mixed-Humid",130.30674216427016,"Metropolitan Area",0.45500777337228371,0.22048011385263097,0.21030952558355584,2.2928937793075282E-2,0.24382909375056469,1.1296265065590354,1064.818,697.25800000000004,{"$f":"T363*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3855898203566041E-2},{"$f":"U363*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0730395895092415E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.46886367157584974},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21938256517306509}]
["Single Family Detached",10363,"West South Central","2000s","Brick","central furnace","central AC",35.598613828355468,22530.768250000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22530.768250000001},"Mixed-Humid",237.05414354442752,"Rural",0.54409365241548524,0.41357126719715304,0.20058645042996676,2.3703404614339497E-2,0.59387193765631796,1.7521233076989231,637.80999999999995,414.23599999999999,{"$f":"T364*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.43703492975325E-2},{"$f":"U364*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.3330553168070006E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55846400171301769},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20991950574677376}]
["Multi-Family (5+ units)",10364,"South Atlantic","1970s","Brick","central furnace","N/A",42.022756644999184,43411.938679999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3453.047788594241},"Mixed-Humid",510.95851829714917,"Metropolitan Area",0.46686040088479941,0.29215197186305547,0,6.3107067020342399E-3,0.97860234058984319,1.7434234573887999,145.36799999999999,0,{"$f":"T365*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0196265093236758E-4},{"$f":"U365*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4673623635357318},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10365,"Pacific","1980s","Siding","central furnace","both central and individual units",15.818166052129945,10325.17366,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10325.17366},"Cold/Very Cold",258.88784948940616,"Micropolitan Area",0.4551623279400539,0.20932994818873035,6.8908577629401724E-2,8.6054953365796803E-3,0.1499244745428667,0.8833253283010527,776.87699999999995,56.570999999999998,{"$f":"T366*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0213899374598201E-3},{"$f":"U366*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8410539911986001E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.46318371787751372},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9492683028521587E-2}]
["Single Family Detached",10366,"New England","Before 1950","Siding","central furnace","window/wall unit",30.229899388402728,11437.72205,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11437.72205},"Cold/Very Cold",73.762212657128572,"Metropolitan Area",1.0207299492784727,0.10761512484681952,6.3727544508262943E-2,1.82504639364179E-2,0.16969865693850375,1.361771275572059,1595.6379999999999,0,{"$f":"T367*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.82504639364179E-2},{"$f":"U367*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0389804132148905},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.3727544508262943E-2}]
["Single Family Detached",10367,"South Atlantic","1960s","Siding","central furnace","central AC",156.19372268577985,25274.065159999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25274.065159999998},"Cold/Very Cold",346.09804402944616,"Micropolitan Area",1.4711333743512374,0.3842973166670926,0.17276001308296457,8.2783835632061348E-2,0.93800985135981008,2.9662005554611044,2774.252,501.19400000000002,{"$f":"T368*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0116625818260309E-2},{"$f":"U368*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2667209813801039E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5412500001694978},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18542722289676561}]
["Mobile Home",10368,"South Atlantic","1960s","Siding","heater burning gas/oil/kerosene","window/wall unit",23.880806808979983,20498.546620000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20498.546620000001},"Mixed-Humid",122.45368481931983,"Micropolitan Area",0.95961115152241783,8.7997493335866303E-2,8.5200466649567305E-2,0,0.24774754579962183,1.3805566573074732,0,0,{"$f":"T369*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U369*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95961115152241783},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5200466649567305E-2}]
["Multi-Family (2-4 units)",10369,"Middle Atlantic","1950s","Concrete","central furnace","window/wall unit",112.4109549138345,55103.409269999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18367.803089999998},"Mixed-Humid",369.07051255038351,"Metropolitan Area",2.9379951446362416,2.3647068788616408,0.56320902566797859,8.0107352673992271E-2,0.6159522457121267,6.535268196660649,1453.7639999999999,0,{"$f":"T370*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6702450891330755E-2},{"$f":"U370*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9646975955275723},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.56320902566797859}]
["Single Family Detached",10370,"Mountain South","1950s","Stucco","central furnace","N/A",155.16510055108725,57298.781589999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":57298.781589999999},"Hot-Dry/Mixed-Dry",222.08027935887,"Metropolitan Area",2.7481246837590647,0.46730210411703749,0.19902989629803655,6.3645710327942709E-2,0.49506233241932346,3.9095190165934621,1110.769,0,{"$f":"T371*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3645710327942709E-2},{"$f":"U371*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8117703940870076},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19902989629803655}]
["Single Family Detached",10371,"East North Central","1960s","Wood","central furnace","central AC",38.769990112804784,20150.72251,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20150.72251},"Cold/Very Cold",129.07901972755769,"Metropolitan Area",0.95551252157859279,0.30655187355633695,0.13961956039983259,5.2866125780272846E-2,0.25455837481435967,1.656242330349122,2294.692,328.84300000000002,{"$f":"T372*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6239701737916916E-2},{"$f":"U372*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6264240423559301E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0017522233165097},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1462459844421885}]
["Single Family Detached",10372,"East North Central","2000s","Siding","central furnace","window/wall unit",63.992591122231119,18553.955089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18553.955089999999},"Cold/Very Cold",381.04257578349103,"Metropolitan Area",2.2585120775790495,0.26292509183966539,4.8583086108242843E-2,4.125401409232158E-2,0.36024238602035902,2.930262641547317,2223.462,0,{"$f":"T373*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.125401409232158E-2},{"$f":"U373*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2997660916713709},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.8583086108242843E-2}]
["Multi-Family (2-4 units)",10373,"Pacific","1970s","Wood","N/A","window/wall unit",18.40325218715817,24835.697960000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8278.5659866666665},"Hot-Dry/Mixed-Dry",86.097467069746102,"Metropolitan Area",0,0.61044195983390137,6.6135774840018716E-2,0,0.32683125336503649,1.0034089880389567,0,0,{"$f":"T374*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U374*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6135774840018716E-2}]
["Multi-Family (5+ units)",10374,"West South Central","1970s","Brick","central furnace","central AC",45.658378213974508,45476.472320000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3617.2637516874706},"Mixed-Humid",281.64788984835559,"Metropolitan Area",0.16490671118486394,0.35048708121729533,8.591446912287079E-2,7.0862803463193607E-3,0.35315172963641345,0.96098261861818357,69.956000000000003,85.867000000000004,{"$f":"T375*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5304930301304872E-4},{"$f":"U375*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1060358656614804E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16515976048787698},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.622507270943694E-2}]
["Single Family Detached",10375,"West North Central","Before 1950","Stucco","central furnace","N/A",7.9783891856209124,9670.77477,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9670.77477},"Cold/Very Cold",21.84686045293185,"Micropolitan Area",0.3975682972947347,2.239872321416625E-2,0,5.6960379856561497E-3,4.6446710028383076E-2,0.46641373053728397,588.995,0,{"$f":"T376*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6960379856561497E-3},{"$f":"U376*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.40326433528039085},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10376,"East North Central","1990s","Siding","central furnace","central AC",117.45404128866161,20070.752100000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20070.752100000002},"Cold/Very Cold",218.15783570482404,"Metropolitan Area",1.5353496740544228,0.47477596913274367,9.2725951447403407E-2,0.113423232144957,0.5431809057324426,2.6460325003670127,5403.2709999999997,247.899,{"$f":"T377*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.1084477127701191},{"$f":"U377*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9755193748379006E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6437973868245419},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.7701470822241301E-2}]
["Multi-Family (2-4 units)",10377,"New England","Before 1950","Brick","built-in electric unit","window/wall unit",109.17066065829154,49623.027569999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16541.009190000001},"Cold/Very Cold",862.84520342107874,"Rural",1.5654300603474609,0.54540148560397517,6.2433460252333345E-2,0,0.77076997346919063,2.9440349796729599,0,0,{"$f":"T378*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U378*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5654300603474609},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2433460252333345E-2}]
["Single Family Detached",10378,"West South Central","Before 1950","Siding","heater burning gas/oil/kerosene","window/wall unit",42.021248132273264,13399.6327,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13399.6327},"Hot-Humid",283.64078516520357,"Metropolitan Area",0.57361111483151705,0.19890934685628761,0.44188100071190456,0,0.5528176452054534,1.7672191076051627,0,0,{"$f":"T379*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U379*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.57361111483151705},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.44188100071190456}]
["Multi-Family (5+ units)",10379,"South Atlantic","1980s","Concrete","N/A","central AC",29.051333141940226,25823.40724,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2054.0308029397252},"Hot-Humid",515.79340493790107,"Metropolitan Area",0,0.29815228266270061,0.45071172064503567,2.1051060818197322E-2,0.99164644323833928,1.759887075831932,0,815.19299999999998,{"$f":"T380*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U380*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6744315323408432E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.45238615217737654}]
["Single Family Detached",10380,"Middle Atlantic","Before 1950","Wood","central furnace","central AC",183.70396501891375,29909.47005,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29909.47005},"Cold/Very Cold",235.76250428334311,"Metropolitan Area",2.4894216015220141,0.82156379164791749,0.15248831853054648,0.11297970316269945,0.66902962189978499,4.1325033336002628,3493.5619999999999,283.827,{"$f":"T381*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.1044905880068181},{"$f":"U381*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4891151558813497E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5939121895288322},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16097743368642783}]
["Multi-Family (5+ units)",10381,"West North Central","1980s","Brick","radiator","central AC",8.9656839253298823,9047.1078959999995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":719.61992169330813},"Cold/Very Cold",37.132307305313091,"Metropolitan Area",8.5138107051989875E-2,0.14317444508745844,1.8556913915582569E-2,1.3074699389141278E-3,0.1068954248120958,0.35496836277419752,55.04,89.477999999999994,{"$f":"T382*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9607880489999679E-5},{"$f":"U382*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4390151353273812E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.5177714932479873E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8621304066935844E-2}]
["Single Family Detached",10382,"Mountain North","1990s","Stucco","radiator","window/wall unit",23.836138648337581,19764.625739999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19764.625739999999},"Cold/Very Cold",271.11073887463505,"Micropolitan Area",0.20222261813771683,0.29490505550193047,1.1196581423207039E-2,1.0518536172570601E-3,0.41670554985596747,0.92502980491882181,53.219000000000001,0,{"$f":"T383*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0518536172570601E-3},{"$f":"U383*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2032744717549739},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1196581423207039E-2}]
["Single Family Detached",10383,"Middle Atlantic","1960s","Siding","radiator","window/wall unit",41.779757403927043,16377.79592,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16377.79592},"Mixed-Humid",107.33689719811898,"Metropolitan Area",1.4711349616689386,0.34516558661791874,3.5775673785443919E-2,1.2175908598764799E-3,0.32924024368800447,2.1813164657603057,74.343999999999994,0,{"$f":"T384*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2175908598764799E-3},{"$f":"U384*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.472352552528815},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5775673785443919E-2}]
["Single Family Attached",10384,"Pacific","2000s","Stucco","central furnace","central AC",12.579048540992396,9373.3595690000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9373.3595690000002},"Hot-Dry/Mixed-Dry",48.834856537834845,"Metropolitan Area",4.991707651594398E-2,8.8766015065936205E-2,4.725117120084598E-2,4.7669344891297779E-3,0.12556915227647722,0.31150341505920337,276.39499999999998,232.167,{"$f":"T385*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5907497180737552E-3},{"$f":"U385*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1761847710560231E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.2507826234017736E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.9427355971902003E-2}]
["Multi-Family (5+ units)",10385,"Middle Atlantic","1950s","Brick","heater burning gas/oil/kerosene","N/A",7.8141287218088245,10418.838299999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":828.72932298023738},"Mixed-Humid",15.835936147366736,"Metropolitan Area",0.36749711948777103,3.1785666859580397E-2,0,0,0.16521954142859088,0.56450232777594234,0,0,{"$f":"T386*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U386*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36749711948777103},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",10386,"West North Central","Before 1950","Stucco","radiator","window/wall unit",18.146223568614818,12707.439469999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4235.8131566666661},"Cold/Very Cold",108.74279504254011,"Metropolitan Area",0.34256553091582098,0.27511351033016651,1.8849631167582377E-2,1.8424262338763598E-3,0.43899093707439102,1.0767478936438784,144.988,0,{"$f":"T387*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1414207795878659E-4},{"$f":"U387*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34317967299377977},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8849631167582377E-2}]
["Single Family Detached",10387,"Pacific","1990s","Stucco","central furnace","central AC",67.686353768902549,28802.703730000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28802.703730000001},"Hot-Dry/Mixed-Dry",156.82113051739123,"Metropolitan Area",0.37137633015657773,0.39294877757734703,0.2783868299669765,2.2501075391728218E-2,0.38572773813331007,1.4284396758342113,274.23599999999999,506.97800000000001,{"$f":"T388*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8987382601002805E-3},{"$f":"U388*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4602337131627941E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37927506841667802},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.29298916709860445}]
["Multi-Family (5+ units)",10388,"Pacific","1960s","Wood","N/A","N/A",23.556781481891651,36692.806049999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2918.59835429653},"Hot-Dry/Mixed-Dry",69.422789040091899,"Metropolitan Area",0,0.20582774514538421,0,0,0.26159593019817956,0.46742367534356377,0,0,{"$f":"T389*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U389*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10389,"Pacific","2010s","Stucco","built-in electric unit","central AC",24.529596371976837,18611.22638,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1480.3636061545685},"Hot-Dry/Mixed-Dry",153.15488997541084,"Metropolitan Area",7.4847447735373024E-2,0.42349884711265395,7.4433907904720403E-2,3.4884510502144394E-3,0.44048283813657152,1.0164740155459229,0,187.43799999999999,{"$f":"T390*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U390*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7747639361039999E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.4847447735373024E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.471138429833081E-2}]
["Single Family Detached",10390,"Mountain North","1980s","Brick","central furnace","central AC",27.002753045347266,21811.59374,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21811.59374},"Cold/Very Cold",304.02547972593885,"Metropolitan Area",1.3772909491761136,0.55250651465119138,3.8177159697028104E-2,1.3479434061757559E-2,1.4346574473789377,3.4026320709032709,541.20899999999995,76.784999999999997,{"$f":"T391*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.180463083643166E-2},{"$f":"U391*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6748032253259E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3890955800125453},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9851962922354003E-2}]
["Single Family Detached",10391,"West South Central","Before 1950","Wood","heater burning gas/oil/kerosene","window/wall unit",25.037094100909595,16385.532790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16385.532790000001},"Hot-Humid",277.87320574697782,"Rural",1.1454209366784727,0.12043794263055821,0.35843980544030862,0,0.22675152322507094,1.8510502079744104,0,0,{"$f":"T392*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U392*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1454209366784727},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35843980544030862}]
["Single Family Detached",10392,"South Atlantic","1970s","Siding","heat pump","central AC",79.728723783079673,31968.213220000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31968.213220000001},"Mixed-Humid",487.80549108868951,"Metropolitan Area",0.42775502466720799,0.28925152609945559,0.17433788355815272,1.7084772191164603E-2,0.77304791546057305,1.6643923497853894,273.55599999999998,260.87400000000002,{"$f":"T393*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7450965356103208E-3},{"$f":"U393*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3396756555542823E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43650012120281834},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18267755921370699}]
["Single Family Detached",10393,"East North Central","1970s","Siding","central furnace","N/A",16.296726259796078,18372.859369999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18372.859369999998},"Cold/Very Cold",165.90607494537841,"Metropolitan Area",1.9201647297550699,0.15706084764592923,0,1.9602756949087169E-2,0.32964255407471321,2.4068681314757123,1066.941,0,{"$f":"T394*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9602756949087169E-2},{"$f":"U394*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.939767486704157},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10394,"East South Central","1980s","Siding","heat pump","central AC",20.450148869736587,15148.25842,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15148.25842},"Mixed-Humid",173.96397821007562,"Metropolitan Area",0.20015618044570618,8.1413451427560055E-2,0.11388956028206333,8.5742778239220815E-3,0.19810589396507591,0.59356508612040559,225.48500000000001,340.53899999999999,{"$f":"T395*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4157050498336999E-3},{"$f":"U395*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1585727740883804E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20357188549553989},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11904813305615171}]
["Multi-Family (5+ units)",10395,"Pacific","1990s","Stucco","heater burning gas/oil/kerosene","window/wall unit",17.576221559086637,35222.888899999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2801.6790385839004},"Hot-Dry/Mixed-Dry",144.69562758462507,"Metropolitan Area",0.10654747777805498,0.59612083657426929,3.6459388414834502E-2,0,0.7197505348966019,1.4588782376637606,0,0,{"$f":"T396*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U396*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10654747777805498},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6459388414834502E-2}]
["Single Family Detached",10396,"Mountain North","1950s","Brick","central furnace","central AC",35.155085945038202,26040.804400000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26040.804400000001},"Cold/Very Cold",155.66244987270696,"Metropolitan Area",2.9930464146722673,5.9237022910618803E-2,8.2323602214656413E-2,6.5893651453759992E-3,0.38437289759219501,3.5189799373897377,199.179,53.860999999999997,{"$f":"T397*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1867813795875998E-3},{"$f":"U397*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4025837657884001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9982331960518547},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.3726185980444817E-2}]
["Single Family Detached",10397,"East North Central","2000s","Siding","central furnace","central AC",33.070484596722501,13228.19384,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13228.19384},"Mixed-Humid",188.82479469485904,"Micropolitan Area",0.67840479923065378,0.52375532109479161,5.8883796864662233E-2,1.091870993386208E-2,0.55383119394509861,1.8148751111352062,626.58199999999999,198.83,{"$f":"T398*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2885481526548798E-3},{"$f":"U398*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6301617812072003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.68669334738330867},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1513958645869435E-2}]
["Single Family Detached",10398,"West South Central","1960s","Brick","central furnace","central AC",57.412897785749827,23763.61663,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23763.61663},"Hot-Humid",425.30500371401513,"Metropolitan Area",1.1869153238599859,0.21453265541274816,0.78669733264291231,5.6678245569963551E-2,0.43530402062660362,2.6234493325422497,614.66300000000001,1770.422,{"$f":"T399*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.460661588864569E-2},{"$f":"U399*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2071629681317856E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2015219397486316},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.82876896232423014}]
["Mobile Home",10399,"East South Central","1980s","Siding","central furnace","both central and individual units",27.964446524859355,19206.350640000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19206.350640000001},"Mixed-Humid",468.38995929031393,"Rural",0.85559308053208927,0.1233742020663636,0.25335233494313547,1.6856011893131278E-2,0.36582689460859752,1.5981465121501859,575.07600000000002,302.55099999999999,{"$f":"T400*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1045111300648641E-2},{"$f":"U400*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8109005924826393E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.86663819183273794},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2591632355356181}]
["Single Family Detached",10400,"Pacific","2000s","Stucco","central furnace","central AC",71.072785412585091,25025.628669999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25025.628669999998},"Hot-Dry/Mixed-Dry",432.81824778544336,"Metropolitan Area",0.29412353601624225,0.43271564277010299,0.28214717105741238,2.1084968051478449E-2,0.958292734667056,1.9672790845108137,219.869,622.66600000000005,{"$f":"T401*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.50235995004423E-3},{"$f":"U401*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.558260810143422E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29962589596628647},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.29772977915884657}]
["Mobile Home",10401,"Pacific","1990s","Siding","central furnace","N/A",17.514254387455676,15229.78642,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15229.78642},"Hot-Dry/Mixed-Dry",82.865267932301165,"Metropolitan Area",0.23528716349182449,0.29727212008506892,0,3.1419506278052602E-3,0.27956857468665469,0.81212785826354816,206.303,0,{"$f":"T402*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1419506278052602E-3},{"$f":"U402*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23842911411962975},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10402,"East North Central","1970s","Brick","radiator","window/wall unit",14.150265458986869,13438.048870000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1068.8816566248508},"Cold/Very Cold",48.969298246205085,"Metropolitan Area",0.31301804011403056,0.24628230645807223,2.1178391895217738E-2,1.769136603199031E-2,0.13051617617669833,0.72727908407960107,1316.5129999999999,0,{"$f":"T403*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4071965964081523E-3},{"$f":"U403*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3144252367104387},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1178391895217738E-2}]
["Mobile Home",10403,"Middle Atlantic","1970s","Brick","heater burning gas/oil/kerosene","central AC",35.80220017833993,42621.666879999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":42621.666879999997},"Cold/Very Cold",394.42018072970791,"Metropolitan Area",1.5465496017375786,0.71420564584813173,7.5122946824344644E-2,2.4818596624223994E-3,0.5564330641801023,2.8923112585901576,0,58.23,{"$f":"T404*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U404*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4818596624223994E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5465496017375786},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.7604806486767042E-2}]
["Single Family Detached",10404,"East North Central","1960s","Siding","central furnace","central AC",107.10258240591772,19256.12772,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19256.12772},"Cold/Very Cold",231.31253975617312,"Metropolitan Area",2.3652964474392126,0.47005992807559643,0.1403910354907584,5.6605909985671318E-2,0.50353705272711513,3.4792844637326827,2482.7289999999998,456.90199999999999,{"$f":"T405*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7807746718147873E-2},{"$f":"U405*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7981632675234404E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4131041941573605},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14918919875828185}]
["Single Family Detached",10405,"Mountain South","1980s","Stucco","heat pump","central AC",7.9126215329755034,10750.84447,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10750.84447},"Hot-Dry/Mixed-Dry",150.68487898162141,"Metropolitan Area",3.6375632776067576E-2,0.13986671266536244,0.18192826281556809,7.9724284777066105E-3,0.15596618826594322,0.51413679652294131,52.521000000000001,689.04200000000003,{"$f":"T406*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6464510240887002E-4},{"$f":"U406*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4077833752977402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.6940277878476445E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18933604619086583}]
["Single Family Detached",10406,"East North Central","1950s","Brick","central furnace","central AC",76.929103945921298,33389.368029999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33389.368029999998},"Cold/Very Cold",198.0424587768033,"Metropolitan Area",3.3578876400021551,9.1231673462346702E-2,7.4166100347269462E-2,3.2852567160181687E-2,0.51630837891547343,4.0395937927272447,865.80499999999995,118.11799999999999,{"$f":"T407*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8908681787214147E-2},{"$f":"U407*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9438853729675391E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.3867963217893693},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.8109985720237002E-2}]
["Single Family Detached",10407,"East North Central","2010s","Concrete","radiator","window/wall unit",26.50263464515789,18468.734939999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18468.734939999998},"Mixed-Humid",130.69117711732341,"Rural",0.62658882571558483,0.15834661169158401,8.003141867730923E-2,2.4360261385859999E-3,0.36345081513052485,1.228417671215003,131.9,0,{"$f":"T408*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4360261385859999E-3},{"$f":"U408*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62902485185417079},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.003141867730923E-2}]
["Multi-Family (5+ units)",10408,"South Atlantic","2010s","Concrete","heat pump","central AC",10.82482596870434,14375.598900000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1143.4557290165878},"Hot-Humid",129.63961086348834,"Metropolitan Area",8.3254691074825652E-4,9.2082812500356603E-2,6.2553851310456127E-2,2.7841366145619001E-3,0.28429847099749289,0.44233036411912141,0.92900000000000005,192.74199999999999,{"$f":"T409*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0622703722564101E-6},{"$f":"U409*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2039194412211516E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.3360918112051292E-4},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2774243254578241E-2}]
["Single Family Detached",10409,"East North Central","1990s","Brick","central furnace","central AC",21.165859029838465,14698.513220000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14698.513220000001},"Cold/Very Cold",110.29133750443334,"Metropolitan Area",1.2350017996348277,9.9464206923671541E-2,3.1898301831673845E-2,1.106861249072846E-2,0.20819221059830118,1.574556518988474,654.81299999999999,98.23,{"$f":"T410*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6247775371278606E-3},{"$f":"U410*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4438349536006001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2446265771719556},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3342136785274444E-2}]
["Single Family Detached",10410,"Middle Atlantic","2010s","Siding","wood-burning stove","N/A",47.80786137608527,12935.02743,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12935.02743},"Cold/Very Cold",239.78559328791911,"Micropolitan Area",0.22521865695335019,0.20086397936185696,0,0,0.41945349943246935,0.8455361357476765,0,0,{"$f":"T411*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U411*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22521865695335019},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10411,"South Atlantic","1980s","Stucco","N/A","central AC",20.920210727362186,16408.008409999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16408.008409999999},"Hot-Humid",155.78540927487165,"Metropolitan Area",0,6.9910487464941135E-2,0.28797122920897489,1.38659156670387E-2,0.22314098930793799,0.58102270598185402,0,845.07,{"$f":"T412*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U412*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.38659156670387E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3018371448760136}]
["Multi-Family (5+ units)",10412,"South Atlantic","1980s","Wood","central furnace","central AC",35.903245242844591,34756.287750000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2764.5649147241129},"Mixed-Humid",168.25518898413421,"Metropolitan Area",8.9782769584126662E-2,0.15750399175175475,0.12780755060881754,6.8209909835130009E-3,0.19271395332575542,0.57408670486032298,30.768999999999998,165.483,{"$f":"T413*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.5062897861146224E-5},{"$f":"U413*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5748849578329038E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.9867832481987805E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12826503910460083}]
["Multi-Family (5+ units)",10413,"West South Central","Before 1950","Brick","central furnace","central AC",33.362222219978179,33563.603840000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2669.6971280473849},"Hot-Humid",461.72093837269915,"Metropolitan Area",0.39693025742318394,0.43095818366777283,0.20601360662086959,1.5592844817571843E-2,0.52713724130518469,1.5753918566216232,189.86199999999999,274.714,{"$f":"T414*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0687403612533258E-4},{"$f":"U414*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3340317683440919E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39743713145930926},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.206747009797704}]
["Single Family Detached",10414,"West South Central","1970s","Brick","central furnace","central AC",14.551406546280175,12426.47869,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12426.47869},"Mixed-Humid",63.64163899408436,"Micropolitan Area",0.50626711860337514,0.16823329703699746,7.5624989452729857E-2,1.260549454200814E-2,0.14911612883777034,0.89924153393087292,741.44899999999996,272.95699999999999,{"$f":"T415*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.2136001982218094E-3},{"$f":"U415*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.39189434378633E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.51548071880159696},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9016883796516182E-2}]
["Single Family Detached",10415,"Mountain South","1960s","Concrete","central furnace","central AC",4.9555243417002313,7463.1390689999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7463.1390689999998},"Hot-Dry/Mixed-Dry",85.827345635719468,"Metropolitan Area",9.1425035780732633E-2,0.13600023844523496,8.5387595094361834E-2,5.4428300073263549E-3,0.19728560352684416,0.51009847284717358,273.34800000000001,455.947,{"$f":"T416*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0400341382330119E-3},{"$f":"U416*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.402795869093343E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.3465069918965651E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.8790390963455174E-2}]
["Mobile Home",10416,"West South Central","2000s","Concrete","central furnace","central AC",45.675794078265916,35135.226210000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35135.226210000001},"Mixed-Humid",432.69031082603436,"Metropolitan Area",0.68173582119787202,0.33577484874843927,0.19751119846001419,1.7260636633603232E-2,0.96228916194044756,2.1773110303467731,282.70800000000003,208.55500000000001,{"$f":"T417*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9330095313766801E-3},{"$f":"U417*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3276271022265508E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.69166883072924867},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20483882556224076}]
["Single Family Detached",10417,"East North Central","Before 1950","Siding","radiator","central AC",95.183113001658967,17918.507720000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17918.507720000001},"Cold/Very Cold",89.825479193771912,"Metropolitan Area",2.3765671037933629,2.5118307469957763E-2,1.2498553341869841E-2,1.4909631903657601E-3,0.2095473793022766,2.6237313439074672,13.693,69.515000000000001,{"$f":"T418*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4535812620996001E-4},{"$f":"U418*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2456050641558001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.376812461919573},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3744158406025641E-2}]
["Single Family Detached",10418,"Middle Atlantic","1990s","Brick","central furnace","central AC",60.709237424331626,17709.812549999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17709.812549999999},"Cold/Very Cold",724.26208796290371,"Metropolitan Area",0.91687207885216138,0.68340555037507944,8.4805757381119035E-2,3.4990569471351145E-2,1.5983753120023698,3.2834586986107297,1703.8019999999999,271.971,{"$f":"T419*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0174014042315095E-2},{"$f":"U419*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8165554290360499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.9470460928944765},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.9622312810155091E-2}]
["Single Family Detached",10419,"East North Central","1980s","Siding","wood-burning stove","central AC",83.306897303318451,25290.497060000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25290.497060000002},"Cold/Very Cold",177.603577778458,"Metropolitan Area",0,0.57738262956123243,8.6223397436599208E-2,4.8660939583204795E-3,0.51976005292581073,1.1833660799236423,0,192.40799999999999,{"$f":"T420*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U420*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8660939583204795E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.1089491394919689E-2}]
["Single Family Detached",10420,"Pacific","Before 1950","Siding","fireplace","window/wall unit",42.076219503992505,18902.165099999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18902.165099999998},"Marine",358.30428127122968,"Micropolitan Area",0.27118424020295789,0.34260945452086072,1.6681009483429196E-2,0,0.59205947493338107,1.2225341791406288,0,0,{"$f":"T421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27118424020295789},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6681009483429196E-2}]
["Multi-Family (2-4 units)",10421,"South Atlantic","1970s","Brick","central furnace","central AC",30.533875677043728,29615.7863,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9871.928766666666},"Mixed-Humid",170.02958961533034,"Metropolitan Area",0.16782071592829234,0.14404612026374269,0.13170450146173274,8.9325653848745003E-3,0.13061462078203517,0.58014100202571928,100.01300000000001,201.602,{"$f":"T422*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8732121174063326E-4},{"$f":"U422*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9902005832175334E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16880803714003298},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13369470204495026}]
["Single Family Detached",10422,"New England","2000s","Wood","central furnace","window/wall unit",54.47728576053678,14739.525369999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14739.525369999999},"Cold/Very Cold",77.900749894523415,"Rural",1.1724588766893835,0.27320666868491511,4.5661133457961895E-3,1.44995658969764E-2,0.29009001380140564,1.7403216725215003,983.72,0,{"$f":"T423*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.44995658969764E-2},{"$f":"U423*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.18695844258636},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.5661133457961895E-3}]
["Multi-Family (5+ units)",10423,"East North Central","2000s","Concrete","central furnace","central AC",52.744803401611414,34006.96544,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2704.9627448103815},"Cold/Very Cold",227.92808114128945,"Metropolitan Area",0.30392416544272405,0.56104402523705765,5.8050601852987882E-2,1.2806921163807678E-2,0.82518540971110277,1.7599924425528726,294.80399999999997,81.793000000000006,{"$f":"T424*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.9743383702107957E-4},{"$f":"U424*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2124701778627556E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30472159927974513},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8271848870774155E-2}]
["Single Family Detached",10424,"East North Central","2000s","Siding","central furnace","central AC",33.513486132546404,13568.213009999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13568.213009999999},"Cold/Very Cold",176.77149579853909,"Metropolitan Area",1.1335550262355751,7.3852801029405737E-2,5.9485162477069552E-2,1.7481814802391388E-2,0.36364626293700719,1.6305392526790576,1063.098,225.34100000000001,{"$f":"T425*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4424340114504977E-2},{"$f":"U425*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0574746878864099E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1479793663500801},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2542637164955964E-2}]
["Multi-Family (5+ units)",10425,"South Atlantic","1970s","Stucco","N/A","window/wall unit",13.478146462608031,29951.436580000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2382.3801698917737},"Hot-Humid",138.38974414273994,"Metropolitan Area",0,0.12306886548108126,0.17552227723777686,0,0.1735946327309246,0.47218577544978274,0,0,{"$f":"T426*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U426*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17552227723777686}]
["Single Family Detached",10426,"New England","2010s","Wood","wood-burning stove","N/A",26.769582854497145,12573.78246,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12573.78246},"Cold/Very Cold",25.645926785078576,"Micropolitan Area",5.7072197405420647E-2,0.34594824818812914,0,0,0.13071827468484104,0.53373872027839087,0,0,{"$f":"T427*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U427*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.7072197405420647E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10427,"East South Central","1980s","Siding","heater burning gas/oil/kerosene","central AC",36.135870348348796,21509.446639999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21509.446639999998},"Mixed-Humid",223.59069778040814,"Rural",0.52390561331992658,0.295579825913797,0.19987814611069796,9.6431151176447991E-3,0.26743908140302491,1.2868026667474466,0,448.32,{"$f":"T428*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U428*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6431151176447991E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52390561331992658},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20952126122834275}]
["Multi-Family (2-4 units)",10428,"Middle Atlantic","2010s","Siding","built-in electric unit","N/A",17.834516438203519,17978.34318,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5992.7810600000003},"Cold/Very Cold",67.940158891099884,"Metropolitan Area",8.5766638992378533E-2,9.0794714142901856E-2,0,0,5.5251403827639642E-2,0.23181275696292,0,0,{"$f":"T429*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U429*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.5766638992378533E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10429,"South Atlantic","1990s","Concrete","N/A","central AC",34.987268792302707,28170.1037,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2240.6904009234963},"Hot-Humid",438.6338676634993,"Metropolitan Area",0,0.56569137381738799,0.35376509848830012,1.6859694384035201E-2,0.56164363978683851,1.4966187622343707,0,598.49599999999998,{"$f":"T430*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U430*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.341044242191109E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35510614273049124}]
["Single Family Detached",10430,"South Atlantic","Before 1950","Siding","heat pump","central AC",45.787086682293257,26760.424709999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26760.424709999999},"Mixed-Humid",596.0349396111734,"Metropolitan Area",0.66584309331877622,0.38762239700697554,0.31981458500110188,2.701542479706159E-2,0.66043192135901618,2.0337119966858701,440.721,568.80799999999999,{"$f":"T431*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.179388113861591E-2},{"$f":"U431*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5221543658445679E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.67763697445739213},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.33503612865954757}]
["Single Family Detached",10431,"West South Central","2000s","Wood","portable electric heaters","window/wall unit",25.480153015226403,20648.42222,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20648.42222},"Hot-Humid",268.75986357065386,"Micropolitan Area",0.28457816561297317,0.1246697015324717,0.16955796734604073,0,0.44732496181183579,1.0261307963033213,0,0,{"$f":"T432*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U432*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28457816561297317},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16955796734604073}]
["Single Family Detached",10432,"Pacific","Before 1950","Stucco","heater burning gas/oil/kerosene","N/A",24.837974309245546,21806.825560000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21806.825560000001},"Marine",108.10426293565162,"Metropolitan Area",0.39466354891792305,0.16588426035301332,0,0,0.42857564864183678,0.98912345791277312,0,0,{"$f":"T433*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U433*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39466354891792305},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",10433,"South Atlantic","1970s","Siding","central furnace","window/wall unit",22.842685893101759,19035.57158,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19035.57158},"Mixed-Humid",288.71811057527248,"Metropolitan Area",0.5877183613550323,0.36965979752322675,0.16615017815672992,6.8533006936610796E-3,0.46903509413447475,1.5925634311694636,360.02600000000001,0,{"$f":"T434*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8533006936610796E-3},{"$f":"U434*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59457166204869338},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16615017815672992}]
["Single Family Detached",10434,"Middle Atlantic","1960s","Stucco","central furnace","central AC",111.76915336702265,33635.014560000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33635.014560000003},"Mixed-Humid",371.07483367405376,"Metropolitan Area",4.0703380916520171,0.17577305441403124,0.2359862220342413,8.9868352717412656E-2,0.95226632527916721,5.4343636933794572,2314.6930000000002,357.17599999999999,{"$f":"T435*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7854732756930098E-2},{"$f":"U435*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2013619960482559E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.1481928244089472},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24799984199472386}]
["Single Family Detached",10435,"East North Central","1970s","Brick","central furnace","central AC",37.220766078479834,16572.024079999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16572.024079999999},"Cold/Very Cold",77.425126227857859,"Metropolitan Area",1.2871456964566395,0.37740491274067328,3.0434207354462482E-2,1.37124384648756E-2,0.23893698438367938,1.9339218009354546,729.49900000000002,97.945999999999998,{"$f":"T436*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.208927499433592E-2},{"$f":"U436*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6231634705396801E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2992349714509754},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2057370825002159E-2}]
["Single Family Detached",10436,"South Atlantic","1990s","Siding","central furnace","central AC",74.66234731874691,16964.859649999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16964.859649999999},"Mixed-Humid",338.6492201815721,"Metropolitan Area",0.70169599522577342,0.504647572659076,0.46152367981231984,5.746481461955024E-2,0.66536299997803494,2.3332302476752043,1684.922,1702.3630000000001,{"$f":"T437*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8584465251197295E-2},{"$f":"U437*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8880349368352948E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.73028046047697071},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.49040402918067277}]
["Single Family Detached",10437,"Middle Atlantic","1950s","Siding","central furnace","central AC",41.462304250941337,28052.979869999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28052.979869999999},"Cold/Very Cold",161.97372588741669,"Micropolitan Area",1.549686078561477,0.46928730347712094,4.8506828287915048E-2,5.2878997412574021E-2,0.53496000262430787,2.6024402129508211,1810.6389999999999,74.33,{"$f":"T438*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0793819418836927E-2},{"$f":"U438*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0851779937371001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6004798979803139},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0592006281652148E-2}]
["Single Family Attached",10438,"West South Central","1960s","Brick","central furnace","central AC",8.8955585207583106,9829.3464320000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9829.3464320000003},"Hot-Humid",76.498205737727446,"Metropolitan Area",2.9151885477372033E-2,3.2826183637771518E-2,5.5180014488000896E-2,3.088763993445248E-3,0.14385380216474195,0.26101188576788636,57.658999999999999,256.58,{"$f":"T439*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6675028592268796E-4},{"$f":"U439*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5220137075225601E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9718635763294723E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7702028195523454E-2}]
["Single Family Detached",10439,"Mountain North","Before 1950","Wood","central furnace","N/A",16.781214187110916,11834.42467,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11834.42467},"Cold/Very Cold",76.82946368235406,"Metropolitan Area",0.36197740535042472,0.11033847143038907,0,7.5358539348145794E-3,0.18799524421502428,0.660311120995838,636.774,0,{"$f":"T440*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5358539348145794E-3},{"$f":"U440*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36951325928523931},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10440,"East South Central","2000s","Brick","heat pump","central AC",61.513021944508004,24361.592850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24361.592850000001},"Hot-Humid",237.01147631006015,"Metropolitan Area",0.13992205097521035,9.1851926494740305E-2,0.2051681703250158,1.3973980189909949E-2,0.44131934135188305,0.87826148914684954,81.819000000000003,491.78800000000001,{"$f":"T441*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9932411653941504E-3},{"$f":"U441*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.19807390245158E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1419152921406045},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2171489093495316}]
["Single Family Detached",10441,"Mountain North","1970s","Wood","central furnace","N/A",15.885848585965212,15728.562959999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15728.562959999999},"Cold/Very Cold",69.848707847511832,"Metropolitan Area",0.50497101882783602,0.32615625807669169,0,9.8524976666476798E-3,0.22847129677221967,1.0595985736767473,626.40800000000002,0,{"$f":"T442*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8524976666476798E-3},{"$f":"U442*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.51482351649448366},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10442,"Pacific","2000s","Stucco","central furnace","central AC",31.177227587711617,13531.782810000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13531.782810000001},"Hot-Dry/Mixed-Dry",123.07054974746879,"Metropolitan Area",0.12532491772581963,0.16377099956032451,0.1867310249796264,1.5137504753583031E-2,0.24041068722566539,0.71623762949143588,410.637,708.02599999999995,{"$f":"T443*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5566506977499704E-3},{"$f":"U443*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5808540558330602E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1308815684235696},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19631187903545946}]
["Multi-Family (5+ units)",10443,"Pacific","Before 1950","Stucco","portable electric heaters","N/A",7.9679564090392425,20535.970130000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1633.4604811533816},"Hot-Dry/Mixed-Dry",30.87993827905234,"Metropolitan Area",1.6371920909438991E-2,0.34634566668095135,0,2.224045565079E-4,0.10838412707301015,0.47130642884289747,10.83,0,{"$f":"T444*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7690377010891122E-5},{"$f":"U444*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6389611286449883E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10444,"Pacific","1970s","Other","central furnace","central AC",15.202207370302292,13477.134190000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13477.134190000001},"Hot-Dry/Mixed-Dry",45.343225000228514,"Metropolitan Area",0.43813165943759946,0.27320355862283485,3.803851044029713E-2,4.6638566263888298E-3,0.11995994447092152,0.86933367297165298,219.07400000000001,126.983,{"$f":"T445*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9524896955400604E-3},{"$f":"U445*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.71136693084877E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44108414913313954},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9749877371145902E-2}]
["Multi-Family (2-4 units)",10445,"Pacific","1970s","Stucco","heater burning gas/oil/kerosene","N/A",26.603626750843695,31335.24941,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10445.083136666666},"Marine",46.803080567847076,"Metropolitan Area",0.74803980553818095,0.77818506751658678,0,0,0.1873777410406828,1.7136026140954503,0,0,{"$f":"T446*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U446*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.74803980553818095},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10446,"South Atlantic","1960s","Concrete","N/A","central AC",84.542286957924404,65791.663,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5233.1631191295037},"Hot-Humid",559.75119236526734,"Metropolitan Area",0,0.290693028507581,0.33904283091228304,6.7631197897480011E-3,1.27391015441977,1.9098711853933881,0,102.79600000000001,{"$f":"T447*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U447*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3794823599403649E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.33958077914827706}]
["Mobile Home",10447,"East South Central","2010s","Siding","heat pump","central AC",10.993793633819251,19086.44728,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19086.44728},"Hot-Humid",368.58269697924447,"Metropolitan Area",5.3757284147276485E-2,9.5728400802443755E-2,0.11144410514700664,4.1888453251997604E-3,0.9966743507106397,1.2576041408073666,33.252000000000002,186.215,{"$f":"T448*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3466254495456013E-4},{"$f":"U448*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5541827802452004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.4391946692231047E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11499828792725185}]
["Single Family Attached",10448,"West South Central","1980s","Brick","central furnace","central AC",23.763206381166221,9520.5153769999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9520.5153769999997},"Hot-Humid",83.96396708798423,"Metropolitan Area",5.0643267647652389E-2,4.0160742273868053E-2,0.10030374201345246,6.7460753473807915E-3,9.5377294208531527E-2,0.28648504614350445,102.71,605.87300000000005,{"$f":"T449*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7785213437167002E-4},{"$f":"U449*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.768223213009121E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.1621119782024057E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10607196522646159}]
["Single Family Detached",10449,"West North Central","1960s","Siding","central furnace","central AC",68.790030411044341,27362.780589999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27362.780589999998},"Mixed-Humid",156.30244146174186,"Metropolitan Area",1.8623014615216571,0.39935860611148466,0.19774865366426339,4.2219019232412232E-2,0.30225004055499649,2.7616587618524018,1217.174,325.762,{"$f":"T450*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3305265101852659E-2},{"$f":"U450*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9137541305595799E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8956067266235097},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20666240779482298}]
["Single Family Detached",10450,"East South Central","1970s","Brick","central furnace","central AC",15.581785973987252,10436.56127,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10436.56127},"Hot-Humid",234.37203001023866,"Metropolitan Area",0.18261756103981111,0.14845935350646111,0.16286051392546358,1.13404718415947E-2,0.30573994951235783,0.79967737798409366,337.03199999999998,749.57799999999997,{"$f":"T451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5174551179506398E-3},{"$f":"U451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8230167236440599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18613501615776176},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17068353064910763}]
["Single Family Detached",10451,"West North Central","2000s","Brick","central furnace","central AC",107.82968804864626,18445.0373,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18445.0373},"Mixed-Humid",310.42997773840511,"Metropolitan Area",1.2757991095117784,0.17325119192774549,0.12828781672672199,3.0725042222922598E-2,1.0092125427339831,2.5865506609002291,1279.2539999999999,386.50799999999998,{"$f":"T452*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3595887746174198E-2},{"$f":"U452*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1291544767483998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2993949972579526},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13541697120347038}]
["Single Family Detached",10452,"Pacific","Before 1950","Stucco","central furnace","central AC",52.654160199984446,25610.000100000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25610.000100000001},"Hot-Dry/Mixed-Dry",306.36738599360632,"Metropolitan Area",0.38830704232623209,0.5136836661357933,0.39617059285693712,2.5713208400403E-2,1.7718537230186009,3.0700150243375637,239.02500000000001,765.005,{"$f":"T453*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1214302739025003E-3},{"$f":"U453*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9591778126500502E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39442847260013458},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4157623709834376}]
["Multi-Family (2-4 units)",10453,"South Atlantic","1990s","Siding","heat pump","central AC",37.023768333449645,36297.812089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12099.270696666666},"Mixed-Humid",505.24525383835362,"Metropolitan Area",0.19470476715166021,1.0275106243163086,8.8442026912153637E-2,7.1373476846929695E-3,0.40848116702946069,1.723896817199378,88.688999999999993,107.944,{"$f":"T454*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0730722188166699E-3},{"$f":"U454*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3060436760809866E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19577783937047688},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.9748070588234627E-2}]
["Single Family Detached",10454,"South Atlantic","1980s","Concrete","heat pump","N/A",12.403941299043925,13223.818020000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13223.818020000001},"Hot-Humid",195.29633986058411,"Metropolitan Area",2.473090676082558E-2,0.13415128317677144,0,3.9318378118866E-4,0.50746893577780339,0.66635112571540045,29.733000000000001,0,{"$f":"T455*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9318378118866E-4},{"$f":"U455*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5124090542014241E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10455,"Mountain South","1990s","Stucco","central furnace","central AC",41.833135911232937,14495.196089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14495.196089999999},"Hot-Dry/Mixed-Dry",214.15973845490649,"Metropolitan Area",1.5597162787878498,0.28219791317865373,9.8424961596004029E-2,1.9721714448975209E-2,0.65328286195491503,2.5936220155174228,985.976,374.59300000000002,{"$f":"T456*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.429191546003384E-2},{"$f":"U456*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4297989889413702E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5740081942478836},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1038547605849454}]
["Multi-Family (2-4 units)",10456,"West North Central","1960s","Siding","central furnace","window/wall unit",18.914910333516556,21494.21629,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7164.7387633333337},"Cold/Very Cold",43.717774323261366,"Metropolitan Area",0.1591506573984289,0.17208953077852024,1.7196447742814501E-2,6.4208597612302508E-3,0.1255477388441063,0.47826494793802338,298.72500000000002,0,{"$f":"T457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.14028658707675E-3},{"$f":"U457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16129094398550564},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7196447742814501E-2}]
["Single Family Detached",10457,"East North Central","1980s","Wood","central furnace","central AC",26.817660219519247,23078.881430000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23078.881430000001},"Cold/Very Cold",108.82901926763192,"Metropolitan Area",1.461246347562642,0.40414253188140054,2.713421015935388E-2,1.6562582337120931E-2,0.32882074816139628,2.2213438377647927,665.96299999999997,51.688000000000002,{"$f":"T458*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5369681113767089E-2},{"$f":"U458*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1929012233538401E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4766160286764092},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8327111382707718E-2}]
["Single Family Detached",10458,"East North Central","2010s","Other","built-in electric unit","central AC",36.435212710840624,12309.19348,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12309.19348},"Cold/Very Cold",77.210006965864153,"Micropolitan Area",0.1069688608121568,0.21533395344075001,1.8389504237348198E-2,1.00441787877452E-3,0.92271116343217363,1.2634034819224287,0,81.599000000000004,{"$f":"T459*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U459*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.00441787877452E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1069688608121568},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9393922116122717E-2}]
["Single Family Detached",10459,"South Atlantic","1990s","Brick","central furnace","central AC",56.994932030002033,27815.97464,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27815.97464},"Mixed-Humid",384.83679069218215,"Metropolitan Area",1.3390183216485274,0.63956928353263931,0.13093137814103448,2.5064835668230801E-2,0.65377732177108094,2.7632963050932822,691.54700000000003,209.548,{"$f":"T460*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9236053814368079E-2},{"$f":"U460*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8287818538627209E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3582543754628955},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13676015999489718}]
["Multi-Family (5+ units)",10460,"Pacific","1950s","Wood","built-in electric unit","N/A",11.859526988212401,14824.408740000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1179.1547065935858},"Marine",51.765352862673602,"Metropolitan Area",3.1027116882601499E-2,6.2114020605651424E-2,0,0,8.348224950047968E-2,0.17662338698873262,0,0,{"$f":"T461*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U461*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.1027116882601499E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10461,"Pacific","2000s","Wood","fireplace","central AC",42.822816835651899,13796.01058,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13796.01058},"Marine",377.47725330576498,"Metropolitan Area",0.16398197540386902,0.4870312078105668,3.0488369417175781E-2,1.71816895364378E-3,0.60645084119609427,1.2879523938277058,0,124.541,{"$f":"T462*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U462*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.71816895364378E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16398197540386902},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2206538370819562E-2}]
["Single Family Detached",10462,"West North Central","1960s","Siding","central furnace","both central and individual units",59.637201015847452,36881.385909999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":36881.385909999997},"Mixed-Humid",465.81042878300099,"Metropolitan Area",2.0027339397194681,0.77580286624633699,0.30776332649407284,4.8983643882507394E-2,0.80687687224956228,3.8931770047094396,996.40099999999995,331.73899999999998,{"$f":"T463*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6748649802109908E-2},{"$f":"U463*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2234994080397488E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0394825895215782},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31999832057447031}]
["Single Family Detached",10463,"South Atlantic","1980s","Siding","central furnace","central AC",19.293722353133813,14875.653319999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14875.653319999999},"Mixed-Humid",137.86419305134336,"Metropolitan Area",0.35457766423042519,0.29254632376690515,0.1275335129866226,1.3130798688177278E-2,0.34707654166554858,1.1217340426495015,498.03,384.67399999999998,{"$f":"T464*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4085216229595992E-3},{"$f":"U464*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7222770652176798E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36198618585338477},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13325579005184029}]
["Single Family Detached",10464,"South Atlantic","1960s","Siding","heat pump","central AC",44.071566742477849,29757.978889999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29757.978889999999},"Mixed-Humid",416.82673567587511,"Metropolitan Area",0.57464445691121291,0.17632664852171373,0.14240603427064386,1.454192081811297E-2,0.52883564912550363,1.4222127888290741,276.16699999999997,212.506,{"$f":"T465*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2181717561146291E-3},{"$f":"U465*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3237490619983397E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58286262866732752},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1487297833326422}]
["Single Family Detached",10465,"West South Central","1960s","Siding","central furnace","window/wall unit",36.867177486684064,38283.6734,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38283.6734},"Hot-Humid",695.75963226543229,"Metropolitan Area",0.93964336174182883,1.2240971422078992,0.86386726190366003,8.1371182138232009E-3,1.7158371831921491,4.7434449490455366,212.548,0,{"$f":"T466*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1371182138232009E-3},{"$f":"U466*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.94778047995565207},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.86386726190366003}]
["Single Family Detached",10466,"South Atlantic","1980s","Concrete","N/A","N/A",18.513345222453619,13223.818020000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13223.818020000001},"Hot-Humid",196.19618100512145,"Metropolitan Area",0,0.20755442250909198,0,0,0.46186696960273804,0.66942139211183005,0,0,{"$f":"T467*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U467*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10467,"South Atlantic","2010s","Concrete","central furnace","central AC",10.437989578637795,12426.17807,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":988.39600372557595},"Mixed-Humid",85.238548956757072,"Metropolitan Area",5.479636620973196E-2,6.4467260350721409E-2,1.9845821729174221E-2,1.7760984839012401E-3,0.1500896663755634,0.29083393973148769,72.028000000000006,70.903999999999996,{"$f":"T468*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1192187356345789E-5},{"$f":"U468*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0081230248158235E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.4867558397088304E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9915902959422378E-2}]
["Single Family Detached",10468,"West North Central","1970s","Siding","central furnace","central AC",23.530643421259242,16594.24783,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16594.24783},"Mixed-Humid",74.655745397319649,"Metropolitan Area",0.60374999568694687,0.22164088860466885,2.8553556298602699E-2,8.4335286321626009E-3,0.25717297329145206,1.1111174138816704,417.30200000000002,90.918000000000006,{"$f":"T469*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9248128079546604E-3},{"$f":"U469*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5087158242079401E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.61067480849490152},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0062272122810638E-2}]
["Multi-Family (5+ units)",10469,"South Atlantic","1980s","Siding","central furnace","central AC",60.893644175682041,56803.772550000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4518.2534379178242},"Mixed-Humid",419.73591303889765,"Metropolitan Area",0.38459946962737174,0.51208839529669703,0.14473371088117357,1.30846353993474E-2,0.37867343151228466,1.432138872073957,112.85599999999999,117.492,{"$f":"T470*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0991200998965391E-4},{"$f":"U470*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3085863292784104E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38510938163736141},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14526456951410141}]
["Multi-Family (5+ units)",10470,"South Atlantic","1990s","Concrete","built-in electric unit","window/wall unit",62.163063252475695,64820.712460000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5155.9323223273786},"Hot-Humid",123.37326203173825,"Metropolitan Area",1.330360856315302E-2,8.7058948745789594E-2,3.8475630294882206E-2,0,0.28211140835416282,0.42094959595798764,0,0,{"$f":"T471*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U471*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.330360856315302E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8475630294882206E-2}]
["Single Family Detached",10471,"West South Central","1970s","Brick","central furnace","central AC",31.210504378107693,20904.557519999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20904.557519999998},"Hot-Humid",279.81864454106164,"Rural",0.32495114522433022,0.29934262326662231,0.39375665670034843,2.4517596718969199E-2,0.54239443655759201,1.5604448617488931,271.73399999999998,901.101,{"$f":"T472*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6804790331396798E-3},{"$f":"U472*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8837117685829519E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33063162425746989},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.41259377438617795}]
["Multi-Family (5+ units)",10472,"East North Central","1960s","Siding","central furnace","central AC",22.416155713509884,16604.559789999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1320.7504711107354},"Cold/Very Cold",148.7768556985545,"Metropolitan Area",0.18391937585338319,0.23252998962620336,4.9248356428292735E-2,9.1464723192833906E-3,0.21687499479691405,0.69099166551381963,413.18,137.661,{"$f":"T473*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4570767965353363E-4},{"$f":"U473*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8181583060357495E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18446508353303673},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.9430172258896309E-2}]
["Multi-Family (5+ units)",10473,"Middle Atlantic","2000s","Concrete","built-in electric unit","window/wall unit",28.930086774976068,38624.948969999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3072.2837698761787},"Mixed-Humid",284.76548761731146,"Metropolitan Area",0.44730657933769713,0.26540160336021451,6.3567782266356898E-2,7.7084196908918691E-3,0.71895823388625502,1.5023294797971776,199.571,0,{"$f":"T474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1313874423795886E-4},{"$f":"U474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44791971808193509},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.3567782266356898E-2}]
["Multi-Family (2-4 units)",10474,"East South Central","2010s","Siding","central furnace","central AC",19.497682046594647,20225.811249999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6741.9370833333332},"Mixed-Humid",225.0001360427695,"Micropolitan Area",0.19271326900976748,0.28802600894441621,2.5426049354676249E-2,4.31732076618E-3,0.25865693768655251,0.76770047883953252,157.84800000000001,55.607999999999997,{"$f":"T475*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0642012847300003E-3},{"$f":"U475*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7490563733E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19377747029449749},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5800954992006249E-2}]
["Single Family Attached",10475,"Pacific","2000s","Stucco","central furnace","central AC",26.550037200551799,10211.55277,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10211.55277},"Hot-Dry/Mixed-Dry",85.680033512011505,"Metropolitan Area",1.976449102099331E-2,8.1117889566501497E-2,5.2273918938695915E-2,3.4337265228874302E-3,0.16867093630381266,0.32182723583000339,44.527000000000001,291.73200000000003,{"$f":"T476*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5468981018979002E-4},{"$f":"U476*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9790367126976405E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0219180831183101E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5252955651393557E-2}]
["Single Family Detached",10476,"South Atlantic","1970s","Siding","built-in electric unit","N/A",47.678206414327832,24079.90223,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24079.90223},"Mixed-Humid",494.095513846259,"Metropolitan Area",1.166707599615965,0.24199656399770236,0,0,0.27717795131309247,1.68588211492676,0,0,{"$f":"T477*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U477*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.166707599615965},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",10477,"West South Central","1990s","Siding","central furnace","central AC",21.532969343918346,20237.753140000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20237.753140000001},"Mixed-Humid",368.20145098933978,"Micropolitan Area",0.52399653167122739,0.35801075058285986,8.7264989162148587E-2,9.7162262335265606E-3,0.2870310813724693,1.2563033527887051,327.34500000000003,152.75899999999999,{"$f":"T478*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6247273016133007E-3},{"$f":"U478*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0914989319132599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53062125897284074},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0356488094061854E-2}]
["Single Family Detached",10478,"Mountain South","1980s","Stucco","built-in electric unit","central AC",17.087774535409071,14395.766250000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14395.766250000001},"Hot-Dry/Mixed-Dry",194.97756806660757,"Metropolitan Area",8.3912863888185016E-2,0.14475970822085249,0.18862657351245002,8.6396191149374999E-3,0.24796430966913002,0.66526345529061759,0,600.15,{"$f":"T479*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U479*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6396191149374999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.3912863888185016E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19726619262738751}]
["Single Family Detached",10479,"Pacific","1990s","Wood","N/A","N/A",12.928356006106561,13753.57022,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13753.57022},"Marine",85.829154953306372,"Metropolitan Area",0,0.10303408734962746,0,0,0.18981497561319122,0.29284906296281871,0,0,{"$f":"T480*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U480*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",10480,"South Atlantic","1970s","Siding","central furnace","window/wall unit",21.337739656028585,20817.306980000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20817.306980000001},"Mixed-Humid",607.04951278163435,"Rural",0.9315655775476126,0.59848267048320236,0.12147608492998019,1.0958063855816162E-2,0.41972857727272439,2.0712529102335195,526.39200000000005,0,{"$f":"T481*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0958063855816162E-2},{"$f":"U481*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.94252364140342881},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12147608492998019}]
["Single Family Detached",10481,"East North Central","1990s","Brick","central furnace","central AC",54.84304129802814,30468.35628,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30468.35628},"Mixed-Humid",358.08758359790352,"Rural",1.1917252111553187,0.25754353133070956,0.35807225805368675,5.6958550685589242E-2,0.78505455375899913,2.5923955542987143,1322.8610000000001,546.572,{"$f":"T482*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0305400256917083E-2},{"$f":"U482*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6653150428672162E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2320306114122357},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37472540848235891}]
["Multi-Family (5+ units)",10482,"Mountain South","1970s","Stucco","central furnace","central AC",14.56636652136838,21080.125209999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1676.7433556984884},"Hot-Dry/Mixed-Dry",97.495579104672601,"Metropolitan Area",3.3351289355403754E-2,7.8124862319654112E-2,6.016938708671301E-2,3.2134753671376102E-3,0.15801988599356756,0.33262329568859,25.648,126.79300000000001,{"$f":"T483*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.300511358695483E-5},{"$f":"U483*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1259932029907844E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.3394294468990712E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0381986407012089E-2}]
["Multi-Family (5+ units)",10483,"East North Central","1980s","Siding","built-in electric unit","central AC",14.798779267388875,14933.17787,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1187.8063590015179},"Cold/Very Cold",58.373792286804353,"Metropolitan Area",5.2051846375743366E-2,7.1043040666026513E-2,1.4443969279650554E-2,6.475473919768099E-4,6.101396320806813E-2,0.19914886007431998,0,43.363,{"$f":"T484*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U484*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1506847145382819E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.2051846375743366E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4495476126795937E-2}]
["Multi-Family (5+ units)",10484,"Middle Atlantic","1960s","Brick","central furnace","window/wall unit",34.470072426709415,41035.800510000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3264.0463548229154},"Mixed-Humid",94.560970007982277,"Metropolitan Area",0.72939710930690549,0.76314425937328845,4.277378976900003E-2,5.3844304923186303E-3,0.37250469506275274,1.91277599868991,131.21299999999999,0,{"$f":"T485*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2828531435537922E-4},{"$f":"U485*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.72982539462126084},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.277378976900003E-2}]
["Single Family Attached",10485,"East North Central","2000s","Brick","central furnace","central AC",27.651086052820176,10869.1376,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10869.1376},"Cold/Very Cold",186.15651311160889,"Metropolitan Area",0.1420230863913888,0.19215646185278401,1.93616404415216E-2,3.2637302928399999E-3,0.28162485499962558,0.63516604368532004,223.06800000000001,77.206999999999994,{"$f":"T486*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4245567861568003E-3},{"$f":"U486*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3917350668319987E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1444476431775456},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0200813948204801E-2}]
["Single Family Detached",10486,"East North Central","Before 1950","Siding","central furnace","window/wall unit",48.111924554500568,24672.78182,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24672.78182},"Cold/Very Cold",121.15816241914384,"Metropolitan Area",2.1254982004378498,0.23245661241245744,6.9383785450149393E-2,2.820054551018724E-2,0.34961460137405492,2.7769531996745114,1142.982,0,{"$f":"T487*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.820054551018724E-2},{"$f":"U487*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.153698745948037},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9383785450149393E-2}]
["Single Family Detached",10487,"Pacific","1980s","Stucco","N/A","central AC",23.309756318484656,24536.585599999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24536.585599999999},"Hot-Dry/Mixed-Dry",222.48188303545348,"Metropolitan Area",0,0.87174094134319047,6.9077383244553592E-2,3.0312007118527997E-3,0.73579142502146888,1.6766097496092129,0,123.538,{"$f":"T488*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U488*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0312007118527997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.2108583956406389E-2}]
["Single Family Detached",10488,"South Atlantic","2000s","Concrete","central furnace","central AC",30.820694024754879,18978.259870000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18978.259870000002},"Hot-Humid",336.65455470195667,"Metropolitan Area",0.10140881335455541,0.1595299239890291,0.50345440483140602,2.5693109820683662E-2,0.38427222336947703,1.1486653655444676,90.307000000000002,1263.511,{"$f":"T489*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7138697140800902E-3},{"$f":"U489*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3979240106603569E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10312268306863551},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.52743364493800959}]
["Single Family Detached",10489,"South Atlantic","Before 1950","Siding","central furnace","both central and individual units",69.306599747255305,27286.062890000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27286.062890000001},"Cold/Very Cold",342.24513038301575,"Micropolitan Area",2.5795388165273772,0.69065410044896425,0.15922154420013032,5.2133024618262899E-2,0.96230693906120157,4.3917214002376728,1693.606,217.00399999999999,{"$f":"T490*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6211839826881339E-2},{"$f":"U490*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9211847913815605E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6257506563542585},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16514272899151189}]
["Single Family Detached",10490,"East North Central","1980s","Wood","central furnace","central AC",25.307985637455072,18746.656029999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18746.656029999998},"Mixed-Humid",109.10289480297308,"Rural",0.96671436050919479,8.7586101664514748E-2,7.2689746329892321E-2,1.2231668153206159E-2,0.24699797252246738,1.3739881810260692,472.36799999999999,180.10400000000001,{"$f":"T491*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8553204155790398E-3},{"$f":"U491*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3763477376271196E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.97556968092477381},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.6066094067519435E-2}]
["Multi-Family (5+ units)",10491,"South Atlantic","1980s","Wood","central furnace","central AC",21.104823154006848,24037.383999999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1911.9679560182817},"Mixed-Humid",251.55122358391986,"Metropolitan Area",0.19031230770465649,0.26528077636619996,5.5103152755148349E-2,5.5326125631279992E-3,0.34249005564340002,0.85827883310399999,129.315,100.852,{"$f":"T492*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4724613623250408E-4},{"$f":"U492*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9282579230035576E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19055955384088899},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5295978547448707E-2}]
["Single Family Detached",10492,"Middle Atlantic","2000s","Siding","central furnace","central AC",32.246538852085493,17553.913369999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17553.913369999998},"Mixed-Humid",168.67488647861356,"Metropolitan Area",0.62691026327251198,0.18512569442353774,5.0661208372787939E-2,1.699731388486404E-2,0.32519988456993842,1.187897050638776,827.846,140.446,{"$f":"T493*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4531936967701017E-2},{"$f":"U493*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4653769171630196E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.64144220024021303},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.3126585289950956E-2}]
["Mobile Home",10493,"West North Central","1970s","Siding","central furnace","window/wall unit",45.085346123150131,29352.438880000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29352.438880000002},"Mixed-Humid",422.64559135101695,"Micropolitan Area",0.6877039555402239,0.17874904402191888,0.10612333183649568,1.117412125234944E-2,0.4694904400343895,1.442066771433028,380.68799999999999,0,{"$f":"T494*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.117412125234944E-2},{"$f":"U494*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6988780767925733},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10612333183649568}]
["Single Family Detached",10494,"East North Central","Before 1950","Siding","central furnace","both central and individual units",75.998215115397755,17371.0206,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17371.0206},"Cold/Very Cold",161.93378312907896,"Micropolitan Area",1.5584077433984274,8.751042475213501E-2,7.2399009140762402E-2,2.35223421887484E-2,0.41781857487499263,2.1361357521663176,1158.421,195.69300000000001,{"$f":"T495*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0122955054472598E-2},{"$f":"U495*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3993871342757999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5785306984528999},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.5798396275038205E-2}]
["Single Family Detached",10495,"Pacific","1970s","Wood","built-in furnace","N/A",16.032527092009154,12604.187970000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12604.187970000001},null,86.498848979576138,"Rural",1.0957024664124235,0.1341443558946348,0,0,0.34072007702373935,1.5705668993307977,0,0,{"$f":"T496*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U496*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0957024664124235},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10496,"Middle Atlantic","1990s","Wood","radiator","central AC",161.92552499741115,35455.55616,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35455.55616},"Mixed-Humid",537.81012100624173,"Metropolitan Area",3.5318459097329447,1.1576675189580767,0.29810737338211868,2.1437776565470079E-2,1.7361839866650399,6.7238047887381791,130.98699999999999,473.65100000000001,{"$f":"T497*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6442169347299198E-3},{"$f":"U497*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6793559630740161E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.5364901266676747},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31490093301285882}]
["Single Family Detached",10497,"East North Central","Before 1950","Siding","central furnace","window/wall unit",94.976721526611968,24947.917399999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24947.917399999998},"Cold/Very Cold",521.51782654847864,"Metropolitan Area",2.0738131473130146,0.95344588563029942,0.23643807429374578,6.1351594147153792E-2,0.52818333635905601,3.7918804435961162,2459.1869999999999,0,{"$f":"T498*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1351594147153792E-2},{"$f":"U498*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1351647414601684},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23643807429374578}]
["Single Family Detached",10498,"South Atlantic","Before 1950","Brick","central furnace","central AC",88.054229986689435,29588.11491,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29588.11491},"Mixed-Humid",498.73726500525441,"Micropolitan Area",1.161694485219402,0.68104076601467622,0.24206311977339662,3.8364186497225276E-2,0.75149660658878137,2.836294977596256,916.93399999999997,379.67399999999998,{"$f":"T499*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7130348556885939E-2},{"$f":"U499*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1233837940339339E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1888248337762879},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25329695771373595}]
["Single Family Detached",10499,"South Atlantic","1990s","Brick","central furnace","central AC",29.589270774101834,16604.529050000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16604.529050000001},"Mixed-Humid",233.36755657105334,"Metropolitan Area",0.37421175476794838,0.31541261011801192,0.32786932781132189,2.5662631737356001E-2,0.45821790287810898,1.475711595575391,612.05499999999995,933.46500000000003,{"$f":"T500*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0162885027697749E-2},{"$f":"U500*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5499746709658252E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38437463979564612},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.34336907452098014}]
["Mobile Home",10500,"South Atlantic","1980s","Siding","portable electric heaters","window/wall unit",16.346576892556008,17427.054260000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17427.054260000001},"Mixed-Humid",302.42927383708519,"Metropolitan Area",0.19468792252752767,0.20019480196547063,0.10944742512900042,0,0.52755851340166449,1.0318886630236632,0,0,{"$f":"T501*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U501*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19468792252752767},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10944742512900042}]
["Single Family Attached",10501,"South Atlantic","2000s","Siding","central furnace","central AC",14.707716154353667,12432.55803,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12432.55803},"Hot-Humid",81.210724767176444,"Metropolitan Area",2.5401978780851459E-2,4.4035225398081843E-2,0.11793239841679112,6.0188997237157196E-3,8.9721395042083416E-2,0.27709099763780787,33.969000000000001,450.15499999999997,{"$f":"T502*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2232156372107001E-4},{"$f":"U502*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.59657815999465E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5824300344572528E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12352897657678577}]
["Single Family Detached",10502,"Mountain South","Before 1950","Stucco","central furnace","both central and individual units",42.243991716459185,16924.676169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16924.676169999999},"Hot-Dry/Mixed-Dry",169.23660687883091,"Metropolitan Area",0.18706893652261891,0.16740826797700523,0.41830508341745959,1.7032164788355671E-2,0.2367039004770255,1.0094861883941093,493.59300000000002,512.75800000000004,{"$f":"T503*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3539016847788087E-3},{"$f":"U503*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6782631035768592E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19542283820739773},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.42698334652103642}]
["Single Family Detached",10503,"West North Central","1950s","Siding","central furnace","central AC",29.951923832063429,14639.258959999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14639.258959999999},"Mixed-Humid",138.37049527835825,"Metropolitan Area",0.52711084930319152,0.2688083567479177,8.9914694513793997E-2,1.7624657678971759E-2,0.36422836418250415,1.2500622647474073,945.48199999999997,258.44900000000001,{"$f":"T504*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3841155840018719E-2},{"$f":"U504*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7835018389530402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54095200514321029},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.3698196352747037E-2}]
["Multi-Family (5+ units)",10504,"East North Central","2000s","Brick","central furnace","central AC",19.979978143181945,17283.718120000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1374.7716975479755},"Cold/Very Cold",58.08533962444389,"Metropolitan Area",6.3111446164573107E-2,0.10714849199222869,2.9558431472774541E-2,2.9507109248826406E-3,0.16578309090509377,0.36831746768580392,94.304000000000002,76.418000000000006,{"$f":"T505*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2964647016556428E-4},{"$f":"U505*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.050573035832212E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.3241092634738677E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.9663488776357761E-2}]
["Single Family Detached",10505,"Middle Atlantic","1970s","Brick","central furnace","central AC",65.733154052479605,24767.57877,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24767.57877},"Cold/Very Cold",293.66279142671635,"Metropolitan Area",2.0663130538521663,0.12405312410951129,8.5153462104294531E-2,2.4557921215711948E-2,0.89727927402524854,3.1727989140912207,817.45699999999999,174.078,{"$f":"T506*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0246430638587887E-2},{"$f":"U506*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3114905771240598E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0865594844907545},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.9464952681418589E-2}]
["Single Family Detached",10506,"East North Central","1990s","Brick","central furnace","central AC",50.333836147954223,15468.2963,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15468.2963},"Cold/Very Cold",222.13106134714417,"Metropolitan Area",1.6739059842908715,0.62797188519969394,5.2953794314308807E-2,2.2573596332219802E-2,0.79937513293391993,3.1542067967387939,1283.52,175.82599999999999,{"$f":"T507*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9853867666975999E-2},{"$f":"U507*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7197286652438E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6937598519578474},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5673522979552609E-2}]
["Single Family Attached",10507,"East North Central","1980s","Siding","central furnace","central AC",68.880380124364095,17812.35586,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17812.35586},"Cold/Very Cold",145.81728880581375,"Metropolitan Area",1.4148946520430346,0.40147591276495065,7.3186214329725371E-2,2.4805433333568421E-2,0.35843841103025315,2.2479951901679636,1146.567,246.03,{"$f":"T508*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0423059421332618E-2},{"$f":"U508*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3823739122358001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4353177114643672},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.7568588241961167E-2}]
["Single Family Detached",10508,"Mountain North","1980s","Siding","central furnace","central AC",81.047807818235285,17789.24667,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17789.24667},"Cold/Very Cold",143.65039049785494,"Metropolitan Area",0.89021049584720024,0.1785264220835788,0.16376220123131896,6.2694695406821016E-2,0.27382201114428212,1.5063211303063799,2954.0839999999998,570.21900000000005,{"$f":"T509*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2550928959900274E-2},{"$f":"U509*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0143766446920732E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.94276142480710057},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17390596767823968}]
["Single Family Detached",10509,"East South Central","1960s","Siding","heater burning gas/oil/kerosene","central AC",38.923095128645294,23661.456010000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23661.456010000002},"Mixed-Humid",279.948529163876,"Rural",1.3272454118956836,0.3437334733527595,0.43676627227510173,2.0242872507131211E-2,0.55354795628740117,2.6612931138109461,0,855.52099999999996,{"$f":"T510*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U510*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0242872507131211E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3272454118956836},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.45700914478223292}]
["Single Family Detached",10510,"South Atlantic","Before 1950","Stone","central furnace","central AC",38.387101165934929,27341.240150000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27341.240150000001},"Hot-Humid",309.68055652134041,"Metropolitan Area",0.1189111545983725,9.8521014637907758E-2,0.33938438061157672,1.924864318420225E-2,0.4998135091313658,1.0566300589792226,75.045000000000002,628.97,{"$f":"T511*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0518233670567504E-3},{"$f":"U511*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7196819817145499E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12096297796542925},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35658120042872221}]
["Mobile Home",10511,"South Atlantic","1990s","Siding","heat pump","central AC",29.580566079550703,19563.866450000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19563.866450000001},"Hot-Humid",282.40206461004288,"Metropolitan Area",2.0465291160550202E-2,0.20492840997285092,0.36651182173827401,1.4588990414295951E-2,0.37165034951683235,0.96355587238850748,13.988,731.72299999999996,{"$f":"T512*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7365936390259999E-4},{"$f":"U512*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.431533105039335E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0738950524452803E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.38082715278866736}]
["Single Family Detached",10512,"West South Central","2000s","Siding","heat pump","central AC",31.701196687131958,13729.40523,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13729.40523},"Mixed-Humid",250.85955989912182,"Metropolitan Area",0.2093324749416989,0.31230105086175103,4.5735024008234794E-2,5.4138889055354395E-3,0.28856426843019878,0.8559328182418835,244.86,149.46799999999999,{"$f":"T513*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3617821646178001E-3},{"$f":"U513*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0521067409176399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2126942571063167},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7787130749152432E-2}]
["Single Family Detached",10513,"West North Central","1980s","Siding","central furnace","central AC",72.703150006772105,17706.563569999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17706.563569999998},"Mixed-Humid",147.37231288609701,"Metropolitan Area",1.5436177171217154,8.8203617420106559E-2,8.4026550541125705E-2,1.641984530193167E-2,0.31952703320356796,2.0353749182865157,625.59500000000003,301.73599999999999,{"$f":"T514*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1077137636574148E-2},{"$f":"U514*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3427076653575186E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5546948547582895},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.9369258206483226E-2}]
["Single Family Detached",10514,"West South Central","1950s","Wood","heater burning gas/oil/kerosene","window/wall unit",5.9733445933458142,17066.698840000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17066.698840000001},"Hot-Humid",232.29603255471832,"Metropolitan Area",0.1978056336938237,0.39650802001149638,0.11159011543107364,0,0.70576356620542291,1.4116673353418168,0,0,{"$f":"T515*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U515*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1978056336938237},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11159011543107364}]
["Single Family Detached",10515,"South Atlantic","2000s","Wood","central furnace","central AC",21.081731491189835,16612.869579999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16612.869579999999},"Hot-Humid",214.94415106886402,"Metropolitan Area",7.07493938090418E-2,0.16160511109058348,0.18805195220559487,9.906885419598041E-3,0.31298297418458815,0.73338943128980827,70.647000000000006,525.69100000000003,{"$f":"T516*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1736493972182599E-3},{"$f":"U516*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7332360223797804E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.1923043206260057E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19678518822797464}]
["Single Family Detached",10516,"South Atlantic","1990s","Siding","central furnace","central AC",81.220119760997605,17059.46645,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17059.46645},"Mixed-Humid",233.15384332459666,"Metropolitan Area",0.78054616352387352,0.44233031658557492,0.31528858934869014,4.2856791615689997E-2,0.49061246207849241,2.028777531536631,1345.7439999999999,1166.4559999999999,{"$f":"T517*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2957674618288799E-2},{"$f":"U517*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9899116997401198E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80350383814216231},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.33518770634609135}]
["Single Family Detached",10517,"West North Central","Before 1950","Siding","central furnace","window/wall unit",14.607055208629125,14874.80164,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14874.80164},null,92.46420644999273,"Micropolitan Area",0.62016885735983107,0.15359265004533815,7.4850596844545604E-3,9.1544735473133992E-3,0.39418054773261307,1.1754271148222371,615.43499999999995,0,{"$f":"T518*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1544735473133992E-3},{"$f":"U518*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62932333090714443},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4850596844545604E-3}]
["Single Family Detached",10518,"East North Central","1990s","Siding","heat pump","central AC",34.386794944800783,10561.054959999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10561.054959999999},"Cold/Very Cold",215.71432112373191,"Micropolitan Area",0.18470374762102446,0.21264193072904361,3.3849406229175358E-2,5.8590937538736797E-3,0.30482216627434594,0.73601725085358938,374.94600000000003,179.83699999999999,{"$f":"T519*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9598253130321602E-3},{"$f":"U519*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8992684408415197E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18866357293405661},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5748674670016876E-2}]
["Single Family Detached",10519,"West North Central","1970s","Siding","central furnace","central AC",21.016612257562109,13326.95768,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13326.95768},"Cold/Very Cold",43.879874405719711,"Metropolitan Area",0.14298894036298165,0.13809685408389188,3.6470685656664796E-3,2.0631729723561603E-3,0.14424735166887337,0.4289802146814134,136.846,17.966000000000001,{"$f":"T520*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.82374085067728E-3},{"$f":"U520*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3943212167888001E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14481268121365892},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8865006873453596E-3}]
["Single Family Detached",10520,"West North Central","1980s","Wood","central furnace","central AC",44.002863421385484,11305.97724,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11305.97724},"Mixed-Humid",125.58304160691006,"Metropolitan Area",0.84699976673347299,0.17992412452174406,8.1195876707031489E-2,1.9023324244251603E-2,0.39967090827271412,1.5077906762349624,1268.9000000000001,413.69,{"$f":"T521*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4346154519836E-2},{"$f":"U521*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6771697244156005E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.861345921253309},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5873046431447095E-2}]
["Multi-Family (2-4 units)",10521,"Pacific","1960s","Wood","N/A","N/A",27.153386197786617,30170.429110000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10056.809703333334},"Hot-Dry/Mixed-Dry",77.081916432399638,"Metropolitan Area",0,0.49766976640088817,0,0,0.26300353520429676,0.76067330160518487,0,0,{"$f":"T522*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U522*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10522,"Pacific","2000s","Stucco","N/A","N/A",41.578337238314774,16765.458559999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16765.458559999999},"Hot-Dry/Mixed-Dry",68.984832352618454,"Metropolitan Area",0,0.40718415064161467,0,0,0.2557295414498445,0.66291369209145912,0,0,{"$f":"T523*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U523*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10523,"East North Central","1970s","Siding","built-in electric unit","N/A",11.156268210728083,16726.0393,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1330.4131253510138},"Cold/Very Cold",154.11874388922303,"Metropolitan Area",0.1972466522706077,0.18742858428378281,0,0,0.14117792439785504,0.52585316095224555,0,0,{"$f":"T524*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U524*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1972466522706077},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10524,"Mountain South","Before 1950","Wood","heat pump","central AC",27.371469107111398,12165.097379999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12165.097379999999},"Hot-Dry/Mixed-Dry",180.84422093808595,"Metropolitan Area",8.0894588670512649E-2,0.11357081879942495,0.33580838935186497,1.7264888678156697E-2,0.21582658856337489,0.74610038538517742,88.137,1331.078,{"$f":"T525*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.07219518778106E-3},{"$f":"U525*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6192693490375637E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.1966783858293715E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35200108284224063}]
["Single Family Attached",10525,"South Atlantic","1990s","Stucco","heat pump","central AC",29.431394114330196,12908.50619,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12908.50619},"Hot-Humid",324.6480916380645,"Metropolitan Area",0.12375856044828937,0.12265987876093988,0.28618990821879259,1.6879743576822551E-2,0.68581407618407553,1.2184224236120973,174.36600000000001,1133.279,{"$f":"T526*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2508045903255405E-3},{"$f":"U526*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4628938986497008E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1260093650386149},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30081884720528962}]
["Multi-Family (2-4 units)",10526,"New England","Before 1950","Siding","built-in furnace","window/wall unit",38.002618879548805,31098.706119999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10366.235373333333},"Cold/Very Cold",189.56461995677677,"Metropolitan Area",1.4869853794967467,0.77190169987476076,6.179487058798272E-2,0,0.58499959564698079,2.9056815456064711,0,0,{"$f":"T527*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U527*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4869853794967467},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.179487058798272E-2}]
["Single Family Detached",10527,"Mountain South","1970s","Brick","heat pump","central AC",20.672708481098557,11963.372960000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11963.372960000001},"Hot-Dry/Mixed-Dry",296.04484973797082,"Metropolitan Area",7.7566538432817286E-2,0.2376832932793827,0.30877406989232498,1.6433271925790721E-2,0.3860811466923858,1.0101050482969107,84.512,1289.1199999999999,{"$f":"T528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0110485755955201E-3},{"$f":"U528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.54222233501952E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.8577587008412803E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32419629324252019}]
["Single Family Detached",10528,"South Atlantic","Before 1950","Concrete","portable electric heaters","window/wall unit",54.172881049967359,35687.009910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35687.009910000001},"Hot-Humid",300.65353009666319,"Metropolitan Area",1.178438597743065E-2,0.29583203658621354,0.39575834085995676,0,0.32245511697123191,1.0258298803948329,0,0,{"$f":"T529*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U529*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.178438597743065E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.39575834085995676}]
["Single Family Detached",10529,"West North Central","1960s","Siding","central furnace","central AC",29.785291275050433,15012.74762,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15012.74762},"Cold/Very Cold",59.694888100381824,"Metropolitan Area",1.1935869982533378,0.14295249378096389,3.2055428896690677E-2,2.0870556601100182E-2,0.15213745791510366,1.5207323788460962,1297.9690000000001,92.22,{"$f":"T530*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.948608101558378E-2},{"$f":"U530*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3844755855163999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2130730792689215},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3439904482207079E-2}]
["Single Family Attached",10530,"Middle Atlantic","1950s","Brick","radiator","window/wall unit",61.106752269259431,47628.02203,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":47628.02203},"Mixed-Humid",209.60025629345475,"Metropolitan Area",2.2915289766782934,0.45299459456140079,0.13914483770844674,4.9375494158280693E-3,0.8271557633389649,3.7108241722871065,103.669,0,{"$f":"T531*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9375494158280693E-3},{"$f":"U531*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2964665260941213},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13914483770844674}]
["Single Family Detached",10531,"Mountain South","1970s","Stucco","central furnace","central AC",18.553913709480067,14405.212509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14405.212509999999},"Hot-Dry/Mixed-Dry",127.10578986430683,"Metropolitan Area",0.79009471888841576,0.22812934354725334,0.10764989379340482,1.307565461096453E-2,0.31523619426354721,1.4411101504926211,749.64800000000002,158.05500000000001,{"$f":"T532*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0798838747696479E-2},{"$f":"U532*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2768158632680501E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80089355763611225},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10992670965667288}]
["Single Family Detached",10532,"Middle Atlantic","1990s","Siding","central furnace","central AC",42.26864821741114,15511.430539999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15511.430539999999},"Cold/Very Cold",326.04076141233941,"Metropolitan Area",1.0852761306534977,0.47713107602176164,6.1040891689618793E-2,3.7015454086240358E-2,0.96116127958481312,2.5846093779496915,2179.2559999999999,207.078,{"$f":"T533*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3803378072878233E-2},{"$f":"U533*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2120760133621199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1190795087263758},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4252967702980918E-2}]
["Multi-Family (5+ units)",10533,"West South Central","1970s","Siding","built-in electric unit","central AC",22.045721704052326,35788.509259999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2846.6692922484226},"Hot-Humid",246.15784025273524,"Micropolitan Area",0.23761562413270515,0.17135148138937065,0.25762122652037311,1.087544798243806E-2,0.33464331891637072,1.0112420502300601,0,303.88099999999997,{"$f":"T534*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U534*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6504871119774283E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23761562413270515},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25848627523157086}]
["Single Family Detached",10534,"New England","1970s","Shingle","central furnace","central AC",65.039084345670091,24729.689869999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24729.689869999998},"Cold/Very Cold",281.97885436677228,"Metropolitan Area",0.62754318202886639,0.70834957043242031,9.5691683330104207E-2,5.123568863367222E-2,0.88938316620699598,2.3209676019983867,1868.1969999999999,203.63200000000001,{"$f":"T535*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6199932426064384E-2},{"$f":"U535*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0357562076078404E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.67374311445493074},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10072743953771204}]
["Single Family Attached",10535,"Pacific","2000s","Wood","built-in electric unit","N/A",14.298725663311785,13215.08841,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13215.08841},"Marine",117.26873874753292,"Metropolitan Area",0.10443205114878726,0.15797298184190228,0,0,0.13771591641051187,0.40012094940120141,0,0,{"$f":"T536*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U536*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10443205114878726},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10536,"Middle Atlantic","1990s","Brick","heat pump","window/wall unit",25.817847071903078,17647.195540000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1403.6832122026565},"Cold/Very Cold",68.625125762392642,"Metropolitan Area",4.9103882573817273E-2,8.2848465373593402E-2,1.4265869344167221E-2,9.7636638764157996E-4,8.7032015431479037E-2,0.23414893752961699,55.326999999999998,0,{"$f":"T537*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7661581081536364E-5},{"$f":"U537*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.918154415489881E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4265869344167221E-2}]
["Single Family Detached",10537,"East North Central","1980s","Wood","central furnace","central AC",56.802456388358607,25290.497060000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25290.497060000002},"Cold/Very Cold",172.26002452693211,"Metropolitan Area",1.0345158751983592,0.40447337265879479,8.2272338952406585E-2,4.9597547851324843E-2,0.47108161231864049,1.992343199128201,1819.212,141.90199999999999,{"$f":"T538*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6008775737516723E-2},{"$f":"U538*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5887721138081197E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0805246509358759},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5861111066214704E-2}]
["Single Family Detached",10538,"Middle Atlantic","1980s","Siding","central furnace","central AC",77.536511956800268,19201.711729999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19201.711729999999},"Cold/Very Cold",335.34364765568228,"Metropolitan Area",1.4179068724213584,0.64326717423140578,0.10361819700859901,7.6809400747660087E-2,1.0632537337890711,3.2280459774504342,3677.3110000000001,322.822,{"$f":"T539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0610665763558025E-2},{"$f":"U539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1987349841020603E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4885175381849165},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10981693199270107}]
["Multi-Family (5+ units)",10539,"East North Central","2000s","Siding","central furnace","central AC",15.283261208901102,22246.37731,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1769.508718345232},"Cold/Very Cold",56.596296618932477,"Metropolitan Area",0.30999176783070975,0.25046713466941373,1.5489858408564752E-2,4.6454885098741999E-3,0.2429930860237049,0.8232178266317024,179.37899999999999,29.440999999999999,{"$f":"T540*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.174127043880494E-4},{"$f":"U540*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2096106176801974E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31030918053509782},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5541954514741553E-2}]
["Single Family Detached",10540,"West South Central","1970s","Brick","central furnace","central AC",14.989746645909634,12822.708850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12822.708850000001},"Mixed-Humid",159.6582663083916,"Micropolitan Area",0.61363207840117928,0.40534972827779647,0.15933058198096445,2.182800751639305E-2,0.45046492910958602,1.6287773177695262,1163.6949999999999,538.59799999999996,{"$f":"T541*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4921722175200752E-2},{"$f":"U541*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9062853411922991E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62855380057638},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16623686732215676}]
["Single Family Detached",10541,"South Atlantic","1950s","Brick","central furnace","central AC",63.409373508803377,22517.533210000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22517.533210000001},"Mixed-Humid",281.48886791969545,"Metropolitan Area",1.2555141298284145,0.30624354061850551,0.43741283269612996,5.0673254077985112E-2,0.64282995262321685,2.6420004557662669,1241.5319999999999,1008.859,{"$f":"T542*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7956238041277722E-2},{"$f":"U542*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2717016036707394E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2834703678696922},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46012984873283735}]
["Single Family Detached",10542,"South Atlantic","1960s","Brick","heat pump","central AC",42.915295383192998,21372.159060000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21372.159060000002},"Mixed-Humid",374.39887152239783,"Rural",0.46109749262860089,0.26612366681682814,0.26480134996362686,2.1397784278712941E-2,0.34978382936060881,1.3418063387696648,382.84199999999998,618.35699999999997,{"$f":"T543*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1821601188485204E-3},{"$f":"U543*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3215624159864421E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.46927965274744943},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2780169741234913}]
["Single Family Detached",10543,"West South Central","1990s","Brick","central furnace","central AC",29.49621285356104,15196.400229999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15196.400229999999},"Mixed-Humid",143.28643230410466,"Metropolitan Area",0.40981023009294476,0.27192435532281956,0.11523158278844882,1.959034817810312E-2,0.3198228769737716,1.1167890451779847,922.38400000000001,366.76,{"$f":"T544*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4016916429748319E-2},{"$f":"U544*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5734317483548002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4238271465226931},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12080501453680362}]
["Multi-Family (5+ units)",10544,"East North Central","1950s","Brick","central furnace","central AC",18.320415555495231,19427.800159999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1545.3150543273282},"Cold/Very Cold",142.58062541015855,"Metropolitan Area",4.1620350317676399E-2,0.14651895131147455,3.5074445062767155E-2,1.0248125728799681E-2,0.54128394344800945,0.77393066526819965,448.35700000000003,79.141000000000005,{"$f":"T545*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9285282181303796E-4},{"$f":"U545*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2229777871451911E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.2313203139489435E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5196742841481672E-2}]
["Single Family Detached",10545,"South Atlantic","Before 1950","Siding","central furnace","N/A",43.444520489913742,17124.367559999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17124.367559999999},"Hot-Humid",224.00660902497455,"Rural",0.65281948971168013,0.36664675144099917,0,1.2638279865939239E-2,0.75167228173887124,1.7711385228915506,738.029,0,{"$f":"T546*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2638279865939239E-2},{"$f":"U546*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.66545776957761937},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10546,"Mountain South","1990s","Stucco","central furnace","central AC",29.360229791457996,22141.953089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1761.2026663026218},"Hot-Dry/Mixed-Dry",81.513297521383336,"Metropolitan Area",0.27728592832291205,0.54635030116481631,2.556561117949422E-2,4.7639519170789499E-3,0.29514127442292049,1.1487281354475536,159.874,55.280999999999999,{"$f":"T547*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8157051507246534E-4},{"$f":"U547*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7361044595875243E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27756749883798448},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5662972224090096E-2}]
["Single Family Detached",10547,"West South Central","1990s","Brick","central furnace","central AC",88.443964596577445,14899.58972,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14899.58972},"Mixed-Humid",154.46321228280001,"Metropolitan Area",0.8015061305637351,0.26093147870503464,0.35631860739370541,5.6590534004454442E-2,0.1658851334324398,1.5846413500949148,1995.5170000000001,1802.61,{"$f":"T548*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9732384579285242E-2},{"$f":"U548*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.68581494251692E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83123851514302038},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.38317675681887459}]
["Single Family Detached",10548,"West South Central","2000s","Brick","central furnace","central AC",98.955073912335166,30004.570619999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30004.570619999999},"Hot-Humid",793.73890093601051,"Metropolitan Area",0.29507172851004015,0.50933940807532418,0.92735687500704589,5.8002525570646259E-2,0.97646907630755708,2.7082370878999673,183.58799999999999,1749.5350000000001,{"$f":"T549*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5084791109845594E-3},{"$f":"U549*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.24940464596617E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30058020762102472},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.9798509214667076}]
["Single Family Detached",10549,"Pacific","Before 1950","Siding","portable electric heaters","N/A",81.064456186401713,21513.921490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21513.921490000001},"Marine",446.49992667000561,"Metropolitan Area",0.80542425172149446,0.22595755486301097,0,0,1.5586337211665644,2.5900155277510701,0,0,{"$f":"T550*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U550*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80542425172149446},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10550,"West North Central","Before 1950","Siding","central furnace","central AC",18.764675488565299,21445.343420000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21445.343420000001},"Mixed-Humid",71.175829520793599,"Metropolitan Area",1.093770459737921,0.32934310863755156,1.6098804851959799E-2,6.1735996823759198E-3,0.22148735672435618,1.6606997299517885,245.54499999999999,42.331000000000003,{"$f":"T551*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2657968500638992E-3},{"$f":"U551*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0780283231202017E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.099036256587985},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.700660768427182E-2}]
["Multi-Family (5+ units)",10551,"Pacific","2000s","Wood","built-in electric unit","N/A",28.40888547641433,24575.160449999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1954.7434651960389},"Marine",149.93816551884336,"Metropolitan Area",0.14137109257983044,0.19259759676012778,0,0,0.17762036352451718,0.51158905286447542,0,0,{"$f":"T552*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U552*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14137109257983044},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10552,"South Atlantic","1980s","Siding","heat pump","N/A",72.064346464429164,25197.323939999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25197.323939999998},"Mixed-Humid",439.25733862998658,"Metropolitan Area",0.52055920046026172,0.58391152178175876,0,7.7288003694401392E-3,0.57116865552685026,1.6756393777688705,306.73099999999999,0,{"$f":"T553*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7288003694401392E-3},{"$f":"U553*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52828800082970184},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10553,"West South Central","2010s","Wood","central furnace","central AC",63.538179425415279,15035.063749999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15035.063749999999},"Hot-Humid",238.44543624696979,"Metropolitan Area",0.55187820770740881,0.11870806785770625,0.33670225402733495,3.3565208489452499E-2,0.4447182114745476,1.4520067410669975,711.49199999999996,1520.97,{"$f":"T554*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0697327577614999E-2},{"$f":"U554*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2867880911837498E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5625755352850238},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35957013493917245}]
["Single Family Detached",10554,"West South Central","Before 1950","Wood","portable electric heaters","window/wall unit",40.056419656948641,30027.301090000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30027.301090000001},"Hot-Humid",553.32508814576875,"Metropolitan Area",0.55554485633894435,0.3871869438231017,0.36672721165210737,0,0.5784861948085217,1.887945206622675,0,0,{"$f":"T555*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U555*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55554485633894435},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36672721165210737}]
["Single Family Detached",10555,"Mountain South","1990s","Stucco","heat pump","central AC",57.295887475497842,29748.643550000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29748.643550000001},"Hot-Dry/Mixed-Dry",590.28377079050824,"Metropolitan Area",0.1233775608487957,0.45319824325294394,0.64246336757407152,3.4788658740241007E-2,0.79500902719398903,2.0140481988698005,72.664000000000001,1096.7560000000001,{"$f":"T556*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1616554349172001E-3},{"$f":"U556*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2627003305323803E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1255392162837129},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.67509037087939527}]
["Single Family Detached",10556,"East North Central","1990s","Wood","wood-burning stove","central AC",46.302690790048693,13460.08453,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13460.08453},"Cold/Very Cold",62.384584427518909,"Micropolitan Area",0,0.34740809290009439,2.6835451287968177E-2,1.5246237747131E-3,0.22380665369691158,0.59805019788497416,0,113.27,{"$f":"T557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5246237747131E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8360075062681275E-2}]
["Single Family Detached",10557,"Pacific","1950s","Wood","central furnace","central AC",12.303300659421703,12829.30204,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12829.30204},"Hot-Dry/Mixed-Dry",63.220080656819967,"Metropolitan Area",1.4581528112623202E-2,0.51034783904891445,2.6549496472261683E-2,1.4777559847794402E-3,0.24921807000401164,0.80069693363781091,14.657999999999999,100.52800000000001,{"$f":"T558*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8805190930232002E-4},{"$f":"U558*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2897040754771202E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4769580021925523E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7839200547738804E-2}]
["Single Family Detached",10558,"South Atlantic","2000s","Stucco","central furnace","central AC",59.635853705688426,18005.994480000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18005.994480000001},"Hot-Humid",386.22503433690719,"Metropolitan Area",0.11314491572977728,0.1915384061611104,0.72888832843866136,4.6003083153084476E-2,0.28422818805370714,1.3177998383832561,122.66200000000001,2432.2139999999999,{"$f":"T559*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2086512949057602E-3},{"$f":"U559*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3794431858178717E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11535356702468304},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.77268276029684002}]
["Single Family Detached",10559,"East North Central","1970s","Siding","central furnace","central AC",25.069314605460978,15494.01397,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15494.01397},"Cold/Very Cold",178.33967992616178,"Metropolitan Area",1.3546074461082682,0.26315718162065471,8.2871283119941991E-2,2.6600557016087163E-2,0.54619873002182051,2.2468346408706856,1468.2840000000001,248.54400000000001,{"$f":"T560*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2749612807927481E-2},{"$f":"U560*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8509442081596798E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3773570589161956},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.672222732810167E-2}]
["Multi-Family (2-4 units)",10560,"West North Central","Before 1950","Siding","central furnace","central AC",41.259947805358252,16503.97912,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5501.3263733333333},"Mixed-Humid",71.240465631416257,"Metropolitan Area",0.40006811668071146,0.12315086025175769,1.6037389624972108E-2,6.4662260112577606E-3,0.22103298969623614,0.76460017359451593,307.42399999999998,84.373999999999995,{"$f":"T561*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6912397589956265E-3},{"$f":"U561*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6416891142362667E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.40175935643970706},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6501558536395733E-2}]
["Single Family Detached",10561,"South Atlantic","1990s","Siding","heat pump","central AC",82.555253271417072,18762.557560000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18762.557560000001},"Mixed-Humid",276.50563075464567,"Metropolitan Area",0.4211993225228533,0.23524558461423703,0.12703112669512007,1.4916383360660482E-2,0.3569920118218925,1.1404680456541028,376.53300000000002,418.47500000000002,{"$f":"T562*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0647220857394805E-3},{"$f":"U562*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8516612749210003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4282640446085928},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13488278797004108}]
["Single Family Detached",10562,"West North Central","Before 1950","Brick","central furnace","central AC",29.719948936524009,8800.6955689999995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8800.6955689999995},"Mixed-Humid",168.47161846977815,"Metropolitan Area",0.36323273634801723,6.6976822359013158E-2,0.1364096460297716,2.9950016720077795E-2,0.73113851883343539,1.2977577235702373,2657.4949999999999,745.64700000000005,{"$f":"T563*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3387804471139653E-2},{"$f":"U563*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5622122489381431E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38662054081915687},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14297185827870973}]
["Single Family Detached",10563,"South Atlantic","2000s","Siding","heat pump","central AC",73.327264064103659,15634.811100000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15634.811100000001},"Mixed-Humid",392.42963104718314,"Metropolitan Area",0.58372190442902494,0.29889043364172246,6.8194652636280911E-2,1.3883524639066801E-2,0.38816292234030186,1.33896991304733,657.51199999999994,230.476,{"$f":"T564*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.02800759159832E-2},{"$f":"U564*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6034487230836004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59400198034500817},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.1798101359364513E-2}]
["Single Family Detached",10564,"New England","1980s","Wood","radiator","window/wall unit",26.62415927972971,9820.789111,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9820.789111},"Cold/Very Cold",29.710332437050177,"Micropolitan Area",0.83983083043325735,0.10199307857389628,1.1361926263032784E-2,1.1529410000531782E-3,8.8856771417444469E-2,1.0420426066876309,117.398,0,{"$f":"T565*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1529410000531782E-3},{"$f":"U565*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84098377143331049},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1361926263032784E-2}]
["Single Family Attached",10565,"Pacific","1970s","Shingle","central furnace","central AC",6.7488014355502042,6301.4019010000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6301.4019010000002},"Hot-Dry/Mixed-Dry",37.621656755514309,"Metropolitan Area",2.5356797139810698E-2,8.9560968228254462E-2,5.4785043473091696E-2,2.974419232319525E-3,7.5926032603282095E-2,0.24562884144443897,103.59699999999999,368.428,{"$f":"T566*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5280633273789694E-4},{"$f":"U566*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3216128995816277E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6009603472548597E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7106656372673321E-2}]
["Single Family Detached",10566,"Pacific","2000s","Wood","central furnace","window/wall unit",10.234060488277317,15229.25668,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15229.25668},"Cold/Very Cold",129.9987320640964,"Micropolitan Area",9.7515961144119326E-2,0.17395709818270078,1.0012185448389081E-2,1.7629692117901601E-3,0.16207040444659734,0.44355564922180646,115.762,0,{"$f":"T567*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7629692117901601E-3},{"$f":"U567*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.9278930355909484E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0012185448389081E-2}]
["Multi-Family (5+ units)",10567,"South Atlantic","2000s","Brick","built-in electric unit","central AC",86.837137828685002,45751.916660000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3639.1729890548399},"Mixed-Humid",761.01784572418001,"Metropolitan Area",0.61146837265981757,1.0001254602084351,0.21394449168112781,1.0916315811242682E-2,0.76100659068252774,2.5965929316463083,0,238.59800000000001,{"$f":"T568*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U568*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6829939684250667E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.61146837265981757},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21481279107797033}]
["Multi-Family (5+ units)",10568,"East North Central","2000s","Siding","central furnace","central AC",14.033426025304227,13839.67064,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1100.8272275188942},"Cold/Very Cold",41.488896785879305,"Metropolitan Area",0.19015937509023123,0.14839704480940441,1.3369863968405442E-2,3.8459199138202401E-3,0.15578100732398747,0.51124730112676642,235.113,42.777999999999999,{"$f":"T569*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5881879194364978E-4},{"$f":"U569*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.709118713880326E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19041819388217487},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3416955155544245E-2}]
["Multi-Family (5+ units)",10569,"Middle Atlantic","1980s","Brick","radiator","N/A",12.543746140447238,24309.58554,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1933.6192564284609},"Mixed-Humid",20.496699979760677,"Metropolitan Area",0.2453906736373376,0.43152766956045252,0,1.92502745974152E-3,0.12935886493944299,0.80804911615529651,79.188000000000002,0,{"$f":"T570*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5311944167805696E-4},{"$f":"U570*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24554379307901567},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10570,"East North Central","1960s","Brick","central furnace","central AC",49.527523768164578,16794.684219999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16794.684219999999},"Cold/Very Cold",115.14047544813356,"Metropolitan Area",1.4684406955730669,0.49643397009087459,9.1021763789396928E-2,2.9431743593233677E-2,0.27743896303276372,2.3333353924861022,1452.7560000000001,299.68799999999999,{"$f":"T571*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4398578268710319E-2},{"$f":"U571*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0331653245233596E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4928392738417773},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.6054929113920287E-2}]
["Single Family Detached",10571,"Pacific","1980s","Stucco","N/A","central AC",18.660897782028151,14443.41934,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14443.41934},"Hot-Dry/Mixed-Dry",152.25362949311688,"Metropolitan Area",0,0.3838232241604464,0.16868275905366842,7.4574984907255009E-3,0.37300059672795238,0.92550657994206731,0,516.32500000000005,{"$f":"T572*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U572*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4574984907255009E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17614025754439391}]
["Mobile Home",10572,"Middle Atlantic","2010s","Siding","central furnace","window/wall unit",24.51985987247394,31435.717789999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31435.717789999999},"Cold/Very Cold",277.37720539266274,"Metropolitan Area",0.60063594123425423,0.58710965484070177,1.0311921378089279E-2,7.7419571416034094E-3,0.4160645821592262,1.6141220996122714,246.279,0,{"$f":"T573*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7419571416034094E-3},{"$f":"U573*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60837789837585765},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0311921378089279E-2}]
["Multi-Family (2-4 units)",10573,"South Atlantic","2000s","Brick","central furnace","central AC",18.522518461036775,23269.49555,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7756.4985166666665},"Hot-Humid",300.76714225310417,"Rural",0.20664554639462371,0.45597949430462448,0.14159425214537016,9.3183858404752504E-3,0.21578594386363709,1.0262174939352389,138.255,262.2,{"$f":"T574*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.07237470242175E-3},{"$f":"U574*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0337539110699999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20771792109704545},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14362800605644016}]
["Single Family Detached",10574,"East North Central","Before 1950","Brick","central furnace","central AC",43.982883116682252,18495.745630000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18495.745630000001},"Cold/Very Cold",246.02265870062297,"Metropolitan Area",0.64767255310904936,0.27162770650937229,8.5876634755880241E-2,5.6680970808705836E-2,0.55436048064394428,1.5595373750182462,2830.1210000000001,234.42,{"$f":"T575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2345198118121238E-2},{"$f":"U575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3357726905845998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.70001775122717058},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0212407446464846E-2}]
["Multi-Family (5+ units)",10575,"West South Central","Before 1950","Brick","central furnace","central AC",18.624511089681572,28048.962479999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2231.0546547544059},"Hot-Humid",171.74379729234983,"Metropolitan Area",0.12750374889322089,0.12441981216048384,0.15314411751683307,8.667241602169919E-3,0.17298145773447002,0.58602697309464002,72.016999999999996,236.98699999999999,{"$f":"T576*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6067386307144806E-4},{"$f":"U576*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2873094946628244E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12766442275629233},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15367284846629936}]
["Mobile Home",10576,"West South Central","1990s","Siding","central furnace","central AC",39.988956862720094,32458.568879999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32458.568879999999},"Hot-Humid",537.67755679151526,"Micropolitan Area",0.66364406920935204,0.18346323186346464,0.45638455166003083,2.5145393642784959E-2,0.53106399351351741,1.8345558462463651,256.79599999999999,517.89599999999996,{"$f":"T577*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.33523065410848E-3},{"$f":"U577*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6810162988676478E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6719792998634605},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.47319471464870733}]
["Single Family Detached",10577,"Mountain North","2010s","Siding","central furnace","central AC",53.069314928918622,14061.82166,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14061.82166},"Cold/Very Cold",114.64667880338111,"Metropolitan Area",0.80224654194421563,0.22850641594999416,5.5606081634125649E-2,3.2372324301817378E-2,0.30643585039669491,1.3927948899250302,2071.7460000000001,230.39699999999999,{"$f":"T578*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9132522776818361E-2},{"$f":"U578*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2398015249990196E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83137906472103396},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8845883159124666E-2}]
["Single Family Detached",10578,"South Atlantic","2000s","Siding","heat pump","central AC",45.485345352960039,22629.52505,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22629.52505},"Mixed-Humid",262.79667441986317,"Micropolitan Area",0.22759047399576177,0.32619835784683621,0.14419854701115709,1.051532929355865E-2,0.49275120962433527,1.1907385884780903,140.24,324.43299999999999,{"$f":"T579*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1735645930120004E-3},{"$f":"U579*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.34176470054665E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23076403858877376},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15154031171170373}]
["Single Family Detached",10579,"East North Central","1970s","Brick","central furnace","central AC",77.217427270658533,19122.69125,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19122.69125},"Cold/Very Cold",87.444242551576849,"Metropolitan Area",2.2358513546504684,0.31469813325877877,9.7789350796572513E-2,4.4235967110578756E-2,0.29856885072898054,2.9469076894348003,1993.0940000000001,320.17700000000002,{"$f":"T580*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8113321194227501E-2},{"$f":"U580*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1226459163512504E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2739646758446961},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10391199671292377}]
["Single Family Detached",10580,"Pacific","1970s","Siding","central furnace","central AC",15.688950807488725,14526.8063,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14526.8063},"Marine",112.2849493208186,"Metropolitan Area",2.9760196458432E-2,0.1171320506467458,1.7410958422801999E-2,1.4579248070743E-3,0.21881304146946043,0.38311624699744024,47.649000000000001,52.712000000000003,{"$f":"T581*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9218779338870004E-4},{"$f":"U581*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6573701368560002E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0452384251820699E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8176695436487599E-2}]
["Single Family Detached",10581,"East North Central","Before 1950","Siding","central furnace","window/wall unit",80.221342052974563,32412.66346,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32412.66346},"Cold/Very Cold",333.67592381415147,"Metropolitan Area",2.1555758547394359,0.93720856614025594,0.1152534349210199,0.1177234419399892,1.0059786114413281,4.2140164672420406,3632.02,0,{"$f":"T582*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.1177234419399892},{"$f":"U582*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2732992966794252},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1152534349210199}]
["Single Family Detached",10582,"Pacific","Before 1950","Siding","central furnace","N/A",33.712388182863855,15932.130520000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15932.130520000001},"Hot-Dry/Mixed-Dry",148.84279076461888,"Metropolitan Area",0.16163076311165711,0.5284855458818376,0,2.5741065317248404E-3,0.57019836492768916,1.2603146739211839,161.56700000000001,0,{"$f":"T583*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5741065317248404E-3},{"$f":"U583*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16420486964338196},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10583,"South Atlantic","1960s","Siding","portable electric heaters","N/A",42.933849013198838,34990.911990000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34990.911990000001},"Mixed-Humid",352.8356548181788,"Metropolitan Area",0.47695279349863645,0.40644988485728134,0,0,0.32047256030655669,1.2038752386624745,0,0,{"$f":"T584*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U584*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.47695279349863645},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10584,"Middle Atlantic","1990s","Brick","central furnace","central AC",76.12285643227122,22764.01209,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22764.01209},"Cold/Very Cold",321.26435958994415,"Metropolitan Area",0.81104846978102441,0.19503998406201981,6.4622614105164539E-2,1.9867428135620039E-2,0.81953748858555464,1.8902485565337634,744.76900000000001,127.98699999999999,{"$f":"T585*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6953930520257208E-2},{"$f":"U585*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9134976153628298E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.82800240030128158},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.753611172052737E-2}]
["Multi-Family (5+ units)",10585,"East North Central","1970s","Brick","built-in electric unit","window/wall unit",15.406908189008833,14715.289580000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1170.475212298049},"Cold/Very Cold",112.01135689077452,"Metropolitan Area",0.29744756478648837,0.31627998637691818,1.156199432177054E-2,0,7.3173204819639209E-2,0.69846275030481642,0,0,{"$f":"T586*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U586*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29744756478648837},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.156199432177054E-2}]
["Multi-Family (5+ units)",10586,"Middle Atlantic","1960s","Siding","radiator","window/wall unit",50.708614150190677,29688.884160000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2361.4963743084004},"Mixed-Humid",209.09881115912933,"Metropolitan Area",1.2107248127639236,0.32131326313186465,0.16586277038113537,2.6982742368816003E-3,0.54486284174678301,2.245247337662609,90.885000000000005,0,{"$f":"T587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1462459797901899E-4},{"$f":"U587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2109394373619027},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16586277038113537}]
["Multi-Family (5+ units)",10587,"Pacific","1970s","Siding","central furnace","N/A",9.2129881738075081,17124.513330000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1362.108320496437},"Marine",131.8930017001216,"Micropolitan Area",0.12479391878201458,0.11582260488020149,0,1.9600546712384703E-3,0.20757728850854118,0.44999796128574004,114.459,0,{"$f":"T588*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.559055562557017E-4},{"$f":"U588*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12494982433827029},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10588,"South Atlantic","1980s","Siding","heat pump","central AC",42.953780741036091,16937.610700000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16937.610700000001},"Mixed-Humid",195.57203592413131,"Metropolitan Area",0.29457675728023036,0.1513983237516916,7.7396361280817907E-2,9.3106384770114004E-3,0.34384188132729659,0.86721332364003645,339.49900000000002,210.203,{"$f":"T589*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7503018950393007E-3},{"$f":"U589*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5603365819721002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30032705917526964},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.0956697862790014E-2}]
["Single Family Detached",10589,"South Atlantic","2000s","Siding","heat pump","central AC",32.341450134753252,19002.027109999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19002.027109999999},"Hot-Humid",163.82223329676771,"Metropolitan Area",4.0316714931449657E-2,0.11862429667608497,0.10749781171804136,5.2913424731048193E-3,0.29252262090906628,0.55896144423464222,33.933999999999997,244.52799999999999,{"$f":"T590*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4481478795073998E-4},{"$f":"U590*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6465276851540794E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.0961529719400397E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11214433940319544}]
["Single Family Detached",10590,"South Atlantic","1970s","Brick","central furnace","both central and individual units",49.26363021417253,17638.24927,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17638.24927},"Mixed-Humid",253.72166509641121,"Metropolitan Area",0.87261687683746958,0.13595581939390197,0.20466916471329025,2.0508803785695421E-2,0.77257270933978028,1.9858145702844419,570.04499999999996,592.70100000000002,{"$f":"T591*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.005459580511715E-2},{"$f":"U591*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.045420798057827E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88267147264258672},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21512337269386853}]
["Single Family Attached",10591,"New England","1990s","Wood","central furnace","central AC",24.774038256267922,7441.885929,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7441.885929},"Cold/Very Cold",34.042006712126337,"Metropolitan Area",0.92050421759411061,4.7463388451877163E-2,8.6299458081352028E-3,4.3454213803461065E-3,0.10359948378843772,1.0801970356425605,527.00400000000002,56.91,{"$f":"T592*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9219036521267164E-3},{"$f":"U592*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2351772821939E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.92442612124623735},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0534635363545921E-3}]
["Single Family Detached",10592,"Mountain South","2000s","Stucco","central furnace","central AC",38.570603510598914,10198.467350000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10198.467350000001},"Hot-Dry/Mixed-Dry",137.80683083537335,"Metropolitan Area",0.72471392066332574,0.24165784428272913,9.0782146642457817E-2,2.4094154472993453E-2,0.36471390772398676,1.4218678193124996,1833.953,528.57399999999996,{"$f":"T593*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8703509791934549E-2},{"$f":"U593*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3906446810589002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.74341743045526032},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.6172791323516721E-2}]
["Single Family Detached",10593,"West South Central","1980s","Brick","central furnace","central AC",24.377557005118735,14156.53717,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14156.53717},"Hot-Humid",164.40861488424684,"Metropolitan Area",0.16353449119454505,5.9224227164124246E-2,0.18637831480775011,1.214074537275219E-2,0.15182513797897434,0.56096217114539371,200.017,657.59,{"$f":"T594*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8315480951318899E-3},{"$f":"U594*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.3091972776203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16636603928967694},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19568751208537041}]
["Single Family Detached",10594,"West South Central","1990s","Brick","central furnace","central AC",168.22071268792646,26218.939009999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26218.939009999998},"Hot-Humid",468.04298495461148,"Metropolitan Area",1.680159453963858,0.23894236782678352,0.67377392761383381,7.7555778905214062E-2,0.64959476962093399,3.2424705190254088,1321.627,1636.3789999999999,{"$f":"T595*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.465165770696927E-2},{"$f":"U595*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2904121198244785E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7148111116708273},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.71667804881207864}]
["Single Family Detached",10595,"Pacific","1970s","Stucco","N/A","N/A",30.001640208144433,16511.634679999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16511.634679999999},"Hot-Dry/Mixed-Dry",43.376064296530231,"Metropolitan Area",0,0.69851644932005996,0,0,0.17734141251235985,0.87585786183241987,0,0,{"$f":"T596*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U596*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10596,"East North Central","1960s","Siding","central furnace","central AC",18.325969872089033,20590.97738,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20590.97738},"Cold/Very Cold",62.484618104445069,"Metropolitan Area",0.82415450795479872,0.18229013133010796,4.8151321100876457E-2,1.7720842224956561E-2,0.23097127886994911,1.2855672392557322,761.27,99.341999999999999,{"$f":"T597*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5675293350072599E-2},{"$f":"U597*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0455488748839599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83982980130487128},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0196869975760415E-2}]
["Single Family Detached",10597,"South Atlantic","1960s","Siding","central furnace","central AC",34.139738384603888,18483.88651,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18483.88651},"Mixed-Humid",221.43696039391153,"Metropolitan Area",0.59857752280043952,0.24812885699509013,0.23177930486039983,2.8369494144937727E-2,0.50674182987031169,1.5852275145262411,920.13800000000003,614.68499999999995,{"$f":"T598*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7007726365538382E-2},{"$f":"U598*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1361767779399349E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6155852491659779},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24314107263979917}]
["Multi-Family (2-4 units)",10598,"Pacific","Before 1950","Stucco","central furnace","both central and individual units",20.799941261229925,24046.174869999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8015.391623333333},"Hot-Dry/Mixed-Dry",127.93045953525484,"Metropolitan Area",0.18533727947327583,0.42380421361380194,5.8879175232583562E-2,3.5306517638123598E-3,0.1899284957951213,0.8603029319573241,65.468000000000004,81.36,{"$f":"T599*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2475165879638664E-4},{"$f":"U599*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.521322624744E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18586203113207223},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9531307495057965E-2}]
["Multi-Family (5+ units)",10599,"Pacific","2000s","Brick","heat pump","central AC",25.202271388857877,19970.10411,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1588.4506873405605},"Hot-Dry/Mixed-Dry",112.03324263115638,"Metropolitan Area",7.1845441153247383E-2,0.33971865022279374,3.4313547307316679E-2,3.0852412942662302E-3,0.37898686443949209,0.82770433990507686,73.959000000000003,80.534000000000006,{"$f":"T600*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1748022438502053E-4},{"$f":"U600*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2792428765428471E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.1962921377632397E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4441471594970963E-2}]
["Single Family Detached",10600,"New England","1950s","Wood","wood-burning stove","window/wall unit",10.727539388411056,14575.46113,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14575.46113},"Cold/Very Cold",104.37487712012442,"Metropolitan Area",2.2316823771748991E-2,0.27041842831666207,2.6175123238393549E-2,0,0.32993255766522755,0.64884293299203222,0,0,{"$f":"T601*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U601*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2316823771748991E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6175123238393549E-2}]
["Single Family Detached",10601,"South Atlantic","1990s","Brick","central furnace","central AC",86.313777185402813,24817.072219999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24817.072219999998},"Mixed-Humid",538.51267335968919,"Metropolitan Area",0.92282990336628268,0.44708613256743823,0.32009355072515422,2.64953267288775E-2,0.85848345400210002,2.5484930406609752,469.74099999999999,597.88400000000001,{"$f":"T602*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1657596321695019E-2},{"$f":"U602*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4837730407182479E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.93448749968797773},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.33493128113233672}]
["Multi-Family (2-4 units)",10602,"East North Central","2000s","Brick","built-in electric unit","window/wall unit",39.551181704512985,31691.652010000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10563.884003333334},"Cold/Very Cold",223.18617745909449,"Metropolitan Area",0.16456818871596393,0.25662007806073006,1.8059170981378402E-2,0,0.3222638208519954,0.76151125861006774,0,0,{"$f":"T603*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U603*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16456818871596393},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8059170981378402E-2}]
["Single Family Detached",10603,"Mountain North","Before 1950","Siding","central furnace","central AC",38.045373050678251,29769.462479999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29769.462479999998},"Cold/Very Cold",260.65986547131467,"Rural",1.673141673368634,0.95070097217067862,0.15952999470256055,6.8830629128182566E-2,0.76292714040129328,3.5462997806431664,2079.1260000000002,232.99600000000001,{"$f":"T604*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1894463448192487E-2},{"$f":"U604*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9361656799900801E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7350361368168263},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16646616038255063}]
["Multi-Family (5+ units)",10604,"Pacific","1960s","Concrete","built-in electric unit","window/wall unit",17.60881826482041,30784.64732,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2448.6549456947596},"Hot-Dry/Mixed-Dry",136.68755902589629,"Metropolitan Area",7.5074950404346474E-2,0.13682316541457029,3.8907361223265921E-2,0,0.21557250975373737,0.46637798679592007,0,0,{"$f":"T605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.5074950404346474E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8907361223265921E-2}]
["Single Family Detached",10605,"Pacific","2000s","Stucco","central furnace","central AC",60.829187107526032,17202.824410000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17202.824410000001},"Marine",43.410759700980599,"Metropolitan Area",0.16489134274267214,0.25919894644073316,7.4473951351039704E-3,1.3642699898350503E-3,0.25230434686522013,0.68384203118372944,49.36,29.945,{"$f":"T606*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.491314128776001E-4},{"$f":"U606*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1513857695744997E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16574047415554974},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.962533712061421E-3}]
["Single Family Detached",10606,"West South Central","1990s","Brick","central furnace","central AC",44.482438996757942,14896.99899,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14896.99899},"Hot-Humid",192.69226487433758,"Metropolitan Area",0.92092747217013937,0.21718787696290295,0.33867484033622169,3.507866368070553E-2,0.40743949195305446,1.8842296814223185,1082.1410000000001,1272.606,{"$f":"T607*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6120653384037592E-2},{"$f":"U607*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8958010296667941E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.93704812555417694},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35763285063288963}]
["Single Family Detached",10607,"Pacific","1970s","Wood","heat pump","central AC",9.4787742326453905,8656.4148239999995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8656.4148239999995},"Marine",33.810969472557417,"Metropolitan Area",4.6749470329071792E-2,6.2035807297528917E-2,7.8694861215946321E-3,9.0055280338519181E-4,0.33689960582787881,0.4535543695760742,63.927999999999997,40.104999999999997,{"$f":"T608*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5338728686867185E-4},{"$f":"U608*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4716551651651996E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.7302857615940462E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.2166516381111526E-3}]
["Single Family Detached",10608,"South Atlantic","1980s","Wood","heat pump","central AC",22.21059248607229,14093.01554,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14093.01554},"Mixed-Humid",368.5773693801973,"Metropolitan Area",0.43483365262970697,0.41445492667061834,9.7222232027414937E-2,1.1914136686407222E-2,0.31107517429346682,1.257585985621207,525.09299999999996,320.3,{"$f":"T609*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4001438089452204E-3},{"$f":"U609*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5139928774620003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44223379643865218},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10173622490487694}]
["Single Family Detached",10609,"Pacific","1990s","Stucco","central furnace","central AC",26.90770167151538,16377.17692,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16377.17692},"Hot-Dry/Mixed-Dry",90.776906528136053,"Metropolitan Area",0.69222519147206107,0.17506509372896284,0.12547559159357194,1.32660046205076E-2,0.25030015765022001,1.2430660344448159,450.21199999999999,359.81799999999998,{"$f":"T610*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3732015755070398E-3},{"$f":"U610*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.89280304500056E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6995983930475681},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1313683946385725}]
["Single Family Attached",10610,"Middle Atlantic","Before 1950","Brick","central furnace","window/wall unit",66.904627462026326,23997.355619999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23997.355619999998},"Cold/Very Cold",276.62044588211177,"Metropolitan Area",2.611303496347317,0.35503422913039323,0.10770322768143498,3.6721617474526326E-2,0.44436990481763555,3.518410857976781,1530.2360000000001,0,{"$f":"T611*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6721617474526326E-2},{"$f":"U611*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6480251138218431},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10770322768143498}]
["Single Family Detached",10611,"New England","Before 1950","Siding","central furnace","N/A",47.316981360735745,21123.652389999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21123.652389999999},"Cold/Very Cold",103.89628294648789,"Rural",2.5896231974776467,0.1696225273423046,0,3.2793181792679212E-2,0.14138578074110555,2.9006315055610568,1552.4390000000001,0,{"$f":"T612*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2793181792679212E-2},{"$f":"U612*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6224163792703261},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",10612,"New England","1950s","Siding","central furnace","central AC",76.192183256544752,72911.18015,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24303.726716666668},"Cold/Very Cold",103.75260935317051,"Metropolitan Area",1.0665733244168187,9.8375045261486743E-2,2.7937935883789983E-2,6.4759710209229999E-3,0.25423895202528524,1.4514425716013293,71.631,17.189,{"$f":"T613*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7409002484415502E-3},{"$f":"U613*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1775675853278338E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0683142246652604},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8355692642322766E-2}]
["Single Family Detached",10613,"East North Central","1990s","Brick","heat pump","central AC",50.439393832593723,21741.118030000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21741.118030000001},"Cold/Very Cold",279.63067283398192,"Metropolitan Area",0.36957946124489105,0.20019704134844268,6.3378924600806921E-2,1.074717817017975E-2,0.32094440628283677,0.95409983347697747,346.26299999999998,148.06200000000001,{"$f":"T614*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5281447524218901E-3},{"$f":"U614*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2190334177578605E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37710760599731297},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6597958018564787E-2}]
["Single Family Detached",10614,"East South Central","1980s","Siding","central furnace","central AC",16.314079194835063,15537.218279999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15537.218279999999},"Hot-Humid",368.04980614719659,"Metropolitan Area",0.32830177961242046,0.36701162474010601,0.26940010742684906,1.685945109284628E-2,0.29107241386576305,1.2557859256451385,331.24700000000001,753.85400000000004,{"$f":"T615*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1466569435951598E-3},{"$f":"U615*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.171279414925112E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33344843655601564},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28111290157610019}]
["Multi-Family (2-4 units)",10615,"New England","Before 1950","Siding","radiator","window/wall unit",15.976625639800901,15976.62564,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5325.5418799999998},"Cold/Very Cold",122.84731010330067,"Metropolitan Area",0.49872227726424367,0.47658633758196894,5.9414242892421712E-2,2.8473382449351599E-3,0.42879223002665773,1.4654133132619154,178.21899999999999,0,{"$f":"T616*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4911274831171999E-4},{"$f":"U616*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49967139001255539},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9414242892421712E-2}]
["Single Family Detached",10616,"Pacific","1980s","Wood","heater burning gas/oil/kerosene","N/A",44.829624767764813,20102.97075,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20102.97075},"Marine",203.98484417870384,"Rural",0.45407705799386999,0.16928609143424178,0,0,0.57188802530587202,1.1952511747339838,0,0,{"$f":"T617*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U617*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45407705799386999},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10617,"East South Central","Before 1950","Siding","central furnace","central AC",22.785005250620422,11530.873100000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11530.873100000001},"Mixed-Humid",119.24485221332478,"Metropolitan Area",7.6977007010736107E-2,9.3966791461118804E-2,5.8407354575176207E-2,4.2934629444195006E-3,0.17751227961715824,0.40686343266418934,150.959,221.386,{"$f":"T618*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7406890723029003E-3},{"$f":"U618*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5527738721166002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.871769608303901E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0960128447292809E-2}]
["Single Family Detached",10618,"East North Central","2010s","Siding","central furnace","central AC",73.596576137285624,14045.14812,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14045.14812},"Cold/Very Cold",114.8841289439698,"Metropolitan Area",1.40187290559348,0.34056881625053365,2.806224807920436E-2,2.9283206850424081E-2,0.38814992971050882,2.1586538996337268,1955.617,129.31700000000001,{"$f":"T619*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7466930430990039E-2},{"$f":"U619*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8162764194340401E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.42933983602447},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.9878524498638401E-2}]
["Multi-Family (5+ units)",10619,"Middle Atlantic","Before 1950","Brick","central furnace","N/A",30.454240403626176,37644.302109999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2994.2817138916362},"Cold/Very Cold",165.88021953822644,"Metropolitan Area",0.49074156097054755,0.60108979832477183,0,9.2354648581568482E-3,0.55674778433905814,1.6570800063882569,245.33500000000001,0,{"$f":"T620*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3460210427760456E-4},{"$f":"U620*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49147616307482517},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10620,"South Atlantic","1970s","Brick","heat pump","central AC",10.818304439640798,13388.99064,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13388.99064},"Mixed-Humid",121.69253595531586,"Rural",0.1194933272693868,0.13829974452416233,6.5222098051416724E-2,4.6320552018143998E-3,9.2204207882714148E-2,0.41521937772768003,142.625,203.33500000000001,{"$f":"T621*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.90960479003E-3},{"$f":"U621*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7224504117844004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1214029320594168},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7944548463201124E-2}]
["Multi-Family (5+ units)",10621,"South Atlantic","2000s","Concrete","N/A","central AC",15.431569084161177,20093.188910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1598.2410286469571},"Hot-Humid",209.41704186219036,"Metropolitan Area",0,0.204295488923534,0.25774684163788553,1.1119691301927458E-2,0.24225343162747048,0.71453097731611814,0,553.40599999999995,{"$f":"T622*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U622*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8447617469939789E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25863131781258492}]
["Single Family Detached",10622,"West South Central","2010s","Brick","central furnace","central AC",79.127442218932757,27970.110359999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27970.110359999999},"Mixed-Humid",471.71565955295904,"Metropolitan Area",1.3752539093175113,0.3775020347973142,0.43475553610904732,6.5342373317513996E-2,1.1840818411212584,3.3715933213451308,1486.347,849.803,{"$f":"T623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1573289623254919E-2},{"$f":"U623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3769083694259077E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4168271989407664},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.45852461980330639}]
["Single Family Detached",10623,"Pacific","1990s","Stucco","central furnace","central AC",120.17478347611558,21191.109759999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21191.109759999999},"Hot-Dry/Mixed-Dry",236.4526066309256,"Metropolitan Area",0.22364116092322109,0.17480429889920318,0.12074516335926017,1.1315755936303358E-2,1.2651233235688808,1.7843139467505653,90.727000000000004,443.25900000000001,{"$f":"T624*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.92260581519552E-3},{"$f":"U624*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.3931501211078402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2255637667384166},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.130138313480368}]
["Single Family Detached",10624,"Mountain South","1980s","Stucco","heater burning gas/oil/kerosene","N/A",47.349651871517949,10550.27894,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10550.27894},"Hot-Dry/Mixed-Dry",98.390382130995292,"Metropolitan Area",0.35722205288364411,0.15695470624296021,0,0,0.22579218509473073,0.73996894422133508,0,0,{"$f":"T625*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U625*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35722205288364411},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",10625,"Middle Atlantic","1970s","Siding","central furnace","N/A",12.334477899098957,16060.518099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16060.518099999999},"Cold/Very Cold",353.79638227123928,"Metropolitan Area",0.7871143963869317,0.21311962217560848,0,9.5286250861394989E-3,0.23709837721186125,1.2373323957744014,593.29499999999996,0,{"$f":"T626*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5286250861394989E-3},{"$f":"U626*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.7966430214730712},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10626,"East South Central","1990s","Brick","heat pump","central AC",54.914061035414058,26075.05272,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26075.05272},"Mixed-Humid",373.72327458789863,"Micropolitan Area",0.79147338904516618,0.20048716910617201,0.15586821684307872,2.1825627453274318E-2,0.2757262383037305,1.4235550132981472,539.83799999999997,297.19299999999998,{"$f":"T627*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4076304310259359E-2},{"$f":"U627*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7493231430149591E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80554969335542559},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16361753998609369}]
["Mobile Home",10627,"South Atlantic","1990s","Siding","central furnace","window/wall unit",22.262082496374536,17460.456859999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17460.456859999998},"Mixed-Humid",214.37159719937117,"Rural",0.29115938644451267,0.10247224350819148,6.6838436795054537E-2,3.8561418975309996E-3,0.27096584427221698,0.73143591101997563,220.85,0,{"$f":"T628*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8561418975309996E-3},{"$f":"U628*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29501552834204364},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6838436795054537E-2}]
["Single Family Detached",10628,"Pacific","1990s","Stucco","central furnace","central AC",54.572483691007776,14141.61277,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14141.61277},"Hot-Dry/Mixed-Dry",113.63914363804948,"Metropolitan Area",0.14895738311701959,0.58988643485180914,0.11528276669974649,9.51618820680117E-3,0.34342878328719451,1.1975553679557698,157.63399999999999,515.28700000000003,{"$f":"T629*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2291989873861797E-3},{"$f":"U629*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.2869892194149903E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15118658210440578},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12256975591916149}]
["Multi-Family (2-4 units)",10629,"South Atlantic","2000s","Concrete","central furnace","central AC",10.640800392359603,18346.207569999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6115.4025233333332},"Hot-Humid",157.2880550797027,"Metropolitan Area",2.0637655010895518E-2,9.0639658654075833E-2,8.9711982668298787E-2,4.0637950540004198E-3,0.33296836665838658,0.53666685969432371,17.556999999999999,203.94900000000001,{"$f":"T630*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0736812210216332E-4},{"$f":"U630*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2472302292313101E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.074502313299768E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0959212897530103E-2}]
["Multi-Family (2-4 units)",10630,"East South Central","1960s","Brick","heat pump","central AC",18.538687811839189,13385.33416,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4461.7780533333334},"Mixed-Humid",87.417890691981242,"Micropolitan Area",0.15334572108516584,0.11546232079485311,0.22272835530573293,1.3503767596647683E-2,6.5447055961953521E-2,0.56598596487880382,244.72499999999999,764.12300000000005,{"$f":"T631*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.091908634102E-3},{"$f":"U631*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4093472314472269E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15443762971926783},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22613770253718016}]
["Multi-Family (5+ units)",10631,"East South Central","1990s","Brick","built-in electric unit","central AC",47.573984296417869,48743.836369999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3877.1545686019113},"Mixed-Humid",430.30585931588138,"Micropolitan Area",0.6159120545258816,0.43535684187840057,9.9464458494318203E-2,4.4156553929219295E-3,0.31340585626020695,1.4682036389965141,0,90.588999999999999,{"$f":"T632*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U632*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5122755521507852E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6159120545258816},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.9815686049533281E-2}]
["Multi-Family (5+ units)",10632,"East North Central","2010s","Siding","built-in electric unit","central AC",12.66770754170479,12310.697319999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":979.21049944869787},"Cold/Very Cold",89.519316066162219,"Metropolitan Area",5.5674574648320596E-2,0.11222669273370275,5.7102264007245765E-3,2.5330490805631996E-4,0.13159526055562659,0.30543991101119417,0,20.576000000000001,{"$f":"T633*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U633*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0148235236656408E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.5674574648320596E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7303746359612332E-3}]
["Single Family Detached",10633,"East South Central","1950s","Siding","heat pump","central AC",20.474539847755462,17499.60671,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17499.60671},"Mixed-Humid",234.98587384212846,"Metropolitan Area",0.27188267464912841,0.16269800848926697,0.15313165598557169,1.1370666953136571E-2,0.2140594766803639,0.80177181580433099,262.15600000000001,387.61099999999999,{"$f":"T634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5876268966667608E-3},{"$f":"U634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7830400564698103E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27647030154579516},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1599146960420415}]
["Single Family Detached",10634,"South Atlantic","Before 1950","Brick","central furnace","central AC",105.83410938566996,26807.01859,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26807.01859},"Cold/Very Cold",223.7036854857665,"Micropolitan Area",2.4384578496868103,0.25343014925849905,0.18248505287584099,7.3210262646494495E-2,0.52914818991309598,3.4035212417342464,2318.7979999999998,412.21300000000002,{"$f":"T635*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.216006109245481E-2},{"$f":"U635*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1050201554039671E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.500617910779265},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19353525442988068}]
["Single Family Attached",10635,"Pacific","1960s","Brick","central furnace","central AC",7.2892287028311307,7035.9350409999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7035.9350409999997},"Hot-Dry/Mixed-Dry",25.050405396314886,"Metropolitan Area",2.1067841011967116E-3,2.3366298055550756E-2,4.1027803692378377E-3,3.3766155855263102E-4,0.17947946995468783,0.20905533248067312,4.9889999999999999,43.002000000000002,{"$f":"T636*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5102279919549003E-5},{"$f":"U636*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0255927863308198E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1418863811162605E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.4053396478709195E-3}]
["Multi-Family (5+ units)",10636,"South Atlantic","1950s","Brick","central furnace","central AC",22.889606944337896,41922.357040000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3334.564331178361},"Mixed-Humid",562.36196669654032,"Metropolitan Area",0.53688221731197294,0.78570776758475402,6.7391026160164624E-2,1.0987262867185443E-2,0.51868469785625626,1.918779029153032,195.46700000000001,66.619,{"$f":"T637*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.517972861224407E-4},{"$f":"U637*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2214534117877122E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53753401459809536},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7613171501343397E-2}]
["Multi-Family (5+ units)",10637,"Pacific","1980s","Stucco","central furnace","central AC",13.876847702413507,18803.31667,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1495.6427429833625},"Hot-Dry/Mixed-Dry",50.814571855071172,"Metropolitan Area",7.4879972647520443E-2,5.450212789402846E-2,2.0944535939641691E-2,1.27140505995872E-3,0.10296318261826932,0.25446009477970905,18.489999999999998,49.125999999999998,{"$f":"T638*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7654434317762371E-5},{"$f":"U638*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.347494539180066E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.4907627081838207E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1018010885033491E-2}]
["Single Family Detached",10638,"West North Central","Before 1950","Siding","heat pump","central AC",49.709464251672379,12884.775600000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12884.775600000001},"Cold/Very Cold",263.96626163452237,"Micropolitan Area",0.92645396842769756,0.1233268358118096,6.237978565971361E-2,4.41143921930316E-2,0.85904057767776132,1.9712011675769823,3187.7719999999999,235.989,{"$f":"T639*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1073726883963206E-2},{"$f":"U639*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0406653090684003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.96752769531166072},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5420450968782004E-2}]
["Multi-Family (2-4 units)",10639,"East South Central","1990s","Brick","central furnace","central AC",22.138984160878916,16447.98229,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5482.6607633333333},"Mixed-Humid",110.12667591227716,"Micropolitan Area",0.39451942265529821,0.21504047636393819,3.8919029284132045E-2,6.4524776604378397E-3,0.11594315944877541,0.76872373952576911,282.32299999999998,109.973,{"$f":"T640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5478812346865565E-3},{"$f":"U640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0294465212605661E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39606730388998479},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9521973936258101E-2}]
["Single Family Detached",10640,"Pacific","1950s","Wood","central furnace","central AC",19.756706877818697,15907.171399999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15907.171399999999},"Hot-Dry/Mixed-Dry",226.26034501222478,"Metropolitan Area",0.9390854311089899,0.10899589071128581,9.9172576084929798E-2,1.31516357270636E-2,0.63256298717526005,1.7798168850804656,550.26,276.51400000000001,{"$f":"T641*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7530801345639987E-3},{"$f":"U641*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3985555924995999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.94783851124355389},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1035711316774294}]
["Multi-Family (2-4 units)",10641,"Middle Atlantic","1950s","Brick","radiator","window/wall unit",81.905192158973904,90803.982440000007,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30267.994146666668},"Cold/Very Cold",167.24005073462678,"Metropolitan Area",2.3924993944898811,0.5931517717821817,2.8508545914915081E-2,2.7313837917952001E-3,0.53938319242414234,3.5553638271389838,30.08,0,{"$f":"T642*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1046126393173334E-4},{"$f":"U642*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3934098557538128},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8508545914915081E-2}]
["Single Family Detached",10642,"East North Central","1970s","Brick","central furnace","central AC",43.588932703864202,20638.699199999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20638.699199999999},"Cold/Very Cold",204.72149022126212,"Metropolitan Area",1.3803873647308416,0.78765911378945275,7.1291783956478394E-2,1.8213115437820799E-2,0.66841186753283066,2.9077501300096036,730.69200000000001,151.78200000000001,{"$f":"T643*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.50805323958464E-2},{"$f":"U643*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1325830419744001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3954678971266881},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4424366998452798E-2}]
["Single Family Detached",10643,"West North Central","1970s","Siding","radiator","central AC",34.998144036377184,8088.3161630000004,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8088.3161630000004},"Cold/Very Cold",102.74509564920913,"Rural",0.12547308612699562,9.281088015083365E-2,1.3918916370473322E-2,2.3232960229762831E-3,0.11836339151318928,0.35056627416149189,209.33099999999999,77.91,{"$f":"T644*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6931353107169529E-3},{"$f":"U644*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3016071225933002E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12716622143771258},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4549077082732653E-2}]
["Multi-Family (5+ units)",10644,"East North Central","Before 1950","Concrete","central furnace","window/wall unit",18.328735848969863,26410.282200000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2100.7116779346711},"Cold/Very Cold",265.3463765790824,"Metropolitan Area",0.65585237173026179,0.32221246797506525,3.4668275648578203E-2,8.9077128009804E-3,0.20664199742774236,1.2275742933464708,337.28199999999998,0,{"$f":"T645*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0853223615716164E-4},{"$f":"U645*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.65656090396641897},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4668275648578203E-2}]
["Single Family Detached",10645,"Pacific","1990s","Siding","central furnace","window/wall unit",17.964584652576232,14464.23885,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14464.23885},"Marine",230.6427605834271,"Micropolitan Area",7.9670850079895106E-2,0.17259311258221768,5.7921610547659501E-3,1.4720689804810501E-3,0.52889698565392862,0.78695310937080742,101.773,0,{"$f":"T646*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4720689804810501E-3},{"$f":"U646*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.1142919060376156E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7921610547659501E-3}]
["Single Family Detached",10646,"East North Central","1950s","Siding","central furnace","central AC",77.211241113716454,27565.598399999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27565.598399999999},"Cold/Very Cold",177.07831676383782,"Metropolitan Area",1.4406631019926703,0.62043361565274713,5.6224641391732791E-2,3.99742249541616E-2,0.51064601191958858,2.627967370956739,1353.8810000000001,96.268000000000001,{"$f":"T647*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7320539927390407E-2},{"$f":"U647*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6536850267712001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4779836419200607},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.887832641850399E-2}]
["Multi-Family (5+ units)",10647,"West North Central","1980s","Siding","central furnace","central AC",8.7517924999878911,10980.91907,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":873.43803258582852},"Mixed-Humid",116.33217509015586,"Metropolitan Area",7.8346486229807555E-2,0.20729719723383022,1.6461985284558604E-2,2.00985957922024E-3,9.296969874501633E-2,0.39692535996245271,117.65,65.382000000000005,{"$f":"T648*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0275998453372273E-4},{"$f":"U648*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7107125446526648E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.8449246214341281E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.651909241000513E-2}]
["Single Family Detached",10648,"South Atlantic","1980s","Brick","central furnace","central AC",58.645149481795642,17097.711220000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17097.711220000001},"Mixed-Humid",198.64221770942308,"Metropolitan Area",0.74095125208219526,0.41379783237690049,0.14322968120155372,2.0783447729984181E-2,0.448011634856462,1.7459904005171116,707.80100000000004,507.76799999999997,{"$f":"T649*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2101777099227221E-2},{"$f":"U649*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6816706307569595E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.75305302918142247},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15191135183231066}]
["Single Family Detached",10649,"Pacific","2000s","Wood","central furnace","N/A",37.380782757583738,12827.99683,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12827.99683},"Hot-Dry/Mixed-Dry",69.928258526204914,"Metropolitan Area",0.27153408295565262,0.17685606459608177,0,5.7024679148303904E-3,0.25638037030037375,0.70477051785210809,444.53300000000002,0,{"$f":"T650*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7024679148303904E-3},{"$f":"U650*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27723655087048299},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10650,"Middle Atlantic","Before 1950","Brick","radiator","N/A",37.624021573117048,42369.393660000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3370.1222642964872},"Mixed-Humid",100.45359543660273,"Metropolitan Area",0.77585045651889917,6.3791359094496E-2,0,1.6305013762177799E-3,0.26960598497215355,1.1107486095466694,38.482999999999997,0,{"$f":"T651*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.296924150969217E-4},{"$f":"U651*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.77598014893399614},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10651,"East North Central","2010s","Siding","central furnace","central AC",65.290990656117486,14271.254790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14271.254790000001},"Cold/Very Cold",102.27133681233443,"Metropolitan Area",0.7920191196918277,0.41678829988695942,2.3696462404724068E-2,1.5326243029095962E-2,0.44817331518226716,1.6806771971657783,983.33100000000002,90.593000000000004,{"$f":"T652*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4033367243905491E-2},{"$f":"U652*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2928757851904701E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80605248693573317},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.4989338189914539E-2}]
["Single Family Detached",10652,"East South Central","1950s","Brick","central furnace","central AC",22.416481247712902,10120.307559999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10120.307559999999},"Mixed-Humid",224.70169479324238,"Metropolitan Area",0.26670586937291701,0.20111084291508799,5.025883382509571E-2,6.2145570227540798E-3,0.24860662024984498,0.76668216636294573,387.60300000000001,226.465,{"$f":"T653*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9226615711786799E-3},{"$f":"U653*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2918954515753999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27062853094409567},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2550729276671107E-2}]
["Mobile Home",10653,"South Atlantic","2010s","Siding","central furnace","both central and individual units",12.060633839116905,9306.044629,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9306.044629},"Hot-Humid",177.40294344034277,"Metropolitan Area",3.5535382679041487E-2,0.12997524535230889,0.18863127256702977,6.4215244237059016E-3,0.2511569485654262,0.60529884916380627,49.222000000000001,640.81600000000003,{"$f":"T654*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5806212872863801E-4},{"$f":"U654*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9634622949772641E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.5993444807770128E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19459473486200704}]
["Single Family Detached",10654,"Pacific","1950s","Wood","central furnace","central AC",20.882354735490399,11588.432150000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11588.432150000001},"Marine",102.46312086915766,"Metropolitan Area",0.29902377771675459,0.25049222347437294,3.06682526170961E-2,1.0605072563047451E-2,0.292018987665637,0.87220324147386064,786.21500000000003,128.928,{"$f":"T655*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1109991828122513E-3},{"$f":"U655*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4940733802352002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30813477689956686},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2162325997331299E-2}]
["Single Family Detached",10655,"East North Central","1950s","Stone","central furnace","central AC",67.030883661516853,28892.62227,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28892.62227},"Cold/Very Cold",211.00097129461349,"Metropolitan Area",6.4864756679843802,0.30878397752305964,0.24120852571211468,7.2297488639020149E-2,0.72768972895532991,7.7641579001748848,2085.444,416.83800000000002,{"$f":"T656*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.025394575723788E-2},{"$f":"U656*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2043542881782259E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.5467296137416184},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25325206859389693}]
["Single Family Detached",10656,"West South Central","2000s","Brick","central furnace","central AC",73.840100452099051,17092.615849999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17092.615849999998},"Hot-Humid",400.34827355986039,"Metropolitan Area",0.20349001884570067,0.23216628336462983,0.9032386196206873,7.3847381926352082E-2,0.54848112126469972,1.8873760430957174,824.21699999999998,3496.2089999999998,{"$f":"T657*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4088024558039449E-2},{"$f":"U657*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9759357368312643E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21757804340374012},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.96299797698899992}]
["Single Family Detached",10657,"Middle Atlantic","1950s","Siding","radiator","window/wall unit",49.057721585281406,17659.367020000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17659.367020000002},"Mixed-Humid",85.544198931613707,"Metropolitan Area",1.4528304560785865,0.17533114907363914,0.14725448612980713,3.9121678727757001E-3,0.18431007189432477,1.9597261631763581,221.535,0,{"$f":"T658*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9121678727757001E-3},{"$f":"U658*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4567426239513621},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14725448612980713}]
["Single Family Detached",10658,"Mountain North","1960s","Brick","built-in furnace","window/wall unit",89.712826350312966,24279.519990000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24279.519990000001},"Cold/Very Cold",264.02960673488843,"Rural",0.58240639397228444,0.7679486647718653,1.590427528992951E-2,0,0.88496470970590968,2.2512240437399886,0,0,{"$f":"T659*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U659*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58240639397228444},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.590427528992951E-2}]
["Single Family Detached",10659,"Pacific","1960s","Wood","heat pump","central AC",43.118916667731703,10210.494119999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10210.494119999999},"Marine",155.06949018817784,"Metropolitan Area",0.12814671455861293,0.10752103654298927,3.6527603663052841E-2,8.9818143100697991E-3,0.2569017499359072,0.52909710470056215,651.65700000000004,228.00800000000001,{"$f":"T660*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.65373996675684E-3},{"$f":"U660*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3280743433129599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13480045452536976},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8855678006365801E-2}]
["Multi-Family (5+ units)",10660,"West North Central","1960s","Concrete","radiator","window/wall unit",17.438883031459781,27946.927940000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2222.9386812821235},"Cold/Very Cold",127.829248374835,"Metropolitan Area",0.50108067226374786,0.28573039734796585,2.7604494231951181E-2,3.9368278450519203E-3,0.40462635433564892,1.2226656050982108,140.86799999999999,0,{"$f":"T661*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1314092615485019E-4},{"$f":"U661*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.50139381318990273},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7604494231951181E-2}]
["Single Family Detached",10661,"East North Central","2010s","Siding","central furnace","central AC",22.733354816942693,10682.967490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10682.967490000001},"Mixed-Humid",208.43537868109442,"Rural",0.26101025714552128,0.16231577950179865,4.2377291586039409E-2,7.2293136620278598E-3,0.24547818388213552,0.71118151211549485,475.98899999999998,200.72499999999999,{"$f":"T662*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0849750125976098E-3},{"$f":"U662*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1443386494302504E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26609523215811892},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.4521630235469657E-2}]
["Single Family Detached",10662,"South Atlantic","2000s","Concrete","central furnace","central AC",15.816869619839627,12911.730299999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12911.730299999999},"Hot-Humid",155.60410376717942,"Metropolitan Area",3.3183069400618201E-2,0.10852455219702388,0.1308286624691529,6.6980246517764994E-3,0.25838492436415261,0.53092120843094759,42.795000000000002,475.96,{"$f":"T663*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5255749818849996E-4},{"$f":"U663*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1454671535879999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.37356268988067E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13697412962274089}]
["Single Family Detached",10663,"Middle Atlantic","1960s","Shingle","central furnace","central AC",65.50098878236011,35832.050759999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35832.050759999998},"Mixed-Humid",222.00890088431817,"Metropolitan Area",3.1523668041026935,0.59026964937320558,0.31359336523113451,6.3965012101401833E-2,0.54220614892602592,4.5984359676330593,1363.338,421.79599999999999,{"$f":"T664*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8851196419036874E-2},{"$f":"U664*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5113815682364959E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2012180005217306},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32870718091349949}]
["Single Family Detached",10664,"Mountain North","2000s","Siding","central furnace","window/wall unit",48.937702083128208,17231.58524,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17231.58524},"Cold/Very Cold",133.60537186787602,"Metropolitan Area",0.77171051391856615,9.9604938373738794E-2,2.1509670907534799E-2,1.470421140126396E-2,0.32004271514690674,1.2128678383467464,853.32899999999995,0,{"$f":"T665*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.470421140126396E-2},{"$f":"U665*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78641472531983014},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1509670907534799E-2}]
["Single Family Detached",10665,"South Atlantic","1950s","Brick","central furnace","central AC",68.380231339963004,38567.53037,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38567.53037},"Mixed-Humid",459.63733654075276,"Metropolitan Area",3.4654977444385384,0.7153395615566045,0.59484672890452905,5.8842712490691222E-2,0.66763877718462472,5.443322812084296,776.17700000000002,749.529,{"$f":"T666*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9935230019995492E-2},{"$f":"U666*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8907482470695731E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.495432974458534},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.6237542113752248}]
["Single Family Detached",10666,"Pacific","1970s","Stucco","central furnace","N/A",31.484054812437588,9639.9432980000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9639.9432980000001},"Hot-Dry/Mixed-Dry",78.513665346730122,"Metropolitan Area",0.11681963810866371,0.14206233091152823,0,3.5422164447366958E-3,0.32024914433939922,0.57913111335959111,367.452,0,{"$f":"T667*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5422164447366958E-3},{"$f":"U667*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1203618545534004},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10667,"East North Central","1960s","Brick","other","window/wall unit",13.766462047226923,12413.4013,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":987.37972113752824},"Cold/Very Cold",66.685412480437691,"Metropolitan Area",5.6637508905393E-2,6.8810090220172995E-2,9.2100486141271989E-3,0,9.2872972104171003E-2,0.22753061984386419,0,0,{"$f":"T668*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U668*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.6637508905393E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2100486141271989E-3}]
["Single Family Detached",10668,"East North Central","1990s","Siding","built-in electric unit","window/wall unit",43.680252605979454,13684.28966,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13684.28966},"Cold/Very Cold",267.44575718397948,"Metropolitan Area",0.46041705303190328,0.14783066961391769,2.0644050959627701E-2,0,0.28364508237165131,0.91253685597709999,0,0,{"$f":"T669*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U669*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.46041705303190328},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0644050959627701E-2}]
["Single Family Attached",10669,"South Atlantic","1980s","Concrete","central furnace","N/A",17.99568279315044,25133.635190000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25133.635190000001},"Hot-Humid",69.615293539895035,"Metropolitan Area",1.18623218006243E-3,6.569404432327011E-3,0,7.0876851235800002E-4,0.23681866154155221,0.24457429815394166,28.2,0,{"$f":"T670*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0876851235800002E-4},{"$f":"U670*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.89500069242043E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10670,"Pacific","2000s","Stucco","central furnace","both central and individual units",32.620365091165397,11263.93822,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11263.93822},"Hot-Dry/Mixed-Dry",229.26595076572806,"Metropolitan Area",0.63262941440336895,0.2293984259006446,0.1974884210793689,1.5390560834464538E-2,0.70776302496953225,1.7672792863529148,587.02300000000002,779.33399999999995,{"$f":"T671*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6121908057190596E-3},{"$f":"U671*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7783700287454806E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63924160520908802},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20626679110811438}]
["Single Family Detached",10671,"South Atlantic","1950s","Brick","central furnace","central AC",55.819840316979025,21143.878909999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21143.878909999999},"Mixed-Humid",374.54341101112783,"Metropolitan Area",0.71870306810133366,0.19210719433913392,0.18176081778434577,2.2559271308114307E-2,0.18537102938883351,1.277942109613647,651.90899999999999,415.03199999999998,{"$f":"T672*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.378388495633919E-2},{"$f":"U672*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7753863517751191E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.73248695305767286},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19053620413612088}]
["Single Family Detached",10672,"Mountain North","1970s","Wood","central furnace","N/A",82.876682230450598,38781.7886,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38781.7886},"Cold/Very Cold",517.14146096126876,"Metropolitan Area",2.3470576352843651,0.62124202000421469,0.11502926702207039,4.4333401638090006E-2,0.9838819932093229,4.0672109155199729,1143.1500000000001,0,{"$f":"T673*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4333401638090006E-2},{"$f":"U673*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3913910369224549},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11502926702207039}]
["Mobile Home",10673,"South Atlantic","2000s","Siding","central furnace","window/wall unit",19.094709732867393,20356.8334,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20356.8334},"Cold/Very Cold",339.396169974342,"Micropolitan Area",0.36930563059360699,0.50352631486266675,2.7637902715844799E-2,5.0384587643338002E-3,0.62181706450705743,1.522286912679176,247.50700000000001,0,{"$f":"T674*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0384587643338002E-3},{"$f":"U674*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37434408935794078},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7637902715844799E-2}]
["Single Family Detached",10674,"East North Central","1990s","Siding","central furnace","central AC",41.153160893466925,14259.584510000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14259.584510000001},"Cold/Very Cold",146.2003686043517,"Metropolitan Area",1.3213377046769472,0.23463928139561999,7.1025578745443518E-2,3.6913971795635624E-2,0.32995619069010879,1.9569587555081198,2320.7959999999998,267.91699999999997,{"$f":"T675*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3093586692469958E-2},{"$f":"U675*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8203851031656699E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3544312913694172},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4845963848609184E-2}]
["Single Family Detached",10675,"New England","2000s","Concrete","central furnace","central AC",93.570970505612735,17428.007170000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17428.007170000001},"Cold/Very Cold",522.77445928416171,"Metropolitan Area",1.972932201281649,0.27057040386649378,6.6707963084107091E-2,5.2840602346981125E-2,1.0055470235808452,3.315757591813095,2819.3440000000001,212.59200000000001,{"$f":"T676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.913554744669648E-2},{"$f":"U676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7050549002846404E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0220677487283454},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0413017984391729E-2}]
["Mobile Home",10676,"Pacific","1990s","Wood","central furnace","N/A",29.368253510739763,22660.689439999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22660.689439999998},"Marine",257.67469959152919,"Metropolitan Area",0.48164289270108857,0.70735008974825231,0,5.1444523773582392E-3,0.492780802846364,1.6817737852957049,227.02099999999999,0,{"$f":"T677*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1444523773582392E-3},{"$f":"U677*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.48678734507844679},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10677,"Mountain South","1980s","Stucco","built-in electric unit","N/A",20.583221436188236,35734.759440000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2842.393954571005},"Hot-Dry/Mixed-Dry",139.43106362157405,"Metropolitan Area",0.193855709748084,0.33027965763650208,0,0,0.28188314382316471,0.80601851120775081,0,0,{"$f":"T678*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U678*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.193855709748084},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10678,"Pacific","1970s","Stucco","central furnace","central AC",7.099003479757573,7783.9950440000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7783.9950440000002},"Hot-Dry/Mixed-Dry",44.83708802628761,"Metropolitan Area",1.1368423569826428E-2,3.9803575417419662E-2,1.6681825290831089E-2,1.0737943323247561E-3,8.513031565428969E-2,0.15298413993236687,43.335000000000001,94.614000000000004,{"$f":"T679*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3731942523174E-4},{"$f":"U679*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3647490709301613E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1705742995058168E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7418300197924105E-2}]
["Single Family Detached",10679,"Middle Atlantic","1980s","Siding","central furnace","both central and individual units",71.545963160556198,21293.441419999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21293.441419999999},"Cold/Very Cold",704.23492172332726,"Micropolitan Area",2.2994119201266239,0.98877398392384896,3.0687575438468499E-2,4.5301392045663025E-2,1.5884715658347226,4.9073450453236633,2078.788,48.692999999999998,{"$f":"T680*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4264550502598955E-2},{"$f":"U680*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.03684154306406E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.343676470629223},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.1724416981532562E-2}]
["Single Family Detached",10680,"Pacific","1970s","Stucco","central furnace","central AC",32.578661650107655,13804.51765,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13804.51765},"Hot-Dry/Mixed-Dry",144.71473255368412,"Metropolitan Area",0.12072254991786222,0.22415484484747586,0.19349495592875524,1.42105637321571E-2,0.35062708680270421,0.88899943749679755,301.51900000000001,727.89499999999998,{"$f":"T681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1623243573103499E-3},{"$f":"U681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.004823937484675E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12488487427517256},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20354319530360199}]
["Multi-Family (5+ units)",10681,"Pacific","Before 1950","Stucco","built-in electric unit","N/A",11.69247724816497,23526.11116,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1871.3005819453604},"Marine",50.981082890892338,"Metropolitan Area",8.1881500639044327E-2,0.13763925455435724,0,0,9.2070565277995647E-2,0.3115913204713972,0,0,{"$f":"T682*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U682*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.1881500639044327E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",10682,"Middle Atlantic","Before 1950","Stucco","built-in electric unit","window/wall unit",34.582125410049123,55331.400659999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18443.800220000001},"Mixed-Humid",770.76641113917492,"Metropolitan Area",0.58245152218755603,0.89343009533434803,0.13316541799161408,0,1.020854437856282,2.6299014733698001,0,0,{"$f":"T683*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U683*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58245152218755603},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13316541799161408}]
["Single Family Attached",10683,"West North Central","1990s","Siding","central furnace","central AC",8.9387849692717065,8082.0840589999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8082.0840589999998},"Cold/Very Cold",55.133472004548921,"Metropolitan Area",6.8391953097379915E-2,0.22330933225820787,1.2837881356425782E-2,1.9093277022662781E-3,0.10688556168027497,0.4114247283922885,166.93299999999999,69.308999999999997,{"$f":"T684*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3491665382210469E-3},{"$f":"U684*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6016116404523095E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.9741119635600965E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3398042520471012E-2}]
["Multi-Family (5+ units)",10684,"Mountain North","1970s","Stucco","central furnace","central AC",26.85179513851946,27177.9303,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2161.7715074360144},"Cold/Very Cold",78.136549618667459,"Metropolitan Area",0.36718503339538461,0.27050433193376638,6.8030888604352371E-2,1.1485855369595101E-2,0.18727800824640381,0.90357051616034412,314.55200000000002,108.065,{"$f":"T685*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7998955120701318E-4},{"$f":"U685*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3361183795107289E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36786502294659162},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.826450044230345E-2}]
["Multi-Family (5+ units)",10685,"Pacific","1970s","Stucco","built-in electric unit","window/wall unit",29.839327421714575,37867.16678,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3012.0086889887843},"Hot-Dry/Mixed-Dry",107.57694770346599,"Metropolitan Area",1.558218766130288E-2,9.8819521647092068E-2,3.3553566343423082E-2,0,0.21909723069340675,0.36705250634522479,0,0,{"$f":"T686*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U686*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.558218766130288E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3553566343423082E-2}]
["Multi-Family (2-4 units)",10686,"New England","1980s","Siding","radiator","window/wall unit",30.438204259276976,25707.942790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8569.3142633333337},"Cold/Very Cold",144.504346403206,"Metropolitan Area",0.51496114070927612,0.79165321814896694,5.0281496896448466E-2,2.7909313931107705E-3,0.5344401860702872,1.8931966627537191,108.563,0,{"$f":"T687*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.3031046437025671E-4},{"$f":"U687*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.51589145117364643},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0281496896448466E-2}]
["Single Family Detached",10687,"New England","1990s","Wood","central furnace","window/wall unit",48.949252722609607,15258.49524,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15258.49524},"Cold/Very Cold",167.58992771655846,"Metropolitan Area",1.7884850305709188,0.27860600897430299,2.3343590405295E-2,2.1000846821631117E-2,0.39667963252736665,2.4871142624778835,1376.338,0,{"$f":"T688*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1000846821631117E-2},{"$f":"U688*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.80948587739255},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3343590405295E-2}]
["Multi-Family (5+ units)",10688,"Pacific","2000s","Stucco","N/A","central AC",16.223267346160586,19131.211490000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1521.7239666632929},"Hot-Dry/Mixed-Dry",109.15565249387843,"Metropolitan Area",0,0.42512389089443969,2.4805996856348295E-2,1.0870163056503101E-3,0.39073789138017795,0.84166833260255447,0,56.819000000000003,{"$f":"T689*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U689*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6462834061841646E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.4892459690410138E-2}]
["Single Family Attached",10689,"Middle Atlantic","1970s","Brick","central furnace","central AC",35.581694111310362,25746.522509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25746.522509999999},"Mixed-Humid",128.43575515444891,"Metropolitan Area",1.5518692241171341,0.42050021280182059,0.12698666361902938,3.0017304170913778E-2,0.42186284750566266,2.5212189480436464,939.67499999999995,226.203,{"$f":"T690*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4193363539584248E-2},{"$f":"U690*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.82394063132953E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5760625876567185},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1328106042503589}]
["Multi-Family (5+ units)",10690,"Mountain South","2000s","Concrete","central furnace","central AC",15.418823138957961,14840.06077,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1180.3996914807365},"Hot-Dry/Mixed-Dry",141.396099006729,"Metropolitan Area",4.5436876896151786E-2,0.10997382854246585,9.5769241071674102E-2,5.0583089137583503E-3,0.22661446534548962,0.48245037563270005,49.415999999999997,291.43900000000002,{"$f":"T691*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.833063115421207E-5},{"$f":"U691*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4401450568545436E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.5495207527306E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.6113255577359558E-2}]
["Single Family Detached",10691,"East North Central","Before 1950","Siding","central furnace","N/A",117.93760067297185,37440.508150000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":37440.508150000001},"Cold/Very Cold",189.34728281962217,"Metropolitan Area",2.001955689659551,1.5056065735909356,0,4.2737029635439745E-2,0.79025777897526217,4.2978200422257489,1141.4649999999999,0,{"$f":"T692*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2737029635439745E-2},{"$f":"U692*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0446927192949906},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10692,"East North Central","1990s","Brick","built-in electric unit","window/wall unit",8.8041338756539744,15338.21233,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15338.21233},"Cold/Very Cold",51.688717205080962,"Metropolitan Area",2.9290739881683136E-2,6.2977288711445645E-2,3.5957371165219001E-3,0,8.0498143994216967E-2,0.17636190970386764,0,0,{"$f":"T693*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U693*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9290739881683136E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5957371165219001E-3}]
["Multi-Family (5+ units)",10693,"Mountain South","2000s","Other","N/A","central AC",13.949738307532121,16034.18196,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1275.3818014675144},"Hot-Dry/Mixed-Dry",58.743037482842155,"Metropolitan Area",0,5.4441242829155044E-2,3.8405037446365427E-2,1.8166247135221198E-3,0.10591282688586239,0.2004312349429441,0,113.297,{"$f":"T694*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U694*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4449693196086499E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.854953437832629E-2}]
["Single Family Detached",10694,"West South Central","1960s","Brick","central furnace","both central and individual units",134.24577067331978,34617.269379999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34617.269379999998},"Hot-Humid",543.95628158629654,"Metropolitan Area",0.42598426228090397,0.37131424726715134,0.80771699217519877,4.9404416785630179E-2,0.85789022389648961,2.462905725619744,408.55700000000002,1018.604,{"$f":"T695*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.414312772608466E-2},{"$f":"U695*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5261289059545516E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44012739000698864},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.84297828123474428}]
["Single Family Detached",10695,"South Atlantic","1970s","Siding","radiator","central AC",63.11991508505541,15596.717339999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15596.717339999999},"Mixed-Humid",454.27200129388928,"Metropolitan Area",1.6466499319932604,0.2488918382331784,0.23451417591719015,1.6057569143962318E-2,0.66564060181585505,2.795696547959484,130.66200000000001,898.88599999999997,{"$f":"T696*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0378982810790799E-3},{"$f":"U696*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4019670862883239E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6486878302743395},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2485338467800734}]
["Single Family Attached",10696,"South Atlantic","1980s","Brick","central furnace","central AC",38.737503032688068,16754.97536,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16754.97536},"Hot-Humid",331.50278366252002,"Rural",0.23218669542439938,0.2291245896375565,0.23431558259364099,1.6997939257695358E-2,0.43546063675812469,1.1310875044137216,253.041,761.46,{"$f":"T697*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2396957200697607E-3},{"$f":"U697*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2758243537625601E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23642639114446914},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24707382613126661}]
["Single Family Detached",10697,"South Atlantic","1990s","Siding","central furnace","central AC",25.788473577936294,19074.314780000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19074.314780000001},"Mixed-Humid",160.1515519096593,"Metropolitan Area",0.60832418889311923,0.57488866992073895,0.14748803805867233,1.9148895350789799E-2,0.38642368198080301,1.7171245788533336,656.66099999999994,347.24900000000002,{"$f":"T698*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2525358617749579E-2},{"$f":"U698*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6235367330402207E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62084954751086885},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15411157479171256}]
["Single Family Detached",10698,"South Atlantic","2000s","Concrete","central furnace","central AC",19.50962448618586,12911.730299999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12911.730299999999},"Hot-Humid",144.00130012462563,"Metropolitan Area",3.9772377283268698E-2,8.2514762417064597E-2,0.16742675541681809,8.8700230111121974E-3,0.20161854083539343,0.49133243595254483,52.515999999999998,634.45799999999997,{"$f":"T699*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7807242843479984E-4},{"$f":"U699*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1919505826773993E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.0450449711703501E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1756187059994955}]
["Single Family Detached",10699,"Pacific","1950s","Stucco","central furnace","central AC",28.841696585805739,18128.03054,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18128.03054},"Marine",97.792168321579794,"Metropolitan Area",0.39597974386867324,0.32806053952628766,3.654172258524932E-2,9.489462018743261E-3,0.30446743349136329,1.0650494394715735,426.53899999999999,96.93,{"$f":"T700*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7323120185010599E-3},{"$f":"U700*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7571500002422002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.40371205588717429},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8298872585491521E-2}]
["Multi-Family (5+ units)",10700,"Pacific","1990s","Siding","central furnace","N/A",22.617832300666876,23984.975930000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1907.7993430578715},"Marine",106.56524805075604,"Metropolitan Area",8.5541301514922452E-2,0.12674522342047889,0,1.4505633742945402E-3,0.14996654170184359,0.36358825012287005,60.478000000000002,0,{"$f":"T701*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1537988866945395E-4},{"$f":"U701*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.5656681403591908E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10701,"West South Central","1970s","Brick","central furnace","central AC",22.592506660042368,16760.019779999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16760.019779999999},"Hot-Humid",254.50287800335997,"Metropolitan Area",0.16182673970622513,0.24358799896000791,0.61452937138113484,3.4426572269880412E-2,0.35213725034869875,1.3720813603960667,408.07900000000001,1646.01,{"$f":"T702*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8394121118026197E-3},{"$f":"U702*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.75871601580778E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16866615181802774},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.64211653153921266}]
["Mobile Home",10702,"East South Central","1990s","Brick","portable electric heaters","window/wall unit",22.892854044110759,28403.044720000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28403.044720000002},"Mixed-Humid",286.66673259915609,"Metropolitan Area",0.12799613399623655,0.44857931153774622,9.4289161511313196E-2,0,0.30724229583957041,0.97810690288486635,0,0,{"$f":"T703*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U703*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12799613399623655},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.4289161511313196E-2}]
["Single Family Detached",10703,"East North Central","2000s","Siding","central furnace","central AC",49.263501273045783,9412.2088789999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9412.2088789999998},"Cold/Very Cold",133.33826415392264,"Metropolitan Area",0.77035905531902182,0.26736796799456675,6.7846505285148517E-2,5.3474598822821622E-2,0.48380905269009711,1.5893825812888343,5203.2209999999995,478.18700000000001,{"$f":"T704*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8973802895599251E-2},{"$f":"U704*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5007959272223728E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.8193328582146211},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.2347301212370888E-2}]
["Single Family Detached",10704,"Mountain North","Before 1950","Brick","central furnace","central AC",108.05516523900815,27692.251469999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27692.251469999999},"Cold/Very Cold",279.97312082213631,"Rural",1.7948567744461736,0.46594004786945109,0.14734836546075827,5.7238028407641507E-2,0.29285375620168497,2.7009989439780679,1774.0039999999999,292.92899999999997,{"$f":"T705*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9126164876785873E-2},{"$f":"U705*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.111863530855629E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8439829393229594},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15546022899161391}]
["Single Family Detached",10705,"South Atlantic","Before 1950","Siding","heat pump","central AC",19.031765584747969,20333.082890000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20333.082890000001},"Mixed-Humid",336.80045861113729,"Metropolitan Area",0.49783048420352954,0.25849061949482094,8.9161503794462929E-2,1.2569240850862629E-2,0.46965909952484891,1.3151417070176623,431.84199999999998,186.32499999999999,{"$f":"T706*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7806791813833801E-3},{"$f":"U706*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.78856166947925E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.50661116338491297},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2950065463942175E-2}]
["Single Family Attached",10706,"West South Central","1950s","Wood","N/A","window/wall unit",6.7385956665803732,11538.691210000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11538.691210000001},"Hot-Humid",44.470115922946505,"Metropolitan Area",0,9.7741749343917425E-2,9.0562606446879634E-2,0,8.5920717898699997E-2,0.27422507368949706,0,0,{"$f":"T707*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U707*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0562606446879634E-2}]
["Single Family Detached",10707,"West South Central","1980s","Wood","central furnace","central AC",42.197971583390206,11040.80889,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11040.80889},"Hot-Humid",168.99703560357415,"Metropolitan Area",0.16196948343615789,0.10223488722138192,0.18373023322819668,1.1720050493721689E-2,0.12868326636627472,0.57661787025201117,199.20400000000001,862.31700000000001,{"$f":"T708*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1993732941235603E-3},{"$f":"U708*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5206771995981297E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16416885673028145},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1932509104277948}]
["Multi-Family (5+ units)",10708,"West North Central","1990s","Brick","central furnace","central AC",21.609051997765636,24307.145100000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1933.4251403350215},"Mixed-Humid",193.00157606450273,"Metropolitan Area",0.21362360896345525,0.14135834817192064,5.5589576071463143E-2,5.9805056732588997E-3,0.24244508017791808,0.65852142106991318,144.99199999999999,101.047,{"$f":"T709*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8033117794745542E-4},{"$f":"U709*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9536681015543291E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21390394014140271},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5784942881618574E-2}]
["Single Family Detached",10709,"East North Central","1970s","Siding","radiator","window/wall unit",65.530788410730565,15890.103880000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15890.103880000001},"Cold/Very Cold",403.00686448706449,"Metropolitan Area",0.80916104995122495,0.16897412523181737,4.585278566810172E-2,1.2918495553401201E-3,0.35107149000552962,1.3750594508566738,81.299000000000007,0,{"$f":"T710*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2918495553401201E-3},{"$f":"U710*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.81045289950656507},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.585278566810172E-2}]
["Single Family Detached",10710,"Pacific","1950s","Stucco","central furnace","central AC",11.995080491224792,14161.84237,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14161.84237},"Marine",94.834777461023407,"Metropolitan Area",0.78450706906268663,0.10415471421808674,1.1775996785926101E-2,6.1914725131097803E-3,0.20195761554375052,1.10239539561045,401.63799999999998,35.555999999999997,{"$f":"T711*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6879340458020596E-3},{"$f":"U711*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0353846730771996E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.79019500310848867},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.227953525323382E-2}]
["Single Family Detached",10711,"South Atlantic","2000s","Siding","heat pump","central AC",87.781788205635465,29656.009529999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29656.009529999999},"Mixed-Humid",722.00425899904678,"Metropolitan Area",0.80689710706550999,0.75749624501447432,0.49916654196786403,3.8134395750541235E-2,2.0753833002073168,4.1389431942551651,374.04199999999997,911.84900000000005,{"$f":"T712*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.109259311662026E-2},{"$f":"U712*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7041802633920971E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.81798970018213024},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.52620834460178501}]
["Mobile Home",10712,"South Atlantic","1980s","Siding","heat pump","central AC",26.64882777866066,23132.663,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23132.663},"Hot-Humid",249.97974536566034,"Metropolitan Area",0.12896674756265902,0.12130773103732601,0.29973590585071702,1.2199310557668999E-2,0.30292053330060098,0.85293091775130303,71.472999999999999,455.89,{"$f":"T713*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.653360822599E-3},{"$f":"U713*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.054594973507E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13062010838525803},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31028185558578703}]
["Single Family Detached",10713,"South Atlantic","2010s","Wood","heat pump","central AC",31.497320862201317,13085.71702,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13085.71702},"Hot-Humid",203.28643067378707,"Metropolitan Area",0.1266257073158277,0.11970968341356836,0.2048409222876186,1.41090855195491E-2,0.24243699860053383,0.69361331161754847,259.339,818.86599999999999,{"$f":"T714*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.39363676624978E-3},{"$f":"U714*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0715448753299319E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13001934408207749},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21555637104091793}]
["Single Family Detached",10714,"East North Central","1950s","Siding","portable electric heaters","N/A",79.703850932997497,30167.998080000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30167.998080000001},"Cold/Very Cold",355.93434991623207,"Metropolitan Area",0.79988730350029258,0.38062389985572481,0,0,0.41456069543186497,1.5950718987878822,0,0,{"$f":"T715*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U715*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.79988730350029258},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10715,"East North Central","2000s","Siding","central furnace","central AC",41.464152802238011,19223.065739999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19223.065739999998},"Cold/Very Cold",104.39253091045309,"Metropolitan Area",0.73827216253100236,0.30480102648876861,4.5234315015568974E-2,3.0046882027827359E-2,0.28301483405526018,1.3713223380906001,1453.366,109.69799999999999,{"$f":"T716*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.793815016228084E-2},{"$f":"U716*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1087318655465198E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.76621031269328321},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7343046881115493E-2}]
["Single Family Detached",10716,"West North Central","1970s","Siding","central furnace","both central and individual units",23.950037069125539,18171.500049999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18171.500049999999},"Mixed-Humid",88.378762283082267,"Metropolitan Area",1.3232125086989004,6.0798840869791745E-2,4.8673126086927095E-2,8.2388309221696505E-3,0.17420003128232242,1.6068845069379416,351.464,101.929,{"$f":"T717*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3866280935731996E-3},{"$f":"U717*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.85220282859645E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3295991367924735},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0525328915523547E-2}]
["Single Family Attached",10717,"Middle Atlantic","Before 1950","Brick","radiator","window/wall unit",55.853146395235505,25457.222600000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25457.222600000001},"Mixed-Humid",206.30986337604691,"Metropolitan Area",1.7196649170082161,0.57303192329418251,0.10280850978287061,3.8061348081486002E-3,0.62206375596846719,3.0175691060537368,149.511,0,{"$f":"T718*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8061348081486002E-3},{"$f":"U718*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7234710518163647},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10280850978287061}]
["Single Family Attached",10718,"West South Central","2000s","Brick","central furnace","central AC",25.336643710546504,14628.54718,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14628.54718},"Hot-Humid",223.75759933461455,"Metropolitan Area",9.0585976471450974E-2,0.11852550684404273,9.7814234204032569E-2,6.6159945189098804E-3,0.4565351902095961,0.76346090772912245,112.577,339.68900000000002,{"$f":"T719*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6468379558828598E-3},{"$f":"U719*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9691565630270206E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.2232814427333831E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10278339076705958}]
["Single Family Detached",10719,"West North Central","2000s","Siding","central furnace","central AC",76.849902986936911,27763.69328,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27763.69328},"Mixed-Humid",404.79384281154393,"Metropolitan Area",1.3492315082358279,0.38691052617762162,0.2622004026273998,4.5053255633187198E-2,0.56326422876229076,2.56160666580314,1151.538,471.202,{"$f":"T720*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1970947832264639E-2},{"$f":"U720*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3082307800922559E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3812024560680927},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27528271042832236}]
["Single Family Detached",10720,"Pacific","2000s","Stucco","central furnace","central AC",48.90522490888565,15806.472169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15806.472169999999},"Hot-Dry/Mixed-Dry",57.405550482698189,"Metropolitan Area",0.24290648268605661,0.11548442503190115,5.8282904509469768E-2,8.992665566372909E-3,0.17638113519881862,0.5930549474262462,335.459,233.464,{"$f":"T721*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3024233476760291E-3},{"$f":"U721*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6902422186968799E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24820890603373263},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1973146728166645E-2}]
["Single Family Detached",10721,"East South Central","1950s","Shingle","central furnace","both central and individual units",22.611517395685908,13017.569020000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13017.569020000001},"Hot-Humid",253.82331695947735,"Metropolitan Area",0.29367387073551721,0.11361242176547044,0.35719339817269469,1.8641275994761178E-2,0.77285227864568973,1.5373319693193721,255.25,1176.759,{"$f":"T722*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.322734492355E-3},{"$f":"U722*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5318541502406182E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29699660522787219},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37251193967510088}]
["Multi-Family (5+ units)",10722,"South Atlantic","1980s","Brick","central furnace","central AC",48.737636849566407,56803.772550000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4518.2534379178242},"Mixed-Humid",506.23499376781865,"Metropolitan Area",0.4743902013625434,0.56463762208647461,0.1991864473173971,1.6471105907460752E-2,0.47389859416983415,1.7272738354855841,134.59,155.375,{"$f":"T723*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0811173020936004E-4},{"$f":"U723*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0202362791648191E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.47499831309275276},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19988847094531359}]
["Single Family Detached",10723,"West South Central","Before 1950","Wood","heat pump","central AC",32.088245230360933,24683.26556,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24683.26556},"Hot-Humid",371.59508531465514,"Metropolitan Area",8.8646295135437106E-2,0.34981521352207517,0.7066395118158334,3.4238429174197157E-2,0.63955219790213946,1.7846532183754851,50.161999999999999,1336.9490000000001,{"$f":"T724*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.23816196702072E-3},{"$f":"U724*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3000267207176442E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.9884457102457821E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.73963977902300981}]
["Single Family Detached",10724,"Pacific","1950s","Stucco","N/A","N/A",22.912720528052841,20294.703740000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20294.703740000001},"Hot-Dry/Mixed-Dry",30.034477082120791,"Metropolitan Area",0,0.38616155464830176,0,0,0.13224420644766183,0.51840576109596359,0,0,{"$f":"T725*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U725*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10725,"South Atlantic","1960s","Concrete","central furnace","central AC",31.727323419668853,18885.311559999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18885.311559999998},"Hot-Humid",152.03773041859591,"Metropolitan Area",6.357045157208592E-2,0.12457742983832899,0.31610833153504447,1.7691212195372757E-2,0.20080846208305794,0.70506467502851733,97.213999999999999,839.55700000000002,{"$f":"T726*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8359166779938398E-3},{"$f":"U726*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5855295517378919E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.5406368250079755E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.33196362705242338}]
["Single Family Detached",10726,"Mountain South","1980s","Wood","central furnace","central AC",11.759134143816809,12509.71717,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12509.71717},"Hot-Dry/Mixed-Dry",124.3465887122756,"Metropolitan Area",9.9882898515077256E-2,5.8498539896778154E-2,0.10314798473531593,6.10869504958572E-3,0.16272512495620867,0.42425454810338004,127.55800000000001,360.75799999999998,{"$f":"T727*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5957145027708599E-3},{"$f":"U727*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5129805468148597E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10147861301784812},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10766096528213079}]
["Multi-Family (5+ units)",10727,"Pacific","1990s","Stucco","central furnace","N/A",17.604091331945611,20759.541669999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1651.2436817028945},"Hot-Dry/Mixed-Dry",89.787467327172095,"Metropolitan Area",5.2438456285323204E-2,0.23794055217887247,0,8.6700149830588001E-4,0.25311837208235116,0.54429541950373006,41.764000000000003,0,{"$f":"T728*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8962541122639693E-5},{"$f":"U728*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.2507418826445842E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10728,"New England","Before 1950","Shingle","central furnace","window/wall unit",46.275257964928549,17535.14891,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17535.14891},"Cold/Very Cold",147.8737879846293,"Metropolitan Area",2.4277758582274056,0.47938266946905922,4.0815198376192019E-2,2.0629138259424949E-2,0.33456436361948966,3.2825380896921472,1176.4449999999999,0,{"$f":"T729*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0629138259424949E-2},{"$f":"U729*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4484049964868304},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.0815198376192019E-2}]
["Single Family Detached",10729,"West South Central","2000s","Brick","central furnace","central AC",45.127674927392327,14977.655140000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14977.655140000001},"Hot-Humid",305.12817539839699,"Metropolitan Area",0.74114184051633869,0.40315662880033887,0.36622283957157925,3.728576412454964E-2,0.25463556436479423,1.7651568732530512,1140.519,1348.9069999999999,{"$f":"T730*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7082300262617662E-2},{"$f":"U730*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0203463861931979E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.75822414077895639},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.38642630343351125}]
["Single Family Detached",10730,"Pacific","2000s","Stucco","central furnace","both central and individual units",67.396390290208316,17929.340329999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17929.340329999999},"Hot-Dry/Mixed-Dry",150.15822524088708,"Metropolitan Area",0.1120353199308356,0.33960512156867101,0.1344062240234252,8.8151215373074698E-3,0.67257764226906513,1.258624307791997,116.95699999999999,374.702,{"$f":"T731*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0969618569758098E-3},{"$f":"U731*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7181596803316595E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1141322817878114},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14112438370375685}]
["Single Family Attached",10731,"Middle Atlantic","Before 1950","Brick","central furnace","window/wall unit",40.776269232776421,28756.184229999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28756.184229999999},"Mixed-Humid",114.51376826735435,"Metropolitan Area",1.2783940418392807,0.46177385163047635,6.7726708879417147E-2,1.521196394530154E-2,0.34845358001834131,2.1563481823675157,528.99800000000005,0,{"$f":"T732*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.521196394530154E-2},{"$f":"U732*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2936060057845822},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7726708879417147E-2}]
["Single Family Detached",10732,"East South Central","2000s","Siding","built-in electric unit","window/wall unit",17.677132601425839,20318.54322,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20318.54322},"Mixed-Humid",200.0970136308525,"Micropolitan Area",0.30653326406334358,0.10524166232125014,4.8157568523475379E-2,0,0.22283151291359091,0.68276400782166002,0,0,{"$f":"T733*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U733*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30653326406334358},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.8157568523475379E-2}]
["Single Family Attached",10733,"South Atlantic","1980s","Brick","heat pump","central AC",33.111109193561276,15307.956169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15307.956169999999},"Mixed-Humid",191.94597254857635,"Metropolitan Area",0.27670306428308855,8.9647968410414836E-2,8.974554132304241E-2,9.4065706789471307E-3,0.19882307187040507,0.65491964588695084,333.40100000000001,281.08800000000002,{"$f":"T734*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.10368789503417E-3},{"$f":"U734*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3028827839129606E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28180675217812273},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.4048424106955367E-2}]
["Single Family Detached",10734,"Middle Atlantic","1990s","Siding","heat pump","central AC",103.96943834651,34043.69298,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34043.69298},"Mixed-Humid",550.00309497005435,"Metropolitan Area",1.218869471782694,0.90206169053733143,0.31904053684945588,6.0123306555337742E-2,1.6980453104142541,4.1380170095837361,1273.6110000000001,492.452,{"$f":"T735*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3358421859950778E-2},{"$f":"U735*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6764884695386961E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2622278936426448},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.33580542154484283}]
["Multi-Family (5+ units)",10735,"West North Central","1960s","Brick","built-in electric unit","window/wall unit",8.2616472411429012,11015.52965,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":876.19100769739669},"Cold/Very Cold",36.495066616202578,"Metropolitan Area",1.2545454532029199E-2,2.5503914317225849E-2,3.2123267254736999E-3,0,8.3259481887259457E-2,0.12452117746198819,0,0,{"$f":"T736*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U736*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2545454532029199E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2123267254736999E-3}]
["Single Family Detached",10736,"South Atlantic","2000s","Stucco","central furnace","central AC",24.061094409998212,11806.228859999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11806.228859999999},"Hot-Humid",292.07568882143579,"Metropolitan Area",6.6842723818990132E-2,0.39964252339549811,0.54239790564928281,2.832935311152036E-2,0.4154822204769994,1.4243653733407704,98.915999999999997,2300.61,{"$f":"T737*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1678249339157599E-3},{"$f":"U737*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7161528177604602E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.8010548752905894E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.56955943382688745}]
["Multi-Family (2-4 units)",10737,"East North Central","Before 1950","Shingle","radiator","window/wall unit",77.493252949885857,52860.336259999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17620.112086666664},"Cold/Very Cold",394.30522933343354,"Metropolitan Area",4.8690499556253828,1.6302857703827751,0.16724296778124487,1.087633134751256E-2,1.4444383429531411,8.1182679243075526,205.756,0,{"$f":"T738*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6254437825041859E-3},{"$f":"U738*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.8726753994078873},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16724296778124487}]
["Single Family Detached",10738,"South Atlantic","1980s","Siding","heater burning gas/oil/kerosene","central AC",39.728328667938108,18107.715889999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18107.715889999999},"Mixed-Humid",236.66784671374251,"Metropolitan Area",0.84595491287032831,0.34178540088823622,0.15702679848607212,7.6967932853398398E-3,0.30869849350569917,1.6534656057503356,0,425.05599999999998,{"$f":"T739*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U739*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6967932853398398E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84595491287032831},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16472359177141196}]
["Single Family Detached",10739,"West North Central","Before 1950","Wood","central furnace","both central and individual units",56.423516382745071,19349.628390000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19349.628390000002},"Cold/Very Cold",98.628345336295155,"Metropolitan Area",0.81550612933848532,0.52765269836938089,6.6616455579639036E-2,2.3841470474082995E-2,0.2228046048831098,1.6325798881706151,1099.0250000000001,133.11600000000001,{"$f":"T740*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1265725341319756E-2},{"$f":"U740*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5757451327632404E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83677185467980508},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9192200712402271E-2}]
["Single Family Detached",10740,"South Atlantic","2000s","Stucco","central furnace","central AC",144.1173396550661,18405.790509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18405.790509999999},"Mixed-Humid",1134.3888462073376,"Metropolitan Area",3.2007077030435576,0.64910170029846559,0.41274064929149495,7.0952757923856649E-2,4.1521024623317411,8.41465251496526,2110.3000000000002,1744.615,{"$f":"T741*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8841739713252998E-2},{"$f":"U741*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2111018210603644E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2395494427568106},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.44485166750209859}]
["Single Family Detached",10741,"East South Central","1950s","Brick","heat pump","central AC",38.201546472902123,16037.592979999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16037.592979999999},"Hot-Humid",171.6579273843017,"Metropolitan Area",6.196002162116352E-2,0.11788517719191795,0.26643484159012915,1.628963979127368E-2,0.31275702327391203,0.75903706367712265,71.421000000000006,944.29499999999996,{"$f":"T742*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1454209282245802E-3},{"$f":"U742*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5144218863049098E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.3105442549388102E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28157906045317826}]
["Single Family Detached",10742,"West North Central","1960s","Siding","central furnace","central AC",27.901163673912002,18600.77578,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18600.77578},"Cold/Very Cold",118.43885872981492,"Metropolitan Area",1.0173965884197387,0.17287765618465581,5.8954526408333478E-2,1.4619223921963661E-2,0.35644711269075846,1.6056758837034866,638.64499999999998,147.30199999999999,{"$f":"T743*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.18792924480181E-2},{"$f":"U743*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.73993147394556E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0292758808677567},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1694457882279036E-2}]
["Single Family Detached",10743,"Pacific","2000s","Stucco","central furnace","central AC",38.22997907342377,12785.946180000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12785.946180000001},"Hot-Dry/Mixed-Dry",82.846090754843416,"Metropolitan Area",0.22016636000973056,0.14468093388522396,9.9784643759587927E-2,1.3928217039828841E-2,0.19909579836023808,0.66372773601478052,646.33600000000001,443.00200000000001,{"$f":"T744*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2640173101964799E-3},{"$f":"U744*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6641997296323606E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22843037731992705},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10544884348922029}]
["Single Family Detached",10744,"South Atlantic","2000s","Siding","central furnace","central AC",50.223981043851772,15155.093860000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15155.093860000001},"Hot-Humid",347.74878365486501,"Metropolitan Area",0.28903641943344016,0.22023224784375858,0.25008778274795856,2.1088767759005801E-2,0.42718131355582273,1.18653776358098,374.40899999999999,1017.121,{"$f":"T745*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6742035370287401E-3},{"$f":"U745*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.541456422197706E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29471062297046891},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26550234696993563}]
["Single Family Detached",10745,"West South Central","1970s","Brick","central furnace","central AC",23.826330203240666,14698.538060000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14698.538060000001},"Hot-Humid",249.86512270073581,"Metropolitan Area",0.22462576316392308,0.10704676285851503,0.28987851182163932,1.800947194924336E-2,0.23098876029009713,0.85253979813417446,250.619,974.63699999999994,{"$f":"T746*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6837329100591399E-3},{"$f":"U746*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4325739039184221E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22830949607398221},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30420425086082353}]
["Single Family Detached",10746,"New England","2000s","Siding","central furnace","window/wall unit",30.232146388131948,15631.92678,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15631.92678},"Cold/Very Cold",121.87011213427729,"Micropolitan Area",0.58630050312638204,0.48281999285345584,7.4937581152106393E-3,5.6237107145192403E-3,0.38119108430762078,1.4578053384026692,359.75799999999998,0,{"$f":"T747*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6237107145192403E-3},{"$f":"U747*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59192421384090133},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4937581152106393E-3}]
["Multi-Family (5+ units)",10747,"South Atlantic","2010s","Brick","built-in electric unit","N/A",25.592042529823924,19417.33121,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1544.4823390479469},"Mixed-Humid",101.78565018310853,"Metropolitan Area",9.3998251851724654E-2,0.14602099087357578,0,0,0.10724030863433957,0.34725955135963998,0,0,{"$f":"T748*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U748*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.3998251851724654E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10748,"South Atlantic","Before 1950","Brick","central furnace","central AC",34.651026170319483,25109.439249999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25109.439249999999},"Mixed-Humid",431.31980328925755,"Metropolitan Area",2.1395492297851195,0.76090163246284248,0.36143747175197549,3.9189883732147747E-2,0.70289418254908087,3.9647825165490183,906.18299999999999,654.58000000000004,{"$f":"T749*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.275374698788275E-2},{"$f":"U749*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6436136744265001E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1623029767730024},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37787360849624052}]
["Multi-Family (2-4 units)",10749,"South Atlantic","1990s","Stucco","central furnace","N/A",30.021292776222499,44475.989300000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14825.329766666668},"Hot-Humid",133.26296197402621,"Metropolitan Area",5.8484739903118662E-3,3.2800374968910501E-2,0,9.4511477262500005E-5,0.4159814372674992,0.45469329387822993,2.125,0,{"$f":"T750*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1503825754166671E-5},{"$f":"U750*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.8799778160660331E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10750,"West South Central","1980s","Siding","central furnace","central AC",66.792303048257139,21237.61623,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21237.61623},"Hot-Humid",270.28714910721641,"Metropolitan Area",0.6159001727459088,0.2534770873761405,0.43682542096158167,3.8079874167422971E-2,0.47389714548656681,1.7800998265701975,541.36,1251.6790000000001,{"$f":"T751*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.14971959222728E-2},{"$f":"U751*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6582678245150173E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62739736866818163},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46340809920673182}]
["Single Family Detached",10751,"Mountain South","2000s","Stucco","central furnace","central AC",71.947676989174468,19930.104429999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19930.104429999999},"Hot-Dry/Mixed-Dry",442.08162433538757,"Metropolitan Area",0.25032952563964794,0.34943322551440209,0.57533193089114532,4.2708918336702047E-2,0.94731473425109525,2.1224094162962905,310.54500000000002,1832.39,{"$f":"T752*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1891942802143494E-3},{"$f":"U752*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.65197240564877E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2565187199198623},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.61185165494763305}]
["Multi-Family (5+ units)",10752,"Pacific","1980s","Concrete","N/A","N/A",11.183793816765897,16642.550319999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1323.7722922869561},"Hot-Dry/Mixed-Dry",29.702658547801189,"Metropolitan Area",0,1.2401728932558238E-2,0,0,0.1023950383115836,0.11479676724414183,0,0,{"$f":"T753*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U753*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10753,"Mountain North","2000s","Siding","central furnace","central AC",15.27753883647498,13913.969800000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13913.969800000001},"Cold/Very Cold",56.954762180167293,"Metropolitan Area",0.54417798861829225,0.33612607148691948,9.8218295399105995E-3,6.3144934305152008E-3,0.17861570350409997,1.0687415931492223,423.46899999999999,30.355,{"$f":"T754*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8921348772362006E-3},{"$f":"U754*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2235855327900005E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55007012349552842},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.02441880931896E-2}]
["Mobile Home",10754,"Pacific","1950s","Siding","N/A","N/A",7.6858558886619717,15249.71406,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15249.71406},"Marine",74.15935949714914,"Metropolitan Area",0,0.18871208530111772,0,0,7.5803888638010353E-2,0.26451597393912807,0,0,{"$f":"T755*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U755*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10755,"South Atlantic","2000s","Concrete","heat pump","central AC",35.143954524580302,15220.422049999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15220.422049999999},"Hot-Humid",204.5818936753281,"Metropolitan Area",1.7824225311359649E-2,0.12819237613096565,0.23802937988229278,1.3641090176403799E-2,0.31398742883758951,0.69803341016220766,21.363,874.87300000000005,{"$f":"T756*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2515387625414998E-4},{"$f":"U756*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3315936300149649E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.81493791876138E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25134531618244244}]
["Single Family Attached",10756,"South Atlantic","1980s","Concrete","central furnace","central AC",10.451872335968034,12502.23964,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12502.23964},"Hot-Humid",144.99209871196021,"Metropolitan Area",2.8560991390390801E-3,6.8295871961271237E-2,9.0009124153801606E-2,4.0429867570228404E-3,0.33355196469990434,0.49471305995401621,3.5310000000000001,319.85000000000002,{"$f":"T757*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4145408168840007E-5},{"$f":"U757*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9988413488539999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9002445472079202E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.400796550265561E-2}]
["Single Family Detached",10757,"West North Central","1990s","Wood","central furnace","central AC",167.01968955642826,34057.848599999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34057.848599999998},null,436.90150650941791,"Micropolitan Area",4.1325320768301435,0.63968050658655362,8.5271486986034997E-2,0.18123693408537841,1.5472569169386348,6.4047409873413672,5166.7820000000002,154.66200000000001,{"$f":"T758*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.17596947910520519},{"$f":"U758*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2674549801731991E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.308501555935349},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0538941966208195E-2}]
["Single Family Detached",10758,"Pacific","1960s","Wood","N/A","N/A",17.573519095812085,11087.393749999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11087.393749999999},"Marine",21.75524052305277,"Metropolitan Area",0,0.11387802248698749,0,0,0.10184671455747502,0.21572473704446249,0,0,{"$f":"T759*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U759*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10759,"Middle Atlantic","Before 1950","Brick","portable electric heaters","N/A",114.47180733156677,43034.514029999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":43034.514029999998},"Mixed-Humid",133.20585018811627,"Metropolitan Area",0.15652427373963537,0.42039749720939529,0,0,0.4053770316739625,0.98229880262299307,0,0,{"$f":"T760*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U760*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15652427373963537},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10760,"Mountain North","2000s","Wood","central furnace","central AC",63.795849267943915,13447.69167,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13447.69167},"Cold/Very Cold",113.34509295471094,"Metropolitan Area",0.86220719657241884,0.22889053761519434,5.4808743491727333E-2,3.6726237649203484E-2,0.29849176883930495,1.4443982465186456,2486.1460000000002,244.898,{"$f":"T761*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3432924854603821E-2},{"$f":"U761*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.29331279459966E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.89564012142702265},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8102056286326989E-2}]
["Single Family Detached",10761,"West South Central","Before 1950","Wood","wood-burning stove","window/wall unit",22.666129214380991,13034.001850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13034.001850000001},"Hot-Humid",152.92794368736756,"Rural",0,9.6347902137279562E-2,0.28135771192891584,0,0.24064372620011706,0.6183493402663125,0,0,{"$f":"T762*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U762*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28135771192891584}]
["Single Family Detached",10762,"South Atlantic","1980s","Concrete","N/A","central AC",47.946050969218845,26755.608800000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26755.608800000002},"Hot-Humid",752.11870499891927,"Metropolitan Area",0,0.41221146422398725,1.5016416343552383,7.4603466685304001E-2,1.1370710466268785,3.0509241452061042,0,2788.33,{"$f":"T763*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U763*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4603466685304001E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5762451010405423}]
["Single Family Detached",10763,"East North Central","1960s","Brick","central furnace","central AC",33.294788854828887,14984.153399999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14984.153399999999},"Cold/Very Cold",84.783546546101149,"Metropolitan Area",1.9630633731058529,0.13857719668155,3.0923651468323796E-2,1.7679697707586196E-2,0.24204992334972192,2.3746141446054487,1088.3409999999999,91.552000000000007,{"$f":"T764*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6307868495509397E-2},{"$f":"U764*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3718292120767999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9793712416013622},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2295480680400598E-2}]
["Single Family Detached",10764,"Pacific","1960s","Siding","built-in electric unit","both central and individual units",30.320899292075158,8896.977492,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8896.977492},"Marine",162.27923240668457,"Metropolitan Area",0.36283295059681475,5.1959611924083861E-2,2.8722059055558649E-2,1.522432994476056E-3,0.11018212659597623,0.55369674817243353,0,171.11799999999999,{"$f":"T765*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U765*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.522432994476056E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36283295059681475},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0244492050034703E-2}]
["Multi-Family (2-4 units)",10765,"East North Central","Before 1950","Wood","central furnace","central AC",28.265865448454264,39588.046849999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13196.015616666666},"Cold/Very Cold",153.8052230896414,"Metropolitan Area",0.32447036195056445,0.56261166395603679,0.15311358033643321,1.3641843004275751E-2,0.36010079175697007,1.4093909600028551,187.518,157.077,{"$f":"T766*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4744904564060997E-3},{"$f":"U766*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0727905450191497E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.32694485240697052},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15518637088145237}]
["Single Family Attached",10766,"Pacific","1990s","Stucco","central furnace","N/A",25.659525859385663,13118.367,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13118.367},"Hot-Dry/Mixed-Dry",78.886775242526213,"Metropolitan Area",6.3335908782110997E-2,0.34921857754796098,0,1.2103267761540001E-3,0.32515076875590604,0.73770525508597806,92.262,0,{"$f":"T767*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2103267761540001E-3},{"$f":"U767*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.4546235558264997E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10767,"West North Central","1980s","Brick","central furnace","central AC",103.90693940173804,18488.77925,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18488.77925},"Cold/Very Cold",263.43674256756674,"Metropolitan Area",1.5670988158677501,0.37911038475553249,9.980461206745149E-2,2.4604257296184744E-2,0.77902079407754921,2.8250346067682832,1082.8579999999999,247.90899999999999,{"$f":"T768*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0020722521096497E-2},{"$f":"U768*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5835347750882499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5871195383888466},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10438814684253973}]
["Single Family Detached",10768,"New England","1980s","Wood","radiator","window/wall unit",58.51562694351027,18337.70822,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18337.70822},"Cold/Very Cold",165.00269860159997,"Metropolitan Area",0.76780310728346324,0.38002993164295118,5.432676257903362E-2,1.7723028240465598E-3,0.53302377854906346,1.7351835800545115,96.647999999999996,0,{"$f":"T769*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7723028240465598E-3},{"$f":"U769*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.76957541010750985},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.432676257903362E-2}]
["Multi-Family (5+ units)",10769,"West North Central","1970s","Brick","built-in electric unit","window/wall unit",12.680692091104055,21492.69846,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1709.5600229993195},null,109.24863284614101,"Metropolitan Area",0.2006408309190349,0.15722394658475197,8.3837643517844992E-3,0,0.16373174224415379,0.5299802840997252,0,0,{"$f":"T770*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U770*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2006408309190349},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.3837643517844992E-3}]
["Single Family Detached",10770,"West North Central","1950s","Wood","central furnace","central AC",23.704773287146878,13545.58474,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13545.58474},"Cold/Very Cold",116.83157589797258,"Rural",0.87096892130131875,0.24840199426427123,2.7737700239640204E-2,1.023562628968782E-2,0.33794592201429507,1.4850545378195252,667.21699999999998,88.426000000000002,{"$f":"T771*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0378444134685803E-3},{"$f":"U771*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1977818762192399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88000676571478731},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8935482115859446E-2}]
["Single Family Detached",10771,"South Atlantic","1990s","Siding","heat pump","central AC",92.398529098099559,24972.575430000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24972.575430000001},"Mixed-Humid",430.87976326622794,"Metropolitan Area",0.35875983943142081,0.23487336500815839,0.11462874115015456,1.3089550219662509E-2,0.76189979117856799,1.4701617367683018,284.45999999999998,239.697,{"$f":"T772*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1036988068177995E-3},{"$f":"U772*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9858514128447102E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36586353823823864},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12061459256299928}]
["Mobile Home",10772,"West South Central","1980s","Siding","portable electric heaters","window/wall unit",24.303732691406339,18987.29117,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18987.29117},"Mixed-Humid",112.99336972387431,"Micropolitan Area",0.11248375085766719,9.184388181339509E-2,9.3048416577928714E-2,0,8.8179885249028978E-2,0.38555593449802,0,0,{"$f":"T773*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U773*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11248375085766719},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.3048416577928714E-2}]
["Single Family Detached",10773,"Middle Atlantic","Before 1950","Siding","central furnace","both central and individual units",53.26107586233411,33539.72032,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33539.72032},"Cold/Very Cold",352.24735741191597,"Metropolitan Area",3.9872152669105669,0.7175593079982604,0.29722004637051458,6.7092152194001289E-2,1.1046877398034649,6.1066823610828065,1636.3510000000001,364.02800000000002,{"$f":"T774*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4882754885352318E-2},{"$f":"U774*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2209397308648961E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.042098021795919},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30942944367916353}]
["Single Family Detached",10774,"Mountain South","1970s","Stucco","heat pump","both central and individual units",28.739431075913352,12495.40482,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12495.40482},"Hot-Dry/Mixed-Dry",162.53421555179713,"Metropolitan Area",8.0145001708477548E-2,1.8484027506462119E-2,0.22247084893650665,1.2110471379115081E-2,0.2334668551597259,0.55456673331117223,116.706,852.48800000000006,{"$f":"T775*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4582887149229202E-3},{"$f":"U775*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0652182664192161E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.1603290423400462E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2331230316006988}]
["Single Family Detached",10775,"Pacific","1980s","Stucco","N/A","N/A",17.252237807432,10782.64863,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10782.64863},"Hot-Dry/Mixed-Dry",24.813979899618484,"Metropolitan Area",0,0.15156348619630255,0,0,9.5924587959557356E-2,0.24748807415585991,0,0,{"$f":"T776*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U776*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10776,"West North Central","Before 1950","Brick","central furnace","central AC",27.251299833191762,18538.299210000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1474.5628745873109},"Cold/Very Cold",79.825916382124987,"Micropolitan Area",0.88107207169674495,0.19558864096619158,4.8436906225724843E-2,2.3940748904077411E-2,0.20014507683752109,1.3472791631681977,1171.684,119.73699999999999,{"$f":"T777*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7277217271479588E-3},{"$f":"U777*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7655973491446082E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88279979342389292},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.8613465960639306E-2}]
["Single Family Detached",10777,"West South Central","1980s","Wood","built-in furnace","central AC",13.168753750953437,14471.15797,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14471.15797},"Hot-Humid",117.24478642454503,"Metropolitan Area",3.8466624327219263E-2,7.5438681930454901E-2,0.10914891158493657,5.0429525428595107E-3,0.17698496807964037,0.40003918592225113,0,348.483,{"$f":"T778*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U778*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0429525428595107E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.8466624327219263E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11419186412779608}]
["Multi-Family (2-4 units)",10778,"New England","Before 1950","Siding","radiator","central AC",56.906920510311203,21711.911680000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7237.3038933333337},"Cold/Very Cold",142.62207391261069,"Metropolitan Area",0.5488766351337353,0.14880810152444673,7.7065533082477225E-2,3.9769925743372805E-2,0.2223733342908249,1.0236368878603994,1639.6030000000001,192.107,{"$f":"T779*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1866305175421015E-2},{"$f":"U779*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3903367390365867E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.56074294030915628},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.8455869821513813E-2}]
["Single Family Detached",10779,"East South Central","1950s","Brick","central furnace","central AC",19.343072150222021,11910.75871,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11910.75871},"Mixed-Humid",271.65451024351438,"Metropolitan Area",0.37317408733237506,0.24079350804871244,9.9527312195250336E-2,1.1407195653258619E-2,0.21339029446626973,0.92688520204260749,562.32399999999996,395.39800000000002,{"$f":"T780*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6977054808420398E-3},{"$f":"U780*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7094901724165795E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37987179281321709},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10423680236766691}]
["Multi-Family (5+ units)",10780,"South Atlantic","2010s","Concrete","N/A","central AC",14.612200547212316,17605.0609,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1400.3317625807524},"Hot-Humid",222.5947633802889,"Metropolitan Area",0,8.3846496824532407E-2,0.10373444386682654,4.5550454319615002E-3,0.56771967670939427,0.75949334799412338,0,258.73500000000001,{"$f":"T781*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U781*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6231483859133095E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10409675870541787}]
["Single Family Detached",10781,"Middle Atlantic","2010s","Siding","central furnace","central AC",116.55207625629211,25969.713960000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25969.713960000001},"Cold/Very Cold",143.85294581534671,"Metropolitan Area",1.6849732138840705,0.43849134869469125,3.2800943338322161E-2,3.2464297936258685E-2,0.42720410594654273,2.5834696118636264,1186.8140000000001,63.268999999999998,{"$f":"T782*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0821220103723443E-2},{"$f":"U782*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6430778325352401E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.715794433987794},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4444021170857403E-2}]
["Single Family Detached",10782,"East South Central","2000s","Brick","heat pump","central AC",31.32525260090426,17211.677250000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17211.677250000001},"Hot-Humid",225.02445291995542,"Micropolitan Area",0.135907396675122,0.1153545542139975,0.32318863789797531,1.678794296778225E-2,0.19333284973227585,0.7677834385193707,128.011,847.37,{"$f":"T783*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2032840164497498E-3},{"$f":"U783*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4584658951332501E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13811068069157176},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.33777329684930779}]
["Multi-Family (2-4 units)",10783,"West South Central","1970s","Siding","central furnace","N/A",17.842664461209726,26952.665349999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8984.2217833333325},"Hot-Humid",144.00809096109299,"Metropolitan Area",0.24067985365564162,0.33187094457908101,0,3.6566950606998498E-3,0.51607729180106987,1.0910658867429257,135.67099999999999,0,{"$f":"T784*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2188983535666165E-3},{"$f":"U784*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24189875200920824},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10784,"Mountain North","1970s","Brick","central furnace","N/A",70.397948942017905,19642.28486,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19642.28486},"Cold/Very Cold",154.27431590198194,"Metropolitan Area",0.83286080939307094,0.44674045374857113,0.11738989588760081,8.2126867927552361E-2,0.40641759285087109,1.8034087518801143,4181.1260000000002,0,{"$f":"T785*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2126867927552361E-2},{"$f":"U785*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.91498767732062336},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11738989588760081}]
["Multi-Family (5+ units)",10785,"East North Central","2000s","Brick","built-in electric unit","window/wall unit",14.69662286185868,19439.977330000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1546.2836438724714},"Cold/Very Cold",197.61780883236813,"Metropolitan Area",0.2331848414306523,0.26158122455610722,1.216963964833063E-2,0,0.16733627278019922,0.67427197841528941,0,0,{"$f":"T786*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U786*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2331848414306523},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.216963964833063E-2}]
["Multi-Family (5+ units)",10786,"Pacific","1950s","Concrete","N/A","N/A",7.0684072389082653,17759.817179999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1412.6412987745657},"Hot-Humid",117.88966646199263,"Metropolitan Area",0,0.19558803189193252,0,0,0.20667182723506747,0.40225985912699996,0,0,{"$f":"T787*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U787*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10787,"East North Central","1960s","Wood","built-in electric unit","N/A",48.268518283657073,22682.574379999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22682.574379999998},"Cold/Very Cold",140.53991527795054,"Metropolitan Area",0.1087175563207656,9.166066867334445E-2,0,0,0.27914398622787084,0.47952221122198085,0,0,{"$f":"T788*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U788*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1087175563207656},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10788,"Pacific","2000s","Siding","built-in electric unit","window/wall unit",11.298632077593581,12348.23178,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":982.19604416381549},"Cold/Very Cold",113.16987724132754,"Micropolitan Area",7.4334750045468592E-2,0.22058557728119366,7.1899431773817003E-3,0,8.4025345988849878E-2,0.3861356164928938,0,0,{"$f":"T789*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U789*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.4334750045468592E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.1899431773817003E-3}]
["Single Family Detached",10789,"East North Central","2000s","Brick","heat pump","central AC",29.545378227126999,12845.81662,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12845.81662},"Cold/Very Cold",226.99842550067882,"Metropolitan Area",0.24647308170825522,0.18386198059481068,3.3990891446233532E-2,6.3994775404851191E-3,0.31021255935360054,0.77453851310290001,364.32,133.85599999999999,{"$f":"T790*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6799879109983991E-3},{"$f":"U790*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7194896294867197E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2511530696192536},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5710381075720249E-2}]
["Multi-Family (5+ units)",10790,"East North Central","Before 1950","Brick","radiator","window/wall unit",18.690751909224964,24496.39831,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1948.4786117566036},"Cold/Very Cold",54.491160195264662,"Metropolitan Area",0.69265407144029845,0.44980901436419585,1.406497453566115E-2,9.2375918027009997E-4,0.29176449904964469,1.449142841441621,37.71,0,{"$f":"T791*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3477128449341524E-5},{"$f":"U791*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.69272754856874774},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.406497453566115E-2}]
["Multi-Family (5+ units)",10791,"Pacific","1980s","Stucco","N/A","N/A",19.849489688531975,21071.645100000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1676.0688356016465},"Hot-Dry/Mixed-Dry",66.507084858358184,"Metropolitan Area",0,0.32442804555205773,0,0,0.25268857622685265,0.57711662177891043,0,0,{"$f":"T792*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U792*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10792,"West North Central","1950s","Siding","radiator","N/A",7.5665275786915416,6439.5979390000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6439.5979390000002},null,73.095876209129941,"Metropolitan Area",0.1627277512540144,4.1183508437575407E-2,0,7.1059031377483303E-4,4.5500808083819212E-2,0.249412067775409,110.34699999999999,0,{"$f":"T793*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1059031377483303E-4},{"$f":"U793*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16343834156778922},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10793,"East South Central","1950s","Shingle","built-in electric unit","window/wall unit",16.384038580224683,18326.665079999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18326.665079999999},"Hot-Humid",308.11522396663253,"Micropolitan Area",0.42306186338592983,0.29484646189976083,0.19109094555592979,0,0.46137885154856206,1.3703781223901825,0,0,{"$f":"T794*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U794*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42306186338592983},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19109094555592979}]
["Multi-Family (5+ units)",10794,"Mountain North","1990s","Brick","radiator","window/wall unit",13.245741887541842,22412.42282,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1782.7162160646474},"Cold/Very Cold",77.255621465916633,"Metropolitan Area",7.8965278928176952E-2,0.11692827693025558,4.2803917474320595E-3,6.5643745197498007E-4,6.281433370343277E-2,0.26359250478602003,29.289000000000001,0,{"$f":"T795*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2213975252317464E-5},{"$f":"U795*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.9017492903429271E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.2803917474320595E-3}]
["Single Family Detached",10795,"East North Central","1970s","Siding","central furnace","central AC",37.776144459171697,16034.017169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16034.017169999999},"Cold/Very Cold",117.67552801135942,"Metropolitan Area",0.94786681471556533,0.26835573346828051,3.9665512865746953E-2,1.7403546712558379E-2,0.34678622465943859,1.6026742857090313,957.98900000000003,127.425,{"$f":"T796*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5360412074671131E-2},{"$f":"U796*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0431346378872498E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.96322722679023642},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1708647503634205E-2}]
["Multi-Family (2-4 units)",10796,"Pacific","1960s","Stucco","portable electric heaters","window/wall unit",14.141665207899363,19668.519069999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6556.1730233333328},"Hot-Dry/Mixed-Dry",174.05935239744775,"Metropolitan Area",0.13917493265229672,0.38806357893268506,6.3320535266171943E-2,0,0.44411757982844557,1.0346766266795993,0,0,{"$f":"T797*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U797*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13917493265229672},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.3320535266171943E-2}]
["Single Family Detached",10797,"West North Central","2000s","Siding","central furnace","central AC",111.49427255867322,22130.661479999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22130.661479999999},"Cold/Very Cold",241.64889757442219,"Metropolitan Area",1.6089621398505562,0.63236712018687435,0.15423265189583232,5.1064221906967557E-2,0.62954700999447777,3.0251089219277412,1840.271,467.12599999999998,{"$f":"T798*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0726414532461078E-2},{"$f":"U798*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0337807374506479E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6496885543830173},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16457045927033881}]
["Multi-Family (5+ units)",10798,"East South Central","1970s","Brick","built-in electric unit","window/wall unit",18.825176188121006,24134.841270000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1919.7198468779955},"Mixed-Humid",320.78339159486734,"Metropolitan Area",0.20143440528640419,0.6973092643121257,5.8640882395703128E-2,0,0.13712837573423528,1.0945129277284682,0,0,{"$f":"T799*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U799*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20143440528640419},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8640882395703128E-2}]
["Multi-Family (5+ units)",10799,"East North Central","1990s","Brick","central furnace","central AC",13.285628272571039,22142.713790000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1761.2631734702964},"Cold/Very Cold",140.29623455835016,"Metropolitan Area",0.39722294894088483,0.30764351401728174,1.4924357429063151E-2,3.9952098491297001E-3,1.0061487725792471,1.7296170181012174,152.173,28.257000000000001,{"$f":"T800*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6801670089649545E-4},{"$f":"U800*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9768013492750166E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39749096564178132},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4974125442555901E-2}]
["Mobile Home",10800,"West South Central","1990s","Siding","central furnace","central AC",18.440194114108159,14406.40165,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14406.40165},"Mixed-Humid",449.61342293871365,"Micropolitan Area",0.28233602565502736,0.15013558006899086,0.13355564138285039,8.5189518940961516E-3,0.96805376100473706,1.5340810081116056,252.15299999999999,339.178,{"$f":"T801*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.63261739525245E-3},{"$f":"U801*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8863344988436998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2859686430502798},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1384419758816941}]
["Single Family Detached",10801,"Middle Atlantic","1950s","Siding","central furnace","central AC",31.886809345257184,18035.52565,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18035.52565},"Cold/Very Cold",231.5573743351662,"Metropolitan Area",0.33324278618108866,0.28397797234051064,6.3815623437638844E-2,1.8172000472593548E-2,0.42676468784579125,1.1078010698050293,860.27300000000002,147.29400000000001,{"$f":"T802*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.551547575750245E-2},{"$f":"U802*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6565247150911E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34875826193859111},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6472148152729948E-2}]
["Mobile Home",10802,"Pacific","1970s","Wood","fireplace","window/wall unit",16.655475254425774,11566.30226,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11566.30226},"Hot-Dry/Mixed-Dry",40.690251350742969,"Metropolitan Area",0.20593036641350615,0.17462397174938674,6.6643391207199087E-2,0,0.10108232221130103,0.54828005158139304,0,0,{"$f":"T803*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U803*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20593036641350615},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6643391207199087E-2}]
["Single Family Detached",10803,"West South Central","1980s","Stone","heat pump","central AC",51.655418005727149,28825.568080000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28825.568080000001},"Hot-Humid",928.67309634328547,"Metropolitan Area",0.53373787941642625,0.34921812526762191,0.65399653521437373,3.9650087754265442E-2,1.6316800153155282,3.16863255521395,231.35400000000001,1144.164,{"$f":"T804*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6689104775803209E-3},{"$f":"U804*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.298117727668512E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54040678989400659},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.68697771249105888}]
["Single Family Detached",10804,"West North Central","Before 1950","Stucco","radiator","central AC",40.566882295612217,9513.8091690000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9513.8091690000001},"Cold/Very Cold",38.898302874548435,"Metropolitan Area",0.3984363300977945,0.27776535326049823,4.542149370128163E-3,8.4896476119571509E-4,0.1790678030632453,0.8598116357916662,53.069000000000003,36.165999999999997,{"$f":"T805*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0488833878966103E-4},{"$f":"U805*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.44076422406054E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39894121843658414},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.8862257925342172E-3}]
["Single Family Detached",10805,"West South Central","1980s","Brick","central furnace","central AC",22.833639417406108,18594.16891,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18594.16891},"Hot-Humid",335.36945082653034,"Metropolitan Area",0.26379599496289946,0.33470495107202908,0.27428794071205609,1.67380989694038E-2,0.27149169380886351,1.144280580555848,229.91,670.27,{"$f":"T806*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2749853740981E-3},{"$f":"U806*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.24631135953057E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26807098033699756},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28675105430736181}]
["Single Family Detached",10806,"New England","1950s","Siding","central furnace","N/A",34.250451565764671,13591.44903,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13591.44903},"Cold/Very Cold",191.62972708526345,"Rural",1.0704369057213783,0.33215629886788567,0,2.8547017433344979E-2,0.29313731460300829,1.6957305191922725,2100.366,0,{"$f":"T807*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8547017433344979E-2},{"$f":"U807*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0989839231547234},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10807,"Pacific","1950s","Concrete","N/A","window/wall unit",9.8335810899662626,19511.07359,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1551.9387422356185},"Hot-Dry/Mixed-Dry",48.006060039622369,"Metropolitan Area",0,0.10289993878314074,2.4924499001839857E-2,0,0.13887215396169914,0.26669659174667976,0,0,{"$f":"T808*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U808*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.4924499001839857E-2}]
["Single Family Detached",10808,"East North Central","1960s","Brick","radiator","window/wall unit",58.419600126825557,14782.287480000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14782.287480000001},"Cold/Very Cold",66.802531881562871,"Metropolitan Area",1.7487482305444328,0.13987448316886644,4.8574641006142442E-2,1.6222082280552001E-3,0.20941321645626998,2.1466105711757115,109.74,0,{"$f":"T809*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6222082280552001E-3},{"$f":"U809*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7503704387724881},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.8574641006142442E-2}]
["Single Family Detached",10809,"Pacific","1980s","Stucco","central furnace","central AC",36.184427307836756,20629.662090000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20629.662090000002},"Hot-Dry/Mixed-Dry",90.646219486859763,"Metropolitan Area",4.4820395820313712E-2,7.3584478080035348E-2,6.172784797941501E-2,4.4572654208274902E-3,0.52977506555368137,0.7099077874334454,64.844999999999999,151.21600000000001,{"$f":"T810*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3377304382260499E-3},{"$f":"U810*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1195349826014405E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.615812625853976E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4847382962016448E-2}]
["Single Family Detached",10810,"East North Central","1970s","Siding","central furnace","central AC",50.101545611861297,23812.521680000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23812.521680000002},"Cold/Very Cold",110.68367257762131,"Metropolitan Area",0.32612398585557145,0.16013032622741338,6.9531825117427934E-2,3.1222025925948801E-2,0.42804841283969369,0.98383455004010645,1174.433,136.727,{"$f":"T811*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7966211274207443E-2},{"$f":"U811*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2558146517413602E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35409019712977891},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.2787639769169299E-2}]
["Single Family Attached",10811,"Pacific","1980s","Stucco","central furnace","N/A",11.481539941370171,10010.06098,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10010.06098},"Marine",28.65646222475721,"Metropolitan Area",9.4950433425790015E-3,1.231199462308276E-2,0,1.362869802427E-4,7.5968805242160098E-2,9.7775843207821858E-2,13.615,0,{"$f":"T812*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.362869802427E-4},{"$f":"U812*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.6313303228217021E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",10812,"Middle Atlantic","2000s","Brick","central furnace","central AC",47.958458448484187,16257.10456,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5419.0348533333336},"Cold/Very Cold",215.54953535328056,"Metropolitan Area",1.1264039227393361,0.25829552715732329,3.8773248565948534E-2,1.3961877766905519E-2,0.89097116815235522,2.3237517851262335,725.178,133.63900000000001,{"$f":"T813*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9297648568705603E-3},{"$f":"U813*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.241943987646134E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1303336875962067},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.949744296471315E-2}]
["Single Family Detached",10813,"East South Central","1980s","Brick","heat pump","central AC",21.447923149342198,15319.945110000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15319.945110000001},"Hot-Humid",154.13621975016775,"Micropolitan Area",5.0252330750370902E-2,8.9165726687136182E-2,0.122234915923174,6.9203715649245297E-3,0.26425983054054381,0.52591280390122486,56.716999999999999,395.00599999999997,{"$f":"T814*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6890132680387004E-4},{"$f":"U814*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0514702381206601E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.1121232077174769E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12828638616129465}]
["Single Family Attached",10814,"West South Central","2000s","Brick","built-in electric unit","central AC",11.975769163188149,17356.187190000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17356.187190000001},"Hot-Humid",193.34277054271666,"Metropolitan Area",9.4400926949148853E-2,0.13391893450687761,0.13890875154306664,5.8103828541578705E-3,0.29245690893909543,0.65968552193818852,0,334.77300000000002,{"$f":"T815*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U815*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8103828541578705E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.4400926949148853E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1447191343972245}]
["Multi-Family (5+ units)",10815,"East North Central","1980s","Wood","built-in electric unit","N/A",17.640850696993308,14135.29703,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1124.3417740532993},"Cold/Very Cold",106.50946314250365,"Metropolitan Area",1.6698719011093471E-2,6.7874063566723292E-2,0,0,0.27883750559120585,0.36341028816902254,0,0,{"$f":"T816*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U816*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6698719011093471E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10816,"West South Central","1950s","Wood","heat pump","central AC",45.207128067594994,39344.758979999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39344.758979999999},"Hot-Humid",581.94652020879573,"Metropolitan Area",0.32745076977646592,0.20453864765240248,0.72265026365956841,3.7345376362913338E-2,0.73096176530457546,1.9856014463930123,133.83099999999999,815.35199999999998,{"$f":"T817*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2655484390523796E-3},{"$f":"U817*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2079827923860958E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33271631821551828},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.75473009158342941}]
["Multi-Family (5+ units)",10817,"West South Central","1970s","Brick","central furnace","central AC",13.210932303931806,23889.570169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1900.2106322422696},"Hot-Humid",106.66693080841866,"Metropolitan Area",0.13519628854673185,0.31668484841884353,0.17664272233779449,9.522549896753189E-3,0.26626249436652411,0.90355146630716099,92.796000000000006,305.81099999999998,{"$f":"T818*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7633194582955368E-4},{"$f":"U818*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8110531365664075E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13537262049256141},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17722382765145112}]
["Single Family Detached",10818,"Middle Atlantic","Before 1950","Siding","other","window/wall unit",157.15473206331933,34892.258450000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34892.258450000001},"Cold/Very Cold",598.09542480614857,"Micropolitan Area",1.0046172423394895,0.92534604375081131,0.16247276584593984,0.20833033522095376,0.74455243465278864,2.8369884865890294,5970.6750000000002,0,{"$f":"T819*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.20833033522095376},{"$f":"U819*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2129475775604432},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16247276584593984}]
["Single Family Detached",10819,"Mountain South","Before 1950","Wood","central furnace","central AC",9.5092396014495826,7924.3663349999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7924.3663349999997},"Hot-Dry/Mixed-Dry",153.05596600513175,"Metropolitan Area",0.27342273224115671,8.5908221849428049E-2,0.14659992929030219,1.0714234595632768E-2,0.28536229575443789,0.79129317913532482,549.76199999999994,802.3,{"$f":"T820*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3565154850622699E-3},{"$f":"U820*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3577191105704993E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27777924772621898},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1529576484008727}]
["Single Family Detached",10820,"Mountain North","2000s","Siding","central furnace","central AC",19.187851801794213,7106.6117780000004,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7106.6117780000004},"Cold/Very Cold",95.002913160878833,"Metropolitan Area",0.36886546504195455,0.17830553621169179,1.9302154544437355E-2,8.8854393457040697E-3,0.3189467264479377,0.88541988224602153,1107.287,143.01900000000001,{"$f":"T821*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8690588358262866E-3},{"$f":"U821*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.016380509877782E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37673452387778084},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0318535054315138E-2}]
["Single Family Detached",10821,"Middle Atlantic","Before 1950","Brick","central furnace","central AC",67.042844563274215,46045.909729999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":46045.909729999999},"Cold/Very Cold",196.27276227950668,"Metropolitan Area",4.4127467221241305,0.14675227425774676,9.7928875252833184E-2,3.4097502660072027E-2,0.52568750279396825,5.1831153744286782,645.18299999999999,95.328000000000003,{"$f":"T822*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.970803817733059E-2},{"$f":"U822*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3894644827414397E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.4424547603014615},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10231833973557462}]
["Single Family Detached",10822,"Pacific","2000s","Siding","central furnace","central AC",46.494635492607429,20545.574680000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20545.574680000002},"Marine",158.71096889932886,"Metropolitan Area",0.68432230393019111,0.35704153097398172,3.3530418968909362E-2,1.2008436397817041E-2,0.54415575016335316,1.6190500040364353,500.661,83.816999999999993,{"$f":"T823*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.028636796486348E-2},{"$f":"U823*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7220684329535599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6946086718950546},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5252487401862924E-2}]
["Multi-Family (2-4 units)",10823,"East North Central","1960s","Brick","built-in electric unit","N/A",46.512708300344265,52855.350339999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17618.450113333332},"Cold/Very Cold",104.17102432715851,"Metropolitan Area",0.11191729304902484,0.11608181895766377,0,0,0.12743250544317877,0.35543161744986734,0,0,{"$f":"T824*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U824*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11191729304902484},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10824,"Mountain North","1950s","Brick","central furnace","central AC",23.143486093000618,9691.5770909999992,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9691.5770909999992},"Cold/Very Cold",61.23190740528765,"Metropolitan Area",0.38303129480824638,0.15876761942788092,4.9879019553315876E-2,1.8439708226922417E-2,0.14288389990189923,0.73456183369134231,1667.4649999999999,235.18799999999999,{"$f":"T825*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6160365594044313E-2},{"$f":"U825*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2793426328781073E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3991916604022907},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2158362186193984E-2}]
["Mobile Home",10825,"East South Central","1980s","Siding","portable electric heaters","window/wall unit",13.160442773149363,17135.993190000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17135.993190000001},"Hot-Humid",1.0123602059272372,"Micropolitan Area",6.2186519286509996E-4,8.4453028837596007E-4,1.8907854885846E-4,0,1.7986966611815403E-3,3.4541706912810601E-3,0,0,{"$f":"T826*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U826*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.2186519286509996E-4},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8907854885846E-4}]
["Multi-Family (5+ units)",10826,"South Atlantic","1970s","Siding","central furnace","central AC",62.799635089377745,59980.549270000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4770.9388088410851},"Mixed-Humid",215.23846163210547,"Metropolitan Area",0.9557233900987655,0.67884588116988021,0.18407546944836559,1.675712593285552E-2,0.42184848130424596,2.2559174621534539,139.57,139.80600000000001,{"$f":"T827*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6587992954995022E-4},{"$f":"U827*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6700587110883689E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95638927002831542},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18474247531947444}]
["Multi-Family (5+ units)",10827,"East North Central","1970s","Siding","built-in electric unit","window/wall unit",24.089216456655116,24431.254010000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1943.2969408178176},"Cold/Very Cold",189.56078059786853,"Metropolitan Area",0.18614399640881293,0.22914955104248763,1.582248632825833E-2,0,0.21566530674176432,0.64678134052132319,0,0,{"$f":"T828*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U828*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18614399640881293},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.582248632825833E-2}]
["Single Family Detached",10828,"South Atlantic","1980s","Siding","central furnace","central AC",29.48224778964866,12751.83728,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12751.83728},"Mixed-Humid",205.59536034156173,"Metropolitan Area",0.48226392740833218,0.1888515859166664,0.1427073412209536,1.8034591917334718E-2,0.56916387292034809,1.3829867274663004,890.44,523.83399999999995,{"$f":"T829*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.13547459876032E-2},{"$f":"U829*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6798459297315186E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4936186733959354},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14938718715068514}]
["Single Family Detached",10829,"South Atlantic","1990s","Stucco","built-in electric unit","window/wall unit",36.554729724404375,26036.132280000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26036.132280000002},"Hot-Humid",509.65728942679181,"Metropolitan Area",0.13247605889406938,0.42493550665282176,0.47669466068602251,0,0.70484444513505817,1.7389506713679719,0,0,{"$f":"T830*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U830*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13247605889406938},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.47669466068602251}]
["Single Family Detached",10830,"South Atlantic","1970s","Brick","heat pump","central AC",47.936448908890448,17913.47119,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17913.47119},"Mixed-Humid",377.01821810006356,"Rural",0.61009771832786774,9.9405828423914183E-2,0.30711254478543537,2.8145251837361818E-2,0.32977804787230514,1.3463941394095222,653.45799999999997,917.72,{"$f":"T831*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1705701056875021E-2},{"$f":"U831*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6439550780486801E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62180341938474282},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32355209556592218}]
["Single Family Detached",10831,"East North Central","Before 1950","Siding","central furnace","central AC",65.9904945822027,35326.817230000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35326.817230000001},"Cold/Very Cold",315.0006801337326,"Metropolitan Area",2.465658559594039,0.54392792338755802,0.40317782902890953,0.13580366873692107,0.61404056296849774,4.0268048749790042,3316.5610000000001,527.64800000000002,{"$f":"T832*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.11716354427914603},{"$f":"U832*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8640124457775041E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5828221038731849},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.42181795348668455}]
["Single Family Detached",10832,"Mountain South","1970s","Stucco","heat pump","central AC",25.554695385070129,18279.467369999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18279.467369999998},"Hot-Dry/Mixed-Dry",124.90685429324944,"Metropolitan Area",2.6113590098097748E-2,8.3396450541085715E-2,5.562476651679002E-2,3.9472681838777996E-3,0.26104737352050461,0.42618218067647806,27.209,188.73099999999999,{"$f":"T833*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9736602767032996E-4},{"$f":"U833*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4499021562074696E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6610956125768078E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9074668672997488E-2}]
["Single Family Detached",10833,"East South Central","2000s","Brick","heat pump","central AC",63.891415010913235,16432.97711,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16432.97711},"Hot-Humid",280.21604595816183,"Metropolitan Area",0.11785576713307166,0.1498917738441311,0.34610004156959123,1.9457630876866597E-2,0.34224959783699288,0.95609718038378677,124.464,1059.596,{"$f":"T834*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.04531406301904E-3},{"$f":"U834*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7412316813847559E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11990108119609071},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36351235838343882}]
["Multi-Family (2-4 units)",10834,"West North Central","1950s","Brick","built-in electric unit","window/wall unit",14.596183746678953,19967.41963,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6655.8065433333331},"Cold/Very Cold",218.88544970585735,"Metropolitan Area",0.41611273861005355,0.13053145488846787,4.757279658428723E-2,0,0.1526201732451197,0.74683716332792838,0,0,{"$f":"T835*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U835*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.41611273861005355},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.757279658428723E-2}]
["Single Family Detached",10835,"South Atlantic","1960s","Siding","wood-burning stove","N/A",29.107029816175583,17325.612990000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17325.612990000001},"Hot-Humid",148.84238336690194,"Metropolitan Area",0.34598050208611097,8.8540015645898473E-2,0,0,7.3329686745847583E-2,0.507850204477857,0,0,{"$f":"T836*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U836*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34598050208611097},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10836,"South Atlantic","1950s","Stucco","heat pump","central AC",36.131660569146575,22414.181489999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22414.181489999999},"Hot-Humid",320.88142227537372,"Metropolitan Area",4.287252391736409E-2,8.6779081269406352E-2,0.49931570027607619,2.5744032292154398E-2,0.46588010712053957,1.0948474125833862,31.385999999999999,1117.174,{"$f":"T837*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.034915002451399E-4},{"$f":"U837*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.504054079190926E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.3576015417609228E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.5243562410679854}]
["Multi-Family (5+ units)",10837,"West North Central","1970s","Brick","central furnace","central AC",15.865445527040347,23679.76944,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1883.5227816463296},"Cold/Very Cold",127.39715960518966,"Metropolitan Area",0.12675619872206231,0.12607123457717664,1.3964129330522655E-2,2.8916787249350403E-3,0.16521261475394691,0.43466584784064,97.058000000000007,25.058,{"$f":"T838*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8281095414102947E-4},{"$f":"U838*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.719731386249373E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12693900967620333},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4011326644385149E-2}]
["Single Family Detached",10838,"South Atlantic","1980s","Brick","central furnace","central AC",79.897468566553897,22255.562269999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22255.562269999999},"Mixed-Humid",171.1201918745752,"Metropolitan Area",0.25436066839549837,0.36190317294078839,0.20059178634023511,1.7708572853740837E-2,0.37535583687719953,1.1922114645537214,355.61900000000003,440.07299999999998,{"$f":"T839*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.9145007988951303E-3},{"$f":"U839*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7940720548457087E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26227516919439348},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21038585839508081}]
["Mobile Home",10839,"South Atlantic","1980s","Wood","central furnace","both central and individual units",15.469234340215481,17420.308939999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17420.308939999999},"Hot-Humid",303.41349266775063,"Metropolitan Area",5.8063109118645796E-2,0.27408380691189621,0.37807369657779544,1.1602970972576399E-2,0.3250262079685366,1.0352468205768741,40.884999999999998,625.17499999999995,{"$f":"T840*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1222933101189995E-4},{"$f":"U840*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0890741641564498E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.8775338449657696E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.38896443821935994}]
["Single Family Detached",10840,"West North Central","Before 1950","Brick","central furnace","central AC",11.909337273881789,9466.8817760000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9466.8817760000002},null,70.065329243552654,"Micropolitan Area",0.78588146116811952,8.2472652901742743E-2,1.1110673260057536E-2,1.8165753301040224E-2,0.12779389150454926,1.0072586788344691,1868.165,50.709000000000003,{"$f":"T841*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.768569719306104E-2},{"$f":"U841*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.80056107979184E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80356715836118053},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.159072936803672E-2}]
["Single Family Detached",10841,"Mountain South","2000s","Stucco","central furnace","central AC",32.449112473066918,17371.04522,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17371.04522},"Cold/Very Cold",146.7002487390377,"Metropolitan Area",0.42907412781423793,0.24975293223444925,5.8855567893781234E-2,1.3022951004117459E-2,0.48644461031007097,1.2241272382525394,589.19299999999998,160.5,{"$f":"T842*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.023489824630746E-2},{"$f":"U842*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7880527578099997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43930902606054539},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1643620651591235E-2}]
["Single Family Detached",10842,"East South Central","1970s","Brick","fireplace","central AC",42.797484600315443,16137.814710000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16137.814710000001},"Hot-Humid",258.26079144583002,"Rural",8.0104529625574378E-2,0.14416652219919657,0.25365362292607985,1.1434271096808691E-2,0.40326112231945599,0.88118579707030675,0,708.53899999999999,{"$f":"T843*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U843*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1434271096808691E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.0104529625574378E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26508789402288851}]
["Single Family Detached",10843,"Middle Atlantic","1950s","Siding","heater burning gas/oil/kerosene","window/wall unit",59.026129069309853,23820.068230000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23820.068230000001},"Mixed-Humid",260.72758282540946,"Metropolitan Area",2.0390322366665243,0.49770036444867333,0.30519138466759577,0,0.60753153098812862,3.449455516770922,0,0,{"$f":"T844*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U844*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0390322366665243},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30519138466759577}]
["Mobile Home",10844,"Mountain North","1970s","Siding","central furnace","window/wall unit",22.685030428287501,30006.654009999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30006.654009999998},"Cold/Very Cold",611.98474823273807,"Metropolitan Area",1.0542778473238561,0.38563474494773037,2.7724677979193507E-2,1.2882246652995128E-2,0.62045466653511638,2.0880919367858963,429.31299999999999,0,{"$f":"T845*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2882246652995128E-2},{"$f":"U845*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0671600939768513},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7724677979193507E-2}]
["Single Family Detached",10845,"New England","1960s","Wood","central furnace","window/wall unit",45.676545871991159,14888.05276,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14888.05276},"Cold/Very Cold",104.88098689315828,"Metropolitan Area",1.3475686766644084,0.42946143987733415,6.9992800463163474E-2,6.0588791713415004E-2,0.30156005451082207,2.1485829715157281,4069.625,0,{"$f":"T846*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0588791713415004E-2},{"$f":"U846*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4081574683778233},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9992800463163474E-2}]
["Single Family Detached",10846,"Middle Atlantic","1950s","Siding","central furnace","central AC",31.642863268044159,19776.789540000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19776.789540000002},"Cold/Very Cold",56.717202094960001,"Metropolitan Area",2.3979514344958952,3.8884530289861809E-2,3.0289399118251022E-2,1.088921898146124E-2,0.75693884030970382,3.2240642042137111,483.88,66.725999999999999,{"$f":"T847*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5695929226151995E-3},{"$f":"U847*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3196260588460402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4075210274185106},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.1609025177097065E-2}]
["Single Family Detached",10847,"West North Central","1980s","Siding","central furnace","central AC",57.514132995283731,22643.35945,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22643.35945},"Mixed-Humid",236.98911348285463,"Metropolitan Area",0.75758360958077509,0.31643755180983252,0.35487687352543357,5.566580085781541E-2,0.41554703796857451,1.8444450728846158,1686.2750000000001,772.09699999999998,{"$f":"T848*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8182930956548754E-2},{"$f":"U848*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.748286990126665E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.79576654053732387},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3723597434267002}]
["Single Family Detached",10848,"East South Central","Before 1950","Siding","central furnace","central AC",24.232962194792588,17623.97251,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17623.97251},"Mixed-Humid",378.12622499921457,"Metropolitan Area",0.42577480252937849,0.35084489724558754,0.10417017293060958,2.194656899958268E-2,0.53196292031238301,1.4127527930179586,977.75400000000002,267.51400000000001,{"$f":"T849*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7231909617542538E-2},{"$f":"U849*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7146593820401404E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44300671214692106},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10888483231264973}]
["Multi-Family (2-4 units)",10849,"East North Central","2000s","Brick","central furnace","central AC",15.35391146407774,19288.833500000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6429.6111666666666},"Cold/Very Cold",48.790525667136578,"Micropolitan Area",0.30904002584956214,0.18457349754315502,1.1481035179758334E-2,3.4852993251149999E-3,0.17665871049310006,0.68407680194898557,154.83699999999999,25.853000000000002,{"$f":"T850*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9554170421316669E-4},{"$f":"U850*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6622473749183334E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31003556755377532},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1647259917250167E-2}]
["Single Family Detached",10850,"Pacific","1990s","Wood","heat pump","central AC",52.130835717470802,15692.60557,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15692.60557},"Marine",306.26382651762412,"Metropolitan Area",0.33278842561913569,0.24789227688613646,2.1422540797407519E-2,8.252615728418438E-3,0.68453841485976907,1.2866416581624489,446.90199999999999,78.989999999999995,{"$f":"T851*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0130568144441399E-3},{"$f":"U851*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2395589139742999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33980148243357983},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.266209971138182E-2}]
["Single Family Detached",10851,"Pacific","Before 1950","Wood","radiator","window/wall unit",36.116618057581157,18998.747009999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18998.747009999999},"Marine",209.64722146704474,"Metropolitan Area",1.4936682857970278,0.26417446137954032,2.3336806909781342E-2,1.2676343980012198E-3,0.96438686653720285,2.7455664206235522,66.721999999999994,0,{"$f":"T852*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2676343980012198E-3},{"$f":"U852*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.494935920195029},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3336806909781342E-2}]
["Multi-Family (5+ units)",10852,"Pacific","1960s","Wood","central furnace","window/wall unit",19.573517888588917,20075.402959999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1596.8263087062455},"Hot-Dry/Mixed-Dry",56.925953168726103,"Metropolitan Area",3.2530255385271142E-2,0.24293927685596639,2.850357908308496E-2,6.5283202885623999E-4,0.22380657466816206,0.52838059082660793,32.518999999999998,0,{"$f":"T853*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1927194732818398E-5},{"$f":"U853*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2582182580003963E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.850357908308496E-2}]
["Single Family Detached",10853,"South Atlantic","1960s","Siding","heat pump","central AC",65.499402324399128,20872.977159999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20872.977159999999},"Mixed-Humid",400.35111181319326,"Metropolitan Area",0.20769010948063754,0.29945324841494497,0.31033107522401604,2.2490987730511721E-2,0.54852355503680783,1.3659979881564062,213.613,863.904,{"$f":"T854*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4587392700790804E-3},{"$f":"U854*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8032248460432637E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21214884875071663},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32836332368444865}]
["Single Family Detached",10854,"South Atlantic","1990s","Stucco","central furnace","both central and individual units",84.574851315817256,27335.11678,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27335.11678},"Hot-Humid",353.57590862666837,"Metropolitan Area",0.25391401364636218,0.28832274793598994,0.39240549668917435,3.046096938914334E-2,0.64895983660043344,1.58360209487196,327.988,786.36500000000001,{"$f":"T855*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9655902824386392E-3},{"$f":"U855*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1495379106704699E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26287960392880083},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.41390087579587903}]
["Single Family Detached",10855,"West South Central","1990s","Brick","central furnace","central AC",81.435739734831429,23700.739150000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23700.739150000001},"Hot-Humid",478.99622814605215,"Metropolitan Area",1.297482270308477,0.3024480711848046,0.69308000394127556,7.0653396552716449E-2,0.49370206268307831,2.7867124081176353,1250.971,1730.0920000000001,{"$f":"T856*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9648937355214653E-2},{"$f":"U856*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.10044591975018E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3271312076636916},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.7340844631387774}]
["Single Family Detached",10856,"East North Central","Before 1950","Siding","central furnace","N/A",45.86009764891152,19108.374019999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19108.374019999999},"Cold/Very Cold",169.23855020597526,"Metropolitan Area",0.28792236188611919,8.941022217747023E-2,0,5.2722296926062395E-3,0.23764396867209281,0.6149765527356823,275.91199999999998,0,{"$f":"T857*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2722296926062395E-3},{"$f":"U857*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29319459157872541},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10857,"New England","1950s","Wood","radiator","window/wall unit",34.214099134204275,15032.55674,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15032.55674},"Cold/Very Cold",91.290447149847679,"Metropolitan Area",1.0570156853311037,0.24004626989349123,2.8539519426684357E-2,2.1812540480874798E-3,0.32881520108954598,1.6544166757408254,145.102,0,{"$f":"T858*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1812540480874798E-3},{"$f":"U858*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0591969393791911},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8539519426684357E-2}]
["Single Family Detached",10858,"South Atlantic","1990s","Siding","heat pump","central AC",30.541411180713059,16967.450659999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16967.450659999999},"Hot-Humid",335.13618176311837,"Metropolitan Area",0.1608809556209484,0.15785616819179016,0.44855430830966825,2.5896266155713117E-2,0.37619325541486764,1.1434846875372744,229.934,1296.298,{"$f":"T859*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9013938000564399E-3},{"$f":"U859*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.199487235565668E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16478234942100484},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.47054918066532492}]
["Multi-Family (5+ units)",10859,"South Atlantic","1990s","Brick","radiator","both central and individual units",40.971105014918024,28995.82804,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2306.3696977464929},"Mixed-Humid",347.28303238759599,"Metropolitan Area",0.2602055170149099,0.27503496858682513,4.0599500404153596E-2,2.3579117403847603E-3,0.60687517095773769,1.18488551702656,27.507999999999999,53.811,{"$f":"T860*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3443617645610528E-5},{"$f":"U860*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2410805980543653E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2602689606325555},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.0723608463959032E-2}]
["Single Family Detached",10860,"South Atlantic","2010s","Stucco","heat pump","central AC",16.192283889511661,9236.8989669999992,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9236.8989669999992},"Hot-Humid",112.0066368763368,"Metropolitan Area",1.7880262517077476E-2,8.0510307774004655E-2,0.10441979906450895,5.5876772921073089E-3,0.1793570885050669,0.38216745786065798,33.634999999999998,571.29499999999996,{"$f":"T861*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1068309675504497E-4},{"$f":"U861*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.276994195352264E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.819094561383252E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10969679325986122}]
["Single Family Detached",10861,"East North Central","1980s","Brick","central furnace","central AC",65.606963433489682,15978.315500000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15978.315500000001},"Cold/Very Cold",119.11599322285457,"Metropolitan Area",1.3896648732706529,0.28295457254054551,5.3127195991618005E-2,1.6872414100433497E-2,0.35417235342800141,2.0799189952308179,848.00099999999998,207.95599999999999,{"$f":"T862*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.35496275223155E-2},{"$f":"U862*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.322786578118E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4032145007929684},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.6449982569736004E-2}]
["Single Family Detached",10862,"East North Central","2000s","Siding","central furnace","central AC",36.02793835947179,12483.69313,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12483.69313},"Cold/Very Cold",76.77504978000249,"Metropolitan Area",0.88777539013609652,0.20241680480530561,6.6349281008001887E-2,3.2958697580238207E-2,0.22342656073446035,1.3799680366838643,2370.5030000000002,269.637,{"$f":"T863*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9592632015744393E-2},{"$f":"U863*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3660655644938099E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.91736802215184088},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9715346572495701E-2}]
["Mobile Home",10863,"West South Central","1990s","Siding","central furnace","central AC",21.424659649722319,18597.794829999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18597.794829999999},"Mixed-Humid",118.84453984546734,"Metropolitan Area",0.55674118691534691,9.4825097237976233E-2,9.4027307633153728E-2,7.3440088092393795E-3,0.2127428345450306,0.9583364263315074,209.828,185.05799999999999,{"$f":"T864*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9023380935892396E-3},{"$f":"U864*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4416707156501398E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.56064352500893611},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.7468978348803872E-2}]
["Multi-Family (5+ units)",10864,"Middle Atlantic","Before 1950","Brick","radiator","window/wall unit",21.967402415420221,45107.602500000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3587.9233178123768},"Mixed-Humid",76.756675172820493,"Metropolitan Area",0.4545647072760795,0.78768889241530504,4.1853630270855001E-2,2.5952208022349999E-3,0.30705214140816023,1.5935481645924676,57.533999999999999,0,{"$f":"T865*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0642758016701729E-4},{"$f":"U865*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45477113485624654},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1853630270855001E-2}]
["Multi-Family (2-4 units)",10865,"New England","1990s","Wood","central furnace","N/A",77.926870820698298,54916.751810000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18305.583936666666},"Cold/Very Cold",144.10155675370845,"Metropolitan Area",1.1096568934201569,1.7917971983488039,0,2.4441688894573082E-2,0.51436682739475437,3.4321153784267646,445.06799999999998,0,{"$f":"T866*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1472296315243595E-3},{"$f":"U866*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1178041230516813},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10866,"East South Central","1950s","Siding","central furnace","both central and individual units",42.712666319738616,16743.49915,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16743.49915},"Mixed-Humid",93.85000841294098,"Metropolitan Area",0.99461143453458423,0.14481199587997837,0.10342633557346161,2.1659407243939149E-2,0.20030273148393726,1.4431524974719614,984.69100000000003,308.91000000000003,{"$f":"T867*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6487172921512649E-2},{"$f":"U867*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1722343224265008E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0110986074560968},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10859856989588811}]
["Single Family Detached",10867,"Middle Atlantic","Before 1950","Siding","central furnace","central AC",44.421429733057479,27420.63564,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27420.63564},"Cold/Very Cold",247.70702667599895,"Metropolitan Area",1.0889229629323658,0.43825102205282662,6.9877349412558368E-2,1.6595215475048761E-2,0.66387717059105011,2.2609285049888008,498.99,106.21899999999999,{"$f":"T868*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.36826229780036E-2},{"$f":"U868*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9125924970451597E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1026055859103694},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.2789941909603528E-2}]
["Single Family Detached",10868,"Mountain North","2000s","Siding","central furnace","central AC",35.881359010414918,9006.3652129999991,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9006.3652129999991},"Cold/Very Cold",120.78261664282795,"Metropolitan Area",0.97601785275792396,0.1459984398200144,3.1737683482299321E-2,1.1857393165731641E-2,0.29623727452234366,1.4499912505825814,1102.529,214.02799999999999,{"$f":"T869*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.929778831923676E-3},{"$f":"U869*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9276143338079637E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.98594763158984766},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3665297816107283E-2}]
["Single Family Detached",10869,"New England","1950s","Siding","radiator","window/wall unit",64.139288643153023,23861.342499999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23861.342499999999},"Cold/Very Cold",180.91199815942093,"Rural",2.1676876442566977,0.30167947817703505,3.3852945613080006E-2,6.2523637139324994E-3,0.27548695409881208,2.7787070221456247,262.029,0,{"$f":"T870*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2523637139324994E-3},{"$f":"U870*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1739400079706304},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3852945613080006E-2}]
["Single Family Detached",10870,"New England","2000s","Siding","central furnace","central AC",81.780858056751498,19792.076010000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19792.076010000001},"Cold/Very Cold",506.11356638907858,"Metropolitan Area",0.85897714781402845,0.17651570906348904,4.5351186919869807E-2,3.9486735421878777E-2,1.7412785051069539,2.8221225489043413,1882.261,112.81699999999999,{"$f":"T871*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7253852782658615E-2},{"$f":"U871*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2328826392201697E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.89623100059668703},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7584069559089975E-2}]
["Single Family Detached",10871,"South Atlantic","1970s","Brick","central furnace","central AC",37.783408755574904,18009.251079999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18009.251079999998},"Mixed-Humid",25.424992427308393,"Rural",1.2662603027730903,1.0606260275548719E-2,2.3674727349503957E-2,3.2651672670593996E-3,4.5674594348568437E-2,1.3462158847467112,115.175,66.13,{"$f":"T872*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0742154931389996E-3},{"$f":"U872*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1909517739203998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2683345182662293},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.4865679123424356E-2}]
["Single Family Detached",10872,"West North Central","2010s","Wood","central furnace","central AC",59.27061373382756,12332.62874,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12332.62874},"Cold/Very Cold",265.64482310167409,"Rural",1.0060485076474672,0.27102836081821474,1.8478335287375462E-2,1.1500681937828341E-2,0.3608871866297283,1.6564423903827856,859.99800000000005,72.543000000000006,{"$f":"T873*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0606036051142522E-2},{"$f":"U873*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9464588668582005E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0166545436986099},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9372981174061284E-2}]
["Single Family Detached",10873,"South Atlantic","1990s","Siding","heat pump","central AC",50.58313004327681,17370.58037,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17370.58037},"Mixed-Humid",435.46125543483919,"Metropolitan Area",0.48212827493051646,0.27319691448631872,0.13404868186238814,1.681036178248713E-2,0.64199198425107451,1.531365855530298,541.18100000000004,426.56799999999998,{"$f":"T874*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4006280552169693E-3},{"$f":"U874*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4097337272701598E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49152890298573343},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1414584155896583}]
["Single Family Attached",10874,"East South Central","1990s","Brick","portable electric heaters","N/A",26.237480352764003,10325.651459999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10325.651459999999},"Mixed-Humid",187.83425607890641,"Metropolitan Area",0.56687868850570988,0.37327056556955468,0,1.4595618108253799E-2,0.1010982572574823,1.0412475113327468,1413.53,0,{"$f":"T875*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4595618108253799E-2},{"$f":"U875*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58147430661396371},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",10875,"Pacific","1970s","Siding","built-in electric unit","N/A",21.363830316683934,18417.095099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6139.0316999999995},"Marine",334.54288591738015,"Metropolitan Area",0.19972114899125848,0.40695463107380692,0,0,0.53478452042254976,1.1414603004876152,0,0,{"$f":"T876*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U876*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19972114899125848},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10876,"East North Central","1990s","Wood","central furnace","central AC",24.282556344485194,11833.60446,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11833.60446},"Cold/Very Cold",78.208291852194264,"Micropolitan Area",1.0222694228155575,0.1106595617195891,3.2937051140136536E-2,1.8888373429291443E-2,0.34020201073487927,1.5060680464101623,1460.585,135.57900000000001,{"$f":"T877*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7283985170209102E-2},{"$f":"U877*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6043882590823402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0395534079857667},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4541439399218873E-2}]
["Single Family Detached",10877,"Pacific","2000s","Stucco","central furnace","central AC",46.277676263126551,27222.162509999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27222.162509999998},"Hot-Dry/Mixed-Dry",218.48330684640976,"Metropolitan Area",0.84437660118057978,0.42629174214488474,0.16796240323861308,1.9762092207109561E-2,0.37246220244301104,1.8110929490070884,430.483,295.47300000000001,{"$f":"T878*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1718678183792328E-2},{"$f":"U878*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0434140233172306E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.85609527936437213},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17600581726193032}]
["Single Family Detached",10878,"Middle Atlantic","1970s","Siding","heat pump","central AC",26.806479411258593,12987.63537,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12987.63537},"Cold/Very Cold",215.48331329144574,"Metropolitan Area",0.33244287911146875,0.13023037066491547,4.8305886304293749E-2,7.9392376005980401E-3,0.22424991515473394,0.73522905123541193,446.90100000000001,164.39099999999999,{"$f":"T879*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8041872344883703E-3},{"$f":"U879*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1350503661096698E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33824706634595714},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0440936670403419E-2}]
["Single Family Detached",10879,"New England","2000s","Siding","central furnace","central AC",16.084539427130213,21853.99379,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21853.99379},"Cold/Very Cold",216.04213564874766,"Metropolitan Area",1.2412717716119674,0.30591574541941396,1.6103880213944148E-2,9.4436352125099599E-3,0.75233708901095553,2.3156284862562808,402.04399999999998,30.08,{"$f":"T880*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7862670793067595E-3},{"$f":"U880*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5736813320319996E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2500580386912743},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6761248347147348E-2}]
["Single Family Detached",10880,"East North Central","1950s","Siding","central furnace","window/wall unit",68.559014735836186,36448.173699999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":36448.173699999999},"Cold/Very Cold",395.75959150338161,"Metropolitan Area",3.3395282689486212,0.4106465928785093,6.4290970037603701E-2,6.6214595300968598E-2,0.78968292394491391,4.6041487558096481,1816.6780000000001,0,{"$f":"T881*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6214595300968598E-2},{"$f":"U881*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.4057428642495897},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4290970037603701E-2}]
["Single Family Detached",10881,"East South Central","1970s","Brick","heat pump","central AC",75.978189274818959,20255.44902,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20255.44902},"Mixed-Humid",321.52345214091963,"Metropolitan Area",0.234593546687385,0.23752311253459663,0.19880307976425088,1.5194503549658879E-2,0.42611831697707536,1.0970380559633079,242.85400000000001,507.29,{"$f":"T882*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9191168163030801E-3},{"$f":"U882*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0275386733355799E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23951266350368808},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20907846649760667}]
["Single Family Attached",10882,"South Atlantic","1980s","Stucco","heat pump","central AC",18.207904736955577,14269.517819999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14269.517819999999},"Hot-Humid",134.25751241634853,"Metropolitan Area",1.243515703472118E-2,5.1415313019757741E-2,0.12022994855056518,6.1378618560591599E-3,0.27400620643079304,0.45808662503583719,22.143000000000001,407.995,{"$f":"T883*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1596993308826002E-4},{"$f":"U883*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8218919229708994E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.275112696780944E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12605184047353607}]
["Multi-Family (5+ units)",10883,"East North Central","2000s","Brick","central furnace","central AC",17.008504024028031,13287.893770000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1056.9381048792566},"Cold/Very Cold",247.65932556187633,"Metropolitan Area",0.27209170591446186,0.35346708977712626,2.2859953360757086E-2,5.6433551962252297E-3,0.19140037654665112,0.84501360023901739,345.30099999999999,79.397999999999996,{"$f":"T884*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6496178455291218E-4},{"$f":"U884*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.39187716512032E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27245666769901478},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.294387213240829E-2}]
["Single Family Detached",10884,"East North Central","1950s","Siding","central furnace","N/A",35.703364294344112,18801.1397,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18801.1397},"Cold/Very Cold",127.74953282067736,"Metropolitan Area",1.4623374169428431,0.17077075189509999,0,4.7459491331033603E-2,0.38842188241619419,2.0215300512541372,2524.288,0,{"$f":"T885*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7459491331033603E-2},{"$f":"U885*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5097969082738767},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10885,"Mountain South","2000s","Stucco","N/A","central AC",55.662624518255065,21549.602989999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21549.602989999999},"Hot-Dry/Mixed-Dry",290.43675683555489,"Metropolitan Area",0,0.20724195011554927,0.44089112852869239,2.5154506776579159E-2,0.34283715938453796,0.99097023802877948,0,1167.2840000000001,{"$f":"T886*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U886*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5154506776579159E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46604563530527154}]
["Single Family Detached",10886,"South Atlantic","2000s","Siding","heat pump","central AC",41.532855922824652,11022.52015,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11022.52015},"Hot-Humid",139.75136951057428,"Metropolitan Area",6.1798530797385509E-2,7.3916678427775356E-2,0.15516393899390898,1.20817402463344E-2,0.18595251624525541,0.47683166446432518,159.309,936.78700000000003,{"$f":"T887*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7559866625763499E-3},{"$f":"U887*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0325753583758051E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.3554517459961865E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16548969257766705}]
["Single Family Detached",10887,"Mountain South","1990s","Stucco","heat pump","central AC",43.32280830158318,21880.20621,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21880.20621},"Hot-Dry/Mixed-Dry",296.68712860740163,"Metropolitan Area",6.8034072507105678E-2,0.15197282314784799,0.29328690076235037,1.6299397053664979E-2,0.49900267409062382,1.0122964705079278,49.960999999999999,694.97699999999998,{"$f":"T888*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0931569824578101E-3},{"$f":"U888*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.520624007120717E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.9127229489563485E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30849314083355756}]
["Single Family Detached",10888,"West North Central","1990s","Siding","central furnace","central AC",29.291722975357477,16814.99597,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16814.99597},"Cold/Very Cold",363.76884631717832,"Metropolitan Area",1.6393893990324258,0.51653575834341336,0.10813310259406139,2.4384283220891471E-2,1.1470361775882554,3.4110944375581562,1151.3810000000001,298.77,{"$f":"T889*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9360466874934572E-2},{"$f":"U889*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0238163459568989E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6587498659073603},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11315691894001829}]
["Single Family Detached",10889,"East North Central","Before 1950","Siding","central furnace","window/wall unit",46.246359514837984,18799.333139999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18799.333139999999},"Mixed-Humid",177.69819615780102,"Rural",1.0315514810541369,0.27184873443629326,0.190571528344819,2.970290876253372E-2,0.38603182327269508,1.880003567107944,1579.998,0,{"$f":"T890*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.970290876253372E-2},{"$f":"U890*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0612543898166706},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.190571528344819}]
["Single Family Detached",10890,"East South Central","2010s","Brick","heat pump","central AC",80.831318745972055,22996.107749999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22996.107749999999},"Hot-Humid",546.82405528536299,"Metropolitan Area",0.27011717980245076,0.24165818568368402,0.61054705169633172,4.269777010762725E-2,0.74344125943418127,1.8657636766166474,229.435,1627.3040000000001,{"$f":"T891*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2761119816212496E-3},{"$f":"U891*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7421658126006001E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27539329178407201},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.64796870982233767}]
["Single Family Detached",10891,"West North Central","1970s","Siding","central furnace","central AC",36.53655549905362,12495.40202,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12495.40202},"Cold/Very Cold",82.951438530824532,"Metropolitan Area",0.76295250350249322,0.12096158930978575,4.4398662457463996E-2,3.3436433769915973E-2,0.20714851228411782,1.1354612675538607,2519.576,156.32300000000001,{"$f":"T892*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.148311503994352E-2},{"$f":"U892*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.95331872997246E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.79443561854243672},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.6351981187436456E-2}]
["Single Family Detached",10892,"East North Central","1980s","Siding","central furnace","central AC",82.101545167395827,20774.682479999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20774.682479999999},"Cold/Very Cold",321.3953277978257,"Metropolitan Area",2.3154687443032449,0.6755097001677749,0.12436364792748385,7.6755699991794005E-2,1.0213582834471397,4.1367003758456438,3338.6759999999999,355.99900000000002,{"$f":"T893*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.935993380359648E-2},{"$f":"U893*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3957661881975207E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3848286781068415},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13175941411568137}]
["Single Family Detached",10893,"East North Central","Before 1950","Siding","central furnace","central AC",44.836630486322171,27918.200799999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27918.200799999999},"Cold/Very Cold",81.075627690386057,"Metropolitan Area",0.84203228344115433,0.4489331559970432,2.7744940445835198E-2,1.8638777136296799E-2,0.21024390186476874,1.5289542817488015,626.55200000000002,41.069000000000003,{"$f":"T894*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7492204547641603E-2},{"$f":"U894*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1465725886552001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.85952448798879588},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8891513034490397E-2}]
["Single Family Detached",10894,"West North Central","1960s","Brick","central furnace","central AC",27.220600262616323,20497.43996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20497.43996},"Mixed-Humid",359.36587272850176,"Metropolitan Area",0.8982950998972502,0.7387277566558399,0.18261394732203562,3.174350387613372E-2,1.0199798125124271,2.8396166163875529,1149.539,399.11799999999999,{"$f":"T895*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3562606634178442E-2},{"$f":"U895*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1808972419552799E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.92185770653142862},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1907948445639909}]
["Single Family Detached",10895,"Pacific","2000s","Stucco","central furnace","central AC",42.270338065798995,12785.946180000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12785.946180000001},"Hot-Dry/Mixed-Dry",82.857994470735491,"Metropolitan Area",0.25433787519525969,0.17576948894188529,6.944331218363195E-2,1.062744831778476E-2,0.29015322833736668,0.78970390465814366,500.33300000000003,330.84899999999999,{"$f":"T896*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3972308100779408E-3},{"$f":"U896*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2302175077068198E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26073510600533761},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.3673529691338766E-2}]
["Single Family Detached",10896,"Pacific","2000s","Stucco","central furnace","central AC",38.860947903768967,10537.133379999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10537.133379999999},"Hot-Dry/Mixed-Dry",112.53763820689885,"Metropolitan Area",0.26673666773018523,0.40318601197848963,0.15880749748785714,1.4675497680794578E-2,0.2543568215389575,1.0830869987354894,465.38299999999998,927.35799999999995,{"$f":"T897*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9038027437845397E-3},{"$f":"U897*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7716949370100382E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27164047047396978},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16857919242486719}]
["Mobile Home",10897,"Middle Atlantic","1980s","Wood","central furnace","window/wall unit",25.028406846948471,25539.19066,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25539.19066},"Cold/Very Cold",84.57119104936416,"Metropolitan Area",0.60368136780540771,0.24922240431226381,2.8938278162511381E-2,1.1833456296357701E-2,0.25948665611689892,1.1413287063970818,463.34500000000003,0,{"$f":"T898*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1833456296357701E-2},{"$f":"U898*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.61551482410176539},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8938278162511381E-2}]
["Mobile Home",10898,"East South Central","1980s","Siding","central furnace","both central and individual units",11.28438427953736,14105.48035,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14105.48035},"Hot-Humid",172.0263477522457,"Rural",0.27722738993029733,8.5408232143878798E-2,0.16407312782423483,6.5597536367675005E-3,0.33480828812325503,0.86151703802166602,179.12200000000001,285.928,{"$f":"T899*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5266018512527001E-3},{"$f":"U899*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0331517855147995E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27975399178155003},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16810627960974964}]
["Multi-Family (5+ units)",10899,"Pacific","1970s","Concrete","N/A","window/wall unit",6.3624693400462462,13801.451929999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1097.787256578614},"Hot-Humid",71.415613015334714,"Metropolitan Area",0,7.65262492571082E-2,7.2586210760131803E-2,0,9.4557611578970427E-2,0.24367007159621043,0,0,{"$f":"T900*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U900*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.2586210760131803E-2}]
["Single Family Attached",10900,"Pacific","1970s","Stucco","heater burning gas/oil/kerosene","central AC",25.749198576674509,15874.9683,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15874.9683},"Hot-Dry/Mixed-Dry",98.805374052318484,"Metropolitan Area",0.21508827862502852,0.18411819984276601,0.1650922567098039,7.7416981659560995E-3,0.22947406377371038,0.79377279895130881,0,487.66699999999997,{"$f":"T901*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U901*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7416981659560995E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21508827862502852},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17283395487576}]
["Mobile Home",10901,"South Atlantic","1960s","Siding","central furnace","N/A",37.375516726967035,24333.018700000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24333.018700000001},"Hot-Humid",160.84412491941791,"Metropolitan Area",0.25997012717384538,0.1335372463227861,0,3.3702204220247998E-3,0.1552927413509512,0.54880011484758273,138.50399999999999,0,{"$f":"T902*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3702204220247998E-3},{"$f":"U902*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26334034759587016},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10902,"West North Central","2010s","Siding","wood-burning stove","central AC",22.119589522584015,18071.56007,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18071.56007},"Cold/Very Cold",184.43510723935285,"Rural",0.13576328174515767,0.18228153752318563,1.5769008386801089E-2,6.5332303965064001E-4,0.29547873570801381,0.6292925633631582,0,36.152000000000001,{"$f":"T903*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U903*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5332303965064001E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13576328174515767},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.642233142645173E-2}]
["Multi-Family (5+ units)",10903,"Mountain South","1970s","Brick","N/A","central AC",12.103794457079124,23548.238239999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1873.0606015847791},"Hot-Dry/Mixed-Dry",139.26983835536541,"Metropolitan Area",0,0.19739920604050415,8.9927658494950991E-2,3.64227665329552E-3,0.18450923010326351,0.47518865938958527,0,154.673,{"$f":"T904*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U904*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8971190242892256E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0217370397379912E-2}]
["Single Family Detached",10904,"West North Central","1950s","Siding","central furnace","central AC",21.479667652833843,20074.455750000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20074.455750000001},"Mixed-Humid",157.38204682816306,"Metropolitan Area",1.1588506134661825,0.18497420558399025,0.194056391226684,3.1047454379786253E-2,0.34904957781815099,1.8869307880950077,1138.422,408.19299999999998,{"$f":"T905*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2853202063826503E-2},{"$f":"U905*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1942523159597505E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.181703815530009},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20225064354264374}]
["Multi-Family (5+ units)",10905,"South Atlantic","2010s","Brick","central furnace","central AC",10.216419717521898,11716.077660000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":931.91359992175762},"Hot-Humid",52.176391956917136,"Metropolitan Area",2.0141047984948375E-2,4.1455665400804621E-2,3.1476453956955787E-2,1.7799416663401802E-3,8.331431700880261E-2,0.17802584690801065,28.472999999999999,123.45,{"$f":"T906*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6534375930572205E-5},{"$f":"U906*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1504473391034098E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0167582360878948E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.1591498690866131E-2}]
["Single Family Detached",10906,"South Atlantic","1990s","Wood","N/A","N/A",34.614714646935141,26874.778450000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26874.778450000002},"Hot-Humid",528.49238389627817,"Metropolitan Area",0,0.54807200368510522,0,0,1.255144038482521,1.8032160421676262,0,0,{"$f":"T907*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U907*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10907,"Mountain South","1970s","Stucco","central furnace","central AC",9.6091334575575882,9845.4236249999994,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9845.4236249999994},"Hot-Dry/Mixed-Dry",182.13020611320448,"Metropolitan Area",0.13272773115640499,0.11803101442188076,0.22382034725351999,1.1906740278518999E-2,0.14684916994309688,0.6214282627749026,240.53,968.83799999999997,{"$f":"T908*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3681197445212499E-3},{"$f":"U908*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5386205339977499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13509585090092624},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23335896778751775}]
["Single Family Detached",10908,"Pacific","1980s","Wood","heat pump","central AC",19.093990089237678,9392.0266059999994,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9392.0266059999994},"Marine",164.45391626318116,"Metropolitan Area",0.18129271171514819,0.20144048719033938,1.5533951797020305E-2,3.920523058169186E-3,0.16284960785299921,0.56111675855550702,335.18299999999999,82.248000000000005,{"$f":"T909*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1480476538788978E-3},{"$f":"U909*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7247540429028799E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1844407593690271},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6306427201310592E-2}]
["Single Family Detached",10909,"East North Central","1950s","Brick","central furnace","central AC",76.372539167837587,26490.64834,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26490.64834},"Cold/Very Cold",136.37229471252758,"Metropolitan Area",2.5264999420404104,0.41705578704727342,0.15019058510901381,0.1008280434454995,0.40216806917084119,3.495914383367539,3502.6280000000002,303.54700000000003,{"$f":"T910*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.2786886613837521E-2},{"$f":"U910*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0411568316619813E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6192868286542481},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1582317419406758}]
["Single Family Detached",10910,"West North Central","Before 1950","Brick","radiator","window/wall unit",55.438314872634166,14685.64632,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14685.64632},"Cold/Very Cold",140.50709467934527,"Micropolitan Area",2.1775478382280729,0.34380863249807669,6.734824185270312E-2,2.7089143201871999E-3,0.44304718121840336,3.0317518937972556,184.46,0,{"$f":"T911*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7089143201871999E-3},{"$f":"U911*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1802567525482601},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.734824185270312E-2}]
["Single Family Detached",10911,"Pacific","1950s","Siding","central furnace","central AC",32.860597392047666,15536.92548,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15536.92548},"Hot-Dry/Mixed-Dry",270.06694045687186,"Metropolitan Area",0.18685119864465766,0.26203234570513978,0.17692361598147852,2.2186403310004921E-2,0.73124796130890446,1.3570551216401803,855.82100000000003,572.15800000000002,{"$f":"T912*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3296827101219081E-2},{"$f":"U912*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.889576208785839E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20014802574587673},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18581319219026435}]
["Single Family Attached",10912,"Middle Atlantic","1990s","Brick","heat pump","central AC",27.086924209938793,13848.12076,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13848.12076},"Cold/Very Cold",243.70144486420065,"Metropolitan Area",0.35539592778907686,0.10114220108803451,6.3630065370327518E-2,9.54127211491544E-3,0.31134112278522114,0.83150931703265996,467.38200000000001,221.61199999999999,{"$f":"T913*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4723623770503195E-3},{"$f":"U913*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0689097378651196E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3618682901661272},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6698975108192643E-2}]
["Single Family Detached",10913,"East North Central","1960s","Siding","central furnace","central AC",34.145993280349572,22029.67308,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22029.67308},"Cold/Very Cold",221.97475306945373,"Metropolitan Area",1.6786157516288014,0.74995133616403553,5.7729463255678556E-2,3.2147285094797758E-2,0.31927063264886235,2.8055671836973777,1338.6659999999999,120.60599999999999,{"$f":"T914*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9490374343311278E-2},{"$f":"U914*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6569107514864796E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7081061259721126},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0386374007165039E-2}]
["Single Family Detached",10914,"Pacific","1970s","Shingle","heat pump","central AC",31.698221623624484,10937.964669999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10937.964669999999},"Marine",349.76329636253973,"Micropolitan Area",0.48039432544789762,0.33849601134230561,2.0370438820785871E-2,1.364573438981119E-2,0.3541315912028481,1.1933923668138371,1144.547,103.01,{"$f":"T915*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2519014649154489E-2},{"$f":"U915*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1267197406567E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49291334009705212},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1497158561442572E-2}]
["Single Family Attached",10915,"East North Central","1970s","Brick","central furnace","central AC",26.166355917657619,16550.509750000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16550.509750000001},"Cold/Very Cold",73.767243913902547,"Metropolitan Area",0.54255502055776728,0.33530811412442879,3.4002674720670256E-2,9.5656153676587519E-3,0.30852655921176125,1.2203923686146276,484.66800000000001,93.296999999999997,{"$f":"T916*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0215024595130004E-3},{"$f":"U916*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5441129081457498E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55057652301728033},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.554678762881601E-2}]
["Single Family Attached",10916,"South Atlantic","1980s","Siding","central furnace","central AC",62.9675453706163,24908.048009999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24908.048009999999},"Hot-Humid",414.53281171642254,"Metropolitan Area",6.8952127340498659E-2,0.10877095485486898,0.71562423520217033,4.1739885625189585E-2,1.0453013550873442,1.9386486724848822,109.991,1565.768,{"$f":"T917*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7396611086679097E-3},{"$f":"U917*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.900022451652168E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.1691788449166571E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.75462445971869196}]
["Single Family Detached",10917,"Pacific","2000s","Wood","central furnace","N/A",21.567896747206714,10414.242759999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10414.242759999999},"Marine",198.00599751551968,"Metropolitan Area",0.31372107542080307,7.8172805342127352E-2,0,5.6141412297890788E-3,0.28370257261996928,0.67559645338289975,539.08299999999997,0,{"$f":"T918*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6141412297890788E-3},{"$f":"U918*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31933521665059217},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10918,"Pacific","1980s","Wood","central furnace","N/A",4.8107509413444136,6626.3787069999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6626.3787069999998},"Hot-Dry/Mixed-Dry",28.095845718044512,"Metropolitan Area",1.7474025705507278E-2,9.9903016037944034E-2,0,2.7771153161036997E-4,0.11294392812468128,0.23032096986813258,41.91,0,{"$f":"T919*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7771153161036997E-4},{"$f":"U919*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7751737237117649E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10919,"West South Central","1970s","Brick","central furnace","central AC",31.935206856089778,14916.02375,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14916.02375},"Mixed-Humid",442.29587291410689,"Micropolitan Area",1.0460375213385211,7.8968487517368749E-2,0.14977198838205874,2.5818906226086253E-2,0.28932618725886894,1.5641041844968175,1212.8119999999999,518.13900000000001,{"$f":"T920*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8090332596285001E-2},{"$f":"U920*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7285736298012501E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.064127853934806},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15750056201186}]
["Single Family Detached",10920,"East North Central","1950s","Brick","central furnace","central AC",39.888385737472461,38280.60052,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38280.60052},"Cold/Very Cold",101.32794567273426,"Metropolitan Area",2.8623224979267134,0.37608588405931448,6.1514436796606203E-2,2.2552479867950719E-2,0.28179383618986037,3.5817166549724946,521.29399999999998,67.841999999999999,{"$f":"T921*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.995544736747288E-2},{"$f":"U921*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5970325004778397E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8822779452941862},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4111469297084042E-2}]
["Multi-Family (5+ units)",10921,"East North Central","1990s","Siding","central furnace","central AC",18.579294363831853,13463.256789999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1070.8867306910583},"Cold/Very Cold",45.120718400770272,"Metropolitan Area",0.30951770746709578,0.46151920414157532,1.2223724716686235E-2,4.9105344285574398E-3,0.1368631737482239,0.92464375355953332,322.22699999999998,42.509,{"$f":"T922*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4506861857038764E-4},{"$f":"U922*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5522324034946196E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30986277608566615},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.226924704072118E-2}]
["Multi-Family (5+ units)",10922,"Pacific","1960s","Stucco","N/A","central AC",14.260738984008739,20519.048900000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1632.1145422801492},"Hot-Dry/Mixed-Dry",98.979952225860757,"Metropolitan Area",0,0.17306533254688861,4.7373372677975673E-2,2.0017973725862002E-3,0.28850363442483867,0.51078491119177338,0,97.558000000000007,{"$f":"T923*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U923*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5922583051576682E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7532598508491439E-2}]
["Single Family Detached",10923,"East North Central","1970s","Siding","central furnace","central AC",94.955126146660305,23691.398740000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23691.398740000001},"Cold/Very Cold",224.32463870724933,"Metropolitan Area",2.4940287507783281,0.39293205909575696,9.8902729156371244E-2,5.495646382920321E-2,0.75534504786583523,3.7412085868962914,2095.4690000000001,224.21100000000001,{"$f":"T924*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9644591626309062E-2},{"$f":"U924*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3118722028941403E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5436733424046372},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10421460135926539}]
["Multi-Family (5+ units)",10924,"West South Central","1970s","Brick","portable electric heaters","window/wall unit",20.436091526646845,28110.167160000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2235.922962675033},"Hot-Humid",205.4974374349882,"Metropolitan Area",5.2956069268712165E-2,7.3127222468549163E-2,0.31495719149533091,0,0.43017832109962795,0.87121880433222021,0,0,{"$f":"T925*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U925*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.2956069268712165E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31495719149533091}]
["Single Family Detached",10925,"West North Central","Before 1950","Siding","central furnace","N/A",37.271145456642735,12781.59995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12781.59995},"Cold/Very Cold",31.435782688687489,"Metropolitan Area",0.48211938101241009,0.12268448109687384,0,7.8665762868269512E-3,0.13612131698671054,0.74092517909599442,615.46100000000001,0,{"$f":"T926*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8665762868269512E-3},{"$f":"U926*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.48998595729923705},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10926,"South Atlantic","1990s","Stucco","heat pump","central AC",54.278850684065254,22578.556860000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22578.556860000001},"Hot-Humid",470.00325492158697,"Metropolitan Area",0.35099190756195392,0.20944666366393158,0.49933553235196537,3.1448271979768683E-2,0.54387699656206379,1.6036511001399147,209.024,1183.8140000000001,{"$f":"T927*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7194602691046396E-3},{"$f":"U927*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.672881171066404E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35571136783105856},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.52606434406262936}]
["Multi-Family (5+ units)",10927,"East North Central","1990s","Brick","built-in electric unit","window/wall unit",33.290831356842205,22755.182059999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1809.9797770041064},"Cold/Very Cold",259.16675557408212,"Metropolitan Area",0.42186232512238253,0.15627514944354637,4.1879729311962884E-2,0,0.26425977488854813,0.88427697876643996,0,0,{"$f":"T928*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U928*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42186232512238253},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1879729311962884E-2}]
["Single Family Detached",10928,"Pacific","Before 1950","Wood","heat pump","central AC",96.55080423641563,26730.56596,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26730.56596},"Marine",250.83219984245474,"Micropolitan Area",0.16422767883410336,0.14231238375670374,3.9150923433314E-2,8.5442917562841992E-3,0.5101484942643485,0.85583948028846957,231.649,87.995999999999995,{"$f":"T929*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1921088740680402E-3},{"$f":"U929*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3521828822161599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1704197877081714},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1503106315530162E-2}]
["Single Family Detached",10929,"East South Central","2000s","Other","central furnace","central AC",40.853640331141172,20790.656660000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20790.656660000001},"Mixed-Humid",208.13522221260743,"Metropolitan Area",0.74873564392108272,0.58080953086891951,0.22996861349607231,2.8543097506037458E-2,0.46261429431565643,2.0221280826017307,845.30700000000002,527.57399999999996,{"$f":"T930*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7574487609294618E-2},{"$f":"U930*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0968609896742839E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.7663101315303773},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24093722339281515}]
["Multi-Family (5+ units)",10930,"East South Central","2010s","Siding","built-in electric unit","central AC",14.165391003466068,20121.294040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1600.4765509467104},"Mixed-Humid",98.871169554558833,"Metropolitan Area",3.8374325928386001E-2,9.4029100876440549E-2,2.2984212918873231E-2,9.9517908192436021E-4,0.18104474362359282,0.33734840445948366,0,49.459000000000003,{"$f":"T931*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U931*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.9157969733273351E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.8374325928386001E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3063370888606504E-2}]
["Multi-Family (5+ units)",10931,"Mountain South","1970s","Wood","central furnace","N/A",26.137906661994876,29269.772300000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2328.1596166018535},"Hot-Dry/Mixed-Dry",300.52858712900951,"Metropolitan Area",8.8547160111618853E-2,0.25205395134239839,0.26724247523545291,1.6998420263225002E-3,0.50440730318565352,1.113815524031712,58.075000000000003,0,{"$f":"T932*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3520786973415265E-4},{"$f":"U932*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.8682367981353011E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26724247523545291}]
["Single Family Detached",10932,"Pacific","1990s","Stucco","central furnace","N/A",30.064346212076213,13880.1229,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13880.1229},"Marine",90.845404412760303,"Metropolitan Area",0.29204719653932615,0.11271289952379661,0,4.9842549725296996E-3,0.32569312801347355,0.73045322407659641,359.09300000000002,0,{"$f":"T933*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9842549725296996E-3},{"$f":"U933*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29703145151185584},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10933,"Middle Atlantic","1970s","Brick","heat pump","central AC",36.312730319586549,22034.423739999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22034.423739999998},"Cold/Very Cold",465.7256616191442,"Metropolitan Area",0.91637651640631101,0.25489018152477555,8.3936589695307845E-2,1.9975505151310656E-2,0.33385265430174471,1.5890559419281389,729.36,177.19900000000001,{"$f":"T934*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6071027299006398E-2},{"$f":"U934*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9044778523042597E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.93244754370531746},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.7841067547612103E-2}]
["Single Family Detached",10934,"East South Central","1990s","Brick","central furnace","central AC",199.13955593385995,34936.764199999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34936.764199999998},"Mixed-Humid",668.12208409620666,"Metropolitan Area",1.4108948798967931,0.43358306147174197,0.35178771165613398,4.82523179498386E-2,1.2816530285976195,3.4779186816222887,791.11300000000006,590.02,{"$f":"T935*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.76389283365546E-2},{"$f":"U935*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0613389613283999E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4385338082333476},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.372401101269418}]
["Single Family Detached",10935,"West South Central","2000s","Brick","central furnace","central AC",24.935431102084273,12116.341640000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12116.341640000001},"Hot-Humid",158.45751601217594,"Metropolitan Area",0.53224884861975685,0.19210613547758829,0.2767378125256571,2.012432262207536E-2,0.39625568433484532,1.3973484809578476,469.45400000000001,1191.47,{"$f":"T936*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6880650482645607E-3},{"$f":"U936*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.44362575738108E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53793691366802143},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.29117407009946789}]
["Multi-Family (5+ units)",10936,"East North Central","1980s","Brick","radiator","window/wall unit",8.0753359141692247,12423.593709999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":988.19044002917633},"Mixed-Humid",49.279277743250283,"Rural",0.13249417609130351,0.12671964953090947,3.7062449887077013E-2,1.1661530471828599E-3,0.1299123019132864,0.42726197298591551,93.866,0,{"$f":"T937*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.2757483843778661E-5},{"$f":"U937*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13258693357514728},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7062449887077013E-2}]
["Single Family Detached",10937,"West South Central","1980s","Brick","central furnace","central AC",15.314709668024896,14407.0646,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14407.0646},"Hot-Humid",183.97536232188489,"Metropolitan Area",0.14976708408632319,0.14635554881730159,8.9979725357108784E-2,6.5608187411294004E-3,0.24162157194570083,0.62772393020643436,177.02600000000001,278.363,{"$f":"T938*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5504250178796E-3},{"$f":"U938*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0103937232498004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1523175091042028},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.3990119080358578E-2}]
["Single Family Detached",10938,"West North Central","1950s","Shingle","central furnace","central AC",29.695634310943323,13145.477779999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13145.477779999999},"Cold/Very Cold",89.385397296839969,"Micropolitan Area",1.3153962922997433,7.249241983896583E-2,3.737159427222872E-2,1.6380027751591239E-2,0.17542373244211076,1.6006840388530486,1114.2529999999999,131.80500000000001,{"$f":"T939*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4647388052798338E-2},{"$f":"U939*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7326396987928999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3300436803525417},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9104233971021619E-2}]
["Multi-Family (5+ units)",10939,"East North Central","1960s","Brick","built-in electric unit","window/wall unit",17.036427505685687,21215.974480000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1687.5490012333137},"Cold/Very Cold",177.56253695756243,"Metropolitan Area",0.18623740948512713,0.18907143935616552,1.649474124701664E-2,0,0.21403979837854517,0.60584338846685448,0,0,{"$f":"T940*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U940*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18623740948512713},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.649474124701664E-2}]
["Single Family Detached",10940,"South Atlantic","1970s","Brick","heat pump","central AC",52.792941807972149,28322.393670000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28322.393670000001},"Mixed-Humid",760.44015469965848,"Metropolitan Area",0.64429149092130267,0.74349022159217892,0.58851319889324261,3.7605058195342503E-2,0.6183268798795426,2.5946217912862668,313.61399999999998,1014.136,{"$f":"T941*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8822991684233792E-3},{"$f":"U941*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.872275902691912E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.65317379008972609},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.61723595792016173}]
["Single Family Detached",10941,"East North Central","1950s","Brick","central furnace","central AC",76.06024394272724,26236.71747,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26236.71747},"Cold/Very Cold",94.836288432266159,"Micropolitan Area",3.2278844336608041,0.27225466533559178,3.8079840552370653E-2,3.31563893355378E-2,0.25425433563407945,3.792473275182846,1190.973,72.766999999999996,{"$f":"T942*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1247222115398311E-2},{"$f":"U942*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.90916722013949E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2591316557762022},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9989007772510146E-2}]
["Single Family Detached",10942,"West South Central","1970s","Brick","central furnace","central AC",27.300814531909353,21910.766080000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21910.766080000001},"Hot-Humid",166.05847521477114,"Metropolitan Area",9.6796878440604167E-2,8.0089437267750418E-2,0.19732099729907712,1.168233843700224E-2,0.19238419495052797,0.56659150795795965,94.924999999999997,438.25299999999999,{"$f":"T943*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0798794701440003E-3},{"$f":"U943*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6024589668582405E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.8876757910748167E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20692345626593536}]
["Single Family Detached",10943,"Middle Atlantic","1950s","Siding","central furnace","central AC",53.981165741086862,21784.166969999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21784.166969999998},"Mixed-Humid",349.95913505362239,"Metropolitan Area",1.6944210638347759,0.64160767558072385,0.17956832608873002,4.3205997890787988E-2,0.97972367405631544,3.4953207395605452,1596.048,387.31900000000002,{"$f":"T944*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4768576124134552E-2},{"$f":"U944*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4374217666534305E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7291896399589104},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18800574785538346}]
["Multi-Family (5+ units)",10944,"East North Central","1960s","Siding","central furnace","central AC",24.226395882473167,26106.030050000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2076.5110260937859},"Cold/Very Cold",122.64015087413993,"Metropolitan Area",0.41798210028423677,0.52027409538853342,4.7706057328961431E-2,1.7258696466055001E-2,0.35364643252558708,1.3554946005540234,582.62400000000002,78.475999999999999,{"$f":"T945*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2098251600668659E-3},{"$f":"U945*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6295627928373594E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.41919192544430361},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7869013608245164E-2}]
["Single Family Detached",10945,"East North Central","2000s","Siding","central furnace","central AC",79.909515252771797,23648.865119999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23648.865119999999},"Cold/Very Cold",357.83097818576204,"Metropolitan Area",1.5684579110306707,1.0201977100645372,0.12487421398979662,3.424175938001088E-2,1.0680526312156295,3.7815824663006339,1184.6980000000001,263.226,{"$f":"T946*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8016763209933761E-2},{"$f":"U946*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2249961700771199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5964746742406044},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13109921015987375}]
["Single Family Detached",10946,"Mountain South","2000s","Stucco","central furnace","central AC",37.410015592884676,9636.7891789999994,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9636.7891789999994},"Cold/Very Cold",106.79957152444889,"Metropolitan Area",0.78918609662246264,0.11609561347484955,4.8157589276595435E-2,1.425935457559354E-2,0.23818930908654631,1.1916286084604539,1182.8430000000001,296.83600000000001,{"$f":"T947*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1398808622855897E-2},{"$f":"U947*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8605459527376439E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80058490524531856},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.1018135229333079E-2}]
["Single Family Detached",10947,"West South Central","1950s","Siding","built-in electric unit","window/wall unit",39.651102992697112,29327.7389,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29327.7389},"Hot-Humid",363.19363341031834,"Metropolitan Area",0.75460747299070174,0.68065511582428417,0.48385736545004759,1.10872050524505E-2,0.49954189886924577,2.4186618531342794,378.04500000000002,0,{"$f":"T948*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.10872050524505E-2},{"$f":"U948*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.76569467804315228},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.48385736545004759}]
["Multi-Family (5+ units)",10948,"East North Central","1960s","Brick","central furnace","central AC",28.699471487577732,21258.867770000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1690.9607949629558},"Cold/Very Cold",99.613229433778997,"Metropolitan Area",0.41284149101480017,0.20000357679223438,5.8028509824058133E-2,1.454931399537476E-2,0.33039150461728956,1.0146571229672139,559.73199999999997,124.65600000000001,{"$f":"T949*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4648486768620504E-4},{"$f":"U949*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1078840885690222E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.41378797588248639},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8239298232915036E-2}]
["Single Family Attached",10949,"West North Central","1970s","Siding","central furnace","central AC",18.263362670511544,8400.8107959999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8400.8107959999998},"Mixed-Humid",64.119432024009583,"Metropolitan Area",0.46088521468366561,7.4400445085857442E-2,6.7759578949187049E-2,1.3494323191344351E-2,0.14056853243379616,0.74361377115250638,1243.6189999999999,362.69299999999998,{"$f":"T950*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0447407921310723E-2},{"$f":"U950*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0469152700336277E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.47133262260497633},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0806494219220681E-2}]
["Single Family Detached",10950,"East North Central","Before 1950","Wood","built-in electric unit","window/wall unit",78.210125475815644,28585.572179999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28585.572179999999},"Mixed-Humid",421.77537226419253,"Rural",0.84450055742866115,0.36603673672957443,0.12500796589836852,0,0.46958905820336722,1.8051343182599713,0,0,{"$f":"T951*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U951*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84450055742866115},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12500796589836852}]
["Single Family Detached",10951,"East North Central","Before 1950","Siding","central furnace","N/A",76.991260690239912,27744.598450000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27744.598450000001},"Cold/Very Cold",152.52964773820773,"Metropolitan Area",1.2987623860983921,0.61739511136655378,0,3.2139564801267596E-2,0.48829158756814578,2.4044490850330917,1158.4079999999999,0,{"$f":"T952*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2139564801267596E-2},{"$f":"U952*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3309019508996598},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10952,"West North Central","Before 1950","Wood","central furnace","window/wall unit",25.524577675879353,11314.085849999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11314.085849999999},"Cold/Very Cold",73.099957935260875,"Metropolitan Area",0.71208592391321401,0.26313456839125587,3.3186125878558646E-2,2.9073546184770451E-2,0.18715738184898317,1.1955640000320118,2569.6770000000001,0,{"$f":"T953*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9073546184770451E-2},{"$f":"U953*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.74115947009798444},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3186125878558646E-2}]
["Single Family Detached",10953,"East South Central","2000s","Wood","heat pump","central AC",34.055667101955819,22375.602559999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22375.602559999999},"Mixed-Humid",287.91336711190871,"Metropolitan Area",0.16357500771547004,0.23132732536503489,0.13218854862413501,8.9942762098380799E-3,0.45526953835393674,0.98236042005857671,124.26300000000001,277.70499999999998,{"$f":"T954*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7804595009132799E-3},{"$f":"U954*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2138167089247996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16635546721638331},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1384023653330598}]
["Single Family Detached",10954,"West North Central","2000s","Wood","central furnace","central AC",60.809600246425362,19898.429400000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19898.429400000001},"Mixed-Humid",119.46439957312383,"Metropolitan Area",1.368442708350154,0.18291165602702039,0.1156640383388268,2.2877622249768002E-2,0.27506926184860991,1.9420876645646112,848.26900000000001,301.45100000000002,{"$f":"T955*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.68792208087086E-2},{"$f":"U955*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9984014410594004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3853219291588625},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12166243977988619}]
["Single Family Detached",10955,"South Atlantic","2000s","Brick","central furnace","central AC",47.906320718807436,19617.657950000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19617.657950000001},"Mixed-Humid",612.58883427263265,"Metropolitan Area",1.3593069504434194,0.93475073891812421,0.15459212753111931,2.2288837491787904E-2,1.9325750142352696,4.3812248311279323,741.44600000000003,394.71600000000001,{"$f":"T956*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4545434016395702E-2},{"$f":"U956*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7434034753921998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3738523844598152},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16233553100651152}]
["Single Family Detached",10956,"South Atlantic","1980s","Concrete","heat pump","central AC",20.425989315789945,15130.36246,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15130.36246},"Hot-Humid",194.35970361342274,"Metropolitan Area",1.6389496093558741E-2,6.1499052819265522E-2,0.23399128239933689,1.1131695138708741E-2,0.35127545204593635,0.66315528335809759,18.071999999999999,717.64700000000005,{"$f":"T957*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7343591037712003E-4},{"$f":"U957*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0858259228331621E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.666293200393586E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2448495416276685}]
["Single Family Detached",10957,"South Atlantic","1970s","Concrete","heat pump","central AC",40.367563845121971,29465.375069999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29465.375069999998},"Hot-Humid",334.67565622450348,"Metropolitan Area",5.9236630198601668E-2,0.16730531307408716,0.34870674372016208,1.8059505172653423E-2,0.56666462766983305,1.1419133146626839,33.932000000000002,578.97400000000005,{"$f":"T958*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9981910687524009E-4},{"$f":"U958*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7059686065778183E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.0236449305476905E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36576642978594026}]
["Single Family Detached",10958,"West South Central","1950s","Brick","central furnace","central AC",34.435767373090734,33367.99164,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33367.99164},"Hot-Humid",525.37902838111791,"Metropolitan Area",0.4252349784938404,0.52918217858696071,0.47159082688786924,2.7699170276263681E-2,0.36662063090704966,1.79262861487572,204.43299999999999,625.67899999999997,{"$f":"T959*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8215186349401191E-3},{"$f":"U959*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0877651641323557E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43205649712878053},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.49246847852919279}]
["Single Family Detached",10959,"East North Central","1990s","Siding","central furnace","central AC",53.659740165752055,19385.744279999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19385.744279999999},"Cold/Very Cold",136.62884526496546,"Metropolitan Area",0.83984400502104561,0.30047064231272674,9.0682653978728253E-2,5.0029526921678641E-2,0.40987680416110611,1.6408741054736067,2335.2750000000001,245.46299999999999,{"$f":"T960*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5271043973476997E-2},{"$f":"U960*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7584829482016392E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88511504899452265},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.544113692692989E-2}]
["Multi-Family (5+ units)",10960,"West South Central","1980s","Brick","central furnace","N/A",17.313437274492081,32852.82215,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2613.160534256458},"Hot-Humid",327.03512646616645,"Metropolitan Area",0.23085199306627324,0.23164823858646566,0,3.4980370912433998E-3,0.65012377476426264,1.1158438046271995,106.476,0,{"$f":"T961*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7823888104549062E-4},{"$f":"U961*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23113023194731874},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10961,"East North Central","2000s","Siding","central furnace","central AC",87.156039471112024,28519.646420000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28519.646420000001},"Cold/Very Cold",284.2658111358308,"Metropolitan Area",0.95157756728074416,0.43700551538638888,9.4982686026560598E-2,6.5059987081282286E-2,0.95420585233587218,2.4377716210295657,2134.42,146.81399999999999,{"$f":"T962*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0872903711776408E-2},{"$f":"U962*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1870833695058802E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0124504709925206},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.9169769396066476E-2}]
["Single Family Detached",10962,"Mountain North","1980s","Siding","central furnace","central AC",35.622646535457491,11237.42793,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11237.42793},"Cold/Very Cold",157.83794601209797,"Metropolitan Area",0.42862240365266435,0.31073489612364336,6.3034857395420307E-2,1.5220298273801971E-2,0.38741291249517379,1.1898050696669018,1073.694,280.73500000000001,{"$f":"T963*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2065558943873419E-2},{"$f":"U963*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1547393299285499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44068796259653775},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6189596725348854E-2}]
["Single Family Detached",10963,"West North Central","Before 1950","Brick","central furnace","central AC",36.381638044967559,24046.026470000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24046.026470000001},"Mixed-Humid",203.57923874998136,"Metropolitan Area",1.4131191135753989,0.51166419180679501,0.15195756579173561,2.300856065795185E-2,0.56173708426931401,2.6384779554432436,660.399,296.45600000000002,{"$f":"T964*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.587997183476153E-2},{"$f":"U964*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1285888231903205E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4289990854101604},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15908615461492592}]
["Single Family Detached",10964,"South Atlantic","1990s","Brick","central furnace","central AC",107.03041486072524,13269.329890000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13269.329890000001},"Mixed-Humid",480.3895498639767,"Metropolitan Area",0.81283183063101228,0.12053292671689698,0.24784936045217007,4.4447955868615642E-2,0.45786658753228071,1.6390807053323599,1651.4179999999999,1698.258,{"$f":"T965*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1913210228284019E-2},{"$f":"U965*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2534745640331623E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83474504085929624},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27038410609250169}]
["Single Family Detached",10965,"East South Central","Before 1950","Wood","central furnace","window/wall unit",26.673056698329681,14599.37422,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14599.37422},"Mixed-Humid",108.63369537509978,"Metropolitan Area",1.155632649961825,0.17782164814515714,7.3172209584382211E-2,5.1228912150495598E-3,0.22371410943451309,1.6303406171258774,350.89800000000002,0,{"$f":"T966*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1228912150495598E-3},{"$f":"U966*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1607555411768746},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.3172209584382211E-2}]
["Multi-Family (5+ units)",10966,"West South Central","1990s","Brick","built-in electric unit","central AC",43.442253807151857,37514.899660000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2983.9888576544413},"Hot-Humid",130.3365903251667,"Metropolitan Area",1.8055996236157321E-2,5.7063763813227364E-2,2.0265231501488654E-2,1.40857193753402E-3,0.34802692462260915,0.44470844828137818,0,37.546999999999997,{"$f":"T967*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U967*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1203982963835129E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8055996236157321E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0377271331127007E-2}]
["Single Family Detached",10967,"West North Central","2000s","Siding","central furnace","central AC",47.426993175503149,14424.268,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14424.268},"Cold/Very Cold",196.7181669487567,"Metropolitan Area",0.70183736734120805,0.41688808779287201,3.4837852680299999E-2,3.3141991491540006E-2,0.60513292048002409,1.7586962282944041,2165.2130000000002,132.44200000000001,{"$f":"T968*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1231612589084003E-2},{"$f":"U968*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9103789024560002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.73306897993029208},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6748231582756002E-2}]
["Mobile Home",10968,"South Atlantic","1980s","Siding","built-in electric unit","central AC",88.633743887388491,36206.594729999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":36206.594729999997},"Mixed-Humid",937.94925172941544,"Metropolitan Area",0.8061284989992995,0.82196106356921284,0.32129141995907901,1.4527063383733708E-2,1.2509018947729322,3.2002828773005239,0,401.22699999999998,{"$f":"T969*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U969*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4527063383733708E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.8061284989992995},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.33581848334281272}]
["Single Family Detached",10969,"West South Central","1980s","Brick","central furnace","central AC",25.375670737765162,20203.559499999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20203.559499999999},"Hot-Humid",294.15942201085983,"Metropolitan Area",0.34474553869843799,0.236111241709652,0.13161879563972301,1.1785887859241499E-2,0.29119636790775905,1.0036719439555719,286.536,296.82100000000003,{"$f":"T970*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7890471248919998E-3},{"$f":"U970*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9968407343495003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35053458582332997},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13761563637407251}]
["Single Family Detached",10970,"West North Central","1990s","Wood","heat pump","central AC",87.691766676595506,27403.677090000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27403.677090000001},"Cold/Very Cold",436.33518542716422,"Metropolitan Area",1.0072444580361013,0.40951992014838695,0.11445321120171877,2.5403701928617621E-2,0.94577428342314673,2.4769918728093536,694.36900000000003,232.649,{"$f":"T971*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9028263857306212E-2},{"$f":"U971*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3754380713114105E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0262727218934076},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12082864927303018}]
["Multi-Family (5+ units)",10971,"East North Central","1990s","Siding","central furnace","central AC",24.078287546074328,21750.937259999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1730.1007070687929},"Cold/Very Cold",111.30317836249552,"Metropolitan Area",0.37001856200980576,7.1010263121784725E-2,1.5071915261670009E-2,4.8301218826418994E-3,0.28890799870656203,0.74945466616894929,190.92699999999999,31.138000000000002,{"$f":"T972*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.303229376985234E-4},{"$f":"U972*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3871875816708077E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37034888494750429},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5125787137486716E-2}]
["Multi-Family (5+ units)",10972,"South Atlantic","1980s","Brick","radiator","central AC",17.432887967769766,32403.137490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2577.391972243513},"Mixed-Humid",148.17954772604298,"Metropolitan Area",0.15420591970927933,0.42616062054138171,5.767087606666952E-2,4.3296100220013307E-3,0.44377720189743247,1.085799844853609,59.304000000000002,74.313000000000002,{"$f":"T973*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5284965352192932E-4},{"$f":"U973*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9153372963333221E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15435876936280127},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7862409796302854E-2}]
["Multi-Family (5+ units)",10973,"New England","1960s","Wood","central furnace","window/wall unit",45.290077481447796,59513.899449999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4733.8208136997791},"Cold/Very Cold",328.33818326563397,"Metropolitan Area",0.49317555864620105,0.79857482136483993,5.1438101350232794E-2,8.5401255432761003E-3,0.56781515152621431,1.91886446461164,143.49799999999999,0,{"$f":"T974*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7929381912429083E-4},{"$f":"U974*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49385485246532534},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.1438101350232794E-2}]
["Single Family Detached",10974,"Middle Atlantic","Before 1950","Siding","wood-burning stove","window/wall unit",74.488536613918171,23639.649829999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23639.649829999998},"Cold/Very Cold",207.63593296407811,"Metropolitan Area",1.9877316111591601,0.97021815372811249,4.1214216541015876E-2,6.3756915699954383E-2,0.60348269675631949,3.602646678184608,2697.0329999999999,0,{"$f":"T975*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3756915699954383E-2},{"$f":"U975*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0514885268591145},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1214216541015876E-2}]
["Single Family Detached",10975,"West South Central","1970s","Brick","central furnace","central AC",60.18257140541786,23591.756720000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23591.756720000001},"Hot-Humid",410.39748163636528,"Metropolitan Area",0.18979690958374945,0.19191478876801729,0.35148509033886077,2.2941214028446E-2,0.72241016568310912,1.4556069543737367,136.202,836.22299999999996,{"$f":"T976*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2132444487774402E-3},{"$f":"U976*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9727969579668558E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19301015403252689},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37121305991852932}]
["Single Family Detached",10976,"West North Central","2000s","Siding","central furnace","central AC",242.48290589282195,33422.8678,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33422.8678},"Mixed-Humid",591.33071285117262,"Metropolitan Area",3.5994063952703148,0.72625398383462114,0.4403309421686798,0.1395526055660114,1.4706422798972234,6.2366336011708396,3190.846,984.51700000000005,{"$f":"T977*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.10664722402815879},{"$f":"U977*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.29053815378526E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.7060536192984737},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4732363237065324}]
["Single Family Detached",10977,"South Atlantic","2000s","Siding","built-in electric unit","central AC",41.769825665060935,15266.74915,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15266.74915},"Mixed-Humid",406.52033986095648,"Micropolitan Area",0.7880145086920668,0.16420165788356733,0.19202865162750621,1.059037595111435E-2,0.57423518214981317,1.7184800003529537,0,693.68899999999996,{"$f":"T978*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U978*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.059037595111435E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.7880145086920668},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20261902757862055}]
["Single Family Detached",10978,"New England","1980s","Siding","central furnace","central AC",53.954183301802217,17117.443940000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17117.443940000001},"Cold/Very Cold",163.26383521874277,"Micropolitan Area",1.3851096710857989,0.13241298040961852,3.3769926750257785E-2,2.6314304220083198E-2,0.36627634375453327,1.9175689220002086,1436.951,100.32899999999999,{"$f":"T979*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.459692818702694E-2},{"$f":"U979*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.71737603305626E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4097065992728257},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5487302783314044E-2}]
["Mobile Home",10979,"New England","1980s","Siding","central furnace","N/A",23.777674242088782,20640.342219999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20640.342219999999},"Cold/Very Cold",147.96795079996286,"Micropolitan Area",1.1395985375963462,0.42706521344591819,0,6.5649085271776405E-3,0.49830174255835985,2.0649654936006239,318.06200000000001,0,{"$f":"T980*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5649085271776405E-3},{"$f":"U980*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1461634461235239},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",10980,"Mountain South","2000s","Stucco","central furnace","central AC",32.30153532390662,15990.85907,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1271.9358367384864},"Hot-Dry/Mixed-Dry",150.69785588737426,"Metropolitan Area",6.2825527688607496E-2,0.12607492319852609,6.9198344883913368E-2,4.8793707823244501E-3,0.25158002812495178,0.51417008253677998,72.968999999999994,232.166,{"$f":"T981*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.28118860709706E-5},{"$f":"U981*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9530025547222743E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.2918339574678461E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9493645139385593E-2}]
["Single Family Detached",10981,"West South Central","1970s","Brick","central furnace","central AC",53.94348323256758,34402.731650000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34402.731650000002},"Hot-Humid",248.26923952990111,"Micropolitan Area",1.4062709665031148,0.45553764745724129,0.11953824279050045,1.4961988813706551E-2,0.71937780412635022,2.7007246608772069,237.73099999999999,197.17599999999999,{"$f":"T982*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1785957978861498E-3},{"$f":"U982*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7833930158204001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4144495623010009},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12632163580632086}]
["Single Family Detached",10982,"East North Central","Before 1950","Brick","central furnace","N/A",73.496892863635125,22939.10514,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22939.10514},"Cold/Very Cold",60.857445932342074,"Metropolitan Area",1.1098859383630217,0.33672943260397353,0,1.8944581127340963E-2,0.29305232121857688,1.7396676921855725,825.86400000000003,0,{"$f":"T983*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8944581127340963E-2},{"$f":"U983*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1288305194903627},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",10983,"Middle Atlantic","1990s","Siding","central furnace","central AC",36.907963864374103,17401.2088,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17401.2088},"Cold/Very Cold",190.8228389807964,"Metropolitan Area",0.68991665325272644,0.1659852236023184,5.4838430430452001E-2,1.6227914895451202E-2,0.64064821054948418,1.5513885178349809,789.44600000000003,143.12799999999999,{"$f":"T984*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3737314682324801E-2},{"$f":"U984*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4906002131264001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.70365396793505119},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7329030643578402E-2}]
["Single Family Detached",10984,"West South Central","1950s","Stone","portable electric heaters","window/wall unit",41.148090357614144,33183.94384,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33183.94384},"Hot-Humid",708.60993669071968,"Metropolitan Area",0.4482801385855365,0.31140413528839506,0.67946965557992711,0,0.97859503478470156,2.4177489642385601,0,0,{"$f":"T985*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U985*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4482801385855365},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.67946965557992711}]
["Single Family Attached",10985,"Pacific","1950s","Wood","N/A","N/A",7.7383708849363879,14739.754070000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14739.754070000001},"Hot-Dry/Mixed-Dry",22.156665655044598,"Metropolitan Area",0,0.20850887060905549,0,0,9.2312868777299495E-2,0.30082173938635498,0,0,{"$f":"T986*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U986*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10986,"East South Central","1980s","Brick","heat pump","central AC",18.68503873667693,13020.932919999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13020.932919999999},"Mixed-Humid",146.0431481893053,"Metropolitan Area",0.16144790145210366,7.7252543967713999E-2,8.8529713551067604E-2,6.8220183219768393E-3,0.17106904274482584,0.49829920171571113,212.768,311.15899999999999,{"$f":"T987*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7704378555225601E-3},{"$f":"U987*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0515804664542797E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16421833930762622},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2581294017521881E-2}]
["Single Family Detached",10987,"South Atlantic","1980s","Brick","central furnace","central AC",17.677140067959265,13951.965330000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13951.965330000001},"Mixed-Humid",102.83280696318312,"Metropolitan Area",0.20030436202876031,0.18064520576087051,0.10737676677361276,8.7977326340340899E-3,0.23954627360239286,0.72787260816563637,282.57799999999997,347.995,{"$f":"T988*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9425184590207397E-3},{"$f":"U988*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8552141750133502E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20424688048778106},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1122319809486261}]
["Multi-Family (5+ units)",10988,"West South Central","1990s","Brick","central furnace","central AC",30.045997134356742,28697.227439999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2282.6185782882426},"Hot-Humid",67.830804290890271,"Metropolitan Area",2.2691934227959204E-2,6.6437812163167201E-2,3.2000016662163559E-2,1.86236396917368E-3,0.1085946993087583,0.23143869123334679,13.000999999999999,51.896000000000001,{"$f":"T989*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9676324136325441E-5},{"$f":"U989*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1845877373884663E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2721610552095529E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2118475435902405E-2}]
["Single Family Detached",10989,"Mountain North","1970s","Siding","central furnace","central AC",104.29746240728062,36724.458590000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":36724.458590000002},"Cold/Very Cold",327.71614148443837,"Metropolitan Area",2.9109519808916398,0.6132137718514914,0.13538023620808701,6.2093530961679057E-2,0.55304074645177648,4.2125867354029944,1492.72,198.07499999999999,{"$f":"T990*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4819333826464804E-2},{"$f":"U990*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.27419713521425E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9657713147181046},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14265443334330125}]
["Single Family Detached",10990,"Mountain South","1980s","Stucco","heat pump","central AC",20.328465610047569,11860.248310000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11860.248310000001},"Hot-Dry/Mixed-Dry",103.39972034415194,"Metropolitan Area",4.2806328427156377E-2,4.5494228361899987E-2,0.1018730217065778,5.8009186099108609E-3,0.16262626601617788,0.35279984451181201,61.000999999999998,428.10500000000002,{"$f":"T991*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.2348700715831006E-4},{"$f":"U991*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0774316027525504E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.3529815434314688E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10695045330933035}]
["Multi-Family (5+ units)",10991,"Pacific","2010s","Siding","built-in electric unit","window/wall unit",7.514169271055902,13966.857379999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1110.9438430087673},"Marine",77.803440522828069,"Metropolitan Area",3.0673341768801762E-2,9.9451035908004762E-2,4.0948870478126793E-3,0,0.1312460559929943,0.26546532071761353,0,0,{"$f":"T992*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U992*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0673341768801762E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.0948870478126793E-3}]
["Multi-Family (5+ units)",10992,"Pacific","1970s","Stucco","central furnace","central AC",12.524451223926704,11152.67251,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":887.09954723384135},"Hot-Dry/Mixed-Dry",43.456711846051554,"Metropolitan Area",6.3787290089255058E-2,0.25568295799457713,2.6407655621111321E-2,2.7594276904417299E-3,0.13253423362001132,0.48095207618412134,140.19499999999999,107.22799999999999,{"$f":"T993*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2436692102444838E-4},{"$f":"U993*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5121910250790324E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.391165701027951E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6502777531362112E-2}]
["Single Family Detached",10993,"West South Central","1960s","Brick","heat pump","central AC",35.438917051603831,17934.674620000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17934.674620000002},"Hot-Humid",278.31896115518282,"Rural",0.19116903262405932,0.15062926096224127,0.49266567322347166,2.4274886987638543E-2,0.26578958223004867,1.1002535490398209,168.72900000000001,1184.788,{"$f":"T994*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0260997139579808E-3},{"$f":"U994*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1248787273680559E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1941951323380173},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.51391446049715217}]
["Single Family Detached",10994,"Middle Atlantic","2000s","Siding","central furnace","central AC",58.862091399822631,11396.339089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11396.339089999999},"Mixed-Humid",257.57320691226715,"Metropolitan Area",1.1211086583702849,0.33949481037569018,7.3680078734570678E-2,3.5575701017793011E-2,0.91767942428547122,2.451962971766017,2742.8049999999998,378.87299999999999,{"$f":"T995*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1257935837747448E-2},{"$f":"U995*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.317765180045569E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1523665942080323},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.7997843914616241E-2}]
["Single Family Detached",10995,"Middle Atlantic","1970s","Siding","central furnace","central AC",19.471926118516929,19869.31237,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19869.31237},"Mixed-Humid",79.688579469657412,"Metropolitan Area",1.6187359898683855,0.34709214980999936,4.9269933883888999E-2,1.3435410462157932E-2,0.21139738320556642,2.2264954567678403,565.20000000000005,110.989,{"$f":"T996*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1230135351524001E-2},{"$f":"U996*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.20527511063393E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6299661252199096},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.1475208994522931E-2}]
["Single Family Detached",10996,"Mountain South","1970s","Other","heater burning gas/oil/kerosene","N/A",89.110916745091956,12661.397660000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12661.397660000001},"Cold/Very Cold",89.55153338372925,"Metropolitan Area",1.0871820267830454,0.37209207821327894,0,0,0.36841717084945202,1.8276912758457766,0,0,{"$f":"T997*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U997*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0871820267830454},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",10997,"South Atlantic","1990s","Siding","central furnace","central AC",121.12036867997068,17838.051350000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17838.051350000002},"Mixed-Humid",232.56883888858761,"Metropolitan Area",0.94699014470737819,0.24432101088143704,0.31750035004316612,5.5307163619496606E-2,0.46039992696298693,1.9692114325949681,1914.655,1185.8610000000001,{"$f":"T998*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4153714207534255E-2},{"$f":"U998*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1153449411962354E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.9811438589149124},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.33865379945512847}]
["Single Family Detached",10998,"West South Central","1980s","Brick","built-in electric unit","central AC",23.81232389590884,19843.60325,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19843.60325},"Hot-Humid",400.21140601696004,"Metropolitan Area",0.31457266519374355,0.37815627294071374,0.16855134772586428,7.6050609455625001E-3,0.50424101987736669,1.3655213057376883,0,383.25,{"$f":"T999*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U999*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6050609455625001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31457266519374355},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17615640867142679}]
["Mobile Home",10999,"East South Central","1990s","Siding","central furnace","both central and individual units",59.696101965626276,32303.085480000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32303.085480000002},"Hot-Humid",717.83186502224191,"Rural",1.1543507596278001E-2,0.15694143970837393,0.38130494264112491,2.4381399827739601E-2,1.8994524694891461,2.4492423594349231,357.35,397.42,{"$f":"T1000*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1543507596278001E-2},{"$f":"U1000*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2837892231461602E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3087015192556001E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3941428348725865}]
["Multi-Family (2-4 units)",11001,"East North Central","1960s","Brick","central furnace","window/wall unit",20.085375572667193,22593.22337,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7531.0744566666663},"Cold/Very Cold",117.91570464740433,"Metropolitan Area",0.72990079368894789,0.41468160225915235,2.3213181419272803E-2,7.6309289728876094E-3,0.32557655010178327,1.4984594134510814,337.75299999999999,0,{"$f":"T1002*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5436429909625365E-3},{"$f":"U1002*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.73244443667991044},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3213181419272803E-2}]
["Single Family Detached",11006,"New England","1980s","Wood","central furnace","central AC",35.824111081486116,18324.353490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18324.353490000001},"Cold/Very Cold",138.89859948729656,"Metropolitan Area",2.1764540127682364,0.38846456640176641,9.4661814342697992E-2,2.9297086305932942E-2,0.35445018680384255,3.0140305803165437,1353.9359999999999,244.87,{"$f":"T1007*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4810001866836642E-2},{"$f":"U1007*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4870844390963007E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2012640146350728},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.9148898781794295E-2}]
["Single Family Attached",11009,"Pacific","1980s","Wood","heat pump","central AC",6.3790481800255936,10423.28134,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10423.28134},"Hot-Dry/Mixed-Dry",124.25732314949843,"Metropolitan Area",3.0312715787673156E-2,0.18676535568512867,1.5765932233162461E-2,1.11538491291206E-3,0.19112199543337105,0.42396599913933536,45.195,61.814,{"$f":"T1010*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7108020016129994E-4},{"$f":"U1010*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4430471275076005E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0783795987834456E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6410236945913221E-2}]
["Single Family Detached",11013,"West North Central","1970s","Brick","central furnace","N/A",10.784801421050249,11522.223739999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11522.223739999999},"Cold/Very Cold",92.462043183183013,"Micropolitan Area",0.24186085539272431,0.20343571406446304,0,1.1268538939916419E-2,8.6168811972905157E-2,0.53146538143009248,977.98299999999995,0,{"$f":"T1014*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1268538939916419E-2},{"$f":"U1014*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25312939433264076},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11019,"Pacific","1970s","Stucco","central furnace","central AC",30.698149150646724,9569.2484879999993,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9569.2484879999993},"Hot-Dry/Mixed-Dry",115.61374638662205,"Metropolitan Area",0.10480780649672322,0.14882782320579038,9.3109227973670453E-2,7.1906012528408633E-3,0.32195742279425099,0.66870228047043501,179.31399999999999,572.11400000000003,{"$f":"T1020*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7159002233772317E-3},{"$f":"U1020*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4747010294636323E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10652370672010045},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.8583929003134091E-2}]
["Single Family Attached",11024,"South Atlantic","1980s","Wood","heat pump","central AC",15.948392310565785,13424.57265,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13424.57265},"Hot-Humid",349.44249872855852,"Metropolitan Area",3.5681091098999099E-2,0.27708637454429075,0.2942593026713331,1.36340228324853E-2,0.6175961894288482,1.2246229577434711,43.429000000000002,972.173,{"$f":"T1025*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8301576561684996E-4},{"$f":"U1025*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.305100706686845E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.6264106864615946E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30731030973820156}]
["Single Family Detached",11029,"Pacific","1960s","Shingle","built-in electric unit","window/wall unit",53.69013544466614,32149.7817,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32149.7817},"Marine",769.67882679059755,"Metropolitan Area",1.3744725790536902,0.223276375932696,3.7125796312399199E-2,0,1.3702521164610226,3.0051268677598082,0,0,{"$f":"T1030*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1030*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3744725790536902},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7125796312399199E-2}]
["Single Family Detached",11031,"South Atlantic","2010s","Brick","central furnace","central AC",28.52216915610693,7488.0990169999995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7488.0990169999995},"Mixed-Humid",168.82778118993249,"Metropolitan Area",0.15870966710549264,8.502344057415008E-2,8.0297499105847936E-2,6.9244248753963077E-3,0.252009785892222,0.57604039267771268,245.994,678.73,{"$f":"T1032*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8420274295878978E-3},{"$f":"U1032*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0823974458084099E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16055169453508053},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5379896551656342E-2}]
["Single Family Detached",11036,"Mountain North","2000s","Wood","central furnace","N/A",30.640369523898922,12521.60585,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12521.60585},"Cold/Very Cold",293.32266160060828,"Metropolitan Area",0.58851016578911952,0.14686061837537545,0,1.1539110568585599E-2,0.26544612345123086,1.0008169076157258,921.53599999999994,0,{"$f":"T1037*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1539110568585599E-2},{"$f":"U1037*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60004927635770511},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",11043,"West South Central","2000s","Siding","heat pump","central AC",119.49891402988807,53347.729480000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":53347.729480000002},"Mixed-Humid",975.11300565441832,"Rural",2.0944093999906892,0.74657896133075941,0.52019018920933435,3.8169073445161961E-2,3.4062255866946125,6.7674041372253955,291.18799999999999,424.28899999999999,{"$f":"T1044*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5534218651822239E-2},{"$f":"U1044*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2634854793339723E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1099436186425113},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.54282504400267406}]
["Single Family Detached",11047,"Pacific","1990s","Siding","built-in electric unit","window/wall unit",52.824669063664082,22010.278780000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22010.278780000001},"Marine",368.07126688594423,"Micropolitan Area",0.76970499552685256,0.23774136299843765,1.0513539813448701E-2,0,0.39215365939921282,1.4101135577379518,0,0,{"$f":"T1048*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1048*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.76970499552685256},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0513539813448701E-2}]
["Single Family Detached",11048,"New England","Before 1950","Siding","heater burning gas/oil/kerosene","window/wall unit",28.526056674048412,11777.89293,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11777.89293},"Cold/Very Cold",36.576376047845073,"Micropolitan Area",1.0833234542982846,0.20704814963892684,2.0305370080750319E-2,0,0.21449177797068691,1.5251687519886483,0,0,{"$f":"T1049*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1049*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0833234542982846},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0305370080750319E-2}]
["Single Family Detached",11054,"East South Central","Before 1950","Brick","central furnace","both central and individual units",34.467425778831092,12434.136280000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12434.136280000001},"Mixed-Humid",154.78213035730153,"Metropolitan Area",0.9734613051280212,0.19040019861475602,0.26615749908414038,3.7911283625359046E-2,0.29369276953483775,1.7237117723617554,2455.2800000000002,593.68799999999999,{"$f":"T1055*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0529286125558403E-2},{"$f":"U1055*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3819974998006405E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0039905912535796},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.273539496583941}]
["Single Family Detached",11057,"Mountain South","2010s","Stucco","central furnace","central AC",27.520455082378497,15357.39681,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15357.39681},"Cold/Very Cold",269.21604143975151,"Metropolitan Area",0.34071281694958711,0.28666427104961562,1.7709259272277022E-2,7.3504954777734895E-3,0.27347877872607301,0.9185651259975528,423.79399999999998,54.835000000000001,{"$f":"T1058*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5083726236971401E-3},{"$f":"U1058*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4212285407634995E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34722118957328424},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.855138212635337E-2}]
["Single Family Detached",11065,"West South Central","1990s","Brick","central furnace","central AC",28.149758270133557,12107.422909999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12107.422909999999},"Mixed-Humid",162.36054124838321,"Metropolitan Area",0.64527557690926718,0.28742553431073387,0.18465821294757023,2.298178954857687E-2,0.4289425658379688,1.5463018900055401,1115.5060000000001,782.65099999999995,{"$f":"T1066*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.350590290064246E-2},{"$f":"U1066*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4758866479344086E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.65878147980990964},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19413409959550465}]
["Single Family Detached",11066,"South Atlantic","Before 1950","Shingle","built-in electric unit","central AC",20.682479562240989,17587.142479999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17587.142479999999},"Hot-Humid",242.40367280507255,"Metropolitan Area",0.17222079128685644,0.17834336802413392,0.1620731507730363,7.3804971031594399E-3,0.31444402024127344,0.82708133032530007,0,419.65300000000002,{"$f":"T1067*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1067*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3804971031594399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17222079128685644},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16945364787619574}]
["Single Family Detached",11072,"East South Central","2010s","Wood","central furnace","central AC",39.783382549288177,23401.989730000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23401.989730000001},"Hot-Humid",198.98711871564552,"Rural",0.5987633326337698,0.1785742650924029,0.23088370304832379,1.5249930009544234E-2,0.25585011579177425,1.2640714165662708,174.404,477.24700000000001,{"$f":"T1073*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0814006168709204E-3},{"$f":"U1073*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1168529392673312E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6028447332506407},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24205223244099711}]
["Single Family Detached",11077,"Mountain South","Before 1950","Wood","portable electric heaters","window/wall unit",41.148527007408035,25526.381519999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25526.381519999999},"Hot-Dry/Mixed-Dry",390.45834724691338,"Metropolitan Area",0.30451844887296819,0.3524724878811108,0.19834769337761904,0,0.47690522513797223,1.3322438552696703,0,0,{"$f":"T1078*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1078*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30451844887296819},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19834769337761904}]
["Mobile Home",11081,"South Atlantic","1980s","Wood","portable electric heaters","window/wall unit",16.414858006189441,12213.436019999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12213.436019999999},"Hot-Humid",206.37939303300558,"Rural",9.2979129685473116E-2,0.36140162969606593,0.1259103271471233,0,0.50655344363279375,1.0868445301614562,0,0,{"$f":"T1082*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1082*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.2979129685473116E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1259103271471233}]
["Single Family Detached",11084,"East North Central","1960s","Brick","central furnace","central AC",25.878127093483869,15740.953219999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15740.953219999999},"Cold/Very Cold",101.44570547521192,"Metropolitan Area",0.80136799319189489,0.34233148022079324,0.10413046671623076,4.2538603836979515E-2,0.2780707387230909,1.52590067885201,2399.7109999999998,302.70499999999998,{"$f":"T1085*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7773738592519417E-2},{"$f":"U1085*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7648652444600998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83914173178441431},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10889533196069086}]
["Single Family Detached",11091,"East North Central","2000s","Brick","central furnace","central AC",62.827594392648713,20438.38464,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20438.38464},"Cold/Very Cold",119.50323500774789,"Metropolitan Area",2.0500223016566781,0.37183808655360001,6.5362281092874244E-2,3.2936129833205763E-2,0.61306557535420414,3.1002882446573565,1435.374,176.11,{"$f":"T1092*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9336725914255363E-2},{"$f":"U1092*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5994039189504003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0793590275709333},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.8961685011824647E-2}]
["Single Family Detached",11095,"South Atlantic","1970s","Siding","heat pump","N/A",37.796261782695517,18527.579310000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18527.579310000001},"Mixed-Humid",520.0416561704792,"Rural",0.38046247008998108,0.45421891056516012,0,7.1123856731021094E-3,0.97509997737738274,1.8097813580325239,383.88099999999997,0,{"$f":"T1096*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1123856731021094E-3},{"$f":"U1096*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3875748557630832},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11101,"West South Central","2000s","Brick","central furnace","central AC",37.250775932723144,18851.607250000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18851.607250000001},"Hot-Humid",367.49315639139735,"Metropolitan Area",0.41590127485359069,0.23141710870579177,0.60108082023802056,3.987610730645675E-2,0.69878280006170135,1.9471820038591043,531.12199999999996,1584.1410000000001,{"$f":"T1102*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0012503345834499E-2},{"$f":"U1102*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9863603960622254E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42591377819942516},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.63094442419864283}]
["Single Family Detached",11102,"New England","1970s","Siding","central furnace","N/A",57.641526666207326,16620.97078,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16620.97078},"Cold/Very Cold",123.66002260570431,"Metropolitan Area",1.6668747926716818,0.27749820998058106,0,5.9038618984923685E-2,0.36290134523615647,2.307274347888419,3552.056,0,{"$f":"T1103*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9038618984923685E-2},{"$f":"U1103*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7259134116566055},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11107,"West South Central","1980s","Brick","central furnace","central AC",34.22173158573851,21150.637569999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21150.637569999999},"Hot-Humid",310.033300146903,"Metropolitan Area",0.11228987699355877,0.12666067769049527,0.30678346240584087,1.7311775700407431E-2,0.51209957525504113,1.057833592344936,92.003,726.49599999999998,{"$f":"T1108*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9459221083527097E-3},{"$f":"U1108*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5365853592054718E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11423579910191148},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32214931599789559}]
["Single Family Detached",11110,"Pacific","Before 1950","Siding","built-in electric unit","window/wall unit",29.45664636244781,14460.798409999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14460.798409999999},"Marine",245.36696639834838,"Metropolitan Area",0.5040415548162035,8.834483513747024E-2,2.1067127398818039E-2,0,0.22373858648099756,0.83719210383348941,0,0,{"$f":"T1111*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1111*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5040415548162035},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1067127398818039E-2}]
["Mobile Home",11118,"East South Central","1990s","Siding","central furnace","window/wall unit",5.9958259206116882,14275.776,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14275.776},"Hot-Humid",123.6270781105323,"Rural",0.11723764048204799,9.5072399702975999E-2,5.9377477804991995E-2,1.2604796419200001E-3,0.150128071909056,0.42181558989907197,88.295000000000002,0,{"$f":"T1119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2604796419200001E-3},{"$f":"U1119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11849812012396799},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9377477804991995E-2}]
["Single Family Detached",11120,"West North Central","2010s","Concrete","central furnace","central AC",125.44534088452855,21337.87054,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21337.87054},"Cold/Very Cold",474.43400183297001,"Metropolitan Area",0.79315796620592205,0.36269687720268257,0.10014413161481932,2.7419334346864315E-2,0.52865799056619001,1.7846569655896136,949.53599999999994,335.47199999999998,{"$f":"T1121*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0261076241069438E-2},{"$f":"U1121*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1582581057948796E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.81341904244699148},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10730238972061419}]
["Single Family Detached",11125,"South Atlantic","2000s","Stucco","built-in electric unit","central AC",64.732499281928995,22793.133549999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22793.133549999999},"Hot-Humid",436.32150219250053,"Metropolitan Area",0.13872445834421843,0.32411954432394458,0.36851172474352717,2.1703849697645501E-2,0.65737323177984974,1.48872895919154,0,952.21,{"$f":"T1126*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1126*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1703849697645501E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13872445834421843},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.39021557444117266}]
["Multi-Family (5+ units)",11130,"South Atlantic","1990s","Brick","radiator","central AC",38.354472081075244,31829.437409999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2531.7590460762926},"Hot-Humid",198.47509882384017,"Metropolitan Area",6.2285831966789919E-2,0.38038001531713594,0.32562100318474951,1.5307604015841659E-2,0.53259455992261351,1.3149714256561373,6.7069999999999999,474.21899999999999,{"$f":"T1131*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6980507922033697E-5},{"$f":"U1131*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2006082430712534E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.2302812474711949E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32682161142782079}]
["Single Family Detached",11136,"East North Central","1980s","Siding","central furnace","central AC",60.125925074240556,24531.18118,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24531.18118},"Cold/Very Cold",138.56729611053919,"Metropolitan Area",2.7344249735066755,0.40555078742036255,7.8969134865516946E-2,3.7843443677407065E-2,0.39416858919583464,3.6131134849883901,1376.0170000000001,166.65,{"$f":"T1137*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3755322333760059E-2},{"$f":"U1137*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0881213436469999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.7681802958404353},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.3057256209163946E-2}]
["Multi-Family (2-4 units)",11137,"Mountain South","1980s","Brick","central furnace","central AC",14.116867562826108,11686.148639999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3895.3828799999997},"Hot-Dry/Mixed-Dry",98.675969372262927,"Metropolitan Area",7.8641403605425445E-2,5.7268660893089754E-2,9.5273465352801109E-2,5.7773981646432005E-3,0.1016472661132867,0.33668239474103184,110.998,383.38200000000001,{"$f":"T1138*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3237970891424002E-4},{"$f":"U1138*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4934196793001599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.9073783314339688E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.6766885032101263E-2}]
["Single Family Detached",11144,"West South Central","1980s","Brick","heat pump","central AC",36.527410232337417,18523.0275,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18523.0275},"Hot-Humid",187.24867374957469,"Metropolitan Area",8.7107685733424992E-2,0.13095465551032501,0.11044651515315,7.5055677890550005E-3,0.31038364795851753,0.63889250435541745,119.907,285.29500000000002,{"$f":"T1145*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2210406584425003E-3},{"$f":"U1145*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2845271306124998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.9328726391867494E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11573104228376251}]
["Single Family Detached",11148,"West South Central","Before 1950","Wood","central furnace","window/wall unit",39.262590730643396,15118.440790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15118.440790000001},"Hot-Humid",211.51029758531809,"Rural",1.8072940462015421,0.35770967177206475,0.40805950712300837,2.1201814113520991E-2,0.27252046302986194,2.8455836881264771,1402.3810000000001,0,{"$f":"T1149*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1201814113520991E-2},{"$f":"U1149*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8284958603150632},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.40805950712300837}]
["Single Family Detached",11153,"East South Central","1970s","Brick","central furnace","both central and individual units",35.333389671342694,23906.217639999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23906.217639999999},"Hot-Humid",499.20346894617239,"Metropolitan Area",0.4243021812799157,0.29631352749701884,0.34242257305151586,1.9098916334772398E-2,0.64024393741374253,1.7032822192421928,337.09,461.82,{"$f":"T1154*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0585469042675981E-3},{"$f":"U1154*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.10403694305048E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43236072818418331},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35346294248202065}]
["Multi-Family (2-4 units)",11155,"East North Central","2000s","Siding","central furnace","central AC",35.40719081885117,27090.429090000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9030.1430300000011},"Cold/Very Cold",463.96333980241599,"Micropolitan Area",0.51117731623607776,0.49077861142745799,2.0895778061849089E-2,1.0002382409467981E-2,0.55352291678538146,1.5830428774504115,334.19299999999998,35.029000000000003,{"$f":"T1156*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0178105896247901E-3},{"$f":"U1156*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1631688019787007E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.51419512682570256},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1212094942046959E-2}]
["Multi-Family (5+ units)",11163,"East South Central","1970s","Brick","central furnace","central AC",25.439019325185072,26307.155460000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2092.5088293098529},"Mixed-Humid",490.06947480049644,"Metropolitan Area",0.30215817369247805,0.89077272716013267,7.9869555163806949E-2,8.4516735274787411E-3,0.39153715532204081,1.6721170266468535,186.846,134.423,{"$f":"T1164*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9097690472122878E-4},{"$f":"U1164*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8128131436231838E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30254915059719928},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.0150836478169271E-2}]
["Single Family Detached",11166,"East North Central","2000s","Concrete","heat pump","central AC",109.81968963106073,14395.03076,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14395.03076},"Mixed-Humid",447.57045458454911,"Metropolitan Area",0.87602307064859131,0.19922394365138674,0.1705909319169783,3.937337450493656E-2,2.1210447034612097,3.3668826496781659,1748.0029999999999,987.20299999999997,{"$f":"T1167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5162556953572276E-2},{"$f":"U1167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4210817551364278E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.90118562760216359},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18480174946834257}]
["Multi-Family (5+ units)",11168,"Middle Atlantic","1970s","Siding","central furnace","window/wall unit",19.460630791865068,20000.648300000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1590.8802159665763},"Cold/Very Cold",153.72498280192693,"Metropolitan Area",0.15828154680680889,0.18552191349789851,1.25732275479603E-2,2.9600159458068004E-3,0.16537574048086767,0.52447700037090006,147.99600000000001,0,{"$f":"T1169*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3544390844218945E-4},{"$f":"U1169*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15851699071525108},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.25732275479603E-2}]
["Multi-Family (5+ units)",11173,"South Atlantic","1970s","Brick","central furnace","central AC",19.435464874132318,32664.646850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2598.1928013403417},"Mixed-Humid",145.91297746680513,"Metropolitan Area",0.18214193899779194,0.16283607370687911,6.1256613917280565E-2,5.5418186552773007E-3,8.6473576911060931E-2,0.49780921799400002,90.411000000000001,79.247,{"$f":"T1174*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3490520936198162E-4},{"$f":"U1174*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0589898492781806E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18237684420715392},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1462512902208381E-2}]
["Single Family Detached",11178,"South Atlantic","1950s","Siding","central furnace","central AC",48.98493111054966,42521.641589999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":42521.641589999999},"Mixed-Humid",548.54567489527903,"Metropolitan Area",0.52907356948806183,0.56199620561896879,0.19659451520556437,1.8530378623581333E-2,0.58397355859640221,1.8716378489089973,226.93100000000001,208.85599999999999,{"$f":"T1179*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6494786476602912E-3},{"$f":"U1179*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8808999759210396E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53872304813572214},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2054754151814854}]
["Multi-Family (5+ units)",11182,"Pacific","1970s","Stucco","heat pump","central AC",28.062481344660426,23581.917099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1875.739466352893},"Hot-Dry/Mixed-Dry",303.8930438817419,"Metropolitan Area",8.274179971362057E-2,0.53844402659093193,6.2359317467357379E-2,4.2799057163961001E-3,0.34939847980867839,1.0368830994654965,58.546999999999997,122.944,{"$f":"T1183*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0981891853656282E-4},{"$f":"U1183*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3061091295129008E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.2851618632157134E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2589928380308663E-2}]
["Multi-Family (5+ units)",11189,"East North Central","Before 1950","Brick","central furnace","window/wall unit",15.001174954900302,14493.888849999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1152.86468108554},"Cold/Very Cold",38.292289067655418,"Metropolitan Area",0.72052147209981121,4.544667553083874E-2,4.9895067427236503E-3,1.2555910971866499E-3,0.11600797032595848,0.88812134428206102,86.629000000000005,0,{"$f":"T1190*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9871514457759264E-5},{"$f":"U1190*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.72062134361426899},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.9895067427236503E-3}]
["Single Family Detached",11192,"South Atlantic","1990s","Siding","central furnace","central AC",160.99022199930047,26804.89877,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26804.89877},"Mixed-Humid",438.5955849662181,"Metropolitan Area",1.1505485998574214,0.23537491510021954,0.46461609201979881,5.7775734492137097E-2,0.77422567318920232,2.6247652801666423,830.87300000000005,1324.5440000000001,{"$f":"T1193*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.227146665572621E-2},{"$f":"U1193*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5504267836410877E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1728200665131476},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.50012035985620973}]
["Single Family Attached",11196,"South Atlantic","1960s","Brick","central furnace","central AC",23.734219949500993,12361.572889999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12361.572889999999},"Mixed-Humid",65.795423550080812,"Metropolitan Area",0.78311203351468417,0.11347178510174734,0.10608013314588027,1.87567090089126E-2,0.10446396874466872,1.1071279205069804,1128.4870000000001,388.85300000000001,{"$f":"T1197*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3949874305917431E-2},{"$f":"U1197*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8068347029951702E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.7970619078206016},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11088696784887545}]
["Single Family Detached",11202,"South Atlantic","1960s","Concrete","N/A","central AC",40.80293197650856,39924.590980000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39924.590980000001},"Hot-Humid",709.92362590176151,"Metropolitan Area",0,0.27939731817650348,1.662022873985151,5.3973695224543185E-2,0.48083919751696108,2.4222593896786155,0,1351.8910000000001,{"$f":"T1203*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1203*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3973695224543185E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7159965692096941}]
["Multi-Family (5+ units)",11207,"South Atlantic","1990s","Wood","central furnace","window/wall unit",16.691195947264024,34992.025049999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2783.3157972510244},"Mixed-Humid",177.52129652261681,"Metropolitan Area",9.237722324526057E-2,0.2580678293689273,3.7122584479219345E-2,1.4648361526430999E-3,0.21678668765669096,0.60570264573683663,41.862000000000002,0,{"$f":"T1208*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.165151659045224E-4},{"$f":"U1208*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.2493738411165094E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7122584479219345E-2}]
["Single Family Detached",11208,"Middle Atlantic","Before 1950","Concrete","radiator","window/wall unit",16.968498925211545,16570.799729999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16570.799729999999},"Cold/Very Cold",109.08895507660971,"Metropolitan Area",1.1834529774179465,0.12389748338604886,2.0968209425149834E-2,3.0105497533469395E-3,0.26716416030650136,1.5954828305356465,181.678,0,{"$f":"T1209*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0105497533469395E-3},{"$f":"U1209*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1864635271712936},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0968209425149834E-2}]
["Single Family Detached",11216,"Mountain South","1970s","Stucco","heat pump","central AC",18.092027850634928,8965.3259909999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8965.3259909999997},"Hot-Dry/Mixed-Dry",145.8188486758223,"Metropolitan Area",0.12792773377501951,6.8186862663669426E-2,0.25272911493176142,1.4854379674708169E-2,0.18392827088292438,0.63277198225337472,195.964,1460.9059999999999,{"$f":"T1217*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7568811425003239E-3},{"$f":"U1217*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3097498532207845E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12968461491751984},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26582661346396924}]
["Single Family Detached",11219,"South Atlantic","1970s","Other","central furnace","both central and individual units",41.856121899595514,19540.673159999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19540.673159999998},"Hot-Humid",62.027802472880879,"Metropolitan Area",4.2570157646659557E-2,0.11241637887110988,4.5122286805394513E-2,8.2432720538923188E-3,0.16167122493974698,0.36178004826291088,247.964,173.88800000000001,{"$f":"T1220*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8453834794462396E-3},{"$f":"U1220*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3978885744460796E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.7415541126105798E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.8520175379840595E-2}]
["Single Family Detached",11221,"South Atlantic","1960s","Brick","central furnace","central AC",112.13848035997427,22904.10138,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22904.10138},"Mixed-Humid",394.28329453313455,"Metropolitan Area",1.4797123464793709,0.41317853684451,0.47577210191724856,6.4325573219094129E-2,0.67031014835740188,3.0389731335985317,1348.6610000000001,1459.8130000000001,{"$f":"T1222*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0889868271252181E-2},{"$f":"U1222*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.343570494784194E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5106022147506231},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.50920780686509048}]
["Single Family Detached",11226,"West South Central","1960s","Brick","central furnace","central AC",86.366277540191561,35806.914400000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35806.914400000001},"Hot-Humid",262.38930901964432,"Metropolitan Area",1.2997830435850031,0.44314042866660963,0.38623486286704006,4.0166334614371205E-2,0.60168846846870827,2.7308468035873612,513.36400000000003,608.38400000000001,{"$f":"T1227*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8381980804041603E-2},{"$f":"U1227*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1784353810329601E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3181650243890446},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.40801921667736968}]
["Single Family Detached",11230,"Middle Atlantic","Before 1950","Siding","central furnace","both central and individual units",144.12017819927561,33539.72032,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33539.72032},"Cold/Very Cold",485.15420091783255,"Metropolitan Area",3.7170364523494506,0.52718520582403527,0.30750748354594626,8.6067316044481937E-2,1.2861242108465356,5.8378533525659684,2054.2550000000001,511.87599999999998,{"$f":"T1231*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8899138165961604E-2},{"$f":"U1231*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7168177878520322E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.785935590515412},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32467566142446658}]
["Single Family Detached",11237,"East North Central","1970s","Brick","central furnace","central AC",29.336460300402823,16234.897790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16234.897790000001},"Cold/Very Cold",139.2304834179605,"Metropolitan Area",1.2391867596954296,0.38047108014429915,6.3837809821481656E-2,2.6991426730151244E-2,0.46379200116601327,2.1472876508272232,1475.307,187.249,{"$f":"T1238*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3951458353871531E-2},{"$f":"U1238*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0399683762797097E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2631382180493012},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6877778197761362E-2}]
["Mobile Home",11240,"Pacific","1970s","Siding","central furnace","window/wall unit",13.359003339418759,16492.596720000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16492.596720000001},"Marine",53.567954131397691,"Metropolitan Area",0.3492217140955941,0.13329722386983311,8.1256715075899207E-3,5.0833976388285603E-3,0.21173418319191717,0.70237879266493441,308.22300000000001,0,{"$f":"T1241*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0833976388285603E-3},{"$f":"U1241*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35430511173442264},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.1256715075899207E-3}]
["Single Family Detached",11244,"South Atlantic","2010s","Wood","heat pump","central AC",30.490466188350215,7449.4175880000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7449.4175880000003},"Mixed-Humid",114.4900989124736,"Micropolitan Area",9.9431980287105384E-2,3.6591338057981128E-2,7.8246030351690671E-2,6.3388956610688999E-3,0.17637066020035486,0.39064000889713202,260.06599999999997,590.85900000000004,{"$f":"T1245*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.937340234440808E-3},{"$f":"U1245*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4015554266280919E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10136932052154619},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.2647585778318766E-2}]
["Single Family Detached",11249,"West North Central","Before 1950","Wood","central furnace","central AC",24.043021245037078,12142.94002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12142.94002},"Cold/Very Cold",110.53250799514808,"Metropolitan Area",1.080783700060562,4.9826040783485862E-2,3.2669475116268179E-2,1.6899256768193878E-2,0.33950473930680058,1.5027839552671167,1268.307,123.387,{"$f":"T1250*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.540097582794614E-2},{"$f":"U1250*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.49828094024774E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0961846758885081},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4167756056515917E-2}]
["Single Family Detached",11254,"Middle Atlantic","2000s","Siding","central furnace","central AC",120.97677835246647,33035.71228,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33035.71228},"Cold/Very Cold",275.40409841936179,"Metropolitan Area",4.2510180794057408,0.35574235875877303,3.9148706551715762E-2,5.6412740324984119E-2,0.90734288419773679,5.553252028913966,1645.4939999999999,62.134999999999998,{"$f":"T1255*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4360066342466318E-2},{"$f":"U1255*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0526739825177998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.3053781457482074},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1201380534233563E-2}]
["Single Family Detached",11260,"Pacific","1950s","Brick","central furnace","N/A",25.560815833118333,12085.492120000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12085.492120000001},"Marine",34.72108709818076,"Metropolitan Area",0.19078357271251981,0.18253234799349524,0,7.2774724479319208E-3,0.16708706489315098,0.540402985599166,602.16600000000005,0,{"$f":"T1261*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.2774724479319208E-3},{"$f":"U1261*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19806104516045173},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11264,"East North Central","1980s","Brick","central furnace","central AC",57.214460928664899,14275.0651,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14275.0651},"Cold/Very Cold",199.99250579821859,"Metropolitan Area",1.4336506550447561,0.33758637515374251,0.11693739338123239,6.6036779479097293E-2,0.50630285566829869,2.3944772792480298,4142.482,483.541,{"$f":"T1265*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9134200225578193E-2},{"$f":"U1265*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9025792535191005E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4927848552703342},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12383997263475149}]
["Single Family Detached",11267,"Middle Atlantic","1970s","Siding","fireplace","central AC",45.786685077991322,12109.676030000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12109.676030000001},"Cold/Very Cold",254.05589287361943,"Metropolitan Area",0,0.21707458914643543,0.11779270785327069,6.2498037990830011E-3,0.53197141978575946,0.86683871678546565,0,516.1,{"$f":"T1268*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1268*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2498037990830011E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12404251165235369}]
["Single Family Attached",11274,"Pacific","1990s","Shingle","central furnace","central AC",20.15729557057195,15224.54348,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15224.54348},"Hot-Dry/Mixed-Dry",107.85675584604225,"Metropolitan Area",5.0076857680742125E-2,0.33973745380324372,5.3140370768874685E-2,3.2434824166096402E-3,0.29966974386527534,0.74262442611813584,54.573,158.47,{"$f":"T1275*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3084901133403998E-4},{"$f":"U1275*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4126334052755999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.0907706692076164E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5553004174150288E-2}]
["Single Family Detached",11278,"East North Central","1960s","Brick","central furnace","central AC",49.454459238882528,21614.711210000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21614.711210000001},"Cold/Very Cold",310.32374889384147,"Metropolitan Area",1.9854828454455073,0.3547205170823835,0.13275377367735824,4.590322704081063E-2,1.1529771777386442,3.6259343139438931,1819.2739999999999,304.42899999999997,{"$f":"T1279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9323082121861537E-2},{"$f":"U1279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.58014491894909E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0248059275673689},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13933391859630734}]
["Single Family Attached",11279,"South Atlantic","1960s","Wood","heat pump","central AC",18.918540387726679,15232.319149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15232.319149999999},"Hot-Humid",101.31020038195756,"Metropolitan Area",3.5375263812215299E-2,7.9987817229607641E-2,9.9780875520947443E-2,5.8259203376196502E-3,0.13052642825071176,0.34567038481348217,40.067,342.404,{"$f":"T1280*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1031333138304993E-4},{"$f":"U1280*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2156070062365995E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.5985577143598346E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10499648252718405}]
["Single Family Detached",11283,"New England","1970s","Siding","radiator","window/wall unit",87.083493921604202,20684.915420000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20684.915420000001},"Cold/Very Cold",161.34291945993888,"Micropolitan Area",2.2125759609031239,0.20942903890592868,4.2148286946916282E-2,2.4108062072855803E-3,0.39882091051823471,2.8629741972742031,116.54900000000001,0,{"$f":"T1284*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4108062072855803E-3},{"$f":"U1284*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2149867671104095},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.2148286946916282E-2}]
["Single Family Detached",11290,"Pacific","1960s","Wood","heat pump","central AC",28.473740915053668,13061.349039999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13061.349039999999},"Marine",81.986427541768649,"Metropolitan Area",0.5167555823635267,0.28776738082229919,5.5103859336054953E-2,1.1010377645644959E-2,0.23515582280331207,1.094782645325193,635.84199999999998,207.13200000000001,{"$f":"T1291*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3049542962916785E-3},{"$f":"U1291*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.70542334935328E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52506053665981833},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7809282685408234E-2}]
["Single Family Detached",11293,"South Atlantic","1970s","Concrete","heat pump","central AC",23.459615613604416,17123.80702,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17123.80702},"Hot-Humid",178.09476785432702,"Metropolitan Area",2.9575811389768499E-2,9.8784263155958521E-2,0.16649366260800372,9.0457538011571182E-3,0.31280561723360395,0.60765935438733465,29.286999999999999,498.96899999999999,{"$f":"T1294*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0150493619473995E-4},{"$f":"U1294*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.5442488649623803E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0077316325963239E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1750379114729661}]
["Multi-Family (2-4 units)",11297,"Pacific","2000s","Siding","built-in electric unit","N/A",47.169516290685259,31134.99425,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10378.331416666666},"Marine",253.127472127891,"Metropolitan Area",0.28882284011029752,0.21986900898966724,0,0,0.35497912972757673,0.86367097882754151,0,0,{"$f":"T1298*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1298*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28882284011029752},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11302,"East North Central","Before 1950","Siding","central furnace","both central and individual units",50.34303792406125,19288.520280000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19288.520280000001},"Cold/Very Cold",134.60248911388697,"Metropolitan Area",1.109474008404336,8.1935589566290337E-2,5.2138895611469407E-2,2.7300180774980521E-2,0.36123805033111811,1.6047865439132136,1286.9670000000001,128.392,{"$f":"T1303*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4823689079190765E-2},{"$f":"U1303*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4764916957897599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1342976974835268},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.4615387307259164E-2}]
["Single Family Detached",11308,"Pacific","Before 1950","Wood","radiator","window/wall unit",62.958985567953221,13452.77469,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13452.77469},"Marine",186.91733137250776,"Metropolitan Area",0.93278627174739615,9.4834675991195189E-2,3.4317153803835147E-2,1.09057608579423E-3,0.1364419960217389,1.1983800975641654,81.066999999999993,0,{"$f":"T1309*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.09057608579423E-3},{"$f":"U1309*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.93387684783319036},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4317153803835147E-2}]
["Single Family Detached",11312,"East South Central","Before 1950","Wood","central furnace","central AC",23.509941996401494,15874.37002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15874.37002},"Mixed-Humid",228.15866916112051,"Metropolitan Area",0.70238290018568705,0.39993352862118325,0.1627489466253762,1.8021251570244843E-2,0.63553235629821248,1.900597731730459,713.40800000000002,421.834,{"$f":"T1313*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1324902567228162E-2},{"$f":"U1313*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6963490030166805E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.71370780275291523},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16944529562839289}]
["Multi-Family (5+ units)",11315,"Pacific","1970s","Stucco","central furnace","window/wall unit",6.4847358660414702,17432.085660000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1386.5730642105566},"Hot-Dry/Mixed-Dry",33.704379799579215,"Metropolitan Area",1.7799283485640284E-2,0.20235571201723879,1.8035340416349962E-2,3.314711088249E-4,0.1151100408183614,0.35360548215959936,19.015000000000001,0,{"$f":"T1316*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6365686815963734E-5},{"$f":"U1316*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7825649172456246E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8035340416349962E-2}]
["Single Family Detached",11320,"West South Central","1970s","Brick","central furnace","central AC",25.814408252052896,24284.485659999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24284.485659999998},"Mixed-Humid",162.46821164095368,"Metropolitan Area",0.59655569986808366,0.46048936244781874,8.4184913687269589E-2,1.3747447332126E-2,0.64476322090352012,1.785993196906692,409.59899999999999,156.501,{"$f":"T1321*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9469010418503402E-3},{"$f":"U1321*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.80054629027566E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60650260090993402},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.7985459977545255E-2}]
["Mobile Home",11326,"South Atlantic","1980s","Siding","portable electric heaters","window/wall unit",14.871573528012734,19671.39356,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19671.39356},"Mixed-Humid",288.33504442368042,"Metropolitan Area",0.3547709665592565,0.2573004704386444,3.5729663579260558E-2,0,0.33599804422871604,0.98379914480587749,0,0,{"$f":"T1327*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1327*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3547709665592565},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5729663579260558E-2}]
["Single Family Detached",11331,"Middle Atlantic","1980s","Siding","central furnace","central AC",72.464238088356197,34838.576000000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34838.576000000001},"Cold/Very Cold",235.77898178264479,"Metropolitan Area",1.5591040705402079,0.341198074031136,3.3256800133872E-2,2.4748418587424003E-2,0.89179480265331224,2.8253537473585282,668.66700000000003,41.707000000000001,{"$f":"T1332*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3295406098192004E-2},{"$f":"U1332*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.453012489232E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5823994766384},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4709812623103999E-2}]
["Single Family Detached",11336,"South Atlantic","1960s","Brick","central furnace","central AC",29.454066908056699,21038.61922,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21038.61922},"Mixed-Humid",216.64358248330632,"Metropolitan Area",0.77439890051255145,0.19530139702616395,0.13355048290391905,1.5890763637535082E-2,0.43698017899056124,1.5402309594331955,456.88600000000002,298.428,{"$f":"T1337*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6122505809489202E-3},{"$f":"U1337*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2785130565861606E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78401115109350039},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13982899596050521}]
["Single Family Detached",11338,"East North Central","1960s","Brick","central furnace","central AC",39.501396071273383,17841.642309999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17841.642309999999},"Cold/Very Cold",95.514001025850561,"Metropolitan Area",1.2530143466453572,0.29037388830200017,2.6480369258436592E-2,1.146550323110606E-2,0.28234199129181148,1.8522105954976054,562.67399999999998,79.951999999999998,{"$f":"T1339*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0039028245136939E-2},{"$f":"U1339*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.42647498596912E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2630533748904942},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7906844244405711E-2}]
["Multi-Family (5+ units)",11341,"Mountain South","1960s","Stucco","central furnace","central AC",8.0636414054058285,14988.181049999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1192.1813907287267},"Hot-Dry/Mixed-Dry",61.166766868886953,"Metropolitan Area",2.9921250436629614E-2,9.1534964982240147E-2,9.988431589391901E-2,4.6807190128287006E-3,0.10445651567634189,0.33010545490672316,38.747,273.54700000000003,{"$f":"T1342*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6193452346565976E-5},{"$f":"U1342*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2611764288967103E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9967443888976181E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10021043353680868}]
["Mobile Home",11349,"South Atlantic","1990s","Stucco","heater burning gas/oil/kerosene","window/wall unit",19.683932061533376,25235.81034,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25235.81034},"Mixed-Humid",258.41971975972052,"Metropolitan Area",0.20312149804222926,0.36228718592681552,7.7323027597966804E-2,0,0.44211787076245762,1.0848495823294693,0,0,{"$f":"T1350*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1350*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20312149804222926},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.7323027597966804E-2}]
["Single Family Detached",11350,"South Atlantic","1990s","Brick","other","N/A",14.382797014972574,13697.90192,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13697.90192},"Hot-Humid",94.628982962843608,"Rural",7.1333700860963037E-2,7.9609562263969438E-2,0,0,0.1719308186034047,0.32287408172833715,0,0,{"$f":"T1351*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1351*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.1333700860963037E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11355,"Middle Atlantic","1980s","Siding","heater burning gas/oil/kerosene","central AC",27.583827631849882,14269.95739,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14269.95739},"Cold/Very Cold",192.16949202210563,"Metropolitan Area",0.38383081663367674,0.1701654888769564,5.4537408331653256E-2,2.6302813559969701E-3,0.28153254587564813,0.89006625971793463,0,184.32300000000001,{"$f":"T1356*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1356*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6302813559969701E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38383081663367674},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7167689687650229E-2}]
["Single Family Detached",11361,"East South Central","1960s","Brick","central furnace","central AC",43.327485457045995,26211.42496,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26211.42496},"Mixed-Humid",370.80537515733596,"Metropolitan Area",0.30414909242555271,0.38953991252891679,0.18917026538741633,1.3496891786103041E-2,2.0235891867941724,2.9064484571360585,167.76,347.16399999999999,{"$f":"T1362*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3972286512895999E-3},{"$f":"U1362*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0996631348134391E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30854632107684232},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19826992852222977}]
["Single Family Detached",11365,"Middle Atlantic","Before 1950","Brick","other","window/wall unit",184.58294944201123,27467.700809999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27467.700809999998},"Cold/Very Cold",490.71319426986986,"Metropolitan Area",0.37626294848628616,0.70130168387671221,0.27491806464230856,0,1.0231323840864361,2.3756150810917429,0,0,{"$f":"T1366*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1366*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37626294848628616},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27491806464230856}]
["Single Family Detached",11368,"South Atlantic","2000s","Wood","built-in electric unit","central AC",28.054562994444378,19925.115760000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19925.115760000001},"Hot-Humid",433.70999481539116,"Metropolitan Area",0.31254090258542977,0.1143036145757616,0.37450414712657232,1.734977462290424E-2,0.6784896832074363,1.4798383474952002,0,870.74900000000002,{"$f":"T1369*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1369*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.734977462290424E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31254090258542977},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.39185392174947653}]
["Mobile Home",11375,"South Atlantic","1970s","Siding","N/A","N/A",40.956274338033708,40631.224540000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":40631.224540000003},"Hot-Humid",148.22270712812198,"Metropolitan Area",0,0.73622580245356084,0,0,0.50577748307392001,1.2420032855274807,0,0,{"$f":"T1376*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1376*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11379,"West North Central","1970s","Siding","central furnace","central AC",46.275712475804184,14142.94391,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14142.94391},"Cold/Very Cold",284.6318942343828,"Metropolitan Area",0.87948494950862388,0.24181578625724573,0.10573131923443246,3.0445656784496098E-2,0.59825536673294377,1.8252874217332458,1793.2280000000001,359.48200000000003,{"$f":"T1380*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.536152302184148E-2},{"$f":"U1380*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0841337626546202E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.90484647253046535},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11081545299708709}]
["Single Family Detached",11384,"New England","2000s","Siding","central furnace","central AC",21.564168693298516,19568.211159999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19568.211159999999},"Cold/Very Cold",203.39190847683301,"Metropolitan Area",0.89575844554344775,0.34593262907698336,3.8161103539363278E-2,1.4838339704094081E-2,0.64261103354905513,1.9224632117088496,674.61699999999996,83.671000000000006,{"$f":"T1385*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3201047908125719E-2},{"$f":"U1385*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6372917959683599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.90895949345157345},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9798395335331638E-2}]
["Single Family Detached",11386,"East South Central","1950s","Shingle","central furnace","window/wall unit",41.502935848782698,18669.78671,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18669.78671},"Hot-Humid",313.75937587900449,"Micropolitan Area",0.94057007614720811,0.26635658211171781,0.37568423931533845,1.251484344616746E-2,0.53660725232604722,2.1192181499003113,670.32600000000002,0,{"$f":"T1387*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.251484344616746E-2},{"$f":"U1387*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.9530849195933756},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37568423931533845}]
["Multi-Family (5+ units)",11391,"Pacific","1960s","Stucco","N/A","N/A",22.058508782673059,24455.109520000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1945.1944422553481},"Hot-Dry/Mixed-Dry",52.710151767220609,"Metropolitan Area",0,0.12616716254324617,0,0,0.17984705723380798,0.30601421977705412,0,0,{"$f":"T1392*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1392*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11398,"South Atlantic","1960s","Brick","central furnace","central AC",28.9794765390252,17531.443759999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17531.443759999998},"Mixed-Humid",179.3093452442082,"Micropolitan Area",0.96283819908042501,0.10066469102917575,0.26595634963725245,2.6290661474365037E-2,0.18592541406151486,1.5153846538083682,785.37699999999995,714.25199999999995,{"$f":"T1399*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3768792705897518E-2},{"$f":"U1399*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2521868768467517E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.97660699178632249},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27847821840571996}]
["Single Family Detached",11402,"Pacific","2000s","Wood","central furnace","central AC",28.609120657979599,14304.56033,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14304.56033},"Hot-Dry/Mixed-Dry",86.296551552729667,"Metropolitan Area",0.20168365806011448,0.27393730830649488,6.1899065378544581E-2,8.172409884933951E-3,0.26489267785543918,0.80241270960059308,353.964,217.351,{"$f":"T1403*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.06329939264812E-3},{"$f":"U1403*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1091104922858302E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20674695745276261},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5008175870830409E-2}]
["Single Family Detached",11403,"Mountain South","2000s","Stucco","radiator","N/A",26.526853386509799,10627.74575,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10627.74575},"Cold/Very Cold",91.99184357097991,"Metropolitan Area",0.82607947947107763,0.20134100656090451,6.3537637878510994E-2,9.5384018106250002E-4,0.25845642521563933,1.3494145491261325,89.75,0,{"$f":"T1404*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5384018106250002E-4},{"$f":"U1404*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.82703331965214011},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.3537637878510994E-2}]
["Single Family Detached",11409,"Pacific","2000s","Wood","built-in electric unit","window/wall unit",37.491352324057232,17904.17972,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17904.17972},"Marine",305.55643718829594,"Micropolitan Area",0.63638596702170314,0.11723388317960201,7.4135299841212397E-3,0,0.28152519658802189,1.0425585767734482,0,0,{"$f":"T1410*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1410*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63638596702170314},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4135299841212397E-3}]
["Single Family Detached",11413,"East North Central","Before 1950","Wood","central furnace","central AC",81.793446677813449,27773.666099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27773.666099999999},"Cold/Very Cold",303.64949152072484,"Metropolitan Area",3.537468832708619,0.27547216290820259,0.2209006584666261,7.3608047338840202E-2,0.4781016373942833,4.5119432914777304,2215.7260000000001,434.55599999999998,{"$f":"T1414*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.15388340930886E-2},{"$f":"U1414*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2069213245751598E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.5990076668017075},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23296987171237771}]
["Multi-Family (5+ units)",11420,"West South Central","1980s","Brick","N/A","N/A",47.040184078231384,41813.496959999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3325.9054444771459},"Hot-Humid",176.8838034372254,"Metropolitan Area",0,0.11242934321745984,0,0,0.49109822557679422,0.60352756879425407,0,0,{"$f":"T1421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11421,"East North Central","2010s","Brick","central furnace","central AC",28.42826114683681,18629.266810000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18629.266810000001},"Cold/Very Cold",117.5502637056324,"Metropolitan Area",2.0031561023661233,7.2572358077704097E-2,2.9135409490900793E-2,1.1670304193124498E-2,0.48192154634683132,2.5867854162815598,556.90599999999995,69.543999999999997,{"$f":"T1422*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.037475046208986E-2},{"$f":"U1422*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.29555373103464E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0135308528282132},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0430963221935434E-2}]
["Single Family Detached",11427,"West South Central","2000s","Siding","heat pump","central AC",41.616346729107839,12422.790069999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12422.790069999999},"Hot-Humid",228.42627606195074,"Metropolitan Area",0.13204979866246488,0.14204057912046095,0.25657441770328682,1.8428103440528767E-2,0.24872567409148072,0.77939046957769331,209.15600000000001,1274.2550000000001,{"$f":"T1428*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5983010798809199E-3},{"$f":"U1428*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5829802360647849E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13464809974234582},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27240422006393467}]
["Single Family Detached",11432,"East North Central","Before 1950","Siding","central furnace","central AC",23.217212480530083,28805.474539999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28805.474539999999},"Cold/Very Cold",211.13859773882041,"Metropolitan Area",1.3014818069085941,1.0300661405999814,0.15263874050825846,4.0575074576824056E-2,0.53335018350523089,3.017536871522065,1194.7729999999999,213.816,{"$f":"T1433*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4416003232579415E-2},{"$f":"U1433*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1590713442446401E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3358978101411734},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15879781185250311}]
["Multi-Family (5+ units)",11437,"East North Central","Before 1950","Brick","portable electric heaters","window/wall unit",26.251925408614465,22304.099750000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1774.1000439080799},"Cold/Very Cold",114.89017984866643,"Metropolitan Area",0.19060541656726074,0.16185005670147101,4.5612553111742504E-2,0,0.17618661902647687,0.57425464540695104,0,0,{"$f":"T1438*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1438*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19060541656726074},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.5612553111742504E-2}]
["Single Family Detached",11439,"Pacific","1970s","Wood","central furnace","central AC",54.386462500264983,15485.89479,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15485.89479},"Marine",174.86319317754618,"Metropolitan Area",0.93439865156410951,0.26353380073325494,0.10037394864897123,2.7488345948253032E-2,0.48698014831963993,1.7852865492659755,1388.519,386.53800000000001,{"$f":"T1440*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1502459147916011E-2},{"$f":"U1440*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9858868003370199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95590111071202555},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10635983544930824}]
["Multi-Family (5+ units)",11447,"Pacific","1950s","Stucco","central furnace","N/A",10.700391861804393,24884.632239999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1979.3592946794643},"Hot-Dry/Mixed-Dry",104.23383601134513,"Metropolitan Area",3.8553439988138309E-2,0.13675172966603094,0,4.3896491271359998E-4,0.3293154092896366,0.50502462795856129,17.64,0,{"$f":"T1448*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4915897958145754E-5},{"$f":"U1448*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.8588355886096458E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11450,"New England","1960s","Siding","wood-burning stove","window/wall unit",35.587824203908944,16970.826990000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16970.826990000001},"Cold/Very Cold",206.46889707293562,"Metropolitan Area",0,0.3291199996486272,5.1322139762711612E-2,0,0.32402973585959266,0.70447187527093147,0,0,{"$f":"T1451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.1322139762711612E-2}]
["Mobile Home",11456,"Middle Atlantic","1970s","Siding","central furnace","central AC",39.230899806320487,25540.950390000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25540.950390000002},"Cold/Very Cold",383.4973701770196,"Metropolitan Area",1.8826822485146977,0.53765138526456957,0.11173877182885593,1.581582487380126E-2,0.52295037179339121,3.0550227774015144,456.178,163.05600000000001,{"$f":"T1457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1651219667009421E-2},{"$f":"U1457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1646052067918406E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.894333468181707},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11590337703564776}]
["Single Family Attached",11457,"South Atlantic","1990s","Brick","radiator","central AC",13.073172118488445,12594.578149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12594.578149999999},"Mixed-Humid",72.167197278953054,"Metropolitan Area",0.30371752160171728,0.11106562746938504,3.1292778546787449E-2,2.1834338518184498E-3,0.2111542992171998,0.65723022683508958,62.234000000000002,111.129,{"$f":"T1458*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8381097658709994E-4},{"$f":"U1458*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3996228752313502E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30450133257830436},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2692401422018798E-2}]
["Single Family Detached",11462,"West North Central","1990s","Siding","central furnace","central AC",32.225075683760934,13046.58935,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13046.58935},"Cold/Very Cold",202.7003314968953,"Metropolitan Area",0.51431173840700339,0.34792176106022332,7.0034783100035553E-2,1.9554997866551647E-2,0.60532415861608246,1.5375924411833448,1245.8869999999999,252.97200000000001,{"$f":"T1463*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.625457606550345E-2},{"$f":"U1463*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3004218010482E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53056631447250679},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.333520490108375E-2}]
["Single Family Detached",11466,"East North Central","Before 1950","Siding","central furnace","window/wall unit",85.015866489497583,39689.947010000004,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39689.947010000004},"Cold/Very Cold",242.83035905056667,"Metropolitan Area",4.8248780454611877,0.32016062453393951,6.9264911024501497E-2,4.793612885053266E-2,0.50051880855794717,5.7148223895775754,1207.7650000000001,0,{"$f":"T1467*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.793612885053266E-2},{"$f":"U1467*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.8728141743117206},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9264911024501497E-2}]
["Single Family Detached",11473,"Pacific","1970s","Siding","heat pump","N/A",10.095424784001557,13196.6337,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13196.6337},"Hot-Dry/Mixed-Dry",31.61913435616697,"Metropolitan Area",0.19908386173958459,5.9764188885706497E-2,0,3.2085239447484002E-3,0.12190389060711634,0.38075194123240746,243.13200000000001,0,{"$f":"T1474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2085239447484002E-3},{"$f":"U1474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.202292385684333},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",11475,"South Atlantic","1950s","Brick","heat pump","central AC",35.504321725157432,37730.416290000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3001.1313591241956},"Mixed-Humid",290.29272929854238,"Micropolitan Area",0.31058943858267923,0.35791631302855093,0.25545359128989742,1.63119908746557E-2,0.40942127423687158,1.3483951288921647,132.06,300.27,{"$f":"T1476*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9632940728594131E-4},{"$f":"U1476*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.011497132042222E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31098576798996519},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25635474100310163}]
["Single Family Detached",11480,"New England","1950s","Shingle","central furnace","window/wall unit",34.935036665662466,20382.168420000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20382.168420000002},"Cold/Very Cold",145.04008115162239,"Metropolitan Area",2.6006463107578166,0.37505813077875655,0.12345136991564545,4.1665840149216607E-2,0.50044468567503886,3.5996004971272577,2044.23,0,{"$f":"T1481*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1665840149216607E-2},{"$f":"U1481*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6423121509070331},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12345136991564545}]
["Single Family Attached",11485,"West South Central","2000s","Brick","central furnace","central AC",17.565951234689166,13347.98726,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13347.98726},"Hot-Humid",247.01359423306522,"Metropolitan Area",0.29106225918733103,0.1735920425948986,0.10860204077267185,9.7933915566874811E-3,0.26955401995989181,0.84281036251479324,361.57100000000003,372.12700000000001,{"$f":"T1486*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8262451015854595E-3},{"$f":"U1486*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9671464551020198E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2958885042889165},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11356918722777387}]
["Multi-Family (5+ units)",11491,"South Atlantic","1970s","Shingle","central furnace","central AC",21.295223326221421,35492.03888,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2823.0876135404333},"Mixed-Humid",341.87621267411339,"Metropolitan Area",0.93091781402864671,0.37227482457503702,0.16021908261707479,2.040107239249616E-2,0.64744311134604382,2.1296331744374224,387.83600000000001,186.971,{"$f":"T1492*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0948950076850677E-3},{"$f":"U1492*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2783551419126838E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.93201270903633182},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16074691813126607}]
["Single Family Detached",11492,"Middle Atlantic","1980s","Brick","central furnace","central AC",158.30916235329803,33754.618840000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33754.618840000003},"Cold/Very Cold",505.20538015816885,"Metropolitan Area",2.4228809880887385,0.80801401523765937,0.32390557562594874,0.12386311390728144,1.2950031077757935,4.8498036867281398,3106.3029999999999,563.21299999999997,{"$f":"T1493*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.10485207376654852},{"$f":"U1493*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9011040140732922E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5277330618552871},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.34291661576668164}]
["Single Family Detached",11499,"Mountain South","2000s","Stucco","central furnace","central AC",26.373457047206813,13069.10656,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13069.10656},"Cold/Very Cold",84.772119344554838,"Metropolitan Area",0.46111686854507011,0.3146217898007917,5.3512162541674242E-2,1.130878939011392E-2,0.24071529954134394,1.06996612042888,667.90700000000004,197.4,{"$f":"T1500*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7289477551699204E-3},{"$f":"U1500*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5798416349440004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.46984581630024003},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.6092004176618242E-2}]
["Single Family Detached",11503,"Pacific","1980s","Stucco","central furnace","central AC",17.894013821286272,14258.17834,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14258.17834},"Hot-Dry/Mixed-Dry",153.61839767434142,"Metropolitan Area",0.12949665390838846,0.18983415636039036,6.4468510204271745E-2,6.9001028258595994E-3,0.45565445106449948,0.83945377153755008,282.15600000000001,201.78399999999999,{"$f":"T1504*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0230305677010402E-3},{"$f":"U1504*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8770722581585601E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1335196844760895},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7345582462430303E-2}]
["Multi-Family (5+ units)",11509,"West North Central","1980s","Brick","central furnace","central AC",11.244953022622925,11849.26557,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":942.50755706988332},null,50.524225640250961,"Metropolitan Area",1.581725048318201E-2,2.750971706866923E-2,3.5629248707123276E-3,6.0663500012171992E-4,0.12494037431358765,0.17238864911938118,37.94,13.256,{"$f":"T1510*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5758736715231374E-5},{"$f":"U1510*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2493880176518374E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5853009219897241E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5754187508888458E-3}]
["Single Family Detached",11510,"East North Central","Before 1950","Siding","central furnace","both central and individual units",87.206717029958654,26203.941419999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26203.941419999999},"Mixed-Humid",351.58842289376378,"Micropolitan Area",1.8970131401122912,0.2834402779734797,0.26638717216040636,6.3280369806103562E-2,0.62253230330716514,3.0693728935533429,1958.789,456.12900000000002,{"$f":"T1511*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.132799221014038E-2},{"$f":"U1511*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.195237759596318E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9483411323224316},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27833954975636954}]
["Single Family Detached",11514,"South Atlantic","1980s","Concrete","N/A","central AC",30.890421969878648,17315.258949999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17315.258949999999},"Hot-Humid",228.60003119024157,"Metropolitan Area",0,0.14619332003365429,0.42436127548528613,2.069784673165935E-2,0.23926856824061693,0.80982316375955721,0,1195.3530000000001,{"$f":"T1515*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1515*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.069784673165935E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.44505912221694549}]
["Single Family Detached",11521,"Pacific","Before 1950","Siding","built-in electric unit","window/wall unit",67.838407343379899,30150.403259999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30150.403259999999},"Cold/Very Cold",378.21995486799824,"Metropolitan Area",0.65334657547483088,0.30752081692416233,2.4811158797896381E-2,0,0.30480794393963384,1.2904864951365236,0,0,{"$f":"T1522*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1522*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.65334657547483088},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.4811158797896381E-2}]
["Single Family Detached",11524,"East North Central","1980s","Siding","central furnace","central AC",56.525727404179058,14883.024590000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14883.024590000001},"Cold/Very Cold",128.5893324834405,"Metropolitan Area",1.0422329257789218,0.13797080235883274,9.1510732390672353E-2,4.6535869212397253E-2,0.16773475303236532,1.4394492135607921,2790.462,336.31299999999999,{"$f":"T1525*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1530514563460581E-2},{"$f":"U1525*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0053546489366701E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0837634403423824},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.6516087039609025E-2}]
["Single Family Detached",11528,"East South Central","1960s","Siding","other","window/wall unit",12.304497940248176,16190.12887,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16190.12887},"Hot-Humid",101.24767463223422,"Rural",0.67135798428749671,0.35162136347165079,5.8548233511550037E-2,0,0.36875353118008042,1.4502811124507777,0,0,{"$f":"T1529*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1529*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.67135798428749671},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8548233511550037E-2}]
["Multi-Family (2-4 units)",11533,"Pacific","2000s","Siding","built-in electric unit","N/A",32.756232562215985,31137.103200000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10379.0344},"Marine",306.94741484627224,"Metropolitan Area",0.196929878584236,0.53532953529120242,0,0,0.31504511676629032,1.0473045306417288,0,0,{"$f":"T1534*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1534*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.196929878584236},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11538,"South Atlantic","1960s","Brick","central furnace","central AC",36.812554952559992,21205.388800000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21205.388800000001},"Mixed-Humid",170.00360199001929,"Micropolitan Area",1.040033985683712,0.50194760537532168,0.12098961477500161,1.75929235855872E-2,0.61600519975699164,2.2789764055910271,532.11800000000005,297.52600000000001,{"$f":"T1539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1283769077478401E-2},{"$f":"U1539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3091545081088007E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0513177547611903},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1272987692831104}]
["Single Family Detached",11544,"East North Central","1960s","Wood","central furnace","central AC",48.318596785108518,15811.059160000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15811.059160000001},"Cold/Very Cold",96.936180698884073,"Metropolitan Area",1.8175577127240981,6.3378219555321844E-2,3.24786033946972E-2,2.1267012966459522E-2,0.21543488309143091,2.1288494187655478,1230.4369999999999,114.63500000000001,{"$f":"T1545*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9454512199652919E-2},{"$f":"U1545*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8125007668066001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.837012224923751},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4291104161503799E-2}]
["Single Family Detached",11547,"New England","1950s","Wood","central furnace","N/A",45.501252777548594,16783.936839999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16783.936839999998},"Cold/Very Cold",84.044086747816365,"Metropolitan Area",1.0294474655837151,0.28572671965552876,0,4.8899697872476874E-2,0.26969767394278144,1.5848718591820252,2913.482,0,{"$f":"T1548*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8899697872476874E-2},{"$f":"U1548*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0783471634561921},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11551,"East North Central","2000s","Wood","heat pump","central AC",69.885563987152622,19358.881990000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19358.881990000002},"Mixed-Humid",466.45516540305829,"Micropolitan Area",0.4789540145904902,0.43428366542291302,0.12036344223630321,1.582516974819137E-2,0.55794392526211312,1.5915450475118196,495.24599999999998,322.21699999999998,{"$f":"T1552*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5874088700195394E-3},{"$f":"U1552*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2377608781718306E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.48854142346050972},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12660120311447504}]
["Multi-Family (2-4 units)",11557,"East North Central","2000s","Siding","central furnace","central AC",41.834957617125767,35214.610789999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11738.203596666666},"Cold/Very Cold",192.13091646383685,"Metropolitan Area",5.0316819202620974E-2,0.15712026870593568,1.6430726557488114E-2,2.30581749991841E-3,0.43014566086380185,0.65555068699645891,44.484000000000002,20.995000000000001,{"$f":"T1558*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2216224879412002E-4},{"$f":"U1558*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4644358451201669E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.0838981451415091E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6677170142000132E-2}]
["Single Family Detached",11562,"West South Central","1980s","Brick","central furnace","central AC",20.37771639614369,10804.72768,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10804.72768},"Hot-Humid",177.90614033465789,"Rural",0.19059002632554303,8.0525550086597758E-2,0.13868523824250176,1.05258036349408E-2,0.22863419640357763,0.6384350110582202,314.25700000000001,659.928,{"$f":"T1563*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.39546130653376E-3},{"$f":"U1563*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1303423284070399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19398548763207679},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14581558057090879}]
["Multi-Family (5+ units)",11563,"West North Central","1990s","Siding","built-in electric unit","central AC",26.866408423355619,22614.821909999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1798.8153296124135},"Cold/Very Cold",270.17927730120334,"Micropolitan Area",0.20987199254904434,0.36336358319445927,1.0947703001058866E-2,4.9560382215764996E-4,0.33720852398855827,0.92184798551732994,0,21.914999999999999,{"$f":"T1564*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1564*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9421037948456037E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20987199254904434},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0987124039007323E-2}]
["Single Family Detached",11571,"South Atlantic","Before 1950","Wood","other","window/wall unit",71.27177873026119,19483.81048,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19483.81048},"Mixed-Humid",264.302000224523,"Micropolitan Area",0.74119822784372957,0.29133286471463926,0.26050550183794136,0,0.34996002064135839,1.6429966150376687,0,0,{"$f":"T1572*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1572*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.74119822784372957},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26050550183794136}]
["Single Family Detached",11574,"South Atlantic","1950s","Concrete","heat pump","central AC",58.858214745490592,27947.87025,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27947.87025},"Mixed-Humid",268.87924912011425,"Metropolitan Area",0.116532781292172,0.21866293507757925,8.0181824894104511E-2,7.4245473670042509E-3,0.50203843707440687,0.91741597833826272,146.22800000000001,119.429,{"$f":"T1575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0867611709170006E-3},{"$f":"U1575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3377861960872499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12061954246308899},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.3519611090191764E-2}]
["Multi-Family (5+ units)",11576,"Middle Atlantic","1990s","Siding","built-in electric unit","window/wall unit",11.533654266994708,17396.16028,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1383.7155080235862},"Cold/Very Cold",147.63447999967232,"Metropolitan Area",0.26260474648403626,0.1567982031445464,9.38387157055816E-3,0,7.4942014828309658E-2,0.50372883602745044,0,0,{"$f":"T1577*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1577*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26260474648403626},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.38387157055816E-3}]
["Single Family Detached",11581,"South Atlantic","2000s","Siding","heat pump","central AC",183.3191618478009,38367.342369999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38367.342369999998},"Mixed-Humid",911.55483922692895,"Metropolitan Area",2.490837217677313,1.3630142638149809,0.34550071885784295,7.7544734439457808E-2,2.7551756604856581,6.9545278608357952,1426.153,594.96,{"$f":"T1582*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4717700423002606E-2},{"$f":"U1582*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2827034016455201E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5455549181003154},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36832775287429814}]
["Multi-Family (2-4 units)",11586,"Mountain South","2000s","Stucco","central furnace","central AC",14.405581294421474,13338.501200000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4446.1670666666669},"Cold/Very Cold",56.962442846391802,"Metropolitan Area",0.13051827019892653,0.28594511986259002,5.2874214465668937E-2,1.9975472627095999E-3,0.17210073201206474,0.64277003471439009,109.952,39.805999999999997,{"$f":"T1587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8886496131413332E-4},{"$f":"U1587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7698412625573334E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13100713516024068},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.305119859192467E-2}]
["Mobile Home",11592,"Pacific","1970s","Siding","built-in electric unit","window/wall unit",2.6780770189936152,8583.5801890000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8583.5801890000002},"Cold/Very Cold",114.52315691235607,"Micropolitan Area",0.23914703322634695,6.1779073791200095E-2,1.1308343300615972E-2,0,7.8518548702703E-2,0.39075299902086597,0,0,{"$f":"T1593*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1593*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23914703322634695},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1308343300615972E-2}]
["Single Family Attached",11597,"West North Central","1990s","Siding","central furnace","central AC",19.029795209446444,8753.3556619999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8753.3556619999999},"Cold/Very Cold",127.78927644215069,"Micropolitan Area",0.18031064463556351,8.5217217384654584E-2,6.5025002803619954E-3,3.270393729013792E-3,0.16398666046854599,0.43601702276912607,341.46199999999999,32.154000000000003,{"$f":"T1598*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9889383310578439E-3},{"$f":"U1598*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8145539795594804E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18329958296662135},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.783955678317943E-3}]
["Single Family Attached",11600,"Pacific","1990s","Siding","central furnace","central AC",9.2562446509214613,8773.6916120000005,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8773.6916120000005},"Cold/Very Cold",43.732334235875122,"Metropolitan Area",0.47147061151614356,3.0347734280252569E-2,7.6981598520513683E-3,3.3547438195307678E-3,0.10814812002307284,0.61766462567152036,344.29199999999997,38.072000000000003,{"$f":"T1601*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0207118324787037E-3},{"$f":"U1601*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3403198705206404E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.47449132334862226},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.0321918391034319E-3}]
["Single Family Detached",11604,"Mountain South","Before 1950","Brick","central furnace","central AC",19.869569821764056,16924.676169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16924.676169999999},"Hot-Dry/Mixed-Dry",270.2346119140754,"Metropolitan Area",0.3311850589622421,0.14793001359115179,0.22428384534240428,1.54769393704182E-2,0.21864158142423046,0.92204049932002863,321.762,592.69799999999998,{"$f":"T1605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4457176538115397E-3},{"$f":"U1605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0031221716606659E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33663077661605362},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23431506705901095}]
["Single Family Attached",11610,"South Atlantic","1990s","Stucco","central furnace","central AC",30.915458425650741,17156.19225,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17156.19225},"Mixed-Humid",130.53692040193877,"Metropolitan Area",0.42433069089707404,0.10726360206160501,9.53467393628325E-2,1.8530317468263748E-2,0.24946163784181047,0.87640267016332196,812.15099999999995,267.94400000000002,{"$f":"T1611*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3933418692029751E-2},{"$f":"U1611*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5968987762340001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43826410958910378},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.9943638139066496E-2}]
["Single Family Detached",11615,"West South Central","1980s","Wood","wood-burning stove","N/A",9.504761753492101,10560.846390000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10560.846390000001},"Hot-Humid",7.8361480234345988,"Rural",0,0.10322265253118872,0,0,5.9331500352342588E-2,0.16255415288353131,0,0,{"$f":"T1616*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1616*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",11620,"Middle Atlantic","Before 1950","Brick","central furnace","both central and individual units",97.359201753207543,37503.544589999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":37503.544589999998},"Cold/Very Cold",466.11944205256174,"Metropolitan Area",3.5893372282033731,0.89933274905552452,0.36078218627502584,0.13469945591249513,1.162317879691821,6.011770043225745,3180.66,410.98599999999999,{"$f":"T1621*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.11928602413562939},{"$f":"U1621*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.541343177686574E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.7086232523390024},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37619561805189156}]
["Single Family Detached",11622,"West North Central","1980s","Stone","central furnace","central AC",43.213523523530633,18498.939859999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18498.939859999999},"Mixed-Humid",116.71351139326174,"Metropolitan Area",0.51363697641567463,0.42393051132713327,5.0596579903665014E-2,1.207901227416602E-2,0.33811267138868306,1.326276739035156,514.47500000000002,138.482,{"$f":"T1623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5172420844734998E-3},{"$f":"U1623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5617701896925196E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52315421850014809},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.315835009335753E-2}]
["Multi-Family (5+ units)",11629,"East North Central","Before 1950","Brick","central furnace","central AC",26.938035968700063,29931.15108,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2380.7666321635497},"Cold/Very Cold",310.23638090619568,"Metropolitan Area",0.42829884776192501,0.32435673070885185,4.1726085891745208E-2,1.0829748946067759E-2,0.79969450832522404,1.6040445078894312,300.64800000000002,61.173999999999999,{"$f":"T1630*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1577272642670703E-4},{"$f":"U1630*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4564101795597298E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42901462048835171},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.187172690970118E-2}]
["Single Family Detached",11633,"West North Central","2000s","Wood","central furnace","central AC",58.174736841585684,26145.949140000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26145.949140000001},"Mixed-Humid",262.60957328777869,"Metropolitan Area",0.47913976107884865,0.69078784653970959,0.11392106406282594,2.6625648868871581E-2,0.76075994937956692,2.0446086210609513,816.29499999999996,202.05199999999999,{"$f":"T1634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1342807553236299E-2},{"$f":"U1634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.28284131563528E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.50048256863208496},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11920390537846122}]
["Multi-Family (5+ units)",11634,"West North Central","Before 1950","Siding","radiator","N/A",7.1549730174691435,10354.519560000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":823.61331826643539},"Cold/Very Cold",40.414787430277741,"Metropolitan Area",0.20058271094772384,0.18560863570331543,0,9.7126428924756004E-4,9.4020694327929616E-2,0.48110604951534974,93.801000000000002,0,{"$f":"T1635*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7255752866709911E-5},{"$f":"U1635*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20065996670059055},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",11639,"South Atlantic","2010s","Wood","built-in electric unit","both central and individual units",7.6841448101773242,8832.3503569999993,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":702.5377994090635},"Hot-Humid",43.866618795464994,"Metropolitan Area",1.3529297120998672E-2,4.0535957142896852E-2,3.3751204001059833E-2,1.1838352477501379E-3,6.076676476786786E-2,0.14967289432916736,0,134.03399999999999,{"$f":"T1640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4163951405994405E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3529297120998672E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.384536795246583E-2}]
["Single Family Attached",11645,"East South Central","1970s","Siding","central furnace","N/A",10.840402140850019,9559.4375139999993,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9559.4375139999993},"Mixed-Humid",23.885640747111282,"Metropolitan Area",2.8822602691836317E-2,1.9843566426498826E-2,0,4.1956371248945998E-4,3.2831639596457622E-2,8.1497808714792772E-2,43.89,0,{"$f":"T1646*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1956371248945998E-4},{"$f":"U1646*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9242166404325778E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",11648,"Middle Atlantic","Before 1950","Brick","radiator","window/wall unit",45.852372840848979,31775.726149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2527.486775516511},"Mixed-Humid",123.32159320536029,"Metropolitan Area",0.80852014336441891,1.1542906842041547,0.19321570285777304,3.4840494937167497E-3,0.28849534482145262,2.4477287984540141,109.645,0,{"$f":"T1649*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7712628750150783E-4},{"$f":"U1649*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80879726965192045},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19321570285777304}]
["Multi-Family (2-4 units)",11652,"Middle Atlantic","Before 1950","Brick","central furnace","window/wall unit",42.981272487388523,41608.201829999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13869.400609999999},"Mixed-Humid",74.506017859099373,"Metropolitan Area",1.6922459006430737,0.72343685384219225,1.6160833631781148E-2,7.31201734859505E-3,0.29076177590980101,2.7274800422592449,175.73500000000001,0,{"$f":"T1653*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4373391161983497E-3},{"$f":"U1653*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6946832397592719},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6160833631781148E-2}]
["Single Family Detached",11658,"East South Central","1970s","Siding","heat pump","central AC",25.080177943892167,12222.308940000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12222.308940000001},"Mixed-Humid",204.14834621053552,"Metropolitan Area",0.23368435022216741,0.12683494545463916,5.0352930589418643E-2,6.0518151600963003E-3,0.28568195136947933,0.69655417763570449,316.46600000000001,178.679,{"$f":"T1659*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8679452210060405E-3},{"$f":"U1659*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1838699390902602E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23755229544317344},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2536800528508905E-2}]
["Single Family Detached",11663,"East North Central","2000s","Siding","heat pump","central AC",53.680773684234147,16456.39904,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16456.39904},"Mixed-Humid",203.52872802508554,"Rural",0.21990745280188545,0.14826662600032259,0.10483369633682466,1.004747089027104E-2,0.22143222045493652,0.69443999559396918,273.31299999999999,337.238,{"$f":"T1664*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.49774779081952E-3},{"$f":"U1664*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5497230994515203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22440520059270497},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11038341943627618}]
["Single Family Detached",11668,"South Atlantic","1970s","Brick","portable electric heaters","central AC",65.41596094365751,27955.538860000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27955.538860000001},"Mixed-Humid",637.26093348141876,"Micropolitan Area",0.79283593925953255,0.34670308334262157,0.2770896541614703,1.4729801380872858E-2,0.75770561135111336,2.1743342881147378,0,526.90099999999995,{"$f":"T1669*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1669*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4729801380872858E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.79283593925953255},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.29181945554234318}]
["Single Family Detached",11672,"South Atlantic","1960s","Brick","heat pump","central AC",36.042714364989422,9578.186119,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9578.186119},"Mixed-Humid",274.03614799490066,"Metropolitan Area",0.3619763290590432,9.9579774815347522E-2,0.16341908450606921,1.5563077402712676E-2,0.31003614365674687,0.93501133203720688,721.24400000000003,903.60199999999998,{"$f":"T1673*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9082092692120366E-3},{"$f":"U1673*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6548681335006372E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36888453832825524},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17207395263956984}]
["Single Family Detached",11675,"South Atlantic","1960s","Stucco","N/A","central AC",41.096012177882862,27036.850119999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27036.850119999999},"Hot-Humid",348.04799413096538,"Metropolitan Area",0,0.11197503438833852,0.33289954445233694,1.7884416727927958E-2,0.74266515120118537,1.1875397300418609,0,661.48299999999995,{"$f":"T1676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7884416727927958E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35078396118026489}]
["Single Family Detached",11682,"West North Central","1980s","Brick","heat pump","central AC",59.234787042660706,15429.74395,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15429.74395},"Mixed-Humid",109.11084804643593,"Metropolitan Area",0.82190871536648136,0.25452854701764965,5.0069750563909249E-2,1.03058654385719E-2,0.31454844570310758,1.4410554586511479,496.96499999999997,170.95699999999999,{"$f":"T1683*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6680427021117497E-3},{"$f":"U1683*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6378227364601495E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.8295767580685931},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2707573300369397E-2}]
["Single Family Detached",11686,"Mountain South","2000s","Stucco","central furnace","central AC",32.129621740250442,15256.23065,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15256.23065},"Hot-Dry/Mixed-Dry",281.20095149249784,"Metropolitan Area",0.39788775875157417,0.19128315385777273,0.5206629309253672,2.9986045061421752E-2,0.48117759384972286,1.5910114373844371,236.52600000000001,1728.9690000000001,{"$f":"T1687*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6084952107219002E-3},{"$f":"U1687*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6377549850699851E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.40149625396229605},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.54704048077606704}]
["Multi-Family (5+ units)",11687,"Pacific","1990s","Stucco","central furnace","central AC",15.682251641015949,13977.051369999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1111.7546875758787},"Hot-Dry/Mixed-Dry",62.675642181919947,"Metropolitan Area",1.9008851016334039E-2,9.2671861996843186E-2,2.0574280870734925E-2,1.1973161515083099E-3,0.29128084204246091,0.42463791583607957,16.888999999999999,68.774000000000001,{"$f":"T1688*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8776424918469017E-5},{"$f":"U1688*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6459816883343488E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9027627441252509E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0650740687618269E-2}]
["Single Family Detached",11693,"East North Central","2000s","Brick","central furnace","central AC",34.132778394376835,14918.17238,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14918.17238},"Cold/Very Cold",233.16651401759461,"Metropolitan Area",1.5292051765369286,0.15213759555720083,9.4589388047664244E-2,3.3013617113492398E-2,0.67948509844191263,2.4554172585837062,1900.421,312.55900000000003,{"$f":"T1694*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8350808072571981E-2},{"$f":"U1694*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6628090409204202E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5575559846095006},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.9252197088584668E-2}]
["Single Family Detached",11696,"New England","1980s","Wood","radiator","window/wall unit",128.00458298612617,32754.499230000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32754.499230000001},"Cold/Very Cold",499.2058527446751,"Metropolitan Area",2.680328971878235,0.56169655687351339,0.11045328110543989,3.31491909457215E-3,1.5895221957621617,4.9420010056193497,101.205,0,{"$f":"T1697*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.31491909457215E-3},{"$f":"U1697*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6836438909728071},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11045328110543989}]
["Single Family Attached",11704,"Pacific","1950s","Siding","central furnace","central AC",19.315407085920636,12911.36837,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12911.36837},"Hot-Dry/Mixed-Dry",108.21879021632829,"Metropolitan Area",0.32694036581693464,0.17467404217858734,0.12744581895670015,1.4846808311399741E-2,0.27884794597593832,0.9079081729281604,701.63300000000004,448.26900000000001,{"$f":"T1705*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0590421235482096E-3},{"$f":"U1705*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7877661878515301E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33599940794048283},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13323358514455169}]
["Single Family Detached",11705,"East North Central","1990s","Siding","central furnace","central AC",43.295612965405915,16035.41221,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16035.41221},"Mixed-Humid",199.43598150993768,"Micropolitan Area",0.59659379105741728,0.41351623909369489,9.8177340424327922E-2,1.7910240534768779E-2,0.54749622920918273,1.6557835997846229,782.82899999999995,334.089,{"$f":"T1706*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.255298570494209E-2},{"$f":"U1706*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3572548298266905E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6091467767623594},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10353459525415461}]
["Mobile Home",11711,"East North Central","1980s","Siding","central furnace","window/wall unit",30.540600617499376,32559.275710000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32559.275710000002},"Mixed-Humid",412.08383574278338,"Rural",0.90245768714173702,0.79341393780978742,7.4463324022975688E-2,6.5058642352693605E-3,0.65441389662374927,2.4247488455982493,199.816,0,{"$f":"T1712*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5058642352693605E-3},{"$f":"U1712*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.90896355137700635},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4463324022975688E-2}]
["Single Family Attached",11716,"Pacific","1980s","Siding","heat pump","N/A",5.9853459748588271,6840.3954000000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6840.3954000000003},"Marine",101.03969250327425,"Metropolitan Area",4.4847171331365003E-2,5.6586124366003805E-2,0,7.1226301142040009E-4,0.24331414353193981,0.34474743922930862,104.126,0,{"$f":"T1717*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1226301142040009E-4},{"$f":"U1717*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.55594343427854E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11720,"Pacific","1970s","Stucco","central furnace","N/A",20.137318319680215,25652.6348,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25652.6348},"Hot-Dry/Mixed-Dry",138.41063806465428,"Metropolitan Area",0.14237458579294079,0.69352583107149157,0.12976959932599522,1.4069187556059999E-3,0.39434464106293882,1.3600146572533665,54.844999999999999,0,{"$f":"T1721*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4069187556059999E-3},{"$f":"U1721*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1437815045485468},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12976959932599522}]
["Single Family Detached",11723,"Pacific","1990s","Wood","built-in electric unit","window/wall unit",25.73779034608571,14362.60622,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14362.60622},"Marine",465.48488628429953,"Metropolitan Area",0.56821642906034009,0.4985441013296123,1.3066653898163179E-2,0,0.5084072477234356,1.5882344320115511,0,0,{"$f":"T1724*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1724*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.56821642906034009},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3066653898163179E-2}]
["Multi-Family (5+ units)",11730,"Pacific","2000s","Brick","built-in electric unit","central AC",13.389195029438071,24255.788100000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1929.3401309880296},"Hot-Dry/Mixed-Dry",157.39580896018776,"Metropolitan Area",1.1870782696140001E-2,0.25744659310733009,1.9128435405362115E-2,8.0451597970079998E-4,0.24781255791083157,0.53699889274590007,0,33.167999999999999,{"$f":"T1731*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1731*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3992353464610967E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1870782696140001E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9192427758826725E-2}]
["Single Family Attached",11734,"Middle Atlantic","Before 1950","Brick","radiator","window/wall unit",67.066232510908236,38323.561430000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38323.561430000002},"Mixed-Humid",170.12963298328276,"Metropolitan Area",3.7003334666988441,1.3624177466432648,0.13577225355146685,4.1833616421373702E-3,0.95124080694026658,6.1497642738338429,109.15900000000001,0,{"$f":"T1735*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1833616421373702E-3},{"$f":"U1735*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.7045168283409815},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13577225355146685}]
["Mobile Home",11739,"South Atlantic","2000s","Wood","heat pump","central AC",19.575133009844997,26888.918969999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26888.918969999999},"Hot-Humid",413.90268925584974,"Metropolitan Area",5.1892790275608149E-2,0.1861763473898968,0.5732683375476908,1.9656471990044246E-2,0.60089855712477469,1.4122360323379706,14.885,716.14,{"$f":"T1740*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0024155886845002E-4},{"$f":"U1740*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9256230431175799E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.2293031834476596E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.59252456797886655}]
["Single Family Detached",11744,"Pacific","1960s","Stucco","central furnace","N/A",72.360661315244798,14901.2894,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14901.2894},"Marine",103.44326086991306,"Metropolitan Area",0.24427643479938618,0.12429916513525761,0,8.5348327141652001E-3,0.43074459888236077,0.79932019881700456,572.75800000000004,0,{"$f":"T1745*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.5348327141652001E-3},{"$f":"U1745*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25281126751355137},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11746,"Mountain North","Before 1950","Wood","central furnace","window/wall unit",43.719794466765414,24728.39054,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24728.39054},"Cold/Very Cold",301.11123162603508,"Metropolitan Area",0.58578898887276953,0.1603291165470967,3.7782681004799777E-2,7.5929759572597004E-3,0.24349071866150726,1.0273915050861733,307.05500000000001,0,{"$f":"T1747*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5929759572597004E-3},{"$f":"U1747*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59338196483002925},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7782681004799777E-2}]
["Single Family Detached",11749,"West South Central","2010s","Brick","central furnace","central AC",291.3281544768476,65261.683349999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":65261.683349999999},"Hot-Humid",825.33050799735872,"Metropolitan Area",2.037946425522188,1.4140247626210833,1.153832957272968,0.114663472412283,1.8716999880666991,6.4775041334829391,487.714,1269.2660000000001,{"$f":"T1750*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1829036633361896E-2},{"$f":"U1750*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2834435778921092E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0697754621555498},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.236667393051889}]
["Single Family Attached",11757,"South Atlantic","Before 1950","Brick","central furnace","window/wall unit",27.147175280444959,13191.047269999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13191.047269999999},"Mixed-Humid",142.21773278260906,"Metropolitan Area",0.68925910321183625,0.14676058436724246,0.10258953154766942,1.00732113372628E-2,0.15027500913615227,1.0888842282629003,763.64,0,{"$f":"T1758*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.00732113372628E-2},{"$f":"U1758*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.69933231454909905},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10258953154766942}]
["Single Family Detached",11759,"Middle Atlantic","Before 1950","Brick","central furnace","window/wall unit",134.12872906742999,38191.55156,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38191.55156},"Cold/Very Cold",335.21217472405539,"Metropolitan Area",0.22326147062220103,0,8.9945763293090314E-2,0.22326147062220103,0.8305367006871085,1.1437439346023999,5845.8339999999998,0,{"$f":"T1760*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.22326147062220103},{"$f":"U1760*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44652294124440206},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.9945763293090314E-2}]
["Single Family Detached",11764,"East South Central","Before 1950","Stone","heater burning gas/oil/kerosene","central AC",47.696971146319342,28458.813330000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28458.813330000001},"Hot-Humid",385.43387357649999,"Micropolitan Area",1.1674653585191366,0.39955283154462773,0.57537974718848672,2.4269277584437379E-2,0.93187595939955759,3.0742738966518086,0,852.78599999999994,{"$f":"T1765*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1765*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4269277584437379E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1674653585191366},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.59964902477292414}]
["Single Family Detached",11769,"South Atlantic","1960s","Concrete","heat pump","central AC",23.434093207313055,17753.100910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17753.100910000001},"Hot-Humid",243.55764969707133,"Metropolitan Area",3.4056128537671205E-3,0.15398966941620273,0.44501327011287978,2.1382686884847683E-2,0.22861016002584839,0.83101871240869796,3.1509999999999998,1201.297,{"$f":"T1770*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5940020967409995E-5},{"$f":"U1770*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1326746863880273E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.4615528747345306E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46634001697676003}]
["Single Family Detached",11775,"Pacific","1960s","Wood","heat pump","central AC",28.199422193090907,10514.32595,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10514.32595},"Marine",135.78110106311237,"Metropolitan Area",0.25094889769053946,7.4654616198962201E-2,2.6135922644256803E-2,7.5181531129620499E-3,0.11154567440045184,0.46328511093421032,596.49900000000002,118.54,{"$f":"T1776*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2717849148490505E-3},{"$f":"U1776*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.246368198113E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2572206826053885},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7382290842369802E-2}]
["Single Family Attached",11776,"South Atlantic","2000s","Brick","heat pump","central AC",20.321181450062863,20341.522970000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20341.522970000002},"Mixed-Humid",159.65733883016011,"Metropolitan Area",0.1312829077324329,0.17813443914699353,8.1466843443270417E-2,5.7223551927825808E-3,0.15386663609637005,0.54475082641906691,107.79600000000001,173.518,{"$f":"T1777*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1927348100741202E-3},{"$f":"U1777*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5296203827084606E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13347564254250702},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.4996463825978877E-2}]
["Single Family Detached",11783,"South Atlantic","1950s","Brick","central furnace","central AC",66.931325687657704,22133.374899999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22133.374899999999},"Mixed-Humid",381.08452522337763,"Metropolitan Area",1.5960563003406656,0.52331764279499249,0.29109447254456661,7.0421891719579396E-2,0.42944778650660276,2.8399162021868274,2548.21,633.49599999999998,{"$f":"T1784*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6400487253928995E-2},{"$f":"U1784*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4021404465650398E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6524567875945946},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30511587701021703}]
["Single Family Detached",11787,"Mountain South","2000s","Stucco","other","central AC",22.779133327488129,6189.981882,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6189.981882},"Cold/Very Cold",39.953058550925441,"Metropolitan Area",0.4093473148854993,0.10156557554882328,4.5371100169353973E-2,1.3815606261892261E-3,9.2157446846298938E-2,0.64844143744997551,0,223.19300000000001,{"$f":"T1788*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1788*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3815606261892261E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4093473148854993},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.6752660795543202E-2}]
["Single Family Detached",11792,"New England","1980s","Wood","central furnace","N/A",33.269005442407959,12032.19003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12032.19003},"Cold/Very Cold",67.444455920983657,"Metropolitan Area",0.94898971679807709,0.31459590257610559,0,1.0986580684202971E-2,0.19796212119629145,1.461547740570474,913.09900000000005,0,{"$f":"T1793*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0986580684202971E-2},{"$f":"U1793*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95997629748228008},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11794,"Middle Atlantic","2000s","Brick","central furnace","central AC",88.443291954706794,21624.276760000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21624.276760000001},"Cold/Very Cold",163.74936004268804,"Metropolitan Area",3.0782872001478618,0.16583670821810056,5.364492193073548E-2,2.2225950636570242E-2,0.68784571123921534,3.9856145415359134,893.90800000000002,133.916,{"$f":"T1795*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9330113989978082E-2},{"$f":"U1795*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8958366465921602E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0976173141378398},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.6540758577327641E-2}]
["Mobile Home",11802,"Pacific","1980s","Shingle","portable electric heaters","N/A",4.2360456482568205,8899.2555639999991,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8899.2555639999991},"Marine",54.356652982253493,"Metropolitan Area",2.4638834924712957E-2,0.11574877264254432,0,0,7.3358023091964486E-2,0.21374563065922178,0,0,{"$f":"T1803*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1803*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4638834924712957E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11805,"South Atlantic","2000s","Concrete","N/A","central AC",27.735503895714309,25896.829030000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25896.829030000001},"Hot-Humid",305.2604001544932,"Metropolitan Area",0,0.19785956873473806,0.36509624072881719,1.6103787751331321E-2,0.47859266771519815,1.0415484771787535,0,621.84400000000005,{"$f":"T1806*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1806*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6103787751331321E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3812000284801485}]
["Single Family Detached",11810,"Mountain South","2000s","Stucco","central furnace","N/A",9.2360439137999659,6668.6237639999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6668.6237639999999},"Hot-Dry/Mixed-Dry",35.383290902391437,"Metropolitan Area",0.13951199709731668,0.12796317443346505,3.8550040272545077E-2,4.0460474277079564E-3,9.6901745240188894E-2,0.40292695704351572,606.72900000000004,0,{"$f":"T1811*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0460474277079564E-3},{"$f":"U1811*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14355804452502463},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8550040272545077E-2}]
["Single Family Detached",11811,"West North Central","1960s","Siding","central furnace","central AC",58.273397650185814,21236.660950000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21236.660950000001},"Cold/Very Cold",308.3138436900137,"Rural",2.401940702994986,0.45952046238567129,7.6274271041170419E-2,4.3913209985731907E-2,0.29733459614425467,3.2350700325660826,1880.5170000000001,187.285,{"$f":"T1812*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9935901939711152E-2},{"$f":"U1812*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9773080460207503E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4418766049346972},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.0251579087191174E-2}]
["Mobile Home",11817,"South Atlantic","Before 1950","Siding","heat pump","central AC",29.763798271565541,32211.902890000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32211.902890000001},"Mixed-Humid",48.66261833360268,"Micropolitan Area",2.8997412676801122E-2,5.7543375534598894E-2,1.6902616227275482E-2,8.8176862971085996E-4,6.2593461033984429E-2,0.16603686547265992,9.2609999999999992,18.113,{"$f":"T1818*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9831443266429002E-4},{"$f":"U1818*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8345419704656999E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9295727109465413E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7486070424322053E-2}]
["Multi-Family (5+ units)",11821,"East North Central","1980s","Brick","radiator","N/A",5.7673242979191937,10012.71579,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":796.42575677945138},"Cold/Very Cold",27.134459804446205,"Metropolitan Area",9.2353749679509572E-2,0.10809528713839778,0,7.1240472845850015E-4,9.1885190897461499E-2,0.29298996675123251,71.150000000000006,0,{"$f":"T1822*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6665692594857964E-5},{"$f":"U1822*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.2410415372104426E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11828,"West South Central","1990s","Siding","central furnace","central AC",18.095682898324327,9554.2148350000007,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9554.2148350000007},"Mixed-Humid",277.41991765985131,"Metropolitan Area",0.36554846344162739,0.21373756937494109,5.6390982341285353E-2,9.2925153364545147E-3,0.3108797334207139,0.94655674857856775,684.33199999999999,288.27699999999999,{"$f":"T1829*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5382549464652207E-3},{"$f":"U1829*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7542603899892949E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3720867183880926},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9145242731274646E-2}]
["Single Family Detached",11831,"West North Central","1980s","Siding","central furnace","central AC",83.127577946925967,13349.538769999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13349.538769999999},"Cold/Very Cold",257.57756180993925,"Metropolitan Area",1.4422416771288948,0.21582411587125441,4.8290728342908158E-2,7.2471976074576006E-2,0.56371092024263481,2.2700674415856925,5181.8469999999998,246.953,{"$f":"T1832*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9175267426708181E-2},{"$f":"U1832*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2967086478678099E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5114169445556029},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.1587436990775969E-2}]
["Single Family Detached",11835,"West North Central","Before 1950","Stucco","central furnace","central AC",56.108212932441766,18052.83556,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18052.83556},"Mixed-Humid",94.789193264664448,"Metropolitan Area",0.84697067838693429,0.348157057550602,0.10126192911748087,2.7835378304595038E-2,0.25743533063333368,1.553824995688351,1234.595,307.28899999999999,{"$f":"T1836*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2287940518198199E-2},{"$f":"U1836*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5474377863968397E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.86925861890513245},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10680936690387771}]
["Single Family Detached",11841,"Middle Atlantic","1950s","Brick","central furnace","central AC",66.41835502166829,29730.687119999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29730.687119999999},"Cold/Very Cold",274.83145283169978,"Metropolitan Area",1.7421532442192684,0.47187859817991523,0.12611686122654914,4.5692290306175762E-2,0.503635045128211,2.8437837487539439,1324.1210000000001,212.75200000000001,{"$f":"T1842*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9367027160021523E-2},{"$f":"U1842*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.32526314615424E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7815202713792899},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13244212437270339}]
["Multi-Family (5+ units)",11846,"New England","Before 1950","Wood","wood-burning stove","N/A",14.003850885676133,28463.111560000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2263.9966658307549},"Cold/Very Cold",58.267234150365873,"Rural",0.29391102914323736,0.3564803773322387,0,8.9531571305326799E-3,0.18985461826440048,0.84848703492718203,314.553,0,{"$f":"T1847*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1214694322706143E-4},{"$f":"U1847*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29462317608646443},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",11847,"East South Central","1990s","Siding","central furnace","central AC",39.890331222988976,20994.911169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20994.911169999999},"Mixed-Humid",288.4770707811399,"Metropolitan Area",0.35231585628270407,0.19949687915366018,0.15076989479376302,1.3740728467630432E-2,0.28170115215530267,0.98428378238542991,296.45499999999998,358.024,{"$f":"T1848*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.22404639090235E-3},{"$f":"U1848*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5166820767280798E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35853990267360641},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15828657687049111}]
["Single Family Detached",11855,"Middle Atlantic","1970s","Siding","radiator","central AC",50.897342698001921,13700.49602,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13700.49602},"Mixed-Humid",111.92903820222482,"Metropolitan Area",1.147453464511774,0.19416799186061467,0.10289250617468261,7.8268604677936594E-3,0.27674160749944327,1.7212555700465149,165.524,405.75900000000001,{"$f":"T1856*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2677609032144804E-3},{"$f":"U1856*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5590995645791808E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1497212254149884},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1084516057392618}]
["Multi-Family (2-4 units)",11858,"West South Central","1970s","Wood","N/A","central AC",51.79768993266179,37399.054100000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12466.351366666668},"Hot-Humid",297.84479530849154,"Rural",0,0.16473127700278309,0.5847532594383883,1.8636995831544798E-2,0.25433727888029956,1.0162464792091674,0,498.32799999999997,{"$f":"T1859*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1859*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2123319438482675E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.59096559138223659}]
["Single Family Detached",11860,"Mountain South","1970s","Stucco","central furnace","N/A",68.170120873112836,20707.813139999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20707.813139999998},"Hot-Dry/Mixed-Dry",175.58394976219475,"Metropolitan Area",0.62444932360561123,0.36998024361281168,0.11790662273623422,4.9183706807581919E-2,0.43200206979373384,1.544338259748391,2375.1280000000002,0,{"$f":"T1861*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9183706807581919E-2},{"$f":"U1861*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.67363303041319311},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11790662273623422}]
["Single Family Detached",11865,"West North Central","Before 1950","Siding","central furnace","central AC",124.11443923353761,22517.133389999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22517.133389999999},"Cold/Very Cold",87.311040362252001,"Metropolitan Area",2.3363103217318972,0.22166798318438344,6.471228237225507E-2,3.5880984505564831E-2,0.2629451086383281,2.8856356959268639,1425.1130000000001,168.38399999999999,{"$f":"T1866*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2089459516823071E-2},{"$f":"U1866*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7915249887417596E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3683997812487201},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.850380736099683E-2}]
["Single Family Detached",11869,"West South Central","2000s","Brick","heat pump","central AC",35.702992607402564,12917.14638,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12917.14638},"Hot-Humid",269.33522551087617,"Metropolitan Area",0.15514987316216164,6.8205542581506545E-2,0.28643482753571092,1.9008265506928142E-2,0.40918153523493367,0.91897177851431278,221.91900000000001,1249.634,{"$f":"T1870*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8665602075032201E-3},{"$f":"U1870*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6141705299424922E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15801643336966487},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30257653283513586}]
["Single Family Detached",11876,"South Atlantic","2000s","Stucco","heat pump","central AC",53.088499520274816,25896.829030000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25896.829030000001},"Hot-Humid",319.96472326747374,"Metropolitan Area",2.187163310020904E-2,0.15462344013721444,0.29081328429941367,1.6237415389126122E-2,0.62441131546635797,1.0917196730031951,15.077,611.92700000000002,{"$f":"T1877*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9044649128531004E-4},{"$f":"U1877*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5846968897840812E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2262079591494351E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30666025319725448}]
["Single Family Detached",11881,"New England","Before 1950","Wood","radiator","window/wall unit",16.212097202707039,10445.938920000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10445.938920000001},"Cold/Very Cold",50.216678599095324,"Metropolitan Area",1.3175520734757007,0.10728848372958144,1.0697592034521719E-2,1.91114720104752E-3,0.14740749101577902,1.5829456402555828,182.95599999999999,0,{"$f":"T1882*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.91114720104752E-3},{"$f":"U1882*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3194632206767483},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0697592034521719E-2}]
["Single Family Detached",11884,"South Atlantic","1960s","Siding","heat pump","central AC",88.043509328851528,32512.374199999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32512.374199999998},"Mixed-Humid",597.09443393268157,"Metropolitan Area",0.92020936641256357,0.32737031454484578,0.23725417386837,2.9874482719282999E-2,0.73647553487064599,2.2213093896964256,551.50300000000004,367.36200000000002,{"$f":"T1885*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.79306719084226E-2},{"$f":"U1885*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1943810810860401E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.93814003832098614},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24919798467923041}]
["Single Family Detached",11888,"South Atlantic","2000s","Siding","heat pump","central AC",24.6326727953115,10947.854579999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10947.854579999999},"Mixed-Humid",142.63888565616972,"Micropolitan Area",0.18575277415587982,6.6747788475274128E-2,7.5229879663929897E-2,7.2461988329741399E-3,0.15895345524237037,0.48668389753745422,313.17500000000001,348.70800000000003,{"$f":"T1889*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4285943580915001E-3},{"$f":"U1889*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8176044748826398E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18918136851397133},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9047484138812532E-2}]
["Single Family Detached",11893,"Mountain North","1980s","Siding","central furnace","N/A",100.00703670871742,12522.79448,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12522.79448},"Cold/Very Cold",142.09606129283242,"Metropolitan Area",0.85472047060967948,0.47894468132981288,5.3117048227407919E-2,2.958564043916264E-2,0.43617970134165285,1.8229619015085532,2362.5430000000001,0,{"$f":"T1894*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.958564043916264E-2},{"$f":"U1894*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88430611104884216},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.3117048227407919E-2}]
["Mobile Home",11899,"East South Central","2000s","Siding","portable electric heaters","N/A",69.675383069626591,31902.647929999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31902.647929999999},"Mixed-Humid",707.36752263465144,"Micropolitan Area",0.62842352715410466,0.88456813273843848,0,0,0.90054635063564303,2.4135380105281863,0,0,{"$f":"T1900*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1900*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62842352715410466},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",11903,"Pacific","1970s","Stucco","wood-burning stove","central AC",24.551420442509151,7981.6061259999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7981.6061259999997},"Marine",152.14164057553393,"Metropolitan Area",3.7078303828543088E-2,0.19694135815858663,1.1338134894985157E-2,5.6370891425487602E-4,0.27374947133394228,0.51910726821605713,0,70.626000000000005,{"$f":"T1904*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1904*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6370891425487602E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.7078303828543088E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1901843809240033E-2}]
["Multi-Family (5+ units)",11906,"Middle Atlantic","1950s","Brick","radiator","window/wall unit",28.424070276858235,36487.895089999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2902.2994430108038},"Mixed-Humid",112.98684696315442,"Metropolitan Area",0.66609014384998655,0.95618331585362437,5.6657308858899295E-2,3.6997266105456401E-3,0.36778550364707924,2.0501217172658115,101.396,0,{"$f":"T1907*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9428155432352347E-4},{"$f":"U1907*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.66638442540431009},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.6657308858899295E-2}]
["Multi-Family (2-4 units)",11913,"Middle Atlantic","Before 1950","Brick","central furnace","window/wall unit",81.559811021263542,63520.102039999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21173.367346666666},"Cold/Very Cold",450.16696316798652,"Metropolitan Area",5.5742500234433621,0.84266936136141524,0.1020113782731788,4.6588628280931875E-2,0.74653238564499858,7.296522234243576,733.447,0,{"$f":"T1914*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5529542760310626E-2},{"$f":"U1914*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.5897795662036724},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1020113782731788}]
["Single Family Detached",11917,"West South Central","1950s","Siding","wood-burning stove","window/wall unit",22.977922285404443,18456.162479999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18456.162479999999},"Mixed-Humid",125.39487756579692,"Micropolitan Area",0.11535937614160344,0.1032277160517624,0.10058442446137679,0,0.10867580911039609,0.42784732576513868,0,0,{"$f":"T1918*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1918*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11535937614160344},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10058442446137679}]
["Multi-Family (5+ units)",11918,"East North Central","Before 1950","Siding","built-in electric unit","window/wall unit",13.206735309662072,17308.958470000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1376.7793511428379},"Cold/Very Cold",120.97231071982729,"Metropolitan Area",0.16306657266356944,9.6590167560773793E-2,2.1216888568564254E-2,0,0.13187579488271253,0.41274942367562001,0,0,{"$f":"T1919*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1919*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16306657266356944},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1216888568564254E-2}]
["Single Family Detached",11922,"South Atlantic","1990s","Stucco","heat pump","central AC",107.47780545127831,30072.133590000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30072.133590000001},"Hot-Humid",644.16281398819024,"Metropolitan Area",5.6277471954463448E-2,0.2987233132721468,0.95155165312765866,6.1301112087073714E-2,0.89133112301687434,2.1978835613711434,37.622,2000.847,{"$f":"T1923*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1313738099229802E-3},{"$f":"U1923*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0169738277150733E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.7408845764386429E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0117213914048093}]
["Multi-Family (2-4 units)",11929,"West North Central","1950s","Siding","radiator","window/wall unit",15.090244500178132,19471.283230000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6490.4277433333336},"Cold/Very Cold",189.72818375449771,"Metropolitan Area",0.28285882522884603,0.13879335134817916,3.4753942954128862E-2,1.6515931861350601E-3,0.34838138729943707,0.80588856895468119,84.822000000000003,0,{"$f":"T1930*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.505310620450201E-4},{"$f":"U1930*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28340935629089103},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4753942954128862E-2}]
["Single Family Detached",11932,"East North Central","Before 1950","Siding","central furnace","window/wall unit",42.912270525618261,18409.382460000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18409.382460000001},"Cold/Very Cold",221.11899557466853,"Metropolitan Area",1.5596578672485224,0.30751361989130038,6.0462487094851802E-2,4.1186133177280558E-2,0.38727812358287261,2.3149120978175475,2237.2359999999999,0,{"$f":"T1933*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1186133177280558E-2},{"$f":"U1933*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6008440004258029},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0462487094851802E-2}]
["Single Family Detached",11936,"Pacific","1950s","Stucco","central furnace","central AC",26.956978560898193,16869.198100000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16869.198100000001},"Hot-Dry/Mixed-Dry",415.3065160719741,"Metropolitan Area",0.62241755597509085,0.14435235973660362,0.18915573530794041,1.9150554712647802E-2,1.3073075555186284,2.2632332065382634,607.06600000000003,528.17200000000003,{"$f":"T1937*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0240716613774601E-2},{"$f":"U1937*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9098380988732011E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63265827258886542},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19806557340681361}]
["Single Family Detached",11941,"South Atlantic","1950s","Siding","heat pump","central AC",34.205390242086729,20097.174060000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20097.174060000001},"Mixed-Humid",177.66036515933777,"Micropolitan Area",0.17336766911336821,9.7814594118292922E-2,0.12583779216994603,8.7076432851946207E-3,0.2091570784285493,0.60617713383015648,142.227,291.05,{"$f":"T1942*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8583607750316204E-3},{"$f":"U1942*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8492825101630012E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17622602988839983},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13168707468010904}]
["Mobile Home",11947,"West North Central","1970s","Siding","radiator","central AC",13.884998437065585,11609.53047,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11609.53047},"Cold/Very Cold",50.753697794546326,"Metropolitan Area",0.81803843309584168,0.1212350760296784,2.9635613602177591E-2,4.0013756003816096E-3,0.14053834682792163,1.1094474695556193,258.20699999999999,86.456000000000003,{"$f":"T1948*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9976620340672901E-3},{"$f":"U1948*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0037135663143199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.82103609512990894},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0639327168491909E-2}]
["Multi-Family (2-4 units)",11952,"South Atlantic","Before 1950","Brick","central furnace","window/wall unit",33.534546204264828,23483.575769999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7827.8585899999998},"Mixed-Humid",157.2950101170444,"Metropolitan Area",0.58324365343117757,0.33037225122048403,0.21304717946192706,1.294644835484946E-2,0.31069693648237728,1.4459909861658657,551.298,0,{"$f":"T1953*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3154827849498194E-3},{"$f":"U1953*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58755913621612743},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21304717946192706}]
["Single Family Detached",11956,"East North Central","2000s","Brick","central furnace","central AC",80.298864774984096,15341.777760000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15341.777760000001},"Cold/Very Cold",126.28997053685633,"Metropolitan Area",1.2210575689330605,0.4881678968774309,3.8592149904613439E-2,3.6971659286935681E-2,0.3736018827452991,2.121419498460404,2265.5070000000001,144.36099999999999,{"$f":"T1957*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4756904907724318E-2},{"$f":"U1957*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.21475437921136E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2558144738407848},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.0806904283824802E-2}]
["Multi-Family (5+ units)",11959,"Pacific","1970s","Concrete","N/A","central AC",17.490688993540896,21540.257379999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1713.3429276225029},"Hot-Humid",198.32114970878209,"Metropolitan Area",0,0.23415562957631486,0.28265876256079553,1.2559262467982798E-2,0.40448224225314655,0.93285691513086022,0,583.05999999999995,{"$f":"T1960*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U1960*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9898172737957641E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28365774428817508}]
["Multi-Family (2-4 units)",11965,"Middle Atlantic","1990s","Brick","heat pump","window/wall unit",35.824882971313194,40525.885710000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13508.628570000001},"Mixed-Humid",523.67549519831346,"Metropolitan Area",0.21604230796069585,0.73059880338913741,7.8245151205153962E-2,3.5990228581336808E-3,0.75946016394111382,1.7867457750681901,88.808000000000007,0,{"$f":"T1966*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1996742860445602E-3},{"$f":"U1966*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21724198224674041},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.8245151205153962E-2}]
["Single Family Detached",11970,"West South Central","1970s","Brick","central furnace","central AC",41.825004698345495,22657.098969999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22657.098969999999},"Mixed-Humid",198.19630383232283,"Metropolitan Area",1.484329336345946,0.34769285005655592,0.23339610090822793,3.8858873244061412E-2,0.32450840710802886,2.3899266944187589,1222.4939999999999,492.59199999999998,{"$f":"T1971*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7698167548231178E-2},{"$f":"U1971*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1160705695830239E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5120275038941773},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24455680660405818}]
["Multi-Family (5+ units)",11975,"New England","Before 1950","Brick","central furnace","window/wall unit",23.447694704687187,27488.504929999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2186.4750583928171},"Cold/Very Cold",36.312315011596446,"Metropolitan Area",0.73682371590569729,0.48771161005395303,4.5208667259570262E-2,1.1925228139762181E-2,0.1064115760896709,1.3871322477199715,433.82600000000002,0,{"$f":"T1976*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.485497286823223E-4},{"$f":"U1976*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.73777226563437959},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.5208667259570262E-2}]
["Single Family Detached",11977,"West South Central","2010s","Siding","central furnace","central AC",35.78209463934683,14725.14183,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14725.14183},"Hot-Humid",133.70333065395789,"Rural",0.32827575926990565,7.9152408282202921E-2,5.6841256235074508E-2,7.9454803794823808E-3,0.35051754117387296,0.81478696496105596,280.71699999999998,258.86900000000003,{"$f":"T1978*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1335976390921101E-3},{"$f":"U1978*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8118827403902703E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33240935690899776},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0653138975464781E-2}]
["Single Family Detached",11980,"Pacific","1980s","Stucco","central furnace","both central and individual units",26.668948942620993,17499.31033,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17499.31033},"Hot-Dry/Mixed-Dry",147.48705734648053,"Metropolitan Area",8.150986259300369E-2,0.25766084275960882,6.6870219559890975E-2,3.9286826656366501E-3,0.60050435586221262,1.0065452807747162,63.307000000000002,161.19800000000001,{"$f":"T1981*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.10782883906131E-3},{"$f":"U1981*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8208538265753402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.2617691432065002E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.969107338646631E-2}]
["Multi-Family (2-4 units)",11988,"Middle Atlantic","1960s","Siding","central furnace","window/wall unit",9.5088514991300528,14150.076639999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4716.6922133333328},"Mixed-Humid",80.982275293107463,"Metropolitan Area",0.2956042466758016,0.23930602538529677,4.7476988046053437E-2,6.7736275374913595E-3,0.25409551568850519,0.84099852748731796,478.69900000000001,0,{"$f":"T1989*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2578758458304529E-3},{"$f":"U1989*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29786212252163202},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7476988046053437E-2}]
["Single Family Detached",11989,"West South Central","1960s","Siding","central furnace","central AC",34.215308289098267,18151.357179999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18151.357179999999},"Mixed-Humid",180.50270459260184,"Micropolitan Area",1.5055184709668632,0.2751376368369387,0.25385600550581899,4.0723332190331557E-2,0.37639249612963488,2.4109046094392559,1561.6569999999999,681.88499999999999,{"$f":"T1990*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8346193999647256E-2},{"$f":"U1990*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2377138190684299E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5338646649665104},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2662331436965033}]
["Single Family Detached",11994,"West North Central","1960s","Brick","radiator","window/wall unit",45.750844147962795,10386.11672,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10386.11672},"Cold/Very Cold",265.832480863282,"Metropolitan Area",1.3942551267912338,0.10125798051918249,1.9629854075850481E-2,1.3824959965992002E-3,0.19273391125291681,1.7078768726391835,133.11000000000001,0,{"$f":"T1995*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3824959965992002E-3},{"$f":"U1995*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3956376227878329},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9629854075850481E-2}]
["Single Family Detached",12000,"West South Central","Before 1950","Stucco","built-in furnace","window/wall unit",37.067008380465936,20036.22075,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20036.22075},"Hot-Humid",92.988100483103992,"Metropolitan Area",1.1414442613555802,0.16359652383635925,0.17670968933927403,0,0.27104572659098031,1.7527962011221936,0,0,{"$f":"T2001*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2001*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1414442613555802},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17670968933927403}]
["Single Family Detached",12004,"East North Central","1950s","Siding","central furnace","central AC",59.150948587161338,19651.477940000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19651.477940000001},"Cold/Very Cold",437.81295806027714,"Metropolitan Area",1.7456484298351187,0.72932351250272753,0.16198502995128042,0.11416752101239312,0.86406819432348492,3.5010251666126111,5436.5330000000004,373.08199999999999,{"$f":"T2005*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.10683590831958203},{"$f":"U2005*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3316126928110806E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8524843381547007},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16931664264409149}]
["Single Family Detached",12007,"South Atlantic","1980s","Brick","central furnace","central AC",25.008747520629221,18443.029149999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18443.029149999998},"Mixed-Humid",415.39450326739808,"Micropolitan Area",0.61851440732959606,0.11921284487002344,0.18634666977291819,1.8514200799489847E-2,0.4932521197971686,1.4173260417697062,543.48099999999999,460.37799999999999,{"$f":"T2008*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.002343592547115E-2},{"$f":"U2008*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.490764874018699E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62853784325506723},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1948374346469369}]
["Single Family Detached",12014,"West South Central","2000s","Siding","central furnace","central AC",40.273663713502842,22287.58368,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22287.58368},"Mixed-Humid",472.74193748041438,"Micropolitan Area",0.86332490998995548,0.20745071157299041,0.12306196309313663,1.8726674147862717E-2,0.41913713384919765,1.6129747185052801,582.37699999999995,257.85199999999998,{"$f":"T2015*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2979776120807359E-2},{"$f":"U2015*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7468980270553591E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.87630468611076284},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12880886112019199}]
["Single Family Detached",12018,"Pacific","2000s","Stucco","central furnace","central AC",47.995540828752091,12502.094510000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12502.094510000001},"Hot-Dry/Mixed-Dry",76.898820576986324,"Metropolitan Area",0.64210503610841441,5.012483505036066E-2,7.2627730021744955E-2,9.7767129193870612E-3,0.16402282919204222,0.9288804303725624,382.21300000000002,399.79300000000001,{"$f":"T2019*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7784630489506302E-3},{"$f":"U2019*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9982498704364301E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.64688349915736498},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.7625979892181382E-2}]
["Single Family Detached",12023,"New England","2010s","Siding","central furnace","window/wall unit",20.566519982346669,16802.7124,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16802.7124},"Cold/Very Cold",109.52007944847679,"Rural",0.62657438879671756,0.18080926657421559,1.1285104912937599E-2,1.7745193341228399E-2,0.3446522127377924,1.1633209730216632,1056.0909999999999,0,{"$f":"T2024*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7745193341228399E-2},{"$f":"U2024*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.64431958213794593},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1285104912937599E-2}]
["Multi-Family (2-4 units)",12028,"South Atlantic","Before 1950","Concrete","built-in electric unit","window/wall unit",21.978593583967989,26258.773700000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8752.9245666666666},"Mixed-Humid",258.45833473100629,"Rural",0.33037512892938181,0.13638355408872363,8.1866689917979296E-2,0,0.33323444679757475,0.88185981973365946,0,0,{"$f":"T2029*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2029*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33037512892938181},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.1866689917979296E-2}]
["Single Family Detached",12030,"East North Central","1950s","Siding","heat pump","central AC",41.025303342291338,35612.242480000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35612.242480000001},"Mixed-Humid",568.81013288207203,"Micropolitan Area",0.95982821054497103,0.22318975831550564,0.22470630566151639,2.5748149884434721E-2,0.53305593992962841,1.9407802144516215,445.142,277.87200000000001,{"$f":"T2031*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5852504842032159E-2},{"$f":"U2031*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8956450424025604E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.97568071538700318},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23460195070391895}]
["Single Family Detached",12037,"East North Central","1980s","Siding","central furnace","central AC",61.167059927404054,26733.854859999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26733.854859999999},"Cold/Very Cold",482.19934218635694,"Metropolitan Area",1.9272887770721137,0.4245103032553621,5.9444437247921034E-2,4.3567762257519099E-2,1.1206704704162864,3.531913987991683,1520.1320000000001,109.553,{"$f":"T2038*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0638988256041522E-2},{"$f":"U2038*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9287740014775801E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9679277653281553},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2373211249398611E-2}]
["Single Family Attached",12041,"Middle Atlantic","1970s","Brick","central furnace","central AC",40.549989970639039,16091.26586,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16091.26586},"Cold/Very Cold",133.31773069672681,"Metropolitan Area",1.6156227265752769,0.26317994248373455,0.13788467330547605,4.0023049284082582E-2,0.28401682837989972,2.3007041707443876,2049.471,437.78199999999998,{"$f":"T2042*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.297858273336006E-2},{"$f":"U2042*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0444665507225198E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6486013093086369},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14492913985619857}]
["Single Family Detached",12042,"Mountain South","1960s","Stucco","central furnace","window/wall unit",28.245230454016472,25446.153559999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25446.153559999999},"Hot-Dry/Mixed-Dry",141.63016085018907,"Metropolitan Area",1.1680500029878107,0.41291531907965184,0.14794317341323318,1.3626796923683399E-2,0.32167213019803192,2.0505806256787276,535.51499999999999,0,{"$f":"T2043*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3626796923683399E-2},{"$f":"U2043*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1816767999114941},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14794317341323318}]
["Multi-Family (5+ units)",12048,"South Atlantic","1990s","Wood","heat pump","both central and individual units",35.096327332833283,34273.757160000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2726.1837403883947},"Mixed-Humid",360.08009273315082,"Metropolitan Area",7.9016576401921307E-2,0.58578803544349622,6.483601801052051E-2,3.31331265217152E-3,0.49588670228380133,1.2285770991573601,53.533999999999999,43.137999999999998,{"$f":"T2049*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4594352035795231E-4},{"$f":"U2049*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1760211419287456E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.9162519922279254E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4953620124713382E-2}]
["Multi-Family (5+ units)",12052,"Pacific","1990s","Siding","built-in electric unit","window/wall unit",12.949735749510317,18849.688139999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1499.3311961325678},"Cold/Very Cold",110.33566932096022,"Micropolitan Area",0.11299275908329738,0.13484693671530826,7.0601318431488596E-3,0,0.12156550300092873,0.37646533064268323,0,0,{"$f":"T2053*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2053*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11299275908329738},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0601318431488596E-3}]
["Single Family Detached",12059,"East South Central","1980s","Siding","portable electric heaters","central AC",40.730933124009454,19395.68244,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19395.68244},"Mixed-Humid",464.30009165857342,"Metropolitan Area",0.44561727813086544,0.53951846833334716,0.26181688646647677,1.316689479417108E-2,0.33723928632494449,1.584191919255634,0,678.85699999999997,{"$f":"T2060*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2060*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.316689479417108E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44561727813086544},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27498378126064787}]
["Mobile Home",12060,"Mountain North","2000s","Other","portable electric heaters","central AC",1.682901075820368,7012.0878160000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7012.0878160000002},"Cold/Very Cold",75.025006160054502,"Metropolitan Area",8.2693355275629155E-2,0.2061983588766243,5.6287220953960722E-3,1.64622785656232E-4,0.17291331732284515,0.46743375357049466,0,23.477,{"$f":"T2061*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2061*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.64622785656232E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.2693355275629155E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7933448810523038E-3}]
["Single Family Detached",12066,"East North Central","Before 1950","Siding","central furnace","both central and individual units",51.600143932869649,27922.15581,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27922.15581},"Cold/Very Cold",195.50289338555231,"Metropolitan Area",0.9258664086474836,0.53906648033133886,0.17669028507944762,7.5342157567032331E-2,0.55867671295550614,2.2002998870137764,2509.4180000000001,188.875,{"$f":"T2067*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0068360388418585E-2},{"$f":"U2067*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2737971786137499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.99593476903590217},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18196408225806138}]
["Single Family Detached",12071,"East North Central","1990s","Siding","central furnace","central AC",40.503657924745461,13065.696099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13065.696099999999},"Mixed-Humid",99.67745083851014,"Rural",0.42385383382030828,0.24238570032271439,0.14276423602828059,2.4211048450006396E-2,0.22237273842381466,1.0313765085951179,1294.191,558.83299999999997,{"$f":"T2072*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6909506301355102E-2},{"$f":"U2072*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.301542148651299E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44076334012166341},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1500657781769319}]
["Single Family Detached",12076,"Mountain North","1990s","Siding","central furnace","central AC",49.807782636279128,18352.167519999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18352.167519999999},"Cold/Very Cold",95.178488323735934,"Metropolitan Area",1.6896960108274555,5.9007522353213278E-2,3.4579154041184001E-2,1.2980616552068638E-2,0.24414842764567041,2.027431114867523,602.03099999999995,105.276,{"$f":"T2077*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1048573764233119E-2},{"$f":"U2077*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9320427878355198E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7007445845916886},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6511196829019522E-2}]
["Single Family Detached",12078,"East South Central","Before 1950","Siding","heater burning gas/oil/kerosene","central AC",65.079556493367264,19555.155200000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19555.155200000001},"Mixed-Humid",121.78543909042691,"Metropolitan Area",0.24895505777331842,0.13501708288660483,0.27247421892875523,1.32217684199104E-2,0.17014883829569924,0.82659519788437774,0,676.12699999999995,{"$f":"T2079*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2079*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.32217684199104E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24895505777331842},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28569598734866564}]
["Single Family Detached",12086,"Pacific","2000s","Wood","central furnace","central AC",19.723037316929286,10288.491040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10288.491040000001},"Cold/Very Cold",214.20012797693218,"Micropolitan Area",0.36220870370463032,0.15097214463298145,2.65989902130776E-2,7.9376428567972824E-3,0.19107100345984734,0.73085084201053663,646.87400000000002,124.633,{"$f":"T2087*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6553573530089604E-3},{"$f":"U2087*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2822855037883201E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3688640610576393},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7881275716865921E-2}]
["Single Family Detached",12089,"South Atlantic","1980s","Concrete","N/A","N/A",52.876182940689489,40799.523869999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":40799.523869999997},"Hot-Humid",433.08119318952487,"Metropolitan Area",0,0.76095138930555961,0,0,0.7167216862657132,1.4776730755712728,0,0,{"$f":"T2090*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2090*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12094,"West North Central","Before 1950","Brick","central furnace","central AC",23.134654210257491,16643.636119999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16643.636119999999},"Mixed-Humid",87.538801975290241,"Metropolitan Area",0.60505186256845744,0.23300992370546891,0.10111641401072559,1.7603358109587557E-2,0.18467339246758438,1.1238515927522363,774.62400000000002,283.03899999999999,{"$f":"T2095*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2892559985818879E-2},{"$f":"U2095*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7107981237686797E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.61794442255427628},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10582721213449427}]
["Single Family Detached",12095,"West North Central","1970s","Wood","central furnace","central AC",69.049970881335938,11850.003580000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11850.003580000001},"Cold/Very Cold",118.91337581048073,"Metropolitan Area",0.81056054392813259,0.26147637249452577,0.1902078439636182,7.3015420508660472E-2,0.20552946014242576,1.4677742205287025,5028.835,1132.8019999999999,{"$f":"T2096*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9591712753229303E-2},{"$f":"U2096*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.342370775543116E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.87015225668136187},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20363155171904937}]
["Single Family Detached",12101,"East South Central","1960s","Brick","central furnace","both central and individual units",30.192358171730056,17512.968779999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17512.968779999999},"Hot-Humid",175.4939049827135,"Metropolitan Area",0.35132335850526014,0.15914821062684223,0.27103839303257443,1.546866242134182E-2,0.34397097638719665,1.1254809385518734,187.85599999999999,695.41300000000001,{"$f":"T2102*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2899162631356794E-3},{"$f":"U2102*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2178746158206138E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35461327476839583},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28321713919078056}]
["Single Family Detached",12105,"South Atlantic","1950s","Siding","central furnace","central AC",110.2208355184101,32171.872599999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32171.872599999999},"Mixed-Humid",170.83872397567737,"Metropolitan Area",3.7085321842835001E-2,0.18746218793732219,0.10820066713142819,8.2068838408969995E-3,0.57564874268199206,0.90839691959357738,29.391999999999999,225.703,{"$f":"T2106*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4559567945919987E-4},{"$f":"U2106*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.2612881614378001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.8030917522294198E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11546195529286599}]
["Single Family Detached",12112,"Middle Atlantic","1950s","Stone","central furnace","central AC",51.294698406474211,18775.511859999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18775.511859999999},"Cold/Very Cold",220.25598026321765,"Metropolitan Area",1.724809693345192,0.20610063368738224,8.8104464913287189E-2,4.0735369306967861E-2,0.44335844073493647,2.4623732326807981,1920.2619999999999,249.339,{"$f":"T2113*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6053901955307319E-2},{"$f":"U2113*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6814673516605392E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7608635953004992},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2785932264947732E-2}]
["Multi-Family (2-4 units)",12114,"West North Central","Before 1950","Siding","radiator","N/A",14.184759777950784,22163.687150000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7387.8957166666669},"Cold/Very Cold",78.861324497249356,"Metropolitan Area",0.54719194325379916,0.23039755644715484,0,3.4806297574103006E-3,0.26559424520671798,1.0455041647459455,157.042,0,{"$f":"T2115*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1602099191367669E-3},{"$f":"U2115*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54835215317293595},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12119,"New England","1960s","Siding","heat pump","N/A",37.699109006193773,13368.478370000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13368.478370000001},"Cold/Very Cold",50.864453348337271,"Micropolitan Area",7.3431728207051378E-2,0.20817252811893278,0,2.0562725004815499E-3,0.10011776441294003,0.38172202073892419,153.815,0,{"$f":"T2120*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0562725004815499E-3},{"$f":"U2120*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.5488000707532921E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12124,"East North Central","1970s","Brick","central furnace","central AC",89.692372990339052,27412.094430000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27412.094430000001},"Cold/Very Cold",267.74214997204723,"Metropolitan Area",3.263101592889635,0.47183454048168966,0.15170979694643072,6.5131218601963303E-2,0.95106809866773656,4.8377140289854914,2106.799,269.20400000000001,{"$f":"T2125*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7751773133029573E-2},{"$f":"U2125*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3794454689337201E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.3208533660226647},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15908924241536443}]
["Single Family Detached",12129,"East North Central","1980s","Siding","central furnace","central AC",13.464791036209681,12513.74632,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12513.74632},"Cold/Very Cold",66.02179976687934,"Metropolitan Area",0.62565966062063283,0.14185823092281344,3.7271154773175441E-2,6.6839923493942407E-3,0.62055914521682509,1.4253481915334467,405.649,128.483,{"$f":"T2130*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.07618868096168E-3},{"$f":"U2130*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6078036684325601E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63073584930159454},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8878958441607998E-2}]
["Single Family Detached",12131,"West North Central","Before 1950","Brick","central furnace","both central and individual units",71.489228832840865,18052.83556,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18052.83556},"Mixed-Humid",505.01783894090272,"Metropolitan Area",1.800685426571526,0.15213619174106341,0.36424106891726393,6.5972408640312924E-2,1.4090674311087132,3.7261301183385664,2699.2620000000002,955.14499999999998,{"$f":"T2132*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8729333019356717E-2},{"$f":"U2132*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7243075620956196E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8494147595908828},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3814841445382201}]
["Single Family Attached",12138,"Mountain South","2000s","Stucco","central furnace","central AC",13.737657203430718,6896.4142590000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6896.4142590000001},"Hot-Dry/Mixed-Dry",12.627334507771909,"Metropolitan Area",8.114261707976772E-2,5.2211069629809807E-2,1.0302870496576015E-2,2.7256284290990162E-3,5.4789783745949325E-2,0.1984463409521029,314.83100000000002,80.393000000000001,{"$f":"T2139*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1712049975752289E-3},{"$f":"U2139*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5442343152378693E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.3313822077342947E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0857293928099802E-2}]
["Mobile Home",12142,"South Atlantic","2000s","Siding","other","central AC",23.249092604813526,12419.38708,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12419.38708},"Mixed-Humid",128.50254112960246,"Rural",0.54955291053516808,0.17763413324301469,8.7942462334866037E-2,3.4380216671951601E-3,0.17287406782115342,0.98800357393420224,0,276.827,{"$f":"T2143*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2143*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4380216671951601E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54955291053516808},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.1380484002061196E-2}]
["Single Family Detached",12148,"Pacific","1970s","Siding","heat pump","central AC",15.292403412314727,16373.022929999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16373.022929999999},"Cold/Very Cold",155.49919954187564,"Micropolitan Area",0.18399749386878583,8.8724805455821593E-2,2.2413669636771265E-2,3.7451488919852697E-3,0.23542728738489677,0.53056325634627544,170.73500000000001,58.003999999999998,{"$f":"T2149*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7954480699535502E-3},{"$f":"U2149*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4970082203171997E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18679294193873938},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3363370458802983E-2}]
["Single Family Detached",12149,"New England","Before 1950","Wood","central furnace","window/wall unit",19.749812216601118,12343.63264,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12343.63264},"Cold/Very Cold",78.858803014279175,"Metropolitan Area",1.1789611154365005,0.12202196828484352,4.1692668284618241E-2,2.2688473190237441E-2,8.2663110623470301E-2,1.4253388626294325,1838.0709999999999,0,{"$f":"T2150*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2688473190237441E-2},{"$f":"U2150*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.201649588626738},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1692668284618241E-2}]
["Single Family Detached",12153,"East North Central","1950s","Stucco","central furnace","central AC",71.519248739506168,37249.608719999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":37249.608719999997},"Mixed-Humid",242.42112403290804,"Micropolitan Area",1.3305056247578018,0.41629346939041029,0.13978556365449982,3.0735136399785354E-2,0.62988212979715064,2.5164667875998625,616.76599999999996,208.34700000000001,{"$f":"T2154*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2974292171799519E-2},{"$f":"U2154*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7608442279858397E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3534799169296012},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14754640788248566}]
["Multi-Family (5+ units)",12160,"South Atlantic","1970s","Concrete","N/A","central AC",58.448899684344674,40477.077340000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3219.6047135309618},"Hot-Humid",388.9624913577739,"Metropolitan Area",0,0.21335722471501242,0.34044392366834764,1.8176312533681682E-2,0.75660837749600718,1.3271400684772283,0,449.05200000000002,{"$f":"T2161*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2161*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4457699358205055E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.34188969360416815}]
["Single Family Detached",12165,"Middle Atlantic","1950s","Siding","heater burning gas/oil/kerosene","window/wall unit",84.678298130242098,41145.917459999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":41145.917459999997},"Mixed-Humid",324.62791632687936,"Metropolitan Area",2.856645429219737,1.3045642709491854,0.23709512017975798,0,0.87053540853668687,5.2688402288853675,0,0,{"$f":"T2166*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2166*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.856645429219737},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23709512017975798}]
["Single Family Detached",12167,"Mountain North","1990s","Stucco","central furnace","central AC",48.695123470528948,12757.43345,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12757.43345},"Cold/Very Cold",161.66943011620396,"Metropolitan Area",1.0469938754293207,0.6250761581111518,9.399416714317621E-2,2.7012551314729651E-2,0.43610324338342882,2.2021674440670771,1686.7560000000001,430.64100000000002,{"$f":"T2168*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1518677416388202E-2},{"$f":"U2168*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4938738983414505E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0685125528457089},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.9488041041517664E-2}]
["Multi-Family (5+ units)",12172,"Pacific","1950s","Concrete","central furnace","N/A",3.668068904012328,12066.01613,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":959.7482070993965},null,26.774489796063673,"Metropolitan Area",0.12560057505319283,0.22816672404010632,0,2.58102944435217E-3,8.8758712659747843E-2,0.44490174241816677,213.90899999999999,0,{"$f":"T2173*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0529877923242481E-4},{"$f":"U2173*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12580587383242525},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",12177,"West South Central","1970s","Brick","central furnace","central AC",22.030664938771594,23714.38637,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1886.276261845994},"Hot-Humid",235.22740929101619,"Metropolitan Area",4.9430229748352386E-2,0.30031906013283916,0.19540312999063658,9.761505432710359E-3,0.24845840058169519,0.80259588176112262,34.037999999999997,377.59,{"$f":"T2178*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.420507140071394E-5},{"$f":"U2178*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1223905371042872E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.9494434819753103E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19611536904434701}]
["Single Family Detached",12183,"West South Central","1950s","Siding","N/A","window/wall unit",24.612372031978516,19364.572800000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19364.572800000002},"Hot-Humid",277.22527688531852,"Metropolitan Area",0,0.33585849224772485,0.65369975994172813,0,0.29219289102040341,1.2817511432098563,0,0,{"$f":"T2184*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2184*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.65369975994172813}]
["Single Family Detached",12186,"Middle Atlantic","1990s","Siding","central furnace","central AC",48.780765144978496,14082.20703,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14082.20703},"Cold/Very Cold",150.99084605708401,"Metropolitan Area",1.0902393845858622,0.23721784734148255,5.7449039524822443E-2,2.2210358352266788E-2,0.67459427088043256,2.0595005423325996,1343.123,234.07,{"$f":"T2187*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8914136152754689E-2},{"$f":"U2187*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2962221995120997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1091535207386169},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0745261724334546E-2}]
["Multi-Family (2-4 units)",12190,"Pacific","1950s","Wood","N/A","window/wall unit",16.129203600906838,21028.948629999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7009.649543333333},"Marine",70.778856785224775,"Metropolitan Area",0,0.37544630658711586,1.2468442163802339E-2,0,0.2575128083277814,0.64542755707869959,0,0,{"$f":"T2191*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2191*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2468442163802339E-2}]
["Single Family Detached",12195,"Middle Atlantic","Before 1950","Shingle","central furnace","window/wall unit",54.300275659209781,23639.649829999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23639.649829999998},"Cold/Very Cold",125.15977142949556,"Metropolitan Area",3.0613364495983868,0.43156381616064171,2.6201644159625906E-2,4.3526836204585112E-2,0.39936545474934004,3.9184673646679946,1841.2639999999999,0,{"$f":"T2196*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3526836204585112E-2},{"$f":"U2196*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.1048632858029719},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6201644159625906E-2}]
["Single Family Detached",12201,"Pacific","1960s","Wood","wood-burning stove","central AC",54.719653071584034,12493.071480000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12493.071480000001},"Marine",294.15251619247033,"Metropolitan Area",9.657029317782384E-2,0.37115458674945434,7.368422304054037E-2,3.6226309287413758E-2,0.90619154863661311,1.4476006516044315,2523.2240000000002,376.488,{"$f":"T2202*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1522817792051523E-2},{"$f":"U2202*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7034914953622397E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12809311096987536},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.8387714535902611E-2}]
["Multi-Family (5+ units)",12202,"Pacific","1950s","Concrete","N/A","window/wall unit",28.493531860349908,24208.608209999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1925.5873749539924},"Hot-Humid",92.413505216759773,"Metropolitan Area",0,7.1243513101208994E-2,6.4849099745836025E-2,0,0.17922223347903324,0.31531484632607826,0,0,{"$f":"T2203*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2203*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4849099745836025E-2}]
["Single Family Detached",12210,"South Atlantic","1960s","Brick","heat pump","central AC",81.169662712538027,27835.961149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27835.961149999999},"Mixed-Humid",459.35521047579732,"Micropolitan Area",0.59609260549149079,0.24975056220098105,0.35081489254385867,3.0103645561045896E-2,0.37066190500784757,1.567319965244178,381.96199999999999,699.50400000000002,{"$f":"T2211*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0632279392776299E-2},{"$f":"U2211*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.94713661682696E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60672488488426712},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37028625871212828}]
["Single Family Detached",12213,"South Atlantic","2000s","Brick","central furnace","central AC",36.57032764077502,14397.76679,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14397.76679},"Mixed-Humid",206.21498075688746,"Metropolitan Area",0.3814093683242073,0.35777213704982741,0.14902864925196743,1.1530825875708041E-2,0.45913438774547766,1.3473445423714798,352.13900000000001,448.73700000000002,{"$f":"T2214*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0700151996638104E-3},{"$f":"U2214*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4608106760442301E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38647938352387112},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15548945992801166}]
["Single Family Attached",12215,"South Atlantic","1970s","Siding","central furnace","central AC",27.997814629752082,18074.767349999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18074.767349999998},"Mixed-Humid",95.856022151615221,"Metropolitan Area",5.6673198053949443E-2,8.2066565227335894E-2,5.4471817914090892E-2,4.0747755513839993E-3,0.20457392219460668,0.39778550338998292,91.174000000000007,134.26599999999999,{"$f":"T2216*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6479488383688999E-3},{"$f":"U2216*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4268267130150996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.8321146892318342E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.689864462710599E-2}]
["Single Family Detached",12220,"South Atlantic","1980s","Siding","central furnace","central AC",22.155386528687643,14111.711160000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14111.711160000001},"Mixed-Humid",105.93753297514809,"Metropolitan Area",0.35235235249469643,0.10796458146550128,8.5504254977844835E-2,9.7613810670175195E-3,0.28657380016907846,0.83239498910712106,396.20800000000003,295.51400000000001,{"$f":"T2221*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.59117285528128E-3},{"$f":"U2221*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1702082117362404E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3579435253499777},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.9674463189581069E-2}]
["Multi-Family (5+ units)",12225,"East South Central","1980s","Brick","central furnace","central AC",38.767582893838252,37169.30287,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2956.4995939232972},"Mixed-Humid",857.66776241545097,"Metropolitan Area",0.19103563588606265,0.22200819458849716,0.11821627284124854,8.5220662541249902E-3,2.3872580592182508,2.926362371430788,84.355000000000004,144.922,{"$f":"T2226*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4939552324539977E-4},{"$f":"U2226*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2846183415055206E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19128503140930805},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11864473467539909}]
["Single Family Detached",12231,"Middle Atlantic","Before 1950","Brick","central furnace","central AC",97.972966709817683,24444.35297,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24444.35297},"Cold/Very Cold",301.68746216991724,"Metropolitan Area",2.1444942860910308,0.39705111639724117,0.25112962245741327,0.15991507935150487,0.69538437332266712,3.4880593982683523,6014.4009999999998,527.60400000000004,{"$f":"T2232*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.14701814094712096},{"$f":"U2232*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2896938404383881E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2915124270381515},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26402656086179715}]
["Multi-Family (5+ units)",12236,"East North Central","1990s","Brick","built-in electric unit","window/wall unit",10.008471709767207,14442.23912,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1148.7563875750236},"Cold/Very Cold",38.88944048452759,"Metropolitan Area",1.11800261475744E-2,1.8565772791303281E-2,5.7657173549211203E-3,0,0.10124006734672174,0.13675158364052054,0,0,{"$f":"T2237*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2237*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.11800261475744E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7657173549211203E-3}]
["Single Family Detached",12239,"South Atlantic","2000s","Brick","heat pump","central AC",33.772012287573602,17091.099340000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17091.099340000001},"Hot-Humid",233.64635167968456,"Metropolitan Area",9.963165777426497E-2,0.21935111697350756,0.20967627291461705,1.2198344876441499E-2,0.26854230890751146,0.79720135656990099,103.824,609.90099999999995,{"$f":"T2240*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7744662978761601E-3},{"$f":"U2240*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0423878578565341E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10140612407214113},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22010015149318238}]
["Single Family Detached",12243,"Pacific","2010s","Siding","central furnace","N/A",7.3813926194320914,8543.2784950000005,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8543.2784950000005},"Marine",61.154854938551871,"Metropolitan Area",9.927950006617664E-2,5.01984334586296E-2,0,1.55858446895683E-3,5.9182425518072665E-2,0.20866035904287888,182.434,0,{"$f":"T2244*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.55858446895683E-3},{"$f":"U2244*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10083808453513347},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12249,"West North Central","Before 1950","Siding","central furnace","central AC",16.350716632737871,13271.685579999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13271.685579999999},"Cold/Very Cold",95.675581335557879,"Micropolitan Area",0.23187301631968846,8.1730928405514922E-2,2.0848318345709459E-2,1.6036058241143781E-2,0.20866878797993094,0.54312105105084374,1145.0730000000001,63.218000000000004,{"$f":"T2250*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5197048822147341E-2},{"$f":"U2250*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3900941899644002E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2470700651418358},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1687327764705899E-2}]
["Single Family Detached",12254,"South Atlantic","1990s","Siding","heat pump","both central and individual units",31.390696807856724,16949.620309999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16949.620309999998},"Mixed-Humid",433.07588394096916,"Metropolitan Area",0.73273171310965302,0.22185769899532531,5.5755131924173217E-2,7.9721691647069506E-3,0.92545106558575274,1.9357956096149045,344.56200000000001,125.783,{"$f":"T2255*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8401950732542189E-3},{"$f":"U2255*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.13197409145273E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.73857190818290719},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7887106015625946E-2}]
["Single Family Detached",12259,"Middle Atlantic","2000s","Siding","central furnace","central AC",66.92394023895362,19977.295590000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19977.295590000002},"Cold/Very Cold",290.20056401075351,"Metropolitan Area",0.81139653915922672,0.44164202911265682,0.11937506895798183,4.8813682727750218E-2,0.84968186747431751,2.2220955047041833,2110.4279999999999,333.03,{"$f":"T2260*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2160643977412524E-2},{"$f":"U2260*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6530387503377E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.8535571831366392},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12602810770831954}]
["Single Family Detached",12261,"Pacific","Before 1950","Stucco","heater burning gas/oil/kerosene","N/A",62.92159702683945,26327.028040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26327.028040000001},"Marine",157.40669430350101,"Metropolitan Area",8.6614132013693279E-2,0.31532034180270635,0,0,0.60668848512976103,1.0086229589461606,0,0,{"$f":"T2262*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2262*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.6614132013693279E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12266,"East North Central","1960s","Brick","central furnace","central AC",40.044887305042543,20705.732840000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20705.732840000001},"Cold/Very Cold",205.1798153304826,"Metropolitan Area",1.0122432940395627,0.54653846105847981,0.11249014678461768,3.8468497754252283E-2,0.56822597692682097,2.2394978788094813,1628.6210000000001,229.24600000000001,{"$f":"T2267*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3721791323613644E-2},{"$f":"U2267*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.74670643063864E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0459650853631763},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11723685321525631}]
["Multi-Family (5+ units)",12268,"Middle Atlantic","1980s","Stone","central furnace","N/A",29.548185631012188,34438.444790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2739.283230387498},"Mixed-Humid",339.35643497435211,"Metropolitan Area",0.5311586456430456,0.22754596278364198,0,8.6230421909680999E-3,0.39121319079499089,1.15785495228459,250.39,0,{"$f":"T2269*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8588912805672556E-4},{"$f":"U2269*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53184453477110227},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",12273,"West North Central","1990s","Siding","central furnace","central AC",20.577146809287797,7994.2295299999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7994.2295299999996},null,154.76223206203463,"Metropolitan Area",0.25291174486394963,8.8629656507169113E-2,1.0783775953345849E-2,6.1034663384825199E-3,0.17572354957355951,0.52804872689802407,700.57600000000002,62.908000000000001,{"$f":"T2274*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6005653472092805E-3},{"$f":"U2274*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0290099127324006E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25851231021115889},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1286676944619089E-2}]
["Single Family Detached",12278,"New England","1990s","Siding","radiator","central AC",100.15883166532184,26982.443879999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26982.443879999999},"Cold/Very Cold",432.03285386308028,"Metropolitan Area",2.9928201733428943,0.80148265452204515,0.12395222052038279,9.6519979300903197E-3,1.4253552070101738,5.3436102553954967,120.675,237.03899999999999,{"$f":"T2279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2561064152189997E-3},{"$f":"U2279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.39589151487132E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9960762797581131},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13034811203525412}]
["Single Family Detached",12284,"New England","Before 1950","Siding","wood-burning stove","window/wall unit",21.151455139511341,10533.593199999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10533.593199999999},"Cold/Very Cold",21.815208447631875,"Micropolitan Area",0.51750380482910718,0.1033029695795864,8.899527420477199E-3,1.8888312646579998E-3,9.1235853747157689E-2,0.72094215557632835,179.315,0,{"$f":"T2285*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8888312646579998E-3},{"$f":"U2285*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.51939263609376518},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.899527420477199E-3}]
["Multi-Family (5+ units)",12287,"East North Central","1960s","Concrete","central furnace","N/A",6.8257606298187881,14190.77054,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1128.7542165024383},"Cold/Very Cold",44.729308742596295,"Metropolitan Area",0.19120393146750653,0.15016163936765614,0,3.3251671621622597E-3,0.14931076076607774,0.49373701020414601,234.31899999999999,0,{"$f":"T2288*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6448855925663482E-4},{"$f":"U2288*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19146842002676318},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12291,"West South Central","1970s","Brick","central furnace","both central and individual units",34.096256110589216,18213.812020000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18213.812020000001},"Hot-Humid",300.23647741824391,"Metropolitan Area",0.34489791009468934,0.23905387853931337,0.39498212289060114,1.1255735124495563E-2,0.28453761026758956,1.2634715217921935,330.86500000000001,287.113,{"$f":"T2292*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0263129139973013E-3},{"$f":"U2292*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2294222104982604E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35092422300868664},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.40021154510109941}]
["Single Family Detached",12297,"West North Central","1990s","Siding","central furnace","central AC",46.264180435040387,21398.788359999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21398.788359999999},"Cold/Very Cold",173.91238255361853,"Metropolitan Area",0.82484336680347548,0.13840353272936357,9.2751764219118404E-2,2.6176667027444079E-2,0.38083335909259702,1.4368320228445544,1008.918,214.36,{"$f":"T2298*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.158962275459448E-2},{"$f":"U2298*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5870442728495999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84643298955807},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.7338808491968007E-2}]
["Multi-Family (5+ units)",12302,"Middle Atlantic","Before 1950","Brick","built-in electric unit","N/A",55.157285268455084,53189.281840000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4230.7516692209574},"Cold/Very Cold",320.78455877922141,"Metropolitan Area",0.43582659268313922,0.31591630337807036,0,0,0.55527136939354427,1.3070142654547539,0,0,{"$f":"T2303*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2303*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43582659268313922},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",12307,"East South Central","2000s","Brick","central furnace","central AC",32.332282858512251,29826.82921,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2372.4687211865521},"Mixed-Humid",129.84149670613709,"Metropolitan Area",0.19466872038484995,0.49753086883495728,8.0472861294019177E-2,7.3680619660878794E-3,0.3554632355077319,1.1349176817843891,126.895,120.133,{"$f":"T2308*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0105441837496752E-4},{"$f":"U2308*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8501178488230401E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19496977480322492},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.0757873078901476E-2}]
["Single Family Detached",12311,"Pacific","1970s","Stucco","central furnace","N/A",16.510287280840355,11505.42668,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11505.42668},"Hot-Dry/Mixed-Dry",74.197346094363311,"Metropolitan Area",1.713386990642932E-2,2.6585750505449521E-2,0,1.1974157762943201E-3,0.31153725898813889,0.35525687940001771,104.074,0,{"$f":"T2312*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1974157762943201E-3},{"$f":"U2312*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8331285682723641E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12314,"West South Central","1990s","Stone","heat pump","central AC",41.587749776338356,21716.840609999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21716.840609999999},"Hot-Humid",405.571141261501,"Metropolitan Area",0.18708252490728366,0.20639585418277193,0.368592247911954,2.318958987280776E-2,0.62173807517691682,1.3838087021789265,214.303,853.51300000000003,{"$f":"T2315*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6539840932448302E-3},{"$f":"U2315*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8535605779562932E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19173650900052849},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.38712785369151692}]
["Single Family Detached",12321,"Pacific","1990s","Stucco","central furnace","N/A",33.347523773735034,25731.114020000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25731.114020000001},"Hot-Dry/Mixed-Dry",102.31601816958826,"Metropolitan Area",5.1848246212528037E-2,0.47275472161800569,0,9.3694705481026E-4,0.35652421758709718,0.88112718541763091,36.412999999999997,0,{"$f":"T2322*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.3694705481026E-4},{"$f":"U2322*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.2785193267338298E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12325,"East South Central","1970s","Brick","heat pump","central AC",50.515608717075608,16821.714520000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16821.714520000001},"Mixed-Humid",373.15923895761517,"Metropolitan Area",0.52039763698044927,0.23801555254469409,0.18497485309625139,2.0374662487198242E-2,0.62666720357595551,1.5700552461973503,596.91200000000003,614.29999999999995,{"$f":"T2326*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.004108325756224E-2},{"$f":"U2326*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0333579229636E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53043872023801153},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1953084323258874}]
["Multi-Family (5+ units)",12326,"New England","1970s","Siding","radiator","window/wall unit",11.417639460715396,31540.440500000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2508.7718178775708},"Cold/Very Cold",40.428820495856741,"Metropolitan Area",0.2910903781124165,0.31666110231128197,9.1525311860520004E-3,2.1039050835524997E-3,0.12668672109168208,0.74552729016087349,66.704999999999998,0,{"$f":"T2327*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6734762411152335E-4},{"$f":"U2327*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29125772573652803},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.1525311860520004E-3}]
["Single Family Detached",12332,"East South Central","Before 1950","Siding","built-in furnace","window/wall unit",27.89845108627151,17094.639149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17094.639149999999},"Mixed-Humid",196.2618938552254,"Metropolitan Area",1.2099919790565381,0.26440507441469607,0.13715620464559589,0,0.20564481653244351,1.8171980746492737,0,0,{"$f":"T2333*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2333*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2099919790565381},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13715620464559589}]
["Single Family Detached",12337,"South Atlantic","1980s","Concrete","heat pump","central AC",39.404963669677926,24399.35831,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24399.35831},"Hot-Humid",320.00612400316436,"Metropolitan Area",2.4130940969231691E-2,0.1487755996817495,0.44692980478652183,2.2726391908116539E-2,0.47202454480835676,1.09186089024586,25.152999999999999,906.28099999999995,{"$f":"T2338*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1371705957142999E-4},{"$f":"U2338*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2112674848545108E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4744658028803122E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46904247963506696}]
["Single Family Attached",12340,"South Atlantic","1970s","Brick","central furnace","central AC",35.259105250916527,13092.87235,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13092.87235},"Mixed-Humid",69.363523903136866,"Metropolitan Area",0.77639041436392375,0.32660670224798771,7.9344495421533143E-2,9.5253264920720001E-3,0.2028508172148285,1.3851924292482733,397.59199999999998,329.928,{"$f":"T2341*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2056213033812001E-3},{"$f":"U2341*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3197051886908E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78159603566730496},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.3664200610223949E-2}]
["Multi-Family (5+ units)",12344,"Pacific","1970s","Wood","built-in electric unit","window/wall unit",11.753248278298466,14160.54009,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1126.3496432054435},"Cold/Very Cold",87.994006801863534,"Metropolitan Area",7.3922295752907166E-2,0.11280177199535307,4.6146651256093801E-3,0,0.1088968472995946,0.30023558017346424,0,0,{"$f":"T2345*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2345*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.3922295752907166E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.6146651256093801E-3}]
["Single Family Detached",12350,"East North Central","1990s","Siding","heat pump","both central and individual units",19.570165490534404,15289.191790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15289.191790000001},"Mixed-Humid",394.44590484436992,"Metropolitan Area",0.51873160731596923,0.53098441148405062,6.5229593804170941E-2,1.0682619460440161E-2,0.23090379587313198,1.3458494084773227,538.69399999999996,160.01,{"$f":"T2351*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2361958821222589E-3},{"$f":"U2351*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4464235783179002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52696780319809144},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7676017382488837E-2}]
["Single Family Detached",12355,"East South Central","1990s","Brick","central furnace","window/wall unit",19.009598147953632,19801.66474,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19801.66474},"Hot-Humid",556.62101365180251,"Micropolitan Area",0.58027731012505246,0.3091360850899435,0.43296199362190346,7.6220567917208003E-3,0.5768155236902115,1.8991909125271111,384.92,0,{"$f":"T2356*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6220567917208003E-3},{"$f":"U2356*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58789936691677325},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.43296199362190346}]
["Multi-Family (5+ units)",12359,"Pacific","1960s","Stucco","central furnace","central AC",12.744030161237831,29985.953320000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2385.1256808353196},"Hot-Dry/Mixed-Dry",124.84351805481784,"Metropolitan Area",0.12979066504115172,0.41687125999246377,3.2120876410243616E-2,3.9242617109884002E-3,0.45066581920149695,1.0330607409584935,87.516000000000005,43.353999999999999,{"$f":"T2360*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0873665908398384E-4},{"$f":"U2360*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0340473876693444E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12999940170023572},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2224281149010554E-2}]
["Single Family Detached",12362,"West South Central","1960s","Brick","heater burning gas/oil/kerosene","window/wall unit",67.916005434954229,39903.645969999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39903.645969999998},"Hot-Humid",468.7082255223105,"Metropolitan Area",0.5933387642743233,0.45777019726313728,0.72637301082630867,0,0.96305921238954373,2.740541184753313,0,0,{"$f":"T2363*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2363*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5933387642743233},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.72637301082630867}]
["Single Family Detached",12369,"Pacific","1960s","Stucco","central furnace","N/A",22.996591004833942,9609.9419159999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9609.9419159999998},"Marine",88.276253743850503,"Metropolitan Area",0.14518163050939695,0.20063806828196715,0,4.8575373402805202E-3,0.25658975441117837,0.60240945320254247,505.47,0,{"$f":"T2370*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8575373402805202E-3},{"$f":"U2370*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15003916784967747},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12373,"Pacific","1950s","Shingle","central furnace","N/A",19.372630844925347,10068.934950000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10068.934950000001},"Cold/Very Cold",132.28717772102701,"Metropolitan Area",0.29616313166750746,0.19130743812602657,0,1.4103678011684401E-2,0.22329742114886678,0.71076799094240084,1400.712,0,{"$f":"T2374*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4103678011684401E-2},{"$f":"U2374*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31026680967919185},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12378,"New England","1970s","Wood","radiator","window/wall unit",20.056647568899994,26217.839960000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26217.839960000001},"Cold/Very Cold",157.30703975607838,"Micropolitan Area",0.11556923482159849,0.17594876294243872,1.4906388869817641E-2,1.105525035809324E-2,0.34564121517090252,0.65206560180475737,421.66899999999998,0,{"$f":"T2379*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.105525035809324E-2},{"$f":"U2379*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12662448517969174},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4906388869817641E-2}]
["Multi-Family (5+ units)",12383,"Pacific","1970s","Stucco","N/A","N/A",12.117340162875482,19203.3917,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1527.4652839621583},"Hot-Dry/Mixed-Dry",21.921785422586069,"Metropolitan Area",0,9.8004855202000599E-2,0,0,7.4797114654541502E-2,0.17280196985654211,0,0,{"$f":"T2384*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2384*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",12385,"East South Central","1960s","Siding","heat pump","central AC",12.275702389621735,9313.8864869999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9313.8864869999998},"Mixed-Humid",110.21677918871062,"Rural",0.10278757626232116,4.8103513364387278E-2,7.5781766801648429E-2,5.2344694028994086E-3,0.14938678519242013,0.37605964162077699,187.21299999999999,374.79399999999998,{"$f":"T2386*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.743680630890731E-3},{"$f":"U2386*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4907887720086778E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10453125689321188},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9272555573657102E-2}]
["Multi-Family (5+ units)",12388,"South Atlantic","1960s","Concrete","radiator","central AC",50.424049975678756,53358.783040000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4244.2340374731202},"Mixed-Humid",156.02108161786737,"Metropolitan Area",0.53664855788079069,0.89887875084729152,0.17324947374788138,1.0198997790265599E-2,0.47913401841445302,2.0972985557867596,46.256,144.88399999999999,{"$f":"T2389*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9632128963735664E-4},{"$f":"U2389*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1492160428525556E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.536844879170428},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17386439535216663}]
["Single Family Detached",12396,"Middle Atlantic","Before 1950","Siding","central furnace","window/wall unit",122.1408117823843,36189.870159999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":36189.870159999999},"Cold/Very Cold",520.21845417677514,"Metropolitan Area",4.3438245522582681,1.1707840265962943,0.55214892141086025,0.14301592507543154,1.2141682258048812,7.2809257260703042,3951.8220000000001,0,{"$f":"T2397*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.14301592507543154},{"$f":"U2397*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.4868404773336996},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.55214892141086025}]
["Single Family Detached",12398,"Pacific","2000s","Wood","N/A","central AC",32.685366375650304,17202.824410000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17202.824410000001},"Marine",113.69461910327369,"Metropolitan Area",0,6.5961374531292943E-2,3.559611867482082E-2,1.8077760059492603E-3,0.32494509643583258,0.42650258964194632,0,105.086,{"$f":"T2399*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2399*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8077760059492603E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7403894680770079E-2}]
["Single Family Detached",12403,"Pacific","1950s","Wood","central furnace","central AC",36.618386889365738,16766.660660000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16766.660660000001},"Hot-Dry/Mixed-Dry",60.175058888605243,"Metropolitan Area",0.12081276021875312,0.44625800296112472,5.6686117992162784E-2,3.9423113876644799E-3,0.20077081877372874,0.82452769994576935,73.197999999999993,161.93,{"$f":"T2404*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.22728602699068E-3},{"$f":"U2404*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7150253606738001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1220400462457438},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9401143352836583E-2}]
["Single Family Detached",12408,"Pacific","2000s","Stucco","central furnace","central AC",31.148627801639076,15062.199130000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15062.199130000001},"Hot-Dry/Mixed-Dry",89.354809374714719,"Metropolitan Area",0.14548859802790734,0.27523108271211782,0.14940999638480543,1.2392394209809242E-2,0.28455244514131151,0.85468212226614204,322.73899999999998,500.00900000000001,{"$f":"T2409*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8611590850170701E-3},{"$f":"U2409*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5312351247921704E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15034975711292442},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1569412315095976}]
["Multi-Family (2-4 units)",12412,"Mountain South","1990s","Stucco","central furnace","central AC",36.12153548552228,44760.267019999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14920.089006666667},"Hot-Dry/Mixed-Dry",252.64632825917343,"Metropolitan Area",0.16496120388574376,0.60005537874558068,0.22549282559068579,1.3838084151903199E-2,0.72773950117270703,1.7274742988293195,93.504999999999995,215.655,{"$f":"T2413*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3951029225683666E-3},{"$f":"U2413*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2175917947326999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16635630680831212},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22871041738541847}]
["Single Family Detached",12415,"South Atlantic","1990s","Siding","heat pump","central AC",109.857136376819,24251.02348,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24251.02348},"Mixed-Humid",485.9342724706832,"Micropolitan Area",0.62636278250155453,0.13352484997663555,0.37009055264610052,3.384487387482888E-2,0.62312844775105025,1.7531066328753406,499.87099999999998,895.73500000000001,{"$f":"T2416*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.212238335797108E-2},{"$f":"U2416*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.17224905168578E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63848516585952564},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.39181304316295834}]
["Single Family Detached",12422,"West South Central","2000s","Stucco","central furnace","central AC",52.51593640883322,14301.7256,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14301.7256},"Hot-Humid",224.47370669621938,"Metropolitan Area",0.41327913852549114,0.28438186179656638,0.26459080497159759,2.5857062229580799E-2,0.9676942554621073,1.9299460607557624,600.995,1206.973,{"$f":"T2423*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.5952655769720009E-3},{"$f":"U2423*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.72617966526088E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42187440410246313},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28185260162420639}]
["Multi-Family (5+ units)",12426,"West South Central","1960s","Wood","central furnace","central AC",55.312895347409366,62149.320619999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4943.4459887043558},"Hot-Humid",430.88123982425742,"Metropolitan Area",0.43971141444337225,0.29543524787477432,0.28502727716328619,2.0023392415992842E-2,0.43166183532544722,1.47026647790734,116.568,205.614,{"$f":"T2427*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.762476120112893E-4},{"$f":"U2427*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0164417035214575E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44028766205538356},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28604371886680763}]
["Single Family Detached",12431,"East North Central","2010s","Brick","central furnace","central AC",76.413657175202232,13531.72608,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13531.72608},"Cold/Very Cold",91.122643424439858,"Metropolitan Area",1.3156814318103132,0.32370891473377156,6.6401952530676489E-2,2.6352495271756801E-2,0.26088862065230584,1.9666809197270669,1655.9559999999999,291.50400000000002,{"$f":"T2432*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.240794299253248E-2},{"$f":"U2432*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9445522792243204E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3380893748028457},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0346504809900803E-2}]
["Single Family Detached",12433,"New England","1980s","Siding","heat pump","N/A",45.655040842155437,14125.940850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14125.940850000001},"Cold/Very Cold",97.454428051907257,"Metropolitan Area",4.5921187678754853E-2,7.713056111075596E-2,0,1.6967091333160501E-3,0.20946277051989973,0.33251451930941056,120.113,0,{"$f":"T2434*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6967091333160501E-3},{"$f":"U2434*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.7617896812070903E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12441,"Mountain South","1990s","Stucco","central furnace","central AC",37.12075367810391,19154.15566,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19154.15566},"Hot-Dry/Mixed-Dry",214.9624537187668,"Metropolitan Area",0.10300007380828684,0.17220825212211205,0.33363125889181389,2.4571602121940442E-2,0.61785757200265279,1.2266971568248657,425.55,857.28399999999999,{"$f":"T2442*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.151050941113E-3},{"$f":"U2442*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6420551180827442E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11115112474939984},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3500518100726413}]
["Single Family Detached",12444,"Mountain North","1980s","Siding","central furnace","central AC",52.884169429896517,10162.215490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10162.215490000001},"Cold/Very Cold",56.706930681072905,"Metropolitan Area",0.24255500106206132,0.25855606989507313,3.5345699644328009E-2,1.035942344379894E-2,0.15487020276001043,0.69132697336147297,771.05600000000004,248.35,{"$f":"T2445*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8356372268574403E-3},{"$f":"U2445*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5237862169415E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25039063828891878},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7869485861269508E-2}]
["Single Family Detached",12449,"Pacific","1950s","Shingle","central furnace","N/A",13.381494796583493,9993.6480929999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9993.6480929999998},"Marine",46.103376950892553,"Metropolitan Area",0.39451679732357819,0.1020057357231923,0,5.7200043971018522E-3,0.15158470360767376,0.64810723665444436,572.36400000000003,0,{"$f":"T2450*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7200043971018522E-3},{"$f":"U2450*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.40023680172068005},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12450,"Pacific","1970s","Stucco","central furnace","N/A",56.535983545239667,21578.61967,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21578.61967},"Marine",115.02985998933821,"Metropolitan Area",0.44576995989739782,0.26757136659299374,0,1.0376510840712899E-2,0.30986608692616413,1.0232074134165559,480.87,0,{"$f":"T2451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0376510840712899E-2},{"$f":"U2451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45614647073811071},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",12456,"West North Central","Before 1950","Siding","central furnace","window/wall unit",18.758894643778245,24393.8812,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8131.293733333333},"Cold/Very Cold",88.512100214161748,"Metropolitan Area",1.0853715193786766,1.3664928267671823,2.0430436564267601E-2,5.2213639075728005E-3,0.30859335488160894,2.7843690468634503,214.04400000000001,0,{"$f":"T2457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7404546358576001E-3},{"$f":"U2457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0871119740145343},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0430436564267601E-2}]
["Single Family Detached",12460,"Pacific","1950s","Wood","heater burning gas/oil/kerosene","N/A",18.129572677198208,9541.8803559999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9541.8803559999997},null,91.800388946721597,"Rural",0.62806614497041047,9.614435860038989E-2,0,0,0.21707857007506956,0.94128907364586989,0,0,{"$f":"T2461*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2461*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62806614497041047},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12467,"South Atlantic","1970s","Stucco","central furnace","both central and individual units",48.551393239361182,25326.75704,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25326.75704},"Mixed-Humid",310.70457771839926,"Metropolitan Area",1.5804055444994214,0.3621335464858873,0.24020157242333515,5.2465896813782401E-2,0.53554567465146785,2.7182863380601114,1679.1890000000001,392.37099999999998,{"$f":"T2468*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2528411827240563E-2},{"$f":"U2468*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9374849865418394E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.622933956326662},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25013905740987696}]
["Multi-Family (2-4 units)",12470,"South Atlantic","1980s","Stucco","central furnace","central AC",33.762996743958098,26817.312740000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8939.1042466666677},"Hot-Humid",178.78150391431657,"Metropolitan Area",3.2812555419737419E-2,0.1330719306724821,0.15074463809828886,8.0975948510939588E-3,0.28797497749259049,0.6100024982504948,20.78,281.17399999999998,{"$f":"T2471*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8575458624573338E-4},{"$f":"U2471*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5134436974522533E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2998310005983154E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15325808179574113}]
["Single Family Attached",12474,"South Atlantic","1970s","Stucco","heat pump","central AC",16.401679791277665,15546.61592,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15546.61592},"Hot-Humid",231.52020421962746,"Metropolitan Area",2.0462875632533836E-2,0.21185637806654642,0.25875042854345431,1.1597728836472239E-2,0.2988694192685854,0.78993910151112001,21.305,724.69200000000001,{"$f":"T2475*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.312206521756E-4},{"$f":"U2475*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.126650818429664E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0794096284709435E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27001693672775096}]
["Single Family Attached",12479,"East North Central","1990s","Siding","central furnace","central AC",34.364830685732791,16164.0784,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16164.0784},"Cold/Very Cold",71.003801726125232,"Metropolitan Area",1.2014227191618287,0.17830027523888159,2.7650321003275198E-2,1.03199073622448E-2,0.18943174864943385,1.5968050640534193,560.30600000000004,78.141000000000005,{"$f":"T2480*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0568301119904014E-3},{"$f":"U2480*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2630772502544001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2104795492738192},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.89133982535296E-2}]
["Single Family Detached",12484,"East North Central","Before 1950","Concrete","central furnace","both central and individual units",54.875508993332048,26768.540969999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26768.540969999998},"Cold/Very Cold",441.83599620174505,"Metropolitan Area",4.8681580996915121,0.32014679782112054,0.28131651290128434,7.7650558405349568E-2,1.0107217516078855,6.4803431620218017,2467.779,433.03500000000003,{"$f":"T2485*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6058843266405626E-2},{"$f":"U2485*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1591715138943949E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.9342169429579181},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.29290822804022831}]
["Single Family Detached",12486,"Pacific","1960s","Wood","central furnace","both central and individual units",28.203396475543581,20348.770909999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20348.770909999999},"Marine",431.31205975043747,"Metropolitan Area",0.93347015629072128,0.81405738256448468,3.9365002556958649E-2,1.0495611152585259E-2,0.60922195401834411,2.3961144954305089,441.91199999999998,73.873999999999995,{"$f":"T2487*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9923660503799189E-3},{"$f":"U2487*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5032451022053397E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.94246252234110117},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.0868247659163991E-2}]
["Multi-Family (2-4 units)",12494,"New England","1980s","Wood","heat pump","central AC",16.981474986317117,25270.052060000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8423.3506866666667},"Cold/Very Cold",268.66154037362924,"Micropolitan Area",0.3521243106208698,0.20678678180098864,2.0315563536362966E-2,5.1123842322586006E-3,0.33403827323765634,0.91667318535071685,168.601,33.709000000000003,{"$f":"T2495*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4201853491226865E-3},{"$f":"U2495*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8394272829684669E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35354449596999249},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0599506264659811E-2}]
["Single Family Detached",12497,"West North Central","1970s","Siding","central furnace","central AC",45.664989415824017,17173.74555,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17173.74555},null,193.57765118395332,"Metropolitan Area",1.2522280532571108,0.14969191333361265,3.8965562799631648E-2,3.4255869167490752E-2,0.43956150213988354,1.8804470315302386,1878.914,115.751,{"$f":"T2498*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2267990946332703E-2},{"$f":"U2498*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.98787822115805E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2844960442034434},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.0953441020789697E-2}]
["Single Family Detached",12499,"South Atlantic","1970s","Siding","N/A","central AC",36.940158713555448,23679.588919999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23679.588919999998},"Hot-Humid",351.6342469391243,"Metropolitan Area",0,0.26026517969080148,0.54916869101734012,2.7608056401416919E-2,0.39034220538080144,1.1997760760889431,0,1165.9010000000001,{"$f":"T2500*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2500*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7608056401416919E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.57677674741875706}]
["Single Family Detached",12504,"Middle Atlantic","1950s","Brick","central furnace","window/wall unit",105.79589189210473,24620.87314,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24620.87314},"Mixed-Humid",120.55728714277438,"Metropolitan Area",2.7801373403769523,0.41191479086112714,2.3502913153332017E-2,9.2954136870218793E-3,0.34683286115428402,3.562387905545696,377.54199999999997,0,{"$f":"T2505*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.2954136870218793E-3},{"$f":"U2505*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.7894327540639741},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3502913153332017E-2}]
["Mobile Home",12508,"Mountain North","1990s","Siding","other","both central and individual units",3.62239197182104,10290.886280000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10290.886280000001},"Cold/Very Cold",104.73077163435673,"Metropolitan Area",0.16146484958587498,0.14786947739427675,2.47966108536996E-3,5.0147488842440004E-5,0.21795046441550808,0.52976445248102977,0,4.8730000000000002,{"$f":"T2509*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2509*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0147488842440004E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16146484958587498},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5298085742124E-3}]
["Single Family Detached",12515,"Pacific","1960s","Stucco","central furnace","N/A",106.99332553777039,20066.265100000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20066.265100000001},"Marine",177.05669677702005,"Metropolitan Area",0.49879317147023,0.56372551844225971,0,5.1351358288493902E-2,0.59128486805710623,1.653803557969596,2559.0889999999999,0,{"$f":"T2516*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1351358288493902E-2},{"$f":"U2516*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55014452975872385},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",12520,"Pacific","1980s","Stucco","central furnace","central AC",17.228259551072295,24061.815019999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1913.911234345609},"Marine",52.851343568796622,"Metropolitan Area",0.15821968091801317,2.6115105942916682E-2,4.6489094579524248E-3,8.7317920526077991E-4,0.14728559402063265,0.33707301561999253,27.853999999999999,8.4350000000000005,{"$f":"T2521*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.331008352146259E-5},{"$f":"U2521*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6143841261705213E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15827299100153464},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.6650532992141298E-3}]
["Single Family Detached",12523,"Pacific","1960s","Stucco","central furnace","central AC",41.283311090130837,23890.80503,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23890.80503},"Hot-Dry/Mixed-Dry",88.695736538039327,"Metropolitan Area",0.57330872339113625,0.17857712595545164,7.6362753496709734E-2,1.168721458504079E-2,0.21879022454516792,1.0470388273884654,312.96100000000001,176.232,{"$f":"T2524*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4768902329938299E-3},{"$f":"U2524*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2103243520469598E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58078561362413006},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.0573077848756697E-2}]
["Single Family Detached",12527,"East North Central","2000s","Siding","central furnace","central AC",54.04600892079403,13338.10684,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13338.10684},"Cold/Very Cold",103.71389097579851,"Metropolitan Area",0.62420491349591978,0.21837463297769424,2.2226541209534958E-2,1.838481964883712E-2,0.35181282848929024,1.216618916172439,1278.3150000000001,100.053,{"$f":"T2528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7050302045174603E-2},{"$f":"U2528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3345176036625201E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.64125521554109444},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3561058813197477E-2}]
["Single Family Detached",12532,"West South Central","1970s","Siding","central furnace","central AC",32.721968211892701,23507.161069999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23507.161069999998},"Hot-Humid",246.89223367687768,"Metropolitan Area",0.37534196725711227,0.31644825425606565,0.59508140826378186,3.7447048627476415E-2,0.26577793387633181,1.5526495636532915,427.93,1165.076,{"$f":"T2533*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.00594194366851E-2},{"$f":"U2533*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.738762919079132E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38540138669379737},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.62246903745457316}]
["Multi-Family (2-4 units)",12538,"New England","Before 1950","Brick","central furnace","window/wall unit",39.614542202681235,47442.56551,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15814.188503333333},"Cold/Very Cold",8.8480384680240132,"Metropolitan Area",0.7134164560492412,0.80928970500949504,0,6.5717441744452009E-4,2.9532332834058046E-2,1.5526766101710907,13.852,0,{"$f":"T2539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1905813914817332E-4},{"$f":"U2539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.71363551418838933},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12542,"East South Central","2000s","Brick","heat pump","central AC",84.104555882698293,31857.786319999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31857.786319999999},"Mixed-Humid",737.11000882737505,"Micropolitan Area",0.69129781124633582,0.33830439563606191,0.53080099167801298,4.1615858127602316E-2,1.1161778756786811,2.6765810742390919,403.14800000000002,903.15300000000002,{"$f":"T2543*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.284340283933536E-2},{"$f":"U2543*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8772455288266961E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.70414121408567121},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.55957344696627997}]
["Single Family Attached",12545,"Mountain South","1980s","Wood","heat pump","central AC",19.330463462459321,17106.60483,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17106.60483},"Hot-Dry/Mixed-Dry",199.42905575425019,"Metropolitan Area",5.5719376653203555E-2,7.3092690559108081E-2,0.15490868897201668,7.9614994209061506E-3,0.39673119591609662,0.68045195210042486,53.420999999999999,411.98399999999998,{"$f":"T2546*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1385193662342999E-4},{"$f":"U2546*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0476474842827196E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.6633228589826987E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16195633645629939}]
["Single Family Detached",12550,"West North Central","1970s","Wood","central furnace","central AC",54.924637343704411,20327.40094,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20327.40094},"Mixed-Humid",216.56290548779774,"Metropolitan Area",1.195335473003698,0.28873414319353297,8.1422136251603841E-2,2.3025741450379358E-2,0.63920144437999249,2.2046931968288273,899.72299999999996,233.02099999999999,{"$f":"T2551*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.828903015593962E-2},{"$f":"U2551*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7367112944397393E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2136245031596375},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.6158847546043582E-2}]
["Single Family Detached",12556,"South Atlantic","2010s","Shingle","heat pump","central AC",27.755012733638381,7765.8121810000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7765.8121810000002},"Hot-Humid",186.21630155840418,"Metropolitan Area",8.058966154764223E-2,0.12524023930113398,0.16111409027296406,1.1388555797624321E-2,0.26842603578842222,0.63537002691016253,212.56899999999999,1253.93,{"$f":"T2557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6507709295029889E-3},{"$f":"U2557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7377848681213311E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.2240432477145214E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17085187514108538}]
["Single Family Detached",12557,"South Atlantic","2000s","Siding","central furnace","N/A",15.382004811352457,12566.99739,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12566.99739},"Mixed-Humid",159.63624301284329,"Metropolitan Area",0.35024337342305989,0.49090887925768523,0,4.4604169506300903E-3,0.54021845932873414,1.3813707120094794,354.93099999999998,0,{"$f":"T2558*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4604169506300903E-3},{"$f":"U2558*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35470379037368999},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12561,"East North Central","1960s","Brick","central furnace","central AC",107.4190470520836,23613.77161,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23613.77161},"Cold/Very Cold",131.15027356167266,"Metropolitan Area",2.5676406459745285,0.39155583913370345,8.0441965953477704E-2,2.766537531530058E-2,0.37758966282514189,3.4172281138868517,934.74300000000005,236.83500000000001,{"$f":"T2562*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2072807716046233E-2},{"$f":"U2562*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5925675992543498E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5897134536905746},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.6034533552732051E-2}]
["Single Family Detached",12568,"West North Central","2000s","Wood","central furnace","central AC",71.227012816231706,34915.202360000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34915.202360000003},"Mixed-Humid",441.95607284100782,"Rural",0.61276134752036937,0.26252353095737807,0.34295377213144584,5.4750738311930162E-2,0.73566366287722373,1.9539023134864169,1090.7760000000001,477.33,{"$f":"T2569*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.808466476943137E-2},{"$f":"U2569*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6666073542498799E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.65084601228980077},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35961984567394467}]
["Multi-Family (5+ units)",12571,"West South Central","1990s","Stucco","central furnace","central AC",46.685804698613687,44378.141349999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3529.9009330154186},"Hot-Humid",363.57085195485058,"Metropolitan Area",0.23329574331994518,0.33595757420941763,0.1864555453571273,1.1842173884823448E-2,0.47389473385073866,1.24050382714778,73.543000000000006,193.304,{"$f":"T2572*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5959950431675297E-4},{"$f":"U2572*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8234396995561243E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23355534282426194},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18713788932708292}]
["Single Family Detached",12575,"Mountain North","1980s","Brick","central furnace","central AC",72.943037444396481,23775.43593,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23775.43593},"Cold/Very Cold",204.61601407944596,"Metropolitan Area",0.79904382839169508,0.23090884068529066,0.14729089404927589,5.6973219771674584E-2,0.53475993421443557,1.7120034973406972,2062.7930000000001,333.51299999999998,{"$f":"T2576*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9043802808352494E-2},{"$f":"U2576*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.9294169633220887E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.8480876312000476},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15522031101259798}]
["Single Family Detached",12580,"West North Central","1970s","Siding","central furnace","central AC",16.699994038244814,13870.426939999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13870.426939999999},null,92.192053550018599,"Micropolitan Area",1.0363343444181794,0.25001637358284462,1.5723196959364381E-2,1.8799199930567358E-2,0.28071486021054198,1.5827887751709304,1306.4659999999999,48.878,{"$f":"T2581*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8121241202594039E-2},{"$f":"U2581*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7795872797331996E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0544555856207734},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6401155687337701E-2}]
["Single Family Attached",12586,"Pacific","Before 1950","Wood","radiator","N/A",38.552450485485835,12416.24814,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12416.24814},"Marine",104.64945350740174,"Metropolitan Area",0.28844567232851898,0.25029436599872612,0,6.7892044829519996E-4,0.30022650655370631,0.83896654488095146,54.68,0,{"$f":"T2587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7892044829519996E-4},{"$f":"U2587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28912459277681418},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12591,"Middle Atlantic","1970s","Stone","wood-burning stove","window/wall unit",49.321176340323618,12241.5429,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12241.5429},"Cold/Very Cold",256.31060966570806,"Metropolitan Area",0.17453912296791152,0.25084132090692812,5.2941086270430301E-2,0,0.39621025492157302,0.87453178506684304,0,0,{"$f":"T2592*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2592*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17453912296791152},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2941086270430301E-2}]
["Single Family Detached",12595,"South Atlantic","2010s","Wood","heat pump","central AC",21.753754929351185,10285.463320000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10285.463320000001},"Hot-Humid",73.759299724327164,"Metropolitan Area",1.7393088750799521E-2,3.22542872798212E-2,5.4298143694561811E-2,3.7369968171289602E-3,0.14772120245392489,0.2516667221791074,31.053999999999998,332.274,{"$f":"T2596*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1940477793928002E-4},{"$f":"U2596*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4175920391896807E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7712493528738802E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7715735733751494E-2}]
["Multi-Family (5+ units)",12598,"East North Central","1990s","Brick","central furnace","central AC",15.301825689564874,16560.417409999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1317.2393229732181},"Cold/Very Cold",152.5150851729737,"Metropolitan Area",0.28685361527309911,0.10034117544767876,2.6326406511599416E-2,6.5514667315700994E-3,0.33239851227842188,0.75195006319380786,326.03899999999999,69.570999999999998,{"$f":"T2599*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2947139162286506E-4},{"$f":"U2599*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1641656938569745E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28728308666472196},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6418048168537985E-2}]
["Single Family Detached",12604,"East North Central","Before 1950","Siding","central furnace","central AC",51.901676059524988,23559.544279999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23559.544279999998},"Mixed-Humid",206.86097398285159,"Rural",2.417035255893492,0.13594542632298548,0.23731232102986069,5.216945382912648E-2,0.2923921796020727,3.0826851828484112,1704.604,509.762,{"$f":"T2605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0159693417865121E-2},{"$f":"U2605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.200976041126136E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.457194949311357},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24932208144112206}]
["Single Family Detached",12609,"West South Central","1990s","Brick","N/A","window/wall unit",10.66261917152868,18805.324820000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18805.324820000002},"Hot-Humid",48.517738029178119,"Metropolitan Area",0,0.20740514978589333,0.11331180439343194,0,7.0039492025848984E-2,0.39075644620517425,0,0,{"$f":"T2610*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2610*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11331180439343194}]
["Single Family Detached",12614,"West South Central","1950s","Siding","central furnace","central AC",27.531498901873093,22790.975910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22790.975910000001},"Hot-Humid",280.21005761611769,"Rural",0.63338973204976345,0.10195761866707236,0.5935449525955877,3.4567506191239293E-2,0.37404025471046043,1.7029325580228842,357.52,1159.1990000000001,{"$f":"T2615*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1482297073431995E-3},{"$f":"U2615*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6419276483896092E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.64153796175710665},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.61996422907948379}]
["Single Family Attached",12616,"South Atlantic","1960s","Siding","heat pump","central AC",90.296396986402073,22871.427810000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22871.427810000001},"Mixed-Humid",414.11121546495582,"Metropolitan Area",0.32544628319391344,0.36579703960771126,0.38851781332272683,3.4018550038893425E-2,0.33318636317909001,1.4129474993034414,430.16,1057.222,{"$f":"T2617*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8383733867496003E-3},{"$f":"U2617*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4180176652143823E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33528465658066303},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.41269798997487067}]
["Single Family Detached",12621,"Mountain North","1950s","Wood","central furnace","central AC",25.712685024324497,17233.703099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17233.703099999999},"Cold/Very Cold",209.18932319637068,"Rural",1.182160857466197,0.28273706367856744,8.4195239261346908E-2,3.1376386445687098E-2,0.43783939202378752,1.9869325524298986,1600.903,219.738,{"$f":"T2622*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7589486993899296E-2},{"$f":"U2622*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7868994517877997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2097503444600963},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.7982138713134705E-2}]
["Single Family Detached",12623,"East South Central","1980s","Wood","central furnace","central AC",34.245425632594653,12143.767949999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12143.767949999999},"Mixed-Humid",217.74947816601332,"Metropolitan Area",0.33547673857636084,0.20086195362395937,9.5912195751409038E-2,1.2077645133512251E-2,0.11071033635615218,0.74296122430788136,560.44000000000005,434.11500000000001,{"$f":"T2624*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8058533098980002E-3},{"$f":"U2624*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2717918236142502E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34228259188625887},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10118398757502328}]
["Multi-Family (2-4 units)",12628,"South Atlantic","2000s","Concrete","N/A","central AC",17.068652455705024,15966.934010000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5322.3113366666666},"Hot-Humid",215.06719244490853,"Metropolitan Area",0,0.25227208069963458,0.24067456737151846,1.0699139108354811E-2,0.23372985587009568,0.73380926334681862,0,670.08100000000002,{"$f":"T2629*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2629*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5663797027849367E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24424094707430341}]
["Multi-Family (5+ units)",12633,"East North Central","Before 1950","Brick","central furnace","central AC",20.933766814310214,17785.698230000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1414.6999145652071},"Cold/Very Cold",67.159579079503146,"Metropolitan Area",0.78866083044417945,0.18590150696652372,7.9155254563406607E-2,1.8940576973168591E-2,0.16745903625798464,1.2386106445811453,866.35400000000004,198.57900000000001,{"$f":"T2634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2256309297832256E-3},{"$f":"U2634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8092969433444429E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78988646137396268},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9436184257741058E-2}]
["Single Family Detached",12639,"West North Central","1960s","Siding","wood-burning stove","window/wall unit",24.29528667812566,11093.73821,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11093.73821},"Mixed-Humid",129.58595602154605,"Rural",7.5121625476114146E-2,0.10404898051447932,7.473602932341096E-2,0,0.31539402324881388,0.56930065856281831,0,0,{"$f":"T2640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.5121625476114146E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.473602932341096E-2}]
["Single Family Detached",12643,"East North Central","2000s","Brick","central furnace","central AC",68.147136414914584,19661.60889,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19661.60889},"Cold/Very Cold",219.51989710296587,"Metropolitan Area",0.8059732527737512,0.43711104934463968,3.9944622928968457E-2,2.776028457661767E-2,0.89574717588504693,2.1787761009324065,1312.6220000000001,99.281000000000006,{"$f":"T2644*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.580826038440958E-2},{"$f":"U2644*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9520241922080901E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83178151315816073},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.189664712117655E-2}]
["Single Family Attached",12646,"Middle Atlantic","1950s","Siding","radiator","window/wall unit",53.591938833541498,37794.033029999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":37794.033029999999},"Mixed-Humid",78.779583174810583,"Metropolitan Area",1.9673153265542758,0.34918470247509148,5.931747028235379E-2,4.3338795615831295E-3,0.28296294265075161,2.6587804419624725,114.67100000000001,0,{"$f":"T2647*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3338795615831295E-3},{"$f":"U2647*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9716492061158588},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.931747028235379E-2}]
["Multi-Family (5+ units)",12653,"East North Central","1990s","Concrete","built-in electric unit","window/wall unit",15.582713057505782,34023.390959999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2706.2692542001278},"Cold/Very Cold",123.72847686953463,"Metropolitan Area",7.588958181697153E-2,0.15424181069501877,1.7562159922341839E-2,0,0.17446807017631055,0.42216162261064266,0,0,{"$f":"T2654*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2654*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.588958181697153E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7562159922341839E-2}]
["Single Family Detached",12657,"Pacific","1990s","Siding","central furnace","central AC",23.134313245377314,13144.496160000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13144.496160000001},"Marine",84.847722726653728,"Metropolitan Area",0.43078345536950641,0.25507471841861423,1.8678723378244801E-2,7.7035159975142415E-3,0.26814158318429338,0.97267848035065874,521.91600000000005,64.147999999999996,{"$f":"T2658*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8603228578425612E-3},{"$f":"U2658*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4319313967167993E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43764377822734896},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9521916517916481E-2}]
["Single Family Attached",12662,"East North Central","1960s","Siding","built-in electric unit","N/A",18.161421466409433,11379.33676,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11379.33676},"Cold/Very Cold",135.06285005792424,"Metropolitan Area",0.24668564332793261,0.11393508586000904,0,0,0.10021371090474963,0.46083444009269131,0,0,{"$f":"T2663*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2663*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24668564332793261},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12667,"Middle Atlantic","1980s","Siding","central furnace","central AC",102.03019532732884,14269.95739,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14269.95739},"Cold/Very Cold",19.806700855151387,"Metropolitan Area",0.37556161891544737,1.1443150180827949E-2,2.0473393266580799E-3,1.2965112486258397E-3,5.2957310219815909E-2,0.4420094186427494,79.373999999999995,11.481999999999999,{"$f":"T2668*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1326635978738599E-3},{"$f":"U2668*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6384765075198E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37669428251332121},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.21118697741006E-3}]
["Single Family Detached",12669,"West North Central","1960s","Siding","central furnace","central AC",34.347144732733739,24781.489710000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24781.489710000002},"Mixed-Humid",186.17002450238607,"Metropolitan Area",0.73281172229162017,0.59438950740357599,0.17123788834351583,3.2234151017936856E-2,0.53089724912141989,2.0293363671601323,1001.0650000000001,299.67,{"$f":"T2670*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4807881996541152E-2},{"$f":"U2670*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4262690213957013E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.75761960428816133},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17866415736491154}]
["Multi-Family (2-4 units)",12672,"South Atlantic","1960s","Brick","built-in electric unit","window/wall unit",31.20206935331862,34668.965949999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11556.321983333333},"Mixed-Humid",316.23650913041098,"Metropolitan Area",0.77730401030966678,0.43773188951920178,8.5074140875739043E-2,0,0.21662078252467895,1.5167308232292864,0,0,{"$f":"T2673*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2673*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.77730401030966678},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5074140875739043E-2}]
["Single Family Detached",12680,"Mountain South","1990s","Stucco","central furnace","central AC",58.197030834614985,13648.45939,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13648.45939},"Hot-Dry/Mixed-Dry",246.94453744052063,"Metropolitan Area",0.32696485433031447,0.17293827773321038,0.39019227054972799,3.5255212614174483E-2,0.47694796564545594,1.3670433682587086,706.11699999999996,1876.9739999999999,{"$f":"T2681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6374091990886288E-3},{"$f":"U2681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.561780341508586E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33660226352940309},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.41581007396481384}]
["Single Family Detached",12681,"East North Central","1970s","Brick","central furnace","central AC",41.120033882415541,18759.13954,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18759.13954},"Cold/Very Cold",87.192142940172246,"Metropolitan Area",2.5696809605110751,0.32455918924596061,5.807769572337472E-2,4.43854372914078E-2,0.28394966659772203,3.2362675120781326,2225.13,140.94,{"$f":"T2682*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1741524164640206E-2},{"$f":"U2682*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6439131267675998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6114224846757152},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0721608850142321E-2}]
["Multi-Family (5+ units)",12687,"Middle Atlantic","1970s","Brick","heat pump","central AC",15.907691217426063,17123.45664,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1362.0242698601678},"Cold/Very Cold",70.257542588911875,"Metropolitan Area",5.6509284897451884E-2,0.11255629902555073,2.7737831206567656E-2,2.2378131779116801E-3,0.15343858600046406,0.35230181544219075,58.631999999999998,72.055000000000007,{"$f":"T2688*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.9858206990441355E-5},{"$f":"U2688*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8140658764774399E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.6589143104442324E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7835971865332432E-2}]
["Single Family Detached",12692,"Mountain South","1980s","Stucco","built-in furnace","N/A",14.446448658125819,11465.435439999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11465.435439999999},"Hot-Dry/Mixed-Dry",66.740104801050165,"Metropolitan Area",0.80087372461496609,0.11542181625204727,7.9031395538580712E-2,0,0.1486858305642991,1.1440127669698932,0,0,{"$f":"T2693*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2693*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80087372461496609},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9031395538580712E-2}]
["Single Family Detached",12695,"East North Central","Before 1950","Siding","central furnace","central AC",57.848686599049749,17728.68115,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17728.68115},"Cold/Very Cold",300.37578602235709,"Metropolitan Area",2.3787079602956758,0.28089570615596099,0.3300915553395305,0.1014967350411123,0.33699201898882009,3.3266872407799877,4701.79,1023.212,{"$f":"T2696*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3356535744258511E-2},{"$f":"U2696*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8140199296853798E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4620644960399343},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.34823175463638428}]
["Multi-Family (5+ units)",12699,"Pacific","1950s","Stucco","built-in electric unit","window/wall unit",20.878921233523108,30391.44284,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2417.378898104771},"Hot-Dry/Mixed-Dry",81.228880817329056,"Metropolitan Area",2.4283522615231E-2,0.23456252345404779,2.4728331772637238E-2,0,0.34534878434457106,0.62892316218648703,0,0,{"$f":"T2700*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2700*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4283522615231E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.4728331772637238E-2}]
["Single Family Detached",12705,"South Atlantic","1990s","Wood","central furnace","central AC",97.029823016821609,66687.163589999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":66687.163589999996},"Cold/Very Cold",950.5664320835732,"Micropolitan Area",1.6271368490595481,0.53143247407376282,0.16119574501960285,5.7392706851807335E-2,2.500570707123464,4.8203357752763774,751.77499999999998,108.851,{"$f":"T2706*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0133742407872245E-2},{"$f":"U2706*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.2589644439350898E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6772705914674204},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16845470946353794}]
["Single Family Detached",12710,"Pacific","2000s","Stucco","central furnace","central AC",69.271840983564715,19242.178049999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19242.178049999999},"Marine",75.622144583952505,"Metropolitan Area",2.9262349847757E-2,0.35322810444068653,1.0384965009228898E-2,1.4094125734502999E-3,0.27187577393258194,0.66475119323025444,47.162999999999997,26.082999999999998,{"$f":"T2711*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0751884337214985E-4},{"$f":"U2711*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0189373007814995E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0169868691129149E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0886858739307049E-2}]
["Multi-Family (5+ units)",12715,"Mountain South","2000s","Concrete","central furnace","central AC",7.57371019481932,10432.10771,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":829.7847908595736},"Hot-Dry/Mixed-Dry",56.774910140922671,"Metropolitan Area",3.8549509131257521E-2,0.25161882845593231,1.8308175661108941E-2,1.1774407009045701E-3,0.24175012758702646,0.55131042621623982,35.28,77.587000000000003,{"$f":"T2716*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9274807421525759E-5},{"$f":"U2716*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4380512568421738E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.857878393867905E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8372556173677362E-2}]
["Single Family Detached",12717,"East South Central","1990s","Siding","central furnace","central AC",51.423942592602167,23122.27635,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23122.27635},"Hot-Humid",337.35401188222374,"Metropolitan Area",0.34940087978078449,0.51389548216329373,0.459193610054136,2.3722923722743951E-2,1.0600571067151294,2.3825470787133436,155.72800000000001,870.24900000000002,{"$f":"T2718*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6007858514328001E-3},{"$f":"U2718*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.012213787131115E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3530016656322173},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.47931574792544718}]
["Multi-Family (2-4 units)",12722,"East South Central","2000s","Siding","central furnace","central AC",16.681804746362214,15605.05589,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5201.6852966666665},"Mixed-Humid",44.079242456071263,"Micropolitan Area",4.0564848625951812E-2,0.15572517787963761,3.1173299453155487E-2,2.0019258049604302E-3,7.732564237422776E-2,0.30612358553627961,37.186,91.100999999999999,{"$f":"T2723*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9342986944184665E-4},{"$f":"U2723*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7387873221162998E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.0758278495393659E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.1647178185367116E-2}]
["Single Family Detached",12729,"South Atlantic","2000s","Siding","central furnace","central AC",24.005973511403099,16003.98234,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16003.98234},"Cold/Very Cold",307.25829642600274,"Micropolitan Area",1.3578726213050352,0.77150035976437115,3.6969871372658288E-2,1.33140329882928E-2,1.0548146020700884,3.2211574545121531,726.85199999999998,105.068,{"$f":"T2730*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1632526571793679E-2},{"$f":"U2730*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6815064164991198E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3695051478768288},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8651377789157407E-2}]
["Single Family Detached",12733,"Pacific","1970s","Stucco","N/A","N/A",52.844427692409226,25652.6348,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25652.6348},"Hot-Dry/Mixed-Dry",80.268813022429057,"Metropolitan Area",0,0.71749457561794994,0,0,0.34887213930058886,1.0663667149185387,0,0,{"$f":"T2734*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2734*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",12734,"South Atlantic","1990s","Siding","central furnace","central AC",19.962540091101804,18065.647140000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18065.647140000001},"Mixed-Humid",262.424444746316,"Metropolitan Area",0.47887244978212617,0.10436692363296403,0.13015847123191501,1.0371560285662561E-2,0.18199437709589411,0.89539222174289934,318.39400000000001,255.71,{"$f":"T2735*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.751993655493161E-3},{"$f":"U2735*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6195666301693996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.48462444343761935},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13477803786208442}]
["Mobile Home",12740,"Pacific","1970s","Siding","central furnace","window/wall unit",14.225770266184986,10976.674590000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10976.674590000001},"Marine",96.188599415570238,"Metropolitan Area",0.31287459914675431,0.3331140064495734,6.80918250176388E-3,4.7105740402509609E-3,0.35179605413823795,1.0045938422363296,429.14400000000001,0,{"$f":"T2741*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7105740402509609E-3},{"$f":"U2741*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31758517318700524},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.80918250176388E-3}]
["Single Family Detached",12744,"West South Central","1960s","Brick","central furnace","central AC",22.192487636033285,22281.614089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22281.614089999999},"Hot-Humid",196.26126975452871,"Metropolitan Area",0.36231370640547117,0.44006564387028124,0.36024978277392861,2.6213806499760926E-2,0.34261983441265581,1.5052489674623368,491.33100000000002,685.14599999999996,{"$f":"T2745*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.094764773245379E-2},{"$f":"U2745*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5266158767307138E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37326135413792494},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37551594154123574}]
["Single Family Attached",12751,"Pacific","1970s","Wood","central furnace","central AC",3.0607671083470014,5223.1520620000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5223.1520620000001},"Marine",23.651722655411238,"Metropolitan Area",0.11635965799705554,6.2673348502682871E-2,3.9092107061312175E-3,1.472192417043258E-3,7.5474489841227357E-2,0.25841670704709696,251.95099999999999,29.908000000000001,{"$f":"T2752*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3159783851729621E-3},{"$f":"U2752*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5621403187029601E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1176756363822285},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.0654247380015138E-3}]
["Mobile Home",12753,"West South Central","2000s","Siding","central furnace","central AC",70.510144661047107,28249.256679999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28249.256679999999},"Hot-Humid",240.93522650253524,"Rural",7.7111967710139312E-2,0.10241533540503556,7.4784567950787473E-2,6.1165855548669596E-3,0.56775915410746269,0.82207102517342501,53.499000000000002,163.023,{"$f":"T2754*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.51130698312332E-3},{"$f":"U2754*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6052785717436403E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.8623274693262635E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9389846522531116E-2}]
["Mobile Home",12758,"South Atlantic","1990s","Siding","central furnace","window/wall unit",22.089865461484187,21240.255249999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21240.255249999998},"Hot-Humid",403.26578698317479,"Metropolitan Area",7.0040994861934741E-2,0.53201421012135719,0.44732058269469949,8.7887928173449993E-4,0.32656705532628799,1.3759428430042793,41.378,0,{"$f":"T2759*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7887928173449993E-4},{"$f":"U2759*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.0919874143669237E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.44732058269469949}]
["Single Family Detached",12763,"South Atlantic","2000s","Brick","heat pump","central AC",131.51721653729783,25557.17383,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25557.17383},"Mixed-Humid",988.32313045723265,"Metropolitan Area",1.5125749325679836,0.55888506958682871,0.23175661810977427,4.8231345108933017E-2,3.6718433013953047,5.9750599216598914,1333.181,554.01300000000003,{"$f":"T2764*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4072338563853236E-2},{"$f":"U2764*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.415900654507979E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5466472711318369},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24591562465485406}]
["Single Family Detached",12768,"Middle Atlantic","Before 1950","Siding","central furnace","window/wall unit",84.166941996731509,33346.648970000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33346.648970000002},"Cold/Very Cold",113.04944172125094,"Metropolitan Area",1.9604379883524052,0.34774309048357921,3.8407069644495445E-2,3.4259513485553748E-2,0.36069976420762778,2.7072879126881078,1027.375,0,{"$f":"T2769*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4259513485553748E-2},{"$f":"U2769*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9946975018379589},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8407069644495445E-2}]
["Single Family Detached",12770,"East North Central","1960s","Siding","central furnace","central AC",42.226642154630241,16019.211740000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16019.211740000001},"Cold/Very Cold",138.99405472287623,"Metropolitan Area",0.50645242521179812,0.44917539723198158,4.2571007141414777E-2,2.5860101857693326E-2,0.37483630682789099,1.3730351364130855,1477.1980000000001,137.12,{"$f":"T2771*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3663547543904526E-2},{"$f":"U2771*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1965543137887999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53011597275570266},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.4767561455203574E-2}]
["Mobile Home",12777,"West South Central","2000s","Siding","central furnace","central AC",28.003640038057377,23029.309239999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23029.309239999999},"Hot-Humid",390.48793828525146,"Metropolitan Area",0.32840050601572562,0.20278925746259571,0.29917932942967607,1.5195152764118319E-2,0.50197574900744535,1.3323448419154427,180.727,479.09100000000001,{"$f":"T2778*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1620179710174796E-3},{"$f":"U2778*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.103313479310084E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33256252398674313},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31021246422277693}]
["Single Family Detached",12781,"South Atlantic","2000s","Siding","heat pump","central AC",17.88292429035744,12050.488069999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12050.488069999999},"Hot-Humid",203.97610499638009,"Metropolitan Area",1.9957223009321377E-2,0.24626396700632908,0.28236087865683618,1.3526106485635708E-2,0.14738438607625223,0.69596645474873886,27.905000000000001,1094.548,{"$f":"T2782*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3626886959334999E-4},{"$f":"U2782*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3189837616042359E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0293491878914726E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.29555071627287854}]
["Multi-Family (2-4 units)",12787,"Middle Atlantic","Before 1950","Stucco","radiator","window/wall unit",64.777034136420554,45746.493029999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15248.83101},"Mixed-Humid",704.68071706547971,"Metropolitan Area",2.4877565519484137,0.83738982939310824,0.23505778699476507,6.9469251920567096E-3,2.0736602119707142,5.6384956637683725,151.857,0,{"$f":"T2788*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.31564173068557E-3},{"$f":"U2788*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4900721936790995},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23505778699476507}]
["Single Family Detached",12788,"East North Central","1950s","Brick","central furnace","central AC",55.102203764031607,20408.223620000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20408.223620000001},"Cold/Very Cold",151.00975268703195,"Metropolitan Area",1.2505815351685767,0.77759852413731823,0.1998055704910873,9.4522871375957343E-2,0.35034105649673319,2.5783266862937153,4123.7340000000004,507.87299999999999,{"$f":"T2789*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4158085621397094E-2},{"$f":"U2789*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0364785754560259E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3347396207899738},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21017035624564756}]
["Single Family Attached",12793,"New England","1970s","Brick","central furnace","central AC",11.094907776507352,8140.0643989999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8140.0643989999999},"Cold/Very Cold",26.972372009841326,"Metropolitan Area",0.39094250658787499,1.9233042979574434E-2,1.0774824163539521E-2,4.6011632614703516E-3,7.047999871281678E-2,0.49143037244380577,503.11799999999999,62.131,{"$f":"T2794*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0954129202960821E-3},{"$f":"U2794*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0575034117426897E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39503791950817108},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.128057450471379E-2}]
["Single Family Detached",12796,"Pacific","1970s","Siding","central furnace","central AC",17.941160878465581,16877.855950000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16877.855950000001},"Cold/Very Cold",209.49665706728888,"Metropolitan Area",1.2233673882245892,0.16644041948167868,3.4542540666533054E-2,1.7484817405673904E-2,0.66425288199406429,2.0886032303668656,948.41200000000003,87.55,{"$f":"T2797*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6007161117251402E-2},{"$f":"U2797*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4776562884225E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2393745493418407},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6020196954955556E-2}]
["Single Family Detached",12804,"South Atlantic","1980s","Wood","central furnace","central AC",31.11733683311115,19184.547989999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19184.547989999999},"Mixed-Humid",256.0639508941361,"Metropolitan Area",0.75711881951543358,0.40776975456592091,0.14997675786021217,1.4435662534199369E-2,1.0245660179370539,2.3394313498786206,427.96499999999997,324.49799999999999,{"$f":"T2805*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.210315080540348E-3},{"$f":"U2805*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2253474536590192E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.76532913459597396},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15620210531387119}]
["Multi-Family (5+ units)",12806,"West South Central","1990s","Siding","central furnace","central AC",30.67267430343869,43140.188889999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3431.4324210261771},"Hot-Humid",326.1123908764269,"Metropolitan Area",0.25725938149625693,0.22498272865043906,0.14352244986273494,1.0861146515701959E-2,0.47693364044149472,1.1126954358145804,108.22799999999999,143.536,{"$f":"T2807*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7137706806282105E-4},{"$f":"U2807*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9253408398441337E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25763075856431977},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14401498394671935}]
["Single Family Detached",12811,"East North Central","Before 1950","Siding","central furnace","central AC",234.71417713172275,35385.824990000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35385.824990000001},"Cold/Very Cold",521.33935951781564,"Metropolitan Area",3.0125352323365351,0.99801543856946184,0.82496035373936716,0.46033249877531046,0.70172925359751703,5.5372402782428809,11290.584999999999,1718.367,{"$f":"T2812*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.3995266648447191},{"$f":"U2812*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.080583393059133E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.4120618971812542},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.88576618766995852}]
["Single Family Detached",12816,"Pacific","1960s","Wood","built-in electric unit","N/A",18.454607050801897,14775.50605,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14775.50605},"Marine",344.54438123118973,"Metropolitan Area",0.60325895619178149,0.19699837947174034,0,0,0.45237113379703653,1.2526284694605585,0,0,{"$f":"T2817*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2817*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60325895619178149},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12822,"East North Central","1960s","Brick","central furnace","central AC",42.999000784170143,20623.021959999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20623.021959999998},"Cold/Very Cold",174.87941095185502,"Metropolitan Area",1.211057535548663,0.45935966589967514,8.2354222938197399E-2,3.0109447077424318E-2,0.42145679944658854,2.1742282238331243,1262.579,197.41300000000001,{"$f":"T2823*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6038194443234838E-2},{"$f":"U2823*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0712526341894796E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2370957299918979},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.6425475572386876E-2}]
["Single Family Detached",12825,"Mountain South","1980s","Stucco","heat pump","central AC",19.683360206358621,8361.6653380000007,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8361.6653380000007},"Hot-Dry/Mixed-Dry",92.08891010706634,"Metropolitan Area",2.0827411618862497E-2,4.9815465779334142E-2,7.5011814090640283E-2,4.9562349807887544E-3,0.16855266048702164,0.31420735197585858,46.543999999999997,546.18899999999996,{"$f":"T2826*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8918535149187197E-4},{"$f":"U2826*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5670496292968821E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1216596970354367E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9578863719937165E-2}]
["Single Family Attached",12829,"West North Central","2000s","Siding","central furnace","central AC",25.957234397136471,12209.42352,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12209.42352},"Cold/Very Cold",124.84040312626409,"Metropolitan Area",0.6204439063876771,0.11695608245296082,4.1521660993733757E-2,1.2155579962276801E-2,0.37432615172074091,1.1532478015551126,827.85500000000002,167.73500000000001,{"$f":"T2830*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.01076323081496E-2},{"$f":"U2830*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0479476541271999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6305515386958267},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.3569608647860955E-2}]
["Single Family Detached",12834,"Pacific","1950s","Wood","central furnace","window/wall unit",19.292423221524476,11678.22229,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11678.22229},"Marine",124.65721020498704,"Metropolitan Area",0.19274091917551386,0.23164488472397041,1.8994745336907901E-2,5.76198816499684E-3,0.39960515339832958,0.84298570263472172,493.39600000000002,0,{"$f":"T2835*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.76198816499684E-3},{"$f":"U2835*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19850290734051071},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8994745336907901E-2}]
["Single Family Detached",12840,"West South Central","1950s","Wood","portable electric heaters","window/wall unit",50.630942409884426,25227.176090000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25227.176090000001},"Hot-Humid",258.84518093255872,"Metropolitan Area",0.2075152439388635,0.18645428552577481,0.15638460162224277,0,0.33282559027849423,0.88317972136537537,0,0,{"$f":"T2841*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2841*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2075152439388635},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15638460162224277}]
["Single Family Detached",12841,"Middle Atlantic","1970s","Wood","built-in electric unit","window/wall unit",53.165790419418478,22152.412670000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22152.412670000002},"Cold/Very Cold",316.12850829776198,"Metropolitan Area",0.54281879908863739,0.24062143368144229,1.4666735837791611E-2,3.6837911601323103E-3,0.2805234891556927,1.0786304577635639,166.29300000000001,0,{"$f":"T2842*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6837911601323103E-3},{"$f":"U2842*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54650259024876968},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4666735837791611E-2}]
["Multi-Family (5+ units)",12849,"West North Central","1950s","Siding","built-in electric unit","window/wall unit",10.499569355127074,13999.425810000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1113.5343825840316},"Cold/Very Cold",51.797875485293567,"Micropolitan Area",0.11185923406514613,9.9028018340713203E-2,8.5517452479998406E-3,0,5.6331771538104057E-2,0.27577076919196325,0,0,{"$f":"T2850*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2850*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11185923406514613},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5517452479998406E-3}]
["Multi-Family (2-4 units)",12852,"East North Central","1950s","Siding","central furnace","N/A",19.587546187412606,30798.028600000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10266.009533333334},"Cold/Very Cold",111.21168126218069,"Metropolitan Area",0.70434727991462509,0.56599834691153561,0,1.27399433087046E-2,0.42561221671064187,1.7044511390759389,413.661,0,{"$f":"T2853*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2466477695682001E-3},{"$f":"U2853*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.70859392768419327},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",12854,"Pacific","1980s","Stucco","central furnace","central AC",13.484698060323804,15716.43131,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1250.1074596005301},"Hot-Dry/Mixed-Dry",108.84048307939914,"Metropolitan Area",3.054344737074428E-2,0.42727233947889326,3.8491493765853743E-2,2.2376583406238698E-3,0.36364977377272878,0.86201672617906844,35.121000000000002,107.256,{"$f":"T2855*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.390502408863022E-5},{"$f":"U2855*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3408152568691444E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0587352394832911E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8625575291540655E-2}]
["Single Family Detached",12859,"Middle Atlantic","1950s","Siding","central furnace","both central and individual units",99.410085315102023,23313.809880000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23313.809880000001},"Cold/Very Cold",401.58091134723145,"Metropolitan Area",3.5537435303534597,0.47933384286521014,0.17224436243966007,9.3782388075196677E-2,0.63467974974478958,4.8400014854031195,3600.2750000000001,422.33600000000001,{"$f":"T2860*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3936126865717012E-2},{"$f":"U2860*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8462612094796804E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.6376796572191767},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18209062364913975}]
["Single Family Detached",12864,"East North Central","1970s","Siding","central furnace","central AC",125.2214597630512,26434.76035,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26434.76035},"Cold/Very Cold",376.0226495961345,"Metropolitan Area",2.5942556743577558,0.45284875121234214,0.10279230579426481,7.675956527966761E-2,0.94668047452474446,4.0965772058891075,2651.4520000000002,252.28399999999999,{"$f":"T2865*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0090498199528201E-2},{"$f":"U2865*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6690670801393993E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6643461725572841},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1094613728744042}]
["Single Family Detached",12868,"East North Central","1950s","Siding","central furnace","N/A",37.320918565051748,28209.311079999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28209.311079999999},"Cold/Very Cold",159.15126306832229,"Metropolitan Area",1.5536613203925629,0.83295675180038187,0,2.8969664850850316E-2,0.77563895784970716,3.1622570300426518,1026.954,0,{"$f":"T2869*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8969664850850316E-2},{"$f":"U2869*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5826309852434133},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12875,"West North Central","Before 1950","Siding","central furnace","central AC",14.213684527873179,7156.94085,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7156.94085},"Cold/Very Cold",149.40309408621792,"Metropolitan Area",0.35737804100915865,0.11754078705614882,2.4791485651701299E-2,2.1654305042571452E-2,0.47417007607052131,0.97388038978753011,2861.0940000000001,164.54300000000001,{"$f":"T2876*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.04766805242899E-2},{"$f":"U2876*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1776245182815502E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37785472153344857},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5969110169982851E-2}]
["Single Family Detached",12878,"West North Central","1950s","Brick","central furnace","central AC",51.698847984697828,24045.97581,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24045.97581},"Mixed-Humid",187.1293184872429,"Metropolitan Area",1.6841855801229331,0.36772871183276457,0.22973833077364367,3.8330175142244974E-2,0.41489323421174862,2.6965458569410896,1131.693,462.34399999999999,{"$f":"T2879*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.721266250234633E-2},{"$f":"U2879*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1117512639898639E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7113982426252794},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2408558434135423}]
["Mobile Home",12882,"West South Central","1980s","Wood","N/A","N/A",29.446971388084176,31393.359690000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31393.359690000001},"Hot-Humid",72.863987837679502,"Micropolitan Area",0,0.1441899835964072,0,0,0.10444542514839279,0.2486354087448,0,0,{"$f":"T2883*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2883*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12888,"Pacific","2010s","Stucco","central furnace","central AC",22.010555720706353,10416.732480000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10416.732480000001},"Hot-Dry/Mixed-Dry",114.46657732151054,"Metropolitan Area",0.1866782211071501,0.13987945668068066,0.1361073807652205,1.087448537210112E-2,0.31047153448826592,0.77313659304131721,393.791,650.15300000000002,{"$f":"T2889*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1020155000316806E-3},{"$f":"U2889*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7724698720694407E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19078023660718177},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14287985063728995}]
["Single Family Detached",12893,"Pacific","2000s","Wood","built-in electric unit","central AC",20.486278598494518,11994.30831,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11994.30831},"Cold/Very Cold",86.781243494370457,"Micropolitan Area",0.11250760747538974,6.7042042367045279E-2,1.341115996773537E-2,6.3260380888601993E-4,0.10313681422203604,0.29609762403220641,0,52.741999999999997,{"$f":"T2894*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2894*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3260380888601993E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11250760747538974},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4043763776621389E-2}]
["Single Family Detached",12898,"West North Central","1950s","Stucco","central furnace","central AC",17.077277236189879,8875.9237190000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8875.9237190000003},"Cold/Very Cold",191.74492031318439,"Metropolitan Area",0.60758454718462118,0.244529772383003,4.1217890303360136E-2,1.8253922939088951E-2,0.31317713390143442,1.2065093437724188,1838.104,218.46199999999999,{"$f":"T2899*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6314870891588777E-2},{"$f":"U2899*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.939052047500178E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62389941807620997},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.3156942350860317E-2}]
["Single Family Detached",12900,"West North Central","2000s","Siding","central furnace","central AC",65.368174041967578,20100.914529999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20100.914529999998},"Cold/Very Cold",100.05147792089726,"Metropolitan Area",1.1982796772524797,0.18439111623061308,5.6084365666734193E-2,1.6890738176815408E-2,0.29540125095148684,1.7341564101013138,677.12400000000002,163.173,{"$f":"T2901*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.361081165021172E-2},{"$f":"U2901*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2799265266036898E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2118904889026916},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9364292193337879E-2}]
["Mobile Home",12905,"East North Central","1990s","Siding","central furnace","central AC",27.545545372063909,32792.315920000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32792.315920000001},"Mixed-Humid",588.5404178816317,"Micropolitan Area",1.3494629902382353,0.25297199257913855,9.5301553203758729E-2,1.9423052680995603E-2,0.3103633659095788,2.0080999019307115,495.62700000000001,96.677999999999997,{"$f":"T2906*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.625275716248184E-2},{"$f":"U2906*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1702955185137602E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3657157474007171},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.8471848722272493E-2}]
["Single Family Detached",12907,"Pacific","2000s","Siding","central furnace","central AC",21.836048710870198,9539.558196,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9539.558196},"Marine",128.32707173062454,"Metropolitan Area",0.35705967243373288,0.20366173550732108,2.1303560111701477E-2,6.2350075391146209E-3,0.42514590324725032,1.0071708713000058,539.50599999999997,114.089,{"$f":"T2908*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1466488840911763E-3},{"$f":"U2908*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0883586550234439E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36220632131782404},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.239191876672492E-2}]
["Multi-Family (5+ units)",12912,"Pacific","1990s","Stucco","N/A","central AC",13.236267650661413,13977.051369999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1111.7546875758787},"Hot-Dry/Mixed-Dry",61.383393897187212,"Metropolitan Area",0,0.15798212243831206,2.5374154603526981E-2,1.14172941820982E-3,0.22910455799032756,0.41351174965696708,0,81.686000000000007,{"$f":"T2913*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2913*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0814793409323228E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5464969396936304E-2}]
["Mobile Home",12917,"Pacific","2000s","Concrete","central furnace","window/wall unit",21.320753912755066,17533.514729999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17533.514729999999},"Marine",82.652988441387649,"Metropolitan Area",0.1820024065442003,0.26174321845288517,9.2872572832747805E-3,1.86765245552487E-3,0.24897939833543134,0.70201228061579157,106.51900000000001,0,{"$f":"T2918*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.86765245552487E-3},{"$f":"U2918*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18387005899972517},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2872572832747805E-3}]
["Single Family Detached",12923,"South Atlantic","2000s","Concrete","portable electric heaters","central AC",17.561048512621287,10553.514730000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10553.514730000001},"Hot-Humid",203.74175458379614,"Metropolitan Area",3.1506072394896993E-2,0.13398933319824616,0.24913246362952651,1.199256033803861E-2,0.28053900582700486,0.69516687504967456,0,1136.357,{"$f":"T2924*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2924*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.199256033803861E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.1506072394896993E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2611250239675651}]
["Single Family Detached",12926,"West South Central","1990s","Brick","central furnace","central AC",22.383912595111205,17218.3943,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17218.3943},"Hot-Humid",352.71818745384593,"Metropolitan Area",0.99872990594153244,0.49843029548217638,0.34684426990501455,2.6314441548832501E-2,0.80786832694300148,2.6518727982717247,633.48099999999999,894.79399999999998,{"$f":"T2927*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.09075256395583E-2},{"$f":"U2927*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.54069159092742E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0096374315810908},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36225118581428872}]
["Single Family Detached",12930,"New England","1980s","Wood","wood-burning stove","N/A",54.368625667019131,12427.114439999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12427.114439999999},"Cold/Very Cold",126.98111280017656,"Micropolitan Area",8.5441320485203809E-2,0.68641548121753315,0,0,0.45458445514380763,1.2264412568465446,0,0,{"$f":"T2931*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2931*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.5441320485203809E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",12935,"South Atlantic","Before 1950","Brick","central furnace","window/wall unit",21.214439756194125,13993.69377,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13993.69377},"Mixed-Humid",133.69026475613077,"Metropolitan Area",0.43522099053448071,0.28959409100435479,7.4438852280682893E-2,6.7360184268209699E-3,0.40913124582554899,1.2083851796450675,481.36099999999999,0,{"$f":"T2936*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7360184268209699E-3},{"$f":"U2936*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44195700896130169},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4438852280682893E-2}]
["Single Family Detached",12940,"Pacific","1980s","Wood","central furnace","window/wall unit",21.058424998429647,10799.19231,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10799.19231},"Hot-Dry/Mixed-Dry",78.762461998511213,"Metropolitan Area",0.23853873688128133,0.29232660879465994,0.13638218974356675,1.0028896721720011E-2,0.16054351427692209,0.82779104969643014,928.67100000000005,0,{"$f":"T2941*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0028896721720011E-2},{"$f":"U2941*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24856763360300133},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13638218974356675}]
["Single Family Detached",12946,"Mountain North","Before 1950","Siding","central furnace","N/A",44.214987169826102,12596.862440000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12596.862440000001},"Cold/Very Cold",75.798785447953108,"Rural",0.85905008833876639,0.10131880684643432,0,1.5183086476969082E-2,0.19929387733307016,1.1596627725182709,1205.307,0,{"$f":"T2947*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5183086476969082E-2},{"$f":"U2947*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.87423317481573548},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12950,"East North Central","Before 1950","Siding","central furnace","window/wall unit",67.358927950848766,29950.612690000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29950.612690000002},"Cold/Very Cold",248.00500014874387,"Metropolitan Area",2.8664301862855308,0.27828306284664056,7.3610279721692193E-2,5.7108450549108257E-2,0.43719130978126958,3.6555148386351326,1906.7539999999999,0,{"$f":"T2951*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7108450549108257E-2},{"$f":"U2951*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.923538636834639},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.3610279721692193E-2}]
["Multi-Family (2-4 units)",12953,"Pacific","Before 1950","Stucco","central furnace","N/A",38.693948060054304,38693.948060000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12897.982686666668},"Hot-Dry/Mixed-Dry",88.208000897985755,"Metropolitan Area",0.52880703625709746,0.66057959882499473,0.10256500338604438,3.4225183998550599E-3,0.32288443555093005,1.6171177529523033,88.450999999999993,0,{"$f":"T2954*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1408394666183532E-3},{"$f":"U2954*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52994787572371582},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10256500338604438}]
["Multi-Family (5+ units)",12960,"Pacific","1960s","Concrete","N/A","N/A",21.249636687135212,23402.683580000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1861.4829754267439},"Hot-Humid",123.05131024334464,"Metropolitan Area",0,0.19413384908097386,0,0,0.22571029434422613,0.41984414342519999,0,0,{"$f":"T2961*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2961*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",12964,"East South Central","1970s","Wood","heater burning gas/oil/kerosene","window/wall unit",20.228223763586072,16079.66913,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16079.66913},"Mixed-Humid",291.30131196925242,"Micropolitan Area",0.5459346751480818,0.31699779708297687,6.5965282877919404E-2,0,0.61095699798921066,1.5398547530981885,0,0,{"$f":"T2965*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2965*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5459346751480818},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5965282877919404E-2}]
["Single Family Detached",12965,"East North Central","2000s","Brick","central furnace","central AC",65.631396551810312,13934.4791,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13934.4791},"Cold/Very Cold",104.09872446717674,"Metropolitan Area",1.7357749064052275,0.23650746129597844,5.6366626162512902E-2,3.8782623379348298E-2,0.28896811362196995,2.3176171074856886,2522.44,260.77300000000002,{"$f":"T2966*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5148887461004003E-2},{"$f":"U2966*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6337359183443003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7709237938662314},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0000362080857204E-2}]
["Single Family Detached",12971,"East North Central","1970s","Brick","central furnace","central AC",56.19675270391275,18245.698929999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18245.698929999999},"Cold/Very Cold",89.123196432490275,"Metropolitan Area",0.81950164461568009,0.17350156236838166,2.0175199837546426E-2,9.2357538499788401E-3,0.27586372847105933,1.2890421352926673,441.16899999999998,65.019000000000005,{"$f":"T2972*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0494367512491689E-3},{"$f":"U2972*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1863170987296699E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.82755108136692923},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1361516936276095E-2}]
["Single Family Detached",12976,"East North Central","2000s","Siding","central furnace","central AC",59.303545443798306,19093.22133,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19093.22133},"Cold/Very Cold",103.69515137812314,"Metropolitan Area",1.0548442871321257,0.34082077883407219,1.5506330584503542E-2,1.6239376631026231E-2,0.3229143348622811,1.7340857314129827,805.89800000000002,44.633000000000003,{"$f":"T2977*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5387188883404341E-2},{"$f":"U2977*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.5218774762189009E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.07023147601553},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.635851833212543E-2}]
["Single Family Detached",12979,"South Atlantic","2000s","Concrete","central furnace","central AC",47.338278807668139,12976.50187,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12976.50187},"Mixed-Humid",340.06732064572412,"Metropolitan Area",0.62569850163230467,0.18351117200417721,0.40658458384953566,4.4289579472422194E-2,0.74059412315802597,1.9563883806440434,2009.4639999999999,1403.596,{"$f":"T2980*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6075813353697679E-2},{"$f":"U2980*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8213766118724523E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.65177431498600236},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.42479834996826016}]
["Single Family Detached",12983,"West North Central","1990s","Wood","central furnace","central AC",36.572621508354679,9551.4811979999995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9551.4811979999995},"Mixed-Humid",162.23129685861264,"Metropolitan Area",0.46596078641911853,0.27324150543519232,0.18471496781334062,4.1302161591587276E-2,0.36867885490267649,1.292596114570328,3180.3580000000002,1143.8050000000001,{"$f":"T2984*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0377129639908882E-2},{"$f":"U2984*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0925031951678389E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49633791605902744},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.195639999765019}]
["Mobile Home",12989,"Pacific","1960s","Siding","built-in electric unit","window/wall unit",5.1383567874307214,11170.340840000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11170.340840000001},"Marine",93.512497190477163,"Metropolitan Area",0.10125930726971259,0.12195630680612912,5.6740304813822006E-3,0,9.0174978054180621E-2,0.31906462261140456,0,0,{"$f":"T2990*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2990*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10125930726971259},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.6740304813822006E-3}]
["Single Family Detached",12994,"South Atlantic","1950s","Wood","central furnace","central AC",46.186503028226234,21724.601610000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21724.601610000002},"Hot-Humid",553.77740961072448,"Metropolitan Area",0.53097659289722543,0.40170806592379571,0.49151302853779927,3.4019878861797213E-2,0.46529082610568406,1.8894885134645045,368.08,1197.8810000000001,{"$f":"T2995*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.9963913606088E-3},{"$f":"U2995*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6023487501188412E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53897298425783424},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.51753651603898765}]
["Multi-Family (2-4 units)",12998,"Pacific","1970s","Concrete","portable electric heaters","N/A",19.674933567884079,19518.783299999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6506.2610999999997},"Marine",75.827701458991086,"Metropolitan Area",7.8478000887311994E-2,0.19883798210858308,0,0,0.18024614582750009,0.4575621288233952,0,0,{"$f":"T2999*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U2999*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.8478000887311994E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13001,"West North Central","1990s","Siding","central furnace","central AC",59.0519188076291,17574.975839999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17574.975839999999},"Mixed-Humid",309.41882059517229,"Metropolitan Area",0.55078759851729453,0.33843949952836849,9.6767447900547351E-2,1.8106197059739839E-2,0.88182824411673311,1.8678227900629434,738.16200000000003,292.06400000000002,{"$f":"T3002*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2973179316006079E-2},{"$f":"U3002*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1330177437337596E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.56376077783330059},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10190046564428111}]
["Mobile Home",13006,"Pacific","1980s","Siding","heat pump","central AC",14.703782211427578,11345.510969999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11345.510969999999},"Marine",65.336800841004802,"Metropolitan Area",6.0485709976768616E-2,7.6040791264011587E-2,1.111342719759768E-2,1.21664721437892E-3,7.5289241926336861E-2,0.22292917036471474,71.575999999999993,35.659999999999997,{"$f":"T3007*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.120662931887199E-4},{"$f":"U3007*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0458092119019995E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.1297776269957333E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.151800811878788E-2}]
["Single Family Detached",13013,"West North Central","Before 1950","Siding","central furnace","window/wall unit",35.544654855367249,13587.406290000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13587.406290000001},"Cold/Very Cold",136.07200423761677,"Micropolitan Area",0.35860609606804517,0.20560065087023704,3.199153452239871E-2,2.1319510063012564E-2,0.41096663364643954,1.0071649151071205,1569.0640000000001,0,{"$f":"T3014*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1319510063012564E-2},{"$f":"U3014*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37992560613105775},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.199153452239871E-2}]
["Single Family Detached",13017,"Middle Atlantic","Before 1950","Brick","central furnace","window/wall unit",96.749546714072522,19825.726790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19825.726790000001},"Cold/Very Cold",276.0577219463899,"Metropolitan Area",2.3593929524043444,0.3334738991224922,0.1153942549803197,4.1997174096612432E-2,0.5752049017732439,3.3834660082804002,2118.317,0,{"$f":"T3018*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1997174096612432E-2},{"$f":"U3018*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.401390126500957},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1153942549803197}]
["Multi-Family (2-4 units)",13022,"Mountain North","1970s","Siding","central furnace","central AC",31.377008639830773,34105.444170000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11368.481390000001},"Cold/Very Cold",86.457300980403261,"Metropolitan Area",0.55529756614785042,0.34296734785260696,6.8264843152676946E-2,1.1810749421515171E-2,0.21592224914915323,1.1903258392499645,259.59199999999998,86.709000000000003,{"$f":"T3023*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9511668209928799E-3},{"$f":"U3023*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8574965284551025E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55824873296884325},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9250592805522454E-2}]
["Single Family Detached",13024,"South Atlantic","2010s","Stucco","central furnace","central AC",20.573504531822067,11878.46682,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11878.46682},"Hot-Humid",197.85526241939783,"Metropolitan Area",4.2899356125166863E-2,0.19634088856700208,0.23872955376817667,1.2346514048108461E-2,0.1971123355946269,0.67508213405497253,58.741999999999997,980.66099999999994,{"$f":"T3025*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.9776489794044002E-4},{"$f":"U3025*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1648749150168019E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.3597121023107303E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25037830291834468}]
["Multi-Family (5+ units)",13027,"Pacific","1980s","Wood","built-in electric unit","N/A",10.090210458013303,15219.0203,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1210.5426753423642},"Marine",85.056060645165545,"Metropolitan Area",6.5403009226275607E-2,0.12872329552449618,0,0,9.6084980283644053E-2,0.29021128503441584,0,0,{"$f":"T3028*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3028*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.5403009226275607E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13035,"South Atlantic","Before 1950","Brick","central furnace","central AC",42.051557817363097,15540.11745,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15540.11745},"Mixed-Humid",188.24003786100323,"Metropolitan Area",0.99684178190857264,0.22138651786785105,0.20994801239725169,2.5752103610740651E-2,0.44718816958465624,1.8753644817583317,900.08600000000001,757.05100000000004,{"$f":"T3036*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3987442155100699E-2},{"$f":"U3036*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.176466145563995E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0108292240636734},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22171267385289165}]
["Single Family Detached",13037,"East South Central","1990s","Brick","central furnace","central AC",142.32889607024708,26593.59045,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26593.59045},"Hot-Humid",629.07481258768462,"Metropolitan Area",0.70119173674767521,0.19272337768088371,0.67607342572788898,6.7942554780411141E-2,0.57641471673063704,2.1464032568870848,604.27,1950.577,{"$f":"T3038*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6069708901221499E-2},{"$f":"U3038*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1872845879189645E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.71726144564889671},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.72794627160707859}]
["Single Family Detached",13042,"South Atlantic","1950s","Brick","built-in electric unit","window/wall unit",53.006099344865596,35056.944009999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35056.944009999999},"Mixed-Humid",695.35560628345775,"Micropolitan Area",0.70192769649716902,0.63995410099017902,0.28371577775904194,0,0.74695578192110135,2.3725533571674915,0,0,{"$f":"T3043*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3043*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.70192769649716902},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28371577775904194}]
["Single Family Detached",13047,"New England","1960s","Wood","central furnace","window/wall unit",33.395563495935377,15812.293320000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15812.293320000001},"Cold/Very Cold",151.02150579016157,"Micropolitan Area",0.48291012608266443,0.20793654315663587,1.9154063390248798E-2,3.2959033510154764E-2,0.25523574547869871,0.96523647810824775,2084.393,0,{"$f":"T3048*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2959033510154764E-2},{"$f":"U3048*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5158691595928192},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9154063390248798E-2}]
["Single Family Detached",13051,"East North Central","1950s","Wood","central furnace","central AC",79.857168648363128,28000.409759999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28000.409759999999},"Cold/Very Cold",220.50322689546272,"Micropolitan Area",3.0129131671868774,1.1192513912049471,0.18073572889958925,0.13794539070271822,0.44235159340487196,4.7552518806962851,4616.2070000000003,310.34199999999998,{"$f":"T3052*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.12925568753698033},{"$f":"U3052*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6897031657379199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.1421688547238578},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18942543206532717}]
["Multi-Family (5+ units)",13054,"South Atlantic","1970s","Brick","built-in electric unit","central AC",59.718892774120633,71605.387019999995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5695.5950556236658},"Mixed-Humid",328.68490923618782,"Metropolitan Area",7.5096579269547117E-2,0.26303415459846269,0.12290612812832548,5.5192000207275596E-3,0.65535577375782161,1.121472830699187,0,77.078000000000003,{"$f":"T3055*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3055*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3900507569736088E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.5096579269547117E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12334513320402284}]
["Single Family Detached",13061,"Mountain North","1980s","Wood","built-in electric unit","N/A",210.18975291330736,38306.862200000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":38306.862200000003},"Cold/Very Cold",213.59546280441555,"Metropolitan Area",0.24696916726803722,0.17548166716764121,0,0,0.30633687415756189,0.72878770859324038,0,0,{"$f":"T3062*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3062*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24696916726803722},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13065,"Pacific","1980s","Stucco","central furnace","N/A",18.448454747223256,10614.76107,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10614.76107},"Hot-Dry/Mixed-Dry",73.547397310551943,"Metropolitan Area",0.24280887000654805,0.21515028429975899,0,2.7269958074494201E-3,0.49262314264694185,0.95058229695324881,256.90600000000001,0,{"$f":"T3066*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7269958074494201E-3},{"$f":"U3066*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24553586581399747},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",13070,"Middle Atlantic","1990s","Siding","central furnace","central AC",70.427061234871744,31867.448520000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31867.448520000002},"Mixed-Humid",89.680640680890349,"Metropolitan Area",1.9567458197340266,0.53791571138361682,9.6480134429483388E-2,2.5064768019332641E-2,0.37358554068440009,2.9647272062315269,623.72299999999996,162.809,{"$f":"T3071*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9876460593239959E-2},{"$f":"U3071*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1883074260926807E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9766222803272666},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10166844185557607}]
["Multi-Family (5+ units)",13072,"South Atlantic","2010s","Wood","central furnace","central AC",41.029507938966098,33824.821049999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2690.4747191147194},"Mixed-Humid",316.94479704663888,"Metropolitan Area",0.17940871220380866,0.3104477930279313,6.8863750409423108E-2,6.3026127310675502E-3,0.51689413817485907,1.0814156877022023,91.613,94.718000000000004,{"$f":"T3073*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4648246044225677E-4},{"$f":"U3073*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.54836384445108E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17965519466425092},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9118586793868217E-2}]
["Single Family Detached",13077,"Mountain South","2000s","Stucco","central furnace","central AC",11.260532019658655,7542.2183649999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7542.2183649999997},"Hot-Dry/Mixed-Dry",107.6134878869582,"Metropolitan Area",8.3893377051017043E-2,4.0420143528432526E-2,0.13479399112177609,7.7246042895024302E-3,0.10806970158460012,0.36717721328582581,183.96299999999999,840.21900000000005,{"$f":"T3078*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.387489117080495E-3},{"$f":"U3078*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3371151724219352E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.5280866168097533E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14113110629419803}]
["Single Family Detached",13080,"New England","1960s","Brick","central furnace","window/wall unit",63.492229337919866,24123.187440000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24123.187440000002},"Cold/Very Cold",337.25542814219432,"Metropolitan Area",2.8117822036230038,0.59988731986694022,7.931653371578376E-2,6.3378970977049198E-2,1.0080200017298193,4.4990060589355467,2627.3049999999998,0,{"$f":"T3081*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3378970977049198E-2},{"$f":"U3081*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8751611746000529},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.931653371578376E-2}]
["Single Family Detached",13088,"West North Central","1950s","Brick","radiator","window/wall unit",41.235765951328688,16560.548569999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16560.548569999999},"Cold/Very Cold",131.06124129631974,"Micropolitan Area",0.78430602358363444,0.14595382793666664,2.7610839572109622E-2,2.5825347467486495E-3,0.25164654445957196,1.2095172355519825,155.94499999999999,0,{"$f":"T3089*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5825347467486495E-3},{"$f":"U3089*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78688855833038307},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7610839572109622E-2}]
["Single Family Detached",13089,"West North Central","Before 1950","Wood","central furnace","central AC",45.83201722416787,23870.8423,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23870.8423},"Cold/Very Cold",224.61569838800929,"Metropolitan Area",1.1171322887938113,0.513761325331338,0.1689143291247294,5.3527236777408706E-2,0.55144643890792922,2.351254382157808,1928.2090000000001,314.16000000000003,{"$f":"T3090*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.60279729604407E-2},{"$f":"U3090*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4992638169680001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.163160261754252},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17641359294169739}]
["Single Family Detached",13095,"South Atlantic","2000s","Stucco","central furnace","central AC",33.422040788253327,14834.461069999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14834.461069999999},"Hot-Humid",436.76035643993572,"Metropolitan Area",0.11400424259675164,0,0.92352165841985467,4.9598753567245739E-2,0.45270045959450889,1.4902263606111152,136.57,3206.9119999999998,{"$f":"T3096*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0259423483298998E-3},{"$f":"U3096*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7572811218915836E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11603018494508154},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.97109446963877055}]
["Multi-Family (5+ units)",13099,"East North Central","1970s","Brick","built-in electric unit","window/wall unit",18.212000893811542,16217.275949999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1289.9453597074432},"Cold/Very Cold",69.945111179883526,"Metropolitan Area",4.2846707968213951E-2,7.7056046113630053E-2,7.262161039513799E-3,0,0.1114878041987004,0.23865271932005819,0,0,{"$f":"T3100*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3100*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.2846707968213951E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.262161039513799E-3}]
["Multi-Family (5+ units)",13106,"Pacific","1980s","Concrete","built-in electric unit","central AC",9.3024870588666246,13842.98669,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1101.0909908860124},"Marine",58.065791989764797,"Metropolitan Area",5.5435375325013581E-2,0.22207604475939155,4.3556059728938811E-3,1.8735098186245999E-4,0.13815706316130019,0.42019653803499102,0,13.534000000000001,{"$f":"T3107*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3107*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4902165470651293E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.5435375325013581E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.370508138364532E-3}]
["Single Family Detached",13109,"Pacific","1980s","Wood","central furnace","central AC",18.538128851214083,14482.91317,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14482.91317},"Marine",102.81104328334312,"Metropolitan Area",0.2048174014988795,0.48429632041151865,2.1881755572418386E-2,4.0332885570606202E-3,0.36061991788369896,1.0716153953665153,217.226,61.26,{"$f":"T3110*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1460652962664198E-3},{"$f":"U3110*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8722326079419996E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20796346679514593},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.2768978833212584E-2}]
["Mobile Home",13113,"East South Central","1980s","Brick","central furnace","central AC",42.488103508910264,30176.209879999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30176.209879999999},"Mixed-Humid",159.38992582050372,"Micropolitan Area",0.38712703575775409,9.5723886637780323E-2,0.12424924660387517,2.5745738745418397E-3,0.38441126739718379,0.99151143639659334,22.661000000000001,62.656999999999996,{"$f":"T3114*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8382309209067999E-4},{"$f":"U3114*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8907507824511597E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38781085884984479},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12613999738632634}]
["Multi-Family (5+ units)",13118,"South Atlantic","2000s","Wood","central furnace","central AC",56.561634150066027,49615.468549999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3946.4854407797807},"Mixed-Humid",400.14875387744081,"Metropolitan Area",0.23249817006595661,0.3998151890606883,9.1753283491983209E-2,8.2490678011229984E-3,0.63360928033998276,1.3652688480903499,79.766000000000005,86.494,{"$f":"T3119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1479535766923997E-4},{"$f":"U3119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4134731171480635E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23281296542362584},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2094630803698022E-2}]
["Single Family Detached",13123,"East North Central","2000s","Siding","central furnace","central AC",127.39255461286851,24316.19672,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24316.19672},"Cold/Very Cold",209.22219793124464,"Metropolitan Area",1.9838445933193636,0.24974282973171064,0.1161672255622592,6.9439884554287595E-2,0.45118279912137077,2.8009374477347042,2531.989,323.71600000000001,{"$f":"T3124*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1568342616876083E-2},{"$f":"U3124*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8715419374115209E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0454129359362399},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12403876749967072}]
["Single Family Detached",13125,"Middle Atlantic","Before 1950","Siding","radiator","window/wall unit",275.55633200462307,67208.86146,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":67208.86146},"Cold/Very Cold",656.96662081590011,"Metropolitan Area",6.9631055385246103,2.2672904708910697,0.47299627475907224,7.6878200358250198E-3,1.0765728480753631,10.779965132250116,114.387,0,{"$f":"T3126*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6878200358250198E-3},{"$f":"U3126*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.9707933585604351},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.47299627475907224}]
["Single Family Detached",13133,"West South Central","1970s","Brick","central furnace","both central and individual units",31.764136035598568,18456.790260000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18456.790260000002},"Hot-Humid",222.78521540054007,"Metropolitan Area",0.25485143373724112,0.16438497794451404,0.47161235280997277,3.0896168561902981E-2,0.42377755727090599,1.3146263217626337,639.03700000000003,1034.9359999999999,{"$f":"T3134*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1794571877379622E-2},{"$f":"U3134*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.910159668452336E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26664600561462076},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.49071394949449615}]
["Multi-Family (5+ units)",13136,"Pacific","1990s","Concrete","N/A","central AC",32.992262323149703,22142.45793,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1761.2428219993865},"Hot-Humid",272.02009573147257,"Metropolitan Area",0,0.30062458637988326,0.25435838377414205,1.301017757855631E-2,0.36120925193835213,0.92816755150973995,0,587.56700000000001,{"$f":"T3137*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3137*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0348481611937136E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25539323193533575}]
["Single Family Attached",13138,"Mountain South","1970s","Stucco","radiator","central AC",28.625244552084968,19354.458790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19354.458790000001},"Hot-Dry/Mixed-Dry",103.95132722830454,"Metropolitan Area",0.35060472423211103,0.2753356210869769,0.14867439126325019,8.1053376699113597E-3,0.25056748791990852,1.0251822245022466,43.064999999999998,375.71899999999999,{"$f":"T3139*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3349976779135005E-4},{"$f":"U3139*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.2718379021200104E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35143822399990238},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15594622916537021}]
["Single Family Detached",13143,"South Atlantic","Before 1950","Siding","central furnace","central AC",125.9847406925829,40173.705580000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":40173.705580000002},"Mixed-Humid",641.3796775192402,"Metropolitan Area",1.2595072562236542,0.36416423609295484,0.35016699394218231,3.8772004818608215E-2,0.46667262828834438,2.4405111145471357,555.23699999999997,409.87200000000001,{"$f":"T3144*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2305927765122458E-2},{"$f":"U3144*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.646607705348576E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2818131839887767},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36663307099566805}]
["Single Family Detached",13148,"East North Central","1960s","Siding","central furnace","N/A",60.380112745994083,18510.15106,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18510.15106},"Cold/Very Cold",51.265251612043699,"Metropolitan Area",1.2374748254222789,2.3998688501555902E-2,0,5.2280440856885199E-3,0.14569030779803277,1.4071638217218678,282.44200000000001,0,{"$f":"T3149*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2280440856885199E-3},{"$f":"U3149*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2427028695079674},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13152,"Pacific","2000s","Stucco","central furnace","central AC",37.742243734074592,16663.242269999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16663.242269999999},"Marine",110.31176357954094,"Metropolitan Area",0.43879550821307001,0.2455017645751319,4.0643614159117852E-2,1.0288818919065119E-2,0.4062921711779659,1.1312330581252856,489.39400000000001,128.06200000000001,{"$f":"T3153*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1548907874843795E-3},{"$f":"U3153*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.13392813158074E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44695039900055439},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.2777542290698592E-2}]
["Single Family Detached",13159,"West South Central","Before 1950","Siding","heat pump","both central and individual units",28.487235933469226,16836.42786,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16836.42786},"Mixed-Humid",363.27911560675142,"Metropolitan Area",1.2480223886979915,0.2093167343066839,0.15786142868165837,2.14245228161286E-2,0.4852903512803316,2.1004909029666656,891.06700000000001,381.44299999999998,{"$f":"T3160*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.500238526392662E-2},{"$f":"U3160*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.42213755220198E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2630247739619183},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16428356623386034}]
["Multi-Family (5+ units)",13162,"West North Central","1980s","Siding","built-in electric unit","window/wall unit",16.49062679418903,22620.88723,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1799.297773853559},"Cold/Very Cold",129.59485938033993,"Micropolitan Area",0.1273228626810782,0.12747182122348774,9.2297065449229113E-3,0,0.17815326305657306,0.44217765350606192,0,0,{"$f":"T3163*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3163*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1273228626810782},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2297065449229113E-3}]
["Single Family Detached",13166,"East North Central","1950s","Siding","central furnace","window/wall unit",43.280051728070127,23650.301490000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23650.301490000002},"Cold/Very Cold",245.73971110560339,"Metropolitan Area",1.1988874450621809,0.50620790760186185,5.3135345210296406E-2,3.3866876979157648E-2,0.24525376835310889,2.003484466227448,1431.9849999999999,0,{"$f":"T3167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3866876979157648E-2},{"$f":"U3167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2327543220413386},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.3135345210296406E-2}]
["Single Family Detached",13171,"South Atlantic","2000s","Siding","central furnace","central AC",50.785705801746005,9868.9673149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9868.9673149999999},"Mixed-Humid",80.956303421105147,"Metropolitan Area",0.10190696636365731,9.5192900650949194E-2,0.11610139349418136,1.2198566656607693E-2,0.15913889410642637,0.47234015461521417,517.79999999999995,718.25300000000004,{"$f":"T3172*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.110151275707E-3},{"$f":"U3172*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0884153809006954E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10701711763936432},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12318980887508206}]
["Single Family Detached",13177,"Pacific","1970s","Siding","central furnace","N/A",35.81212743572253,13789.806479999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13789.806479999999},"Marine",333.92639697251519,"Metropolitan Area",0.38067897068093953,0.18912119730738119,0,7.6155998960642408E-3,0.56955668137530335,1.1393568493636241,552.26300000000003,0,{"$f":"T3178*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6155998960642408E-3},{"$f":"U3178*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38829457057700378},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13181,"West North Central","1970s","Siding","central furnace","central AC",43.918005917949856,17823.866040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17823.866040000001},"Cold/Very Cold",170.442786558069,"Rural",0.96671598117324264,0.15557483048003426,3.3671760466939558E-2,5.8557495703585684E-2,0.33544025730963922,1.4914028294298556,3190.326,95.016000000000005,{"$f":"T3182*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6863943247929045E-2},{"$f":"U3182*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6935524556566403E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0235799244211716},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5365312922596197E-2}]
["Single Family Detached",13184,"South Atlantic","2000s","Brick","heat pump","central AC",72.60347921687881,11076.04565,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11076.04565},"Mixed-Humid",515.99932874874185,"Metropolitan Area",0.3866763502612956,0,0.15014032888842083,2.1758581550146799E-2,1.8015006602576342,2.3383173394073506,919.43499999999995,1045.037,{"$f":"T3185*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.018370403220775E-2},{"$f":"U3185*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.157487751793905E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39686005429350335},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16171520640635989}]
["Single Family Detached",13189,"Pacific","Before 1950","Wood","wood-burning stove","window/wall unit",31.3121715826931,25771.334640000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25771.334640000001},"Marine",470.17331149453457,"Metropolitan Area",6.1045385044476479E-2,0.83482568728227269,2.5457903668108323E-2,0,0.68290240678407521,1.6042313827789327,0,0,{"$f":"T3190*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3190*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.1045385044476479E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5457903668108323E-2}]
["Multi-Family (5+ units)",13195,"Middle Atlantic","1970s","Brick","radiator","central AC",24.748599239671258,19657.3465,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1563.57349902752},"Cold/Very Cold",41.027339307465347,"Metropolitan Area",0.36892744128144567,0.19361701974374651,4.4266106856960141E-2,3.0273493050790002E-3,8.4958422537911887E-2,0.69455554002485187,48.234999999999999,105.771,{"$f":"T3196*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5418967725592438E-5},{"$f":"U3196*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6538073256563984E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36900286024917128},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.4431487589525781E-2}]
["Single Family Detached",13196,"West North Central","2010s","Siding","central furnace","central AC",49.401612919011839,13409.77549,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13409.77549},"Cold/Very Cold",182.42653217800907,"Metropolitan Area",1.051244786522368,0.31077354503729804,2.4994735321545308E-2,3.0955434165952266E-2,0.56782825358953237,1.9548413204707435,2208.5619999999999,99.861000000000004,{"$f":"T3197*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9616320575745377E-2},{"$f":"U3197*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3391135902068902E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0808611070981133},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6333848911752198E-2}]
["Mobile Home",13200,"South Atlantic","1990s","Wood","N/A","window/wall unit",22.525026554764011,27536.707279999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27536.707279999999},"Hot-Humid",506.64740911448848,"Metropolitan Area",0,0.49393550125549346,0.46797279216361826,0,0.76677266661085053,1.7286809600299624,0,0,{"$f":"T3201*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3201*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46797279216361826}]
["Single Family Detached",13207,"South Atlantic","1990s","Siding","central furnace","central AC",68.397195473725915,18946.591540000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18946.591540000001},"Hot-Humid",339.48857029744454,"Rural",0.40284161462004381,9.2104099177233459E-2,0.29559905617620957,2.1708625654701198E-2,0.38848703268522738,1.1790318026587143,353.41199999999998,792.36800000000005,{"$f":"T3208*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6959528093344803E-3},{"$f":"U3208*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5012672845366722E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4095375674293783},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3106117290215763}]
["Multi-Family (5+ units)",13210,"West South Central","2000s","Stucco","central furnace","central AC",21.464620341612967,26931.769560000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2142.1915295603126},"Mixed-Humid",328.31095583493476,"Metropolitan Area",0.17897774533316174,0.53316191301347338,3.4262190928741436E-2,4.4118278304714001E-3,0.36973425272001614,1.1201970067204492,108.411,55.404000000000003,{"$f":"T3211*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3223712591116305E-4},{"$f":"U3211*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1868597950375956E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17920998245907291},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4380876908245192E-2}]
["Multi-Family (5+ units)",13214,"Pacific","1980s","Stucco","N/A","central AC",7.1290264672567618,13201.900869999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1050.0981064316265},"Hot-Dry/Mixed-Dry",68.832612009386054,"Metropolitan Area",0,0.11134976944850537,2.3688697871587415E-2,9.7857770008787982E-4,0.21026745406864136,0.34620666161678088,0,74.123999999999995,{"$f":"T3215*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3215*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7837472041137874E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.3766535343628555E-2}]
["Single Family Detached",13219,"West South Central","1960s","Shingle","central furnace","central AC",82.172640693702945,43408.684990000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":43408.684990000002},"Hot-Humid",309.03840926957355,"Metropolitan Area",1.9038652481233191,0.39417360586013472,0.37070109739943707,3.7256024796887374E-2,0.85291858563396505,3.5216585370168558,359.91300000000001,498.34899999999999,{"$f":"T3220*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.562335004080587E-2},{"$f":"U3220*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1632674756081511E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.919488598164125},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.39233377215551857}]
["Single Family Attached",13224,"West South Central","2000s","Stone","central furnace","central AC",24.134633529144406,13116.648660000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13116.648660000001},"Hot-Humid",373.47136031344786,"Metropolitan Area",0.50270596139688739,0.22649797426131216,0.2192274027924255,1.9318147679853358E-2,0.32585294143248472,1.2742842798831098,641.57299999999998,831.22299999999996,{"$f":"T3225*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4152876307421812E-3},{"$f":"U3225*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0902860049111181E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.51112124902762957},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23013026284153668}]
["Single Family Detached",13230,"South Atlantic","1990s","Siding","built-in electric unit","window/wall unit",45.173125241291864,22884.055339999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22884.055339999999},"Mixed-Humid",584.15169224669762,"Micropolitan Area",1.2064579928424224,0.29446948398497724,0.19727971098511954,0,0.29491835473047112,1.9931255425429903,0,0,{"$f":"T3231*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3231*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2064579928424224},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19727971098511954}]
["Single Family Detached",13234,"Pacific","2000s","Stucco","central furnace","central AC",60.946600611592281,17052.77018,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17052.77018},"Hot-Dry/Mixed-Dry",251.06738962318232,"Metropolitan Area",0.31750581787851301,0.32269968240885677,0.1073052555212274,1.0813178623908178E-2,0.92448506979467404,1.6719958256032712,256.96800000000002,377.13299999999998,{"$f":"T3235*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3820162476142406E-3},{"$f":"U3235*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4311623762939394E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.32188783412612726},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11373641789752134}]
["Multi-Family (5+ units)",13237,"Mountain North","Before 1950","Stucco","radiator","window/wall unit",4.8567050606377951,9180.9169390000006,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":730.26328465000404},"Cold/Very Cold",18.16426972604107,"Metropolitan Area",9.4599254987991155E-2,9.4585542938772166E-2,2.7538343976869282E-3,5.8745015125885396E-4,5.8635220540211919E-2,0.25111457638938939,63.985999999999997,0,{"$f":"T3238*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6726626531615156E-5},{"$f":"U3238*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.464598161452277E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7538343976869282E-3}]
["Single Family Attached",13243,"South Atlantic","Before 1950","Wood","central furnace","central AC",20.282140118698749,13449.695040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13449.695040000001},"Hot-Humid",228.16958413721795,"Metropolitan Area",6.7306914124948811E-2,0.14979100212083518,0.18209517905204931,1.02458431845216E-2,0.37932152056830437,0.77851461586613757,86.641999999999996,675.14800000000002,{"$f":"T3244*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1653084776556799E-3},{"$f":"U3244*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0805347068659194E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.8472222602604493E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19117571375891523}]
["Single Family Detached",13248,"Pacific","Before 1950","Siding","central furnace","window/wall unit",18.848621429753628,13217.827090000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13217.827090000001},"Cold/Very Cold",49.736568485788325,"Metropolitan Area",0.35036384559498152,0.12226126568005026,1.2330844803125551E-2,1.0113554308778049E-2,0.14725675829163212,0.63221271436978943,765.14499999999998,0,{"$f":"T3249*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0113554308778049E-2},{"$f":"U3249*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36047739990375954},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2330844803125551E-2}]
["Single Family Detached",13249,"Middle Atlantic","2000s","Siding","radiator","central AC",72.259266185954672,21252.725350000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21252.725350000001},"Mixed-Humid",546.69484180645009,"Metropolitan Area",1.9893699849932422,0.68359493101356683,9.1592360375486598E-2,7.5378316162366E-3,1.0869349546998872,3.8514922310821831,150.59399999999999,204.08199999999999,{"$f":"T3250*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2005329213579E-3},{"$f":"U3250*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3372986948787004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9925705179146},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.5929659070365297E-2}]
["Single Family Detached",13253,"West North Central","Before 1950","Brick","central furnace","central AC",21.233420430196791,15275.84204,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15275.84204},"Mixed-Humid",105.19329777286585,"Metropolitan Area",0.64939266523653949,0.23349883767489385,9.3671661975226528E-2,1.7406883107948159E-2,0.25171381282675792,1.2282769777134177,885.97799999999995,253.52600000000001,{"$f":"T3254*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.353405997891512E-2},{"$f":"U3254*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8728231290330404E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.66292672521545459},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.7544485104259573E-2}]
["Single Family Detached",13260,"Pacific","2000s","Stucco","central furnace","central AC",60.823304928698121,15806.472169999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15806.472169999999},"Hot-Dry/Mixed-Dry",46.024495355025152,"Metropolitan Area",0.18755389263276662,0.17023289171885375,1.1367840913470128E-2,2.8394272412022897E-3,0.23167709066232348,0.60083171592741391,112.839,66.798000000000002,{"$f":"T3261*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7835865131906299E-3},{"$f":"U3261*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.05584072801166E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18933747914595725},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2423681641481788E-2}]
["Single Family Detached",13262,"Pacific","2000s","Wood","heat pump","central AC",116.60812948079241,18137.833170000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18137.833170000002},"Marine",452.14052206775483,"Micropolitan Area",0.64846954304912185,0.37382320837901117,2.8645007374048324E-2,2.2953319049635979E-2,0.56220715117609132,1.6131449099782726,1157.6389999999999,107.855,{"$f":"T3263*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0997063053085629E-2},{"$f":"U3263*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9562559965503501E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.66946660610220743},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0601263370598673E-2}]
["Multi-Family (5+ units)",13267,"Middle Atlantic","1950s","Brick","central furnace","window/wall unit",26.567171373046616,32008.640210000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2546.0130934896365},"Mixed-Humid",149.54219046653063,"Metropolitan Area",0.64573330142140872,0.57446117841912392,8.5836866261072384E-2,7.3519685439142708E-3,0.34323325821602013,1.656031786752135,229.68700000000001,0,{"$f":"T3268*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8478610940435407E-4},{"$f":"U3268*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6463180875308131},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5836866261072384E-2}]
["Single Family Detached",13272,"South Atlantic","2010s","Stucco","central furnace","central AC",16.565218871670744,10898.17031,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10898.17031},"Hot-Humid",209.88260908816497,"Metropolitan Area",6.1339392550847714E-2,0.22045615559317661,0.233975455742605,1.1974146664706298E-2,0.20034846466637046,0.71611946855299968,94.072999999999993,1004.657,{"$f":"T3273*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0252235755726299E-3},{"$f":"U3273*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.094892308913367E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.2364616126420344E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24492437883173868}]
["Single Family Detached",13278,"West North Central","Before 1950","Siding","other","both central and individual units",28.976564199478677,8649.7206569999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8649.7206569999998},"Mixed-Humid",113.96871937084509,"Metropolitan Area",0.86054558845322149,0.12847495829719091,0.15774441933902827,7.246433226211605E-3,0.33526318131504085,1.4820281474044814,0,837.76499999999999,{"$f":"T3279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.246433226211605E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.86054558845322149},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16499085256523988}]
["Single Family Detached",13282,"Pacific","1990s","Stucco","central furnace","central AC",112.21176045612059,23338.552510000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23338.552510000001},"Hot-Dry/Mixed-Dry",205.30691255333758,"Metropolitan Area",4.5595503142476568E-2,0.44447101659958999,4.3412601649111239E-2,4.4449206797395405E-3,0.82405313216049925,1.3575322535516769,63.847999999999999,126.60599999999999,{"$f":"T3283*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4901199006584801E-3},{"$f":"U3283*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9548007790810601E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.7085623043135051E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.6367402428192296E-2}]
["Single Family Attached",13285,"Mountain North","1990s","Siding","built-in electric unit","central AC",20.540998658596273,13785.905140000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13785.905140000001},"Cold/Very Cold",56.75198075495809,"Metropolitan Area",2.9731978900007162E-2,3.1448365447652581E-2,7.0643940863210405E-3,3.6520241306374002E-4,0.12539300881810359,0.19363774725208438,0,26.491,{"$f":"T3286*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3286*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6520241306374002E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9731978900007162E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4295964993847802E-3}]
["Single Family Detached",13290,"South Atlantic","2000s","Siding","central furnace","central AC",22.664686545358975,18045.132600000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18045.132600000001},"Mixed-Humid",172.06430926834219,"Metropolitan Area",9.8337617773606223E-2,0.2111392574473446,6.6439291011984009E-2,5.0445889988603998E-3,0.21116722740287458,0.58708339363580941,109.643,169.911,{"$f":"T3291*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9785224736618002E-3},{"$f":"U3291*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0660665251986004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10031614024726802},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9505357537182608E-2}]
["Single Family Detached",13296,"West North Central","1950s","Siding","central furnace","central AC",18.474981917383129,13485.38826,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13485.38826},"Cold/Very Cold",130.04061040362726,"Micropolitan Area",0.83848197027536298,8.6524489650611158E-2,2.4763676965038839E-2,1.2110067452915641E-2,0.20362183787935079,1.1533919747703638,816.33600000000001,81.677999999999997,{"$f":"T3297*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1008607910615361E-2},{"$f":"U3297*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1014595423002799E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84949057818597828},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5865136507339119E-2}]
["Multi-Family (5+ units)",13301,"South Atlantic","2010s","Concrete","N/A","central AC",8.6779000504565484,9311.0515560000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":740.61437849918127},"Hot-Humid",66.887586910690487,"Metropolitan Area",0,5.1427181707212999E-2,0.11915950531569698,5.2846455984842527E-3,5.2769472210577491E-2,0.22822045655101006,0,567.56700000000001,{"$f":"T3302*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3302*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2034828096164481E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11957985359665863}]
["Multi-Family (5+ units)",13306,"Pacific","1980s","Stucco","built-in electric unit","window/wall unit",36.151338736470031,28714.327829999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2283.978767804515},"Hot-Dry/Mixed-Dry",103.7675220501424,"Metropolitan Area",2.8430055984483001E-2,8.4815663686058251E-2,2.5131210431733449E-2,0,0.2156778531949271,0.3540547832972018,0,0,{"$f":"T3307*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3307*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8430055984483001E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5131210431733449E-2}]
["Multi-Family (5+ units)",13308,"Pacific","1960s","Stucco","heater burning gas/oil/kerosene","N/A",20.505638047567011,23624.006969999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1879.0873549048658},"Marine",56.039570007310886,"Metropolitan Area",0.1117741540977186,0.40589039498543794,0,0,0.19120699540549321,0.70887154448864975,0,0,{"$f":"T3309*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3309*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1117741540977186},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",13311,"New England","Before 1950","Siding","central furnace","window/wall unit",47.250137792365003,47250.137790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15750.04593},"Cold/Very Cold",387.35662962180828,"Metropolitan Area",0.83758821430965058,0.91348308663290911,8.1395497114081297E-2,3.0133302874194599E-2,1.4471490591499969,3.2997047257894345,637.74,0,{"$f":"T3312*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.00444342913982E-2},{"$f":"U3312*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84763264860104881},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.1395497114081297E-2}]
["Multi-Family (5+ units)",13319,"Mountain South","1980s","Stucco","built-in electric unit","window/wall unit",10.906253230180342,19757.705129999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1571.5561682177238},"Hot-Dry/Mixed-Dry",63.086352470952583,"Metropolitan Area",3.6256613891268052E-2,7.642132161495524E-2,4.9499887516624978E-2,0,5.30428589582417E-2,0.21522068198108998,0,0,{"$f":"T3320*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3320*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.6256613891268052E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.9499887516624978E-2}]
["Single Family Attached",13320,"South Atlantic","1980s","Brick","heat pump","central AC",25.579814900212369,12669.546759999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12669.546759999999},"Mixed-Humid",255.39410448653052,"Metropolitan Area",0.2094061330610418,0.22408614684865238,6.292082075237504E-2,6.8445832720756402E-3,0.37499159796140108,0.87140469862347025,292.738,247.501,{"$f":"T3321*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7088577794288798E-3},{"$f":"U3321*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.13572549264676E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2131149908404707},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6056546245021802E-2}]
["Multi-Family (5+ units)",13325,"Mountain North","1970s","Siding","central furnace","central AC",11.51926912374921,16841.03673,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1339.5601856627538},"Cold/Very Cold",58.430835829785366,"Metropolitan Area",0.10731967843281798,0.12620834599414607,1.2732775249432516E-2,4.6206584065733702E-3,0.18205490789449907,0.43256883218888892,242.744,31.625,{"$f":"T3326*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2517019770851954E-4},{"$f":"U3326*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2363590871584585E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10764484863052649},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2775138840304101E-2}]
["Single Family Detached",13331,"Pacific","1970s","Wood","heat pump","central AC",35.673339089913966,19472.346659999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19472.346659999999},"Marine",365.85534800069195,"Metropolitan Area",0.35699348294553762,0.59461591177413042,3.9376044743212317E-2,8.1879465194100599E-3,0.25731302154995822,1.2482984610128387,322.68200000000002,97.808999999999997,{"$f":"T3332*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.28337576494212E-3},{"$f":"U3332*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9045707544679399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36327685871047977},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1280615497680258E-2}]
["Single Family Detached",13334,"Pacific","1970s","Wood","heat pump","central AC",32.483341339957711,8867.9610539999994,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8867.9610539999994},"Marine",213.46043335441533,"Metropolitan Area",0.37683715892379632,0.11742981518386067,1.7515571011730208E-2,8.6075090378440189E-3,0.95405073090149717,1.4658332760208843,851.98099999999999,118.649,{"$f":"T3335*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5553343267479737E-3},{"$f":"U3335*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0521747110960461E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38439249325054431},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8567745722826254E-2}]
["Single Family Detached",13338,"New England","1980s","Siding","radiator","N/A",43.575527156155317,14129.548360000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14129.548360000001},"Cold/Very Cold",41.996804458291649,"Metropolitan Area",0.95788506541051122,0.22803370074049753,0,9.4802204721419997E-4,0.12999914988850189,1.3159179160395107,67.094999999999999,0,{"$f":"T3339*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4802204721419997E-4},{"$f":"U3339*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95883308745772544},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",13344,"Pacific","1990s","Stucco","central furnace","N/A",33.703502345778169,11964.32458,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11964.32458},"Hot-Dry/Mixed-Dry",42.519941343857631,"Metropolitan Area",1.9075931074676582E-2,5.2222218927872245E-2,0,4.0169023344892004E-4,0.17258233116373206,0.24388048116628089,33.573999999999998,0,{"$f":"T3345*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0169023344892004E-4},{"$f":"U3345*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9477621308125501E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13349,"Pacific","2000s","Shingle","heat pump","central AC",55.415096276995556,15914.73184,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15914.73184},"Marine",178.91581850244739,"Metropolitan Area",0.25892495247712577,0.14768075410928,2.3740100974119039E-2,4.4323483058310402E-3,0.32572837621300027,0.75607418377352509,200.93700000000001,77.569000000000003,{"$f":"T3350*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1978584717340807E-3},{"$f":"U3350*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.23448983409696E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26212281094885986},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.4974590808215999E-2}]
["Single Family Detached",13354,"South Atlantic","1980s","Siding","heat pump","central AC",53.110126433459683,18415.439119999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18415.439119999999},"Hot-Humid",367.47128513843717,"Metropolitan Area",4.1908419945044628E-2,8.2286645807291101E-2,0.67569942109911385,3.9024212285509362E-2,0.45391755500910019,1.2538120418605496,43.097999999999999,2076.0050000000001,{"$f":"T3355*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.9366859519375992E-4},{"$f":"U3355*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8230543690315595E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.2702088540238388E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.71392996478942949}]
["Single Family Attached",13356,"West North Central","2000s","Siding","central furnace","central AC",88.258419555313139,24300.22565,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24300.22565},"Mixed-Humid",174.36646354254017,"Metropolitan Area",1.1889749758288872,0.22172638833394773,0.15419030209911866,3.0710212072633952E-2,0.45452281736342981,2.0194144836253836,940.44500000000005,323.33800000000002,{"$f":"T3357*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2853025711414253E-2},{"$f":"U3357*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8571863612197004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2118280015403016},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16204748846033837}]
["Single Family Detached",13361,"South Atlantic","2000s","Siding","heat pump","both central and individual units",47.373856989317552,13122.952069999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13122.952069999999},"Hot-Humid",416.42104530541684,"Metropolitan Area",0.20911246963692054,0.26109034374500312,0.3330613765284845,2.187111873137617E-2,0.61756441843043064,1.420828608340839,323.83300000000003,1342.798,{"$f":"T3362*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2496449376843107E-3},{"$f":"U3362*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7621473793691857E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21336211457460486},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35068285032217633}]
["Single Family Detached",13368,"Pacific","Before 1950","Shingle","central furnace","N/A",101.67930651450652,16644.181779999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16644.181779999999},"Marine",200.66420294937842,"Micropolitan Area",0.79479558149509943,0.1707678736631669,0,4.362060557193416E-2,0.32037886182868602,1.2859423169869524,2620.7719999999999,0,{"$f":"T3369*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.362060557193416E-2},{"$f":"U3369*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83841618706703358},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13372,"South Atlantic","Before 1950","Brick","central furnace","both central and individual units",130.8065345935911,37491.12485,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":37491.12485},"Mixed-Humid",338.54002101953711,"Metropolitan Area",4.6546476956442513,0.21968243280418723,0.42606121493760168,5.7376230014815746E-2,0.46443896739918039,5.7648303107852206,1198.0419999999999,332.35300000000001,{"$f":"T3373*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4915942197543697E-2},{"$f":"U3373*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2460287817272051E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.6995636378417949},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.43852150275487373}]
["Single Family Attached",13373,"Pacific","1980s","Concrete","N/A","central AC",14.952182352138937,8490.7338739999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8490.7338739999996},"Hot-Dry/Mixed-Dry",54.576739195388221,"Metropolitan Area",0,9.5095285408073854E-2,2.9800123964456901E-2,1.4473899312991581E-3,6.1320428158116815E-2,0.18621583753064758,0,170.46700000000001,{"$f":"T3374*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3374*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4473899312991581E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.1247513895756061E-2}]
["Single Family Attached",13379,"South Atlantic","1990s","Siding","central furnace","central AC",42.395516893671761,16457.886989999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16457.886989999999},"Mixed-Humid",199.13055788171278,"Metropolitan Area",0.34802339919875003,0.21212577124565796,0.16085991409264366,3.0298805369720093E-2,0.53270982419187851,1.2537189087289302,1398.1479999999999,442.84199999999998,{"$f":"T3380*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3010561779294517E-2},{"$f":"U3380*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.2882435904255789E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37103396097804453},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16814815768306923}]
["Single Family Detached",13383,"South Atlantic","1960s","Siding","central furnace","central AC",78.585593366659651,23458.38608,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23458.38608},"Mixed-Humid",228.41407067320341,"Metropolitan Area",1.1378852365585075,0.45416709241244146,0.15503628593563137,4.2360238706206879E-2,0.66817602503262308,2.4152646399392035,1400.9670000000001,404.79399999999998,{"$f":"T3384*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2864424771339364E-2},{"$f":"U3384*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4958139348675207E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1707496613298469},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16453209987049888}]
["Multi-Family (5+ units)",13390,"Pacific","1950s","Stucco","N/A","N/A",15.071829310461586,24192.342390000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1924.2935683310106},"Hot-Dry/Mixed-Dry",41.201470289296324,"Metropolitan Area",0,0.2109711362376743,0,0,0.14057942754810529,0.35155056378577959,0,0,{"$f":"T3391*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3391*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13391,"South Atlantic","1980s","Brick","central furnace","central AC",67.080759096765405,23889.159220000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23889.159220000001},"Mixed-Humid",307.34851022788439,"Metropolitan Area",1.4844956936393581,0.25228968381358169,0.36112370038562469,3.2708248461769743E-2,0.68437930892039223,2.7822883867589567,556.20299999999997,812.96400000000006,{"$f":"T3392*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3287222025641659E-2},{"$f":"U3392*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9421026436128083E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4977829156649998},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.38054472682175278}]
["Single Family Detached",13397,"South Atlantic","Before 1950","Wood","central furnace","N/A",79.169234116530234,32987.18088,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32987.18088},"Mixed-Humid",569.77675557751525,"Metropolitan Area",1.1970911374423154,0.31209283986982989,0,1.9558264479656397E-2,0.43489431709334875,1.9440782944054942,592.90499999999997,0,{"$f":"T3398*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9558264479656397E-2},{"$f":"U3398*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2166494019219718},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",13402,"East North Central","Before 1950","Brick","radiator","central AC",34.134890419873066,34340.936040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2731.5272447348411},"Cold/Very Cold",64.990530516723908,"Metropolitan Area",0.67293776238045155,0.36488934116553168,6.3587953580224302E-2,5.9972667290895598E-3,0.15238330199207042,1.2593185946608743,93.796999999999997,80.841999999999999,{"$f":"T3403*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5620906097439391E-4},{"$f":"U3403*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2082212551885401E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6731939714414259},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.3808775705743156E-2}]
["Multi-Family (5+ units)",13407,"West South Central","1980s","Wood","central furnace","window/wall unit",29.490220865216877,37001.53183,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2943.1548450759242},"Hot-Humid",197.99519680022019,"Metropolitan Area",6.0998950562452754E-2,0.21215905019306752,0.22390514947096921,8.3641962701715004E-4,0.17770392678207625,0.67553696662030993,22.605,0,{"$f":"T3408*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6530015272941266E-5},{"$f":"U3408*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.1065480577725692E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22390514947096921}]
["Single Family Detached",13409,"West North Central","2010s","Siding","central furnace","central AC",23.821877300872629,9393.4847399999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9393.4847399999999},null,146.68800015734064,"Metropolitan Area",0.58960209661556573,0.19314965985053711,1.3049081441872619E-2,1.4311979104257182E-2,0.28058644206634042,1.0763872799743159,1459.9760000000001,63.631,{"$f":"T3410*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.371426227676624E-2},{"$f":"U3410*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9771682749094001E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60331635889233193},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3646798269363559E-2}]
["Single Family Detached",13416,"Middle Atlantic","2000s","Siding","central furnace","central AC",37.014010516801179,13459.64019,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13459.64019},"Cold/Very Cold",192.43446779355014,"Metropolitan Area",0.4200414789559016,0.38330899026761561,6.0245416788640954E-2,1.766221094472465E-2,0.58156784819021223,1.4451637342023704,1097.587,214.648,{"$f":"T3417*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4773126097221529E-2},{"$f":"U3417*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8890848475031199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43481460505312314},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.3134501636144078E-2}]
["Multi-Family (5+ units)",13420,"East North Central","1970s","Brick","built-in electric unit","window/wall unit",11.507356450625508,14715.289580000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1170.475212298049},"Cold/Very Cold",84.842650179033058,"Metropolitan Area",4.1704410899913461E-2,0.1118893965798317,5.6225649956222002E-3,0,0.13026676255528971,0.28948313503065704,0,0,{"$f":"T3421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.1704410899913461E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.6225649956222002E-3}]
["Multi-Family (5+ units)",13426,"Middle Atlantic","1970s","Brick","radiator","window/wall unit",17.293572302830597,20490.014579999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1629.8051108767656},"Mixed-Humid",99.7044109307745,"Metropolitan Area",0.44572659621159522,0.23450971263916434,5.221771618635726E-2,2.0414201526053996E-3,0.38103474944141508,1.1153678171479406,99.63,0,{"$f":"T3427*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6237748319665216E-4},{"$f":"U3427*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44588897369479186},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.221771618635726E-2}]
["Single Family Detached",13427,"South Atlantic","1980s","Concrete","N/A","central AC",15.664838356710144,16116.08884,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16116.08884},"Hot-Humid",188.09243616305008,"Metropolitan Area",0,0.20160787169614669,0.26792852651700444,1.1520344365941402E-2,0.17223499438205064,0.64177139259520177,0,714.83500000000004,{"$f":"T3428*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3428*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1520344365941402E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27944887088294584}]
["Mobile Home",13432,"New England","1980s","Siding","central furnace","window/wall unit",14.317457362625424,17044.592100000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17044.592100000002},"Cold/Very Cold",108.56977347395943,"Rural",1.0690248171191619,5.6721828775392905E-2,9.7120256231721033E-3,6.0252121735737008E-3,1.0140750123168534,2.14953368383458,353.49700000000001,0,{"$f":"T3433*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0252121735737008E-3},{"$f":"U3433*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0750500292927356},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.7120256231721033E-3}]
["Multi-Family (2-4 units)",13435,"New England","1950s","Wood","central furnace","N/A",51.196338937803525,55952.28299,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18650.760996666668},"Cold/Very Cold",223.13770457263436,"Rural",1.9179123440646704,0.33808624259562498,0,3.124744767229334E-2,0.52968023214901971,2.806510450590844,558.46600000000001,0,{"$f":"T3436*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0415815890764447E-2},{"$f":"U3436*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9283281599554347},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13443,"Pacific","1990s","Stucco","central furnace","central AC",69.265619362154993,14141.61277,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14141.61277},"Hot-Dry/Mixed-Dry",175.53227358841795,"Metropolitan Area",0.17168496294742297,0.45374576508759384,0.20829831963120421,1.8220958956085279E-2,0.34865063036896815,1.1823796780351892,272.2,1016.264,{"$f":"T3444*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.849346995994E-3},{"$f":"U3444*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.437161196009128E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17553430994341698},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2226699315912955}]
["Mobile Home",13445,"Pacific","1980s","Siding","central furnace","window/wall unit",12.23504737678253,16489.282179999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16489.282179999998},"Hot-Dry/Mixed-Dry",86.304902924635812,"Metropolitan Area",0.14487056250939534,0.21128162467852857,9.9457100671813778E-2,2.1405231876323394E-3,0.24738738140396566,0.7029966692637033,129.81299999999999,0,{"$f":"T3446*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1405231876323394E-3},{"$f":"U3446*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14701108569702767},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.9457100671813778E-2}]
["Multi-Family (5+ units)",13450,"Pacific","1990s","Stucco","built-in electric unit","window/wall unit",24.549374388970598,21938.67238,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1745.0334274371678},"Hot-Dry/Mixed-Dry",75.724333304578465,"Metropolitan Area",2.9467147193920802E-2,8.3037699448920962E-2,2.1068321369340639E-2,0,0.22820778131320565,0.36178094932538807,0,0,{"$f":"T3451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9467147193920802E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1068321369340639E-2}]
["Multi-Family (5+ units)",13455,"West North Central","1970s","Brick","built-in electric unit","window/wall unit",10.439157370345093,10502.170389999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":835.35767678895593},null,83.019961517245179,"Metropolitan Area",0.13674804650060346,7.6826852621249081E-2,5.0597776591757588E-3,0,0.14145629551248512,0.36009097229351344,0,0,{"$f":"T3456*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3456*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13674804650060346},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0597776591757588E-3}]
["Single Family Detached",13461,"West South Central","1950s","Brick","central furnace","central AC",24.034416656523625,21138.449130000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21138.449130000001},"Hot-Humid",179.5492047555808,"Metropolitan Area",0.75482738398639637,0.35853500649054254,0.27290268401903167,1.866425707468089E-2,0.33354587177477596,1.7198109462707465,292.04399999999998,590.90899999999999,{"$f":"T3462*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1733572377217199E-3},{"$f":"U3462*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.249089983695917E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.76100074122411809},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28539358385599084}]
["Multi-Family (2-4 units)",13462,"West South Central","1990s","Brick","central furnace","central AC",17.738553248917228,24332.720509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8110.9068366666661},"Hot-Humid",104.61242430295495,"Metropolitan Area",0.17541542569090102,0.17021509343985167,0.1548603600400785,1.0742141790829191E-2,0.19348053216284203,0.70113283919422598,176.96,264.50900000000001,{"$f":"T3463*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4353060738165333E-3},{"$f":"U3463*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1454078564598633E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17685073176471755},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15700576789653836}]
["Single Family Detached",13469,"West South Central","Before 1950","Wood","central furnace","central AC",43.175932770995161,24828.023450000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24828.023450000001},"Hot-Humid",553.69729856786978,"Metropolitan Area",0.53351742880974706,0.33308233483535099,0.44298715587215276,3.0005858084450603E-2,0.57962825741329815,1.8892151769305492,315.90600000000001,892.64200000000005,{"$f":"T3470*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8433215759957011E-3},{"$f":"U3470*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.21625365084549E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54136075038574272},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46514969238060766}]
["Single Family Attached",13473,"Middle Atlantic","Before 1950","Siding","central furnace","both central and individual units",75.502303465361564,40332.427060000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":40332.427060000002},"Cold/Very Cold",247.59342924926494,"Metropolitan Area",3.1794376120787287,0.43618192928539729,6.3434800947540948E-2,4.6906209346509402E-2,0.56382942270118575,4.242883765012853,1107.395,55.594999999999999,{"$f":"T3474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4663928064108696E-2},{"$f":"U3474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2422812824007001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2241015401428372},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5677082229941647E-2}]
["Single Family Detached",13479,"South Atlantic","1970s","Brick","heat pump","central AC",37.407849611799342,25258.5075,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25258.5075},"Mixed-Humid",508.81063348594591,"Micropolitan Area",0.7891100500946775,0.1661375047206525,0.30011817621648751,2.639200828257E-2,0.63321209172945003,1.8885778227612675,528.03099999999995,516.84500000000003,{"$f":"T3480*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3337274973732499E-2},{"$f":"U3480*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3054733308837501E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.80244732506840999},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31317290952532501}]
["Mobile Home",13480,"West South Central","2010s","Siding","portable electric heaters","window/wall unit",11.701888048206847,18284.200079999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18284.200079999999},"Hot-Humid",213.45037334212557,"Metropolitan Area",0.20634290257322493,9.6960491361437279E-2,0.15649913095574036,0,0.26849016727714181,0.72829269216754433,0,0,{"$f":"T3481*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3481*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20634290257322493},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15649913095574036}]
["Single Family Detached",13488,"Middle Atlantic","1990s","Brick","heat pump","both central and individual units",29.76064246557414,22393.25994,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22393.25994},"Cold/Very Cold",588.62103495480767,"Metropolitan Area",1.0074877681847598,0.37410657032200723,5.0748075934486735E-2,1.7715934949812318E-2,0.7925535643927496,2.2248959788340033,712.63199999999995,78.495999999999995,{"$f":"T3489*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5958153617562077E-2},{"$f":"U3489*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7577813322502398E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.023445921802322},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2505857266736976E-2}]
["Single Family Detached",13491,"Pacific","1960s","Brick","N/A","central AC",40.766156356715243,14611.52558,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14611.52558},"Hot-Dry/Mixed-Dry",342.34804424295271,"Metropolitan Area",0,0.34702364485584647,0.22534075932393191,1.244802621042056E-2,0.59572478526216166,1.1680891894419401,0,851.93200000000002,{"$f":"T3492*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3492*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.244802621042056E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23778878553435248}]
["Single Family Detached",13493,"West North Central","1990s","Siding","central furnace","central AC",58.809960262913499,21669.10842,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21669.10842},"Cold/Very Cold",88.997476906888537,"Metropolitan Area",1.3379908663058437,0.3500755844468279,7.2194210104119305E-2,3.2821830148930857E-2,0.20249877162567068,1.9627594324824615,1336.76,177.923,{"$f":"T3494*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8966397371519202E-2},{"$f":"U3494*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.85543277741166E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.366957263677363},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.604964288153096E-2}]
["Single Family Detached",13498,"Pacific","1990s","Wood","N/A","central AC",19.147175121861775,13976.040230000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13976.040230000001},"Hot-Dry/Mixed-Dry",139.84343400439175,"Metropolitan Area",0,0.55126747875018323,9.3430667499963788E-2,4.2217424722760999E-3,0.42339115502647651,1.0680893012766235,0,302.07,{"$f":"T3499*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3499*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2217424722760999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.7652409972239881E-2}]
["Single Family Detached",13503,"Mountain North","Before 1950","Siding","central furnace","central AC",43.782659392381163,10575.52159,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10575.52159},"Cold/Very Cold",96.228236146102958,"Metropolitan Area",0.3726184247515747,0.33363837411103348,5.6383044364872528E-2,1.3123355100419622E-2,0.24927043739231086,1.0119102806197917,881.12900000000002,359.78899999999999,{"$f":"T3504*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.3183987630751103E-3},{"$f":"U3504*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8049563373445099E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3819368235146498},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.018800070221704E-2}]
["Single Family Attached",13507,"South Atlantic","2000s","Concrete","N/A","central AC",32.784842255134393,16392.421129999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16392.421129999999},"Hot-Humid",147.77608640016894,"Metropolitan Area",0,9.8546859057118283E-2,6.5721543909348312E-2,4.3975456392817093E-3,0.33994361970803388,0.50421202267450049,0,268.267,{"$f":"T3508*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3508*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3975456392817093E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0119089548630026E-2}]
["Single Family Detached",13514,"New England","Before 1950","Wood","central furnace","N/A",61.936502136509546,17716.390770000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17716.390770000002},"Cold/Very Cold",105.30378188275684,"Micropolitan Area",1.6273861997777983,0.13648544458412917,0,2.7578946064142074E-2,0.16651543559491039,1.9303870799568377,1556.691,0,{"$f":"T3515*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7578946064142074E-2},{"$f":"U3515*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6549651458419403},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13517,"Middle Atlantic","Before 1950","Wood","wood-burning stove","window/wall unit",86.469641802465262,28594.458269999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28594.458269999999},"Cold/Very Cold",233.47835546609099,"Metropolitan Area",0.69746970674656228,0.30871669456597911,8.6696767590518614E-2,0,0.48306465557515238,1.5759478244782124,0,0,{"$f":"T3518*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3518*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.69746970674656228},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.6696767590518614E-2}]
["Single Family Detached",13521,"Pacific","1980s","Wood","heater burning gas/oil/kerosene","N/A",20.647962806666385,13168.343629999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13168.343629999999},null,43.132132616983512,"Rural",0.31178631905707754,2.2595639844778779E-2,0,0,0.1980492413581304,0.53243120025998669,0,0,{"$f":"T3522*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3522*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31178631905707754},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13527,"South Atlantic","2010s","Stucco","central furnace","central AC",47.710967427468368,11013.612059999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11013.612059999999},"Hot-Humid",222.10471893879316,"Metropolitan Area",9.2671252235018833E-2,0.15632585490535661,0.21798769866400625,1.7401562122860301E-2,0.29083649772286807,0.75782130352724986,181.952,1398.0530000000001,{"$f":"T3528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0039487415411199E-3},{"$f":"U3528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.539761338131918E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.4675200976559959E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23338531204532542}]
["Single Family Detached",13532,"New England","2010s","Wood","wood-burning stove","central AC",40.535979684350977,18096.4195,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18096.4195},"Cold/Very Cold",97.413026178955946,"Rural",0.42666764309730898,0.19437431141702152,1.8335147466043998E-2,9.0138265529500006E-4,0.49922529137181759,1.1386023933521923,0,49.81,{"$f":"T3533*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3533*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0138265529500006E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42666764309730898},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9236530121339E-2}]
["Mobile Home",13533,"West South Central","1990s","Siding","central furnace","central AC",88.025138179247122,41365.196510000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":41365.196510000002},"Hot-Humid",93.298621621878453,"Metropolitan Area",4.6268668269491907E-2,6.0201128297204066E-2,6.1730234151392734E-2,3.3146759267393203E-3,0.46268548310422031,0.63088551382230906,13.845000000000001,66.287000000000006,{"$f":"T3534*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7270114568095006E-4},{"$f":"U3534*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7419747810583702E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.6841369415172855E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4472208932451106E-2}]
["Multi-Family (5+ units)",13541,"West South Central","2000s","Brick","central furnace","central AC",28.061094536363697,28633.769939999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2277.5710778377347},"Hot-Humid",377.70370688041226,"Metropolitan Area",0.24904301190115885,0.40709435332633315,0.19596767459119341,1.2780339607479718E-2,0.42485622442535448,1.2887250373317798,138.37899999999999,307.959,{"$f":"T3542*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1516800818010785E-4},{"$f":"U3542*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0139851155983095E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24935817990933895},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19666907310275325}]
["Single Family Detached",13544,"Pacific","1960s","Wood","built-in furnace","central AC",8.8835085104627876,10353.739519999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10353.739519999999},"Cold/Very Cold",390.97017761216591,"Micropolitan Area",0.78075632207760892,0.27333024361533309,4.8333927344156154E-2,2.0181094922803199E-3,0.23156975018633222,1.3339902432234303,0,194.916,{"$f":"T3545*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3545*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0181094922803199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78075632207760892},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0352036836436471E-2}]
["Single Family Detached",13546,"Pacific","1970s","Stucco","central furnace","both central and individual units",18.518331076145927,9639.9432980000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9639.9432980000001},"Hot-Dry/Mixed-Dry",38.638897848025366,"Metropolitan Area",1.9879134391233576E-2,3.9271393806258367E-2,4.6217763427817797E-2,2.6550813828516498E-3,0.12705693977301089,0.23242523139832061,108.876,166.54900000000001,{"$f":"T3547*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0495584665130482E-3},{"$f":"U3547*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6055229163386021E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0928692857746626E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7823286344156397E-2}]
["Mobile Home",13551,"South Atlantic","1980s","Siding","built-in electric unit","window/wall unit",24.719093191352624,27588.273649999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27588.273649999999},"Mixed-Humid",322.27721901451002,"Metropolitan Area",0.45585348783036611,0.28270128868569211,8.3263230701760893E-2,0,0.27779190021312727,1.0996099074309464,0,0,{"$f":"T3552*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3552*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45585348783036611},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.3263230701760893E-2}]
["Multi-Family (5+ units)",13556,"East North Central","Before 1950","Brick","radiator","N/A",10.682807319733968,39713.038359999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3158.8319586043481},"Cold/Very Cold",48.052776419621189,"Metropolitan Area",0.30971945629096842,0.38758233663925862,0,4.3703007324029201E-3,0.13385084985350049,0.83517532353558188,110.047,0,{"$f":"T3557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4761998054853269E-4},{"$f":"U3557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31006707627151697},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13562,"East South Central","1970s","Brick","central furnace","central AC",16.036666123205425,11603.95523,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11603.95523},"Hot-Humid",181.00877472933675,"Metropolitan Area",0.18275822188421426,5.31153296601748E-2,0.16234992807882501,1.0668618418685849E-2,0.21937844795725744,0.6176019275804715,261.29000000000002,658.10500000000002,{"$f":"T3563*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0319974620467002E-3},{"$f":"U3563*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6366209566391501E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18579021934626094},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16998654903546415}]
["Single Family Detached",13565,"New England","2000s","Siding","wood-burning stove","N/A",38.201374761388003,14404.741609999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14404.741609999999},"Cold/Very Cold",120.90954064051843,"Rural",0,0.1566293817066706,0,0,0.43367970958626012,0.59030909129293074,0,0,{"$f":"T3566*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3566*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13569,"West South Central","1990s","Brick","central furnace","central AC",96.372536015196005,31535.51571,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31535.51571},"Mixed-Humid",564.72931156419827,"Metropolitan Area",0.94106952029467461,0.42664291983305586,0.81614214244879246,8.881186458277178E-2,1.199101056783854,3.382955639360377,1371.319,1444.93,{"$f":"T3570*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3245251867921483E-2},{"$f":"U3570*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5566612714850296E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.98431477216259611},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.86170875516364276}]
["Single Family Detached",13574,"East North Central","1970s","Siding","central furnace","central AC",37.133576146233679,25609.362860000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25609.362860000001},"Cold/Very Cold",184.53251523815658,"Metropolitan Area",2.9902299282453351,0.26484383570200482,0.28971360016260794,6.6752135981458724E-2,0.28581342224584388,3.8306007863557916,2112.4290000000001,494.12299999999999,{"$f":"T3575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4097960776986941E-2},{"$f":"U3575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.265417520447178E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.044327889022322},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30236777536707971}]
["Multi-Family (5+ units)",13579,"South Atlantic","1990s","Siding","central furnace","central AC",58.025969568120459,44635.361210000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3550.3605691376988},"Mixed-Humid",291.99033896640105,"Metropolitan Area",0.33426651240042315,0.25020440996987925,8.7692470450722218E-2,9.9266365209367408E-3,0.31497067616847896,0.99627112662202755,129.886,92.507999999999996,{"$f":"T3580*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6114213288301909E-4},{"$f":"U3580*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2843675552979024E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33472765453330616},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.8020907206252011E-2}]
["Single Family Detached",13585,"East North Central","1960s","Brick","radiator","central AC",72.846147401497277,27489.112229999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27489.112229999999},"Cold/Very Cold",194.10062143470651,"Metropolitan Area",2.6177798559510066,0.62782683053420307,0.14659872080567202,1.3591029423195448E-2,0.97390590201576477,4.3661113093066461,260.12099999999998,234.29400000000001,{"$f":"T3586*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.150495362379829E-3},{"$f":"U3586*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4405340608156203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6249303513133864},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15303925486648765}]
["Multi-Family (5+ units)",13589,"West South Central","1990s","Siding","central furnace","central AC",78.596036827154961,77664.068010000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6177.511220403374},"Hot-Humid",1148.8068940190478,"Metropolitan Area",0.47783152853427607,1.2317133642686631,0.29610866548575432,2.141594441782551E-2,1.8942618005867087,3.9196278483966904,101.848,173.90299999999999,{"$f":"T3590*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2916716277564282E-4},{"$f":"U3590*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.074287733761808E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.47846069569705174},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2971829532195161}]
["Single Family Detached",13592,"East South Central","1970s","Brick","heater burning gas/oil/kerosene","central AC",57.307747586593138,15963.160889999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15963.160889999999},"Mixed-Humid",206.61832690151704,"Micropolitan Area",0.84217122473740302,0.1544375156096118,0.1816915000129132,8.7170351935240802E-3,0.36885271325214147,1.5471529536120696,0,546.072,{"$f":"T3593*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3593*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7170351935240802E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84217122473740302},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19040853520643727}]
["Mobile Home",13599,"East North Central","1960s","Siding","central furnace","window/wall unit",33.10327098955824,34482.573949999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34482.573949999998},"Cold/Very Cold",315.2878976660258,"Metropolitan Area",3.6626521433652202,0.40386649227402444,4.4326762608967847E-2,2.3355357679500546E-2,0.74370294814919802,4.8545483463974106,677.30899999999997,0,{"$f":"T3600*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3355357679500546E-2},{"$f":"U3600*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.6860075010447209},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.4326762608967847E-2}]
["Single Family Detached",13603,"Pacific","Before 1950","Wood","central furnace","N/A",41.22842912473169,16360.48775,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16360.48775},"Marine",47.619931791744207,"Metropolitan Area",0.71594201167070803,0.25586531631101828,0,1.0294476985956999E-2,0.17713670235997617,1.1489440303417024,629.22799999999995,0,{"$f":"T3604*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0294476985956999E-2},{"$f":"U3604*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.72623648865666501},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",13604,"South Atlantic","2000s","Siding","central furnace","central AC",17.856367364201745,9909.1938759999994,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9909.1938759999994},"Mixed-Humid",73.266369767472526,"Metropolitan Area",0.12166780743784388,7.3666086831479724E-2,7.5620090681082053E-2,1.2719104346641816E-2,0.18004298747168643,0.45099697242209208,924.33100000000002,359.23500000000001,{"$f":"T3605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1593750845969553E-3},{"$f":"U3605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.55972926204486E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13082718252244083},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9179819943126908E-2}]
["Single Family Detached",13608,"Pacific","1970s","Wood","central furnace","central AC",24.280304049440922,19740.084589999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19740.084589999999},"Hot-Dry/Mixed-Dry",135.63536486411681,"Metropolitan Area",0.4032991467932035,0.14436739126160564,8.8447284833361867E-2,1.1642978252366262E-2,0.36670191826715004,1.0028157411553211,386.96300000000002,202.851,{"$f":"T3609*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6386823532001704E-3},{"$f":"U3609*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0042958991660894E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.41093782914640364},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.245158073252796E-2}]
["Single Family Detached",13615,"South Atlantic","2000s","Siding","heat pump","central AC",100.928069776206,14952.306629999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14952.306629999999},"Hot-Humid",290.20776440994456,"Rural",0.11792072328830991,0.10443345861422394,0.22984189335055882,1.646162236584546E-2,0.73737682924894721,1.18957290450204,155.65600000000001,945.28599999999994,{"$f":"T3616*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3274162407992799E-3},{"$f":"U3616*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4134206125046178E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12024813952910919},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.243976099475605}]
["Single Family Detached",13618,"West South Central","1970s","Wood","central furnace","central AC",43.527380582472979,23656.185099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23656.185099999999},"Hot-Humid",309.48135553052492,"Metropolitan Area",0.63105771636924757,0.40667286299328731,0.49728400040448095,3.3725298350704404E-2,0.46554608182021284,2.0005606615872287,365.02800000000002,1060.616,{"$f":"T3619*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6351699346827997E-3},{"$f":"U3619*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5090128416021595E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6396928863039304},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.5223741288205026}]
["Multi-Family (5+ units)",13622,"West South Central","Before 1950","Wood","central furnace","central AC",26.224401238127339,25337.585739999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2015.3878649085011},"Hot-Humid",207.31096097381732,"Rural",0.29437190727765344,0.11278582884410548,0.17552217358187944,1.30634257679005E-2,0.11264072049057257,0.70734497236366112,192.309,323.26600000000002,{"$f":"T3623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8757722491268896E-4},{"$f":"U3623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5150637353751152E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29475948450256612},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17617367995541694}]
["Single Family Detached",13628,"East South Central","1980s","Wood","heater burning gas/oil/kerosene","central AC",28.92592461377664,18078.702880000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18078.702880000001},"Hot-Humid",176.40207560909005,"Rural",0.32949694276520447,8.1246847779704326E-2,0.18817517999115807,9.0130830847153613E-3,0.35100967717855763,0.94992864771462449,0,498.54700000000003,{"$f":"T3629*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3629*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0130830847153613E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.32949694276520447},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19718826307587342}]
["Single Family Detached",13633,"Mountain North","1990s","Stucco","central furnace","central AC",71.470248368744748,20064.640189999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20064.640189999998},"Cold/Very Cold",121.67157683972509,"Metropolitan Area",1.1521334499736862,0.21409233929516486,0.11035522007539715,2.6474028658373033E-2,0.34180411520339798,1.8183851245476466,1025.171,294.26600000000002,{"$f":"T3634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0569687248222487E-2},{"$f":"U3634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9043414101505398E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1727031372219086},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1162595614855477}]
["Single Family Detached",13637,"East South Central","1950s","Brick","central furnace","central AC",29.54780530230255,10470.51924,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10470.51924},"Mixed-Humid",124.79092560450086,"Metropolitan Area",0.45169682837557956,8.497935191247516E-2,0.25884590481025521,2.436130688338068E-2,0.16765929403569246,0.96318137913400248,1114.4780000000001,1212.1790000000001,{"$f":"T3638*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.166916334155672E-2},{"$f":"U3638*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.269214354182396E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.46336599171713627},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27153804835207918}]
["Single Family Detached",13640,"West South Central","2000s","Wood","other","window/wall unit",33.369154963158813,30557.834220000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30557.834220000001},"Hot-Humid",507.84941692326993,"Rural",0.19388004631296024,0.43519339912041283,0.3199989814202629,0,1.4423374757582232,2.3914099026118594,0,0,{"$f":"T3641*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3641*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19388004631296024},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3199989814202629}]
["Single Family Detached",13645,"East North Central","1990s","Brick","central furnace","central AC",22.488725219203367,14698.513220000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14698.513220000001},"Cold/Very Cold",58.3551993515972,"Metropolitan Area",1.106997857054713,0.15805738992200702,3.7638453405427555E-2,1.0504145487540801E-2,0.19437644598675441,1.497070146368902,596.16899999999998,118.471,{"$f":"T3646*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7627979278541799E-3},{"$f":"U3646*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7413475596866203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1157606549825672},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9379800965114176E-2}]
["Multi-Family (5+ units)",13652,"Middle Atlantic","Before 1950","Brick","radiator","window/wall unit",36.158713340208344,50360.324990000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4005.7323889965191},"Mixed-Humid",87.21688134990697,"Metropolitan Area",0.98913536651444178,0.55383238624340103,9.1636906359928758E-2,4.0402074326477402E-3,0.26996155814139389,1.9082850608051736,80.225999999999999,0,{"$f":"T3653*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2136388663963472E-4},{"$f":"U3653*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.9894567304010814},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.1636906359928758E-2}]
["Single Family Detached",13656,"Pacific","Before 1950","Wood","central furnace","N/A",41.130266198244229,16360.48775,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16360.48775},"Marine",73.833785053636021,"Metropolitan Area",0.70223661839619234,0.54609002916776028,0,1.0498721315028001E-2,0.42637001683324005,1.6746966643971926,641.71199999999999,0,{"$f":"T3657*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0498721315028001E-2},{"$f":"U3657*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.71273533971122038},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13661,"South Atlantic","1950s","Brick","central furnace","central AC",66.102549654426213,21399.336240000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21399.336240000001},"Mixed-Humid",449.36046749548848,"Metropolitan Area",1.7594925864381192,0.33734050604487936,0.2353585666986972,3.5203363269664327E-2,0.72432753636456726,3.0565191955462634,1113.69,531.37800000000004,{"$f":"T3662*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3832226777125601E-2},{"$f":"U3662*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.137113649253872E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7833248132152448},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24672970319123591}]
["Single Family Detached",13663,"Mountain North","1960s","Wood","wood-burning stove","N/A",53.743111905165208,23790.664850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23790.664850000001},"Cold/Very Cold",263.66158963756851,"Metropolitan Area",0.11734945278847241,0.38086308823711051,0,0,2.4796685468486448,2.9778810878742275,0,0,{"$f":"T3664*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3664*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11734945278847241},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",13666,"South Atlantic","1980s","Brick","heat pump","central AC",9.6556602951000237,9882.9685719999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9882.9685719999998},"Mixed-Humid",151.66881906672242,"Metropolitan Area",7.5998101139808455E-2,0.18218604239743677,7.4772583387974739E-2,4.3970908451799514E-3,0.1845372796844641,0.51749400660968414,124.553,320.363,{"$f":"T3667*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2309533845483161E-3},{"$f":"U3667*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.166137460631636E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.7229054524356772E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.7938720848606369E-2}]
["Multi-Family (5+ units)",13674,"South Atlantic","2000s","Shingle","central furnace","central AC",23.042666116033935,22480.649870000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1788.1430933543581},"Mixed-Humid",270.21507344141645,"Metropolitan Area",0.22171536185077628,0.38864916177913866,5.6712610021485248E-2,6.1115220317085909E-3,0.24927131320817603,0.92197384967435481,157.95400000000001,113.90300000000001,{"$f":"T3675*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8244435416769427E-4},{"$f":"U3675*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0367486276234148E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22199780620494397},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.6916284884247589E-2}]
["Single Family Attached",13675,"Middle Atlantic","1980s","Siding","heat pump","both central and individual units",26.481304103365762,19747.430349999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19747.430349999999},"Mixed-Humid",630.44473147607584,"Metropolitan Area",0.86826001372867856,0.44121107006038773,0.16498237528786874,2.0516533519841448E-2,0.67662395902193495,2.1510774180988697,724.05,314.89699999999999,{"$f":"T3676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4298126944917498E-2},{"$f":"U3676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2184065749239497E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88255814067359606},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17120078186279269}]
["Single Family Detached",13680,"Mountain North","1950s","Stucco","central furnace","central AC",40.842902437337223,16396.187249999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16396.187249999999},"Cold/Very Cold",161.83609041728985,"Rural",0.58248115971971171,0.25066527139411948,0.12777765153596699,6.5334182466445484E-2,0.50598691240155391,1.4669109950513519,3639.665,345.053,{"$f":"T3681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9676628867271243E-2},{"$f":"U3681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6575535991742502E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.64215778858698291},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13343520513514123}]
["Single Family Detached",13686,"Pacific","1960s","Siding","heat pump","central AC",12.687319954104144,14255.41568,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14255.41568},"Marine",68.487906528382652,"Metropolitan Area",2.246329913232064E-2,7.4107106287040633E-2,1.36011633773664E-2,1.244141403472E-3,0.12350917804900226,0.23368074684572995,46.459000000000003,40.816000000000003,{"$f":"T3687*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6229235707712013E-4},{"$f":"U3687*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8184904639488008E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3125591489397759E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.418301242376128E-2}]
["Single Family Attached",13690,"West North Central","1990s","Siding","central furnace","central AC",13.355434094283634,12075.4377,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12075.4377},"Cold/Very Cold",60.228201741015283,"Metropolitan Area",0.19490883086137409,0.17309202888984482,2.5540528845953699E-2,5.8307096215088998E-3,0.17524215717583139,0.56878354577300394,390.53899999999999,92.317999999999998,{"$f":"T3691*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7159293639202999E-3},{"$f":"U3691*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1147802575886001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19962476022529438},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6655309103542298E-2}]
["Single Family Attached",13693,"East North Central","1990s","Brick","built-in electric unit","window/wall unit",19.904017020360126,14875.94695,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14875.94695},"Cold/Very Cold",67.260761085654096,"Metropolitan Area",3.7438608083950949E-2,4.5742778197955546E-2,6.8912675486405501E-3,0,0.33421360097698144,0.42428625480752852,0,0,{"$f":"T3694*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3694*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.7438608083950949E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.8912675486405501E-3}]
["Multi-Family (5+ units)",13700,"Pacific","1980s","Wood","N/A","N/A",9.2420451763991256,12372.215759999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":984.10376428917448},"Marine",18.072503850946482,"Metropolitan Area",0,0.2848027774370292,0,0,8.3200998220457734E-2,0.36800377565748693,0,0,{"$f":"T3701*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3701*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13704,"West North Central","1980s","Siding","central furnace","central AC",45.869341399422723,19112.225579999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19112.225579999998},"Mixed-Humid",295.69168281605022,"Metropolitan Area",1.0870181695765386,0.28467476524044433,0.18516960024530435,2.9757964574766961E-2,0.57596732971021936,2.1328298647725066,1053.4010000000001,503.61099999999999,{"$f":"T3705*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0132837538197581E-2},{"$f":"U3705*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6251270365693784E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1071510071147361},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19479472728187372}]
["Single Family Detached",13709,"Middle Atlantic","Before 1950","Brick","radiator","window/wall unit",66.652788408454796,24586.052530000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24586.052530000001},"Cold/Very Cold",96.627661103916523,"Metropolitan Area",2.3976131327396248,0.41833426533346563,2.844943106640661E-2,1.4519785042642101E-3,0.33859677976816938,3.1829936089076667,59.057000000000002,0,{"$f":"T3710*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4519785042642101E-3},{"$f":"U3710*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.399065111243889},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.844943106640661E-2}]
["Multi-Family (2-4 units)",13711,"New England","Before 1950","Siding","central furnace","window/wall unit",35.602847738853058,37516.17254,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12505.390846666667},"Cold/Very Cold",461.788293517954,"Metropolitan Area",0.96998052847318239,1.169832068339048,5.2853459165457715E-2,1.8138656745192057E-2,1.5804928717462625,3.7852513655540787,483.48899999999998,0,{"$f":"T3712*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0462189150640201E-3},{"$f":"U3712*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.97602674738824646},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2853459165457715E-2}]
["Single Family Detached",13716,"Middle Atlantic","Before 1950","Siding","central furnace","window/wall unit",54.449419753214585,22509.06149,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22509.06149},"Mixed-Humid",289.54808113853056,"Metropolitan Area",1.5420396200624209,0.29347404406907962,9.8194205115820707E-2,2.9977230456459652E-2,0.566292580334676,2.5000004495819974,1331.7850000000001,0,{"$f":"T3717*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9977230456459652E-2},{"$f":"U3717*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5720168505188805},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.8194205115820707E-2}]
["Single Family Detached",13719,"Pacific","1970s","Stucco","central furnace","central AC",41.680843834201497,11061.79507,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11061.79507},"Hot-Dry/Mixed-Dry",89.371925970676941,"Metropolitan Area",9.864059297564623E-2,9.593495533408973E-2,6.4520021486838303E-2,4.2772532379218306E-3,0.28072028404071231,0.53981585383728659,99.197999999999993,287.471,{"$f":"T3720*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0973079473538599E-3},{"$f":"U3720*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1799452905679699E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.9737900923000083E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7699966777406279E-2}]
["Multi-Family (5+ units)",13727,"New England","1980s","Siding","central furnace","window/wall unit",35.684518523303055,41016.687960000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3262.5261152178987},"Cold/Very Cold",186.52552135595843,"Metropolitan Area",0.61390760812730538,0.13611096681041485,5.6312139033787685E-2,8.9634178365867595E-3,0.43503853782849694,1.2496197065421069,218.53100000000001,0,{"$f":"T3728*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1296309448468261E-4},{"$f":"U3728*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.61462057122179004},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.6312139033787685E-2}]
["Single Family Detached",13728,"Pacific","1970s","Stucco","central furnace","central AC",27.607070162791256,9051.4984139999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9051.4984139999997},"Hot-Dry/Mixed-Dry",113.64156258814565,"Metropolitan Area",0.37952493852228919,0.16595098655713325,0.171305925430843,1.5500256562051127E-2,0.21653211741932737,0.93331396792959287,638.19100000000003,1074.261,{"$f":"T3729*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7765848243290742E-3},{"$f":"U3729*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7236717377220533E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38530152334661827},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18102959716856504}]
["Single Family Detached",13734,"East North Central","1950s","Wood","central furnace","window/wall unit",81.852979943428011,20062.00489,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20062.00489},"Cold/Very Cold",247.94746194624597,"Metropolitan Area",1.2937872800753176,0.29525988872192466,3.7549332320436959E-2,2.5271204769712952E-2,0.30443386238002873,1.9310303634977077,1259.655,0,{"$f":"T3735*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5271204769712952E-2},{"$f":"U3735*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3190584848450306},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7549332320436959E-2}]
["Single Family Detached",13738,"Pacific","2000s","Stucco","central furnace","central AC",66.149291238259991,21435.28556,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21435.28556},"Hot-Dry/Mixed-Dry",181.98261633526778,"Metropolitan Area",0.35556478712959261,0.3153104997886183,0.18561045267488047,2.3461391621702316E-2,0.42894323559929048,1.2854289751923818,592.27200000000005,502.25,{"$f":"T3739*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2695519449192321E-2},{"$f":"U3739*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.076587217251E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36826030657878495},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19637632484739045}]
["Single Family Attached",13745,"South Atlantic","Before 1950","Brick","radiator","window/wall unit",17.585443688971402,19803.42758,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19803.42758},"Mixed-Humid",105.88892725780417,"Metropolitan Area",0.72213687815131233,0.31534300801168763,0.15309425857556808,5.3897998673106996E-3,0.21283789241202211,1.4034120371505903,272.16500000000002,0,{"$f":"T3746*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3897998673106996E-3},{"$f":"U3746*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.72752667801862303},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15309425857556808}]
["Single Family Detached",13746,"Pacific","1970s","Shingle","N/A","central AC",73.157403401404011,17860.694189999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17860.694189999998},"Marine",135.06464130376261,"Metropolitan Area",0,0.63462822207821767,7.8402696350570816E-2,4.2332881548312294E-3,0.43525699079444363,1.1482879092232321,0,237.017,{"$f":"T3747*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3747*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2332881548312294E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.2635984505402049E-2}]
["Single Family Detached",13752,"West South Central","1990s","Wood","central furnace","central AC",41.763496438850744,13765.160330000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13765.160330000001},"Hot-Humid",266.20605989568696,"Metropolitan Area",0.66256641842656083,0.24565826824494508,0.20414009449112633,1.49080815921999E-2,0.57169689631185439,1.6840616774744863,379.47199999999998,703.55799999999999,{"$f":"T3753*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2234929207457606E-3},{"$f":"U3753*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6845886714541415E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.66778991134730659},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21382468316258046}]
["Single Family Detached",13757,"South Atlantic","1980s","Concrete","heat pump","central AC",24.852782614495094,22511.578460000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22511.578460000001},"Hot-Humid",249.60680610030673,"Metropolitan Area",4.2915285270897906E-2,8.7698378718200465E-2,0.3492012484167476,1.6691975242834639E-2,0.37184352910128621,0.85165844150713221,43.04,698.44399999999996,{"$f":"T3758*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6889833691840002E-4},{"$f":"U3758*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.572307690591624E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.3884183607816304E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36492432532266383}]
["Single Family Detached",13762,"East South Central","2000s","Siding","central furnace","central AC",28.049620256311826,17574.95004,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17574.95004},"Hot-Humid",320.24803300062325,"Metropolitan Area",0.29285900246988728,0.14759805087562824,0.29566412267082171,1.8675405536754602E-2,0.35656510317368029,1.0926862791900174,239.16499999999999,823.45,{"$f":"T3763*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2033129263165997E-3},{"$f":"U3763*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4472092610438001E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29706231539620387},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31013621528125973}]
["Single Family Detached",13764,"Mountain South","1980s","Wood","heat pump","central AC",26.566408523364149,8307.1946599999992,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8307.1946599999992},"Hot-Dry/Mixed-Dry",137.71667307702654,"Metropolitan Area",6.4429596612406145E-2,6.9123302817615362E-2,0.18422859782445736,1.23338995915685E-2,0.15209835429910112,0.46987985155357992,150.374,1334.3510000000001,{"$f":"T3765*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2491860898028399E-3},{"$f":"U3765*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.108471350176566E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.567878270220899E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19531331132622301}]
["Single Family Detached",13772,"West South Central","1990s","Brick","central furnace","central AC",66.392070191870232,20082.295880000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20082.295880000001},"Mixed-Humid",247.55777493852577,"Metropolitan Area",1.0212886111322914,0.38297789732505316,0.45736822381364434,5.7348751274669568E-2,0.42206497349961136,2.2836997057706001,1545.299,1310.3879999999999,{"$f":"T3773*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1033151741068122E-2},{"$f":"U3773*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6315599533601439E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0523217628733594},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4836838233472458}]
["Single Family Detached",13775,"Pacific","1950s","Wood","heater burning gas/oil/kerosene","N/A",30.490494441865899,30490.494439999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30490.494439999999},"Marine",62.999459615783316,"Metropolitan Area",0.77205224895479529,0.79642808816831423,0,0,0.23263823439847303,1.8011185715215823,0,0,{"$f":"T3776*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3776*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.77205224895479529},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",13780,"West North Central","2000s","Siding","central furnace","both central and individual units",36.935829157181111,34977.110939999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34977.110939999999},"Mixed-Humid",783.62719359610389,"Micropolitan Area",1.0795683193004344,0.81102147665063362,0.12624285153863107,1.6787649143873342E-2,0.65690333673148227,2.6737359842211812,372.423,107.538,{"$f":"T3781*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.302628058760762E-2},{"$f":"U3781*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7613685562657199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.092594599888042},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13000422009489679}]
["Single Family Detached",13781,"South Atlantic","1980s","Concrete","central furnace","central AC",86.84642077448764,13535.91346,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13535.91346},"Hot-Humid",309.34532648910948,"Metropolitan Area",0.10674715083878082,0.13003776094147021,0.44315416579482436,3.2293088962579639E-2,0.37554716452688358,1.0554862421019588,165.47800000000001,2220.2559999999999,{"$f":"T3782*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2398958875338802E-3},{"$f":"U3782*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0053193075045757E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10898704672631471},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.47320735886987014}]
["Single Family Attached",13787,"Middle Atlantic","1970s","Brick","heat pump","central AC",62.964501343829731,29491.56972,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29491.56972},"Cold/Very Cold",270.03849640877218,"Metropolitan Area",7.4666726725526281E-2,0.32311954701974588,6.2201348002555557E-2,5.2480838148134396E-3,0.46138369367523313,0.92137131542306094,79.775999999999996,98.176000000000002,{"$f":"T3788*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3527194659827199E-3},{"$f":"U3788*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.89536434883072E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.7019446191508995E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5096712351386282E-2}]
["Single Family Detached",13791,"East North Central","Before 1950","Siding","central furnace","central AC",70.341090529446646,30477.07562,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30477.07562},"Cold/Very Cold",305.62411431078465,"Metropolitan Area",2.9775760013639276,0.4991965781351354,0.1461557419349695,6.7690011631078684E-2,0.33713463709455871,3.9600629585285914,1979.0830000000001,241.93100000000001,{"$f":"T3792*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0316662249256463E-2},{"$f":"U3792*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3733493818222201E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0378926636131842},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15352909131679171}]
["Multi-Family (5+ units)",13798,"Pacific","2000s","Stucco","central furnace","central AC",33.001339825621478,19131.211490000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1521.7239666632929},"Hot-Dry/Mixed-Dry",103.72059009595375,"Metropolitan Area",0.10821396839885628,0.32504653394425476,3.9080583025800752E-2,4.9444233471675194E-3,0.43881902603319078,0.91571124823353389,155.084,103.364,{"$f":"T3799*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3599503964601013E-4},{"$f":"U3799*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5729147609018461E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10844996343850229},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9237874501890938E-2}]
["Mobile Home",13801,"South Atlantic","1990s","Siding","central furnace","N/A",13.301904334521499,13196.33367,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13196.33367},"Hot-Humid",204.48246867573852,"Metropolitan Area",3.8600701188786356E-2,0.12514245534165142,0,4.7980549590753002E-4,0.53395102948423157,0.69769418601466926,36.359000000000002,0,{"$f":"T3802*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7980549590753002E-4},{"$f":"U3802*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.9080506684693886E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",13805,"New England","1960s","Brick","built-in electric unit","window/wall unit",41.035075254669465,30396.352040000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2417.7693829050172},"Cold/Very Cold",138.13883593430913,"Metropolitan Area",5.6605363415673682E-2,0.11479693006620273,1.9740515679801483E-2,0,0.28018691630362325,0.47132972546530116,0,0,{"$f":"T3806*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3806*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.6605363415673682E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9740515679801483E-2}]
["Single Family Detached",13810,"West North Central","Before 1950","Siding","central furnace","window/wall unit",52.763353548576355,18565.57127,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18565.57127},"Mixed-Humid",204.48051503868354,"Metropolitan Area",0.10402560639921542,0.13476349025110695,9.8228191155446329E-2,2.5599323601352198E-3,0.36067021548074552,0.69768750328651419,137.886,0,{"$f":"T3811*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5599323601352198E-3},{"$f":"U3811*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10658553875935063},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.8228191155446329E-2}]
["Mobile Home",13816,"South Atlantic","2010s","Siding","heat pump","central AC",7.123273032458016,12366.793460000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12366.793460000001},"Mixed-Humid",77.031631078706639,"Micropolitan Area",3.4257440065447904E-2,5.3786523791774205E-2,2.9057463118180565E-2,1.36112638858798E-3,0.14573050436812882,0.2628319313435315,34.173000000000002,75.89,{"$f":"T3817*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2261043290858004E-4},{"$f":"U3817*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.3851595567939999E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.4680050498356485E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.9995979073859966E-2}]
["Multi-Family (5+ units)",13817,"West North Central","Before 1950","Concrete","radiator","window/wall unit",6.1318254731199922,19590.496719999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1558.2561717664973},null,26.140069944394124,"Metropolitan Area",0.2302700628925026,0.19757188338491136,6.7425200276125599E-3,2.2138632628370403E-3,8.0233506212654945E-2,0.51685574192531569,113.00700000000001,0,{"$f":"T3818*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7609385520281657E-4},{"$f":"U3818*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23044615674770541},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7425200276125599E-3}]
["Single Family Detached",13824,"East South Central","1960s","Brick","central furnace","central AC",46.294964382041464,16002.40732,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16002.40732},"Mixed-Humid",292.47775888581191,"Metropolitan Area",1.1251919721034869,0.2393094244811915,0.36983854861248222,6.2941692625092485E-2,0.54908404138415912,2.2834239865813197,2688.5909999999999,1244.673,{"$f":"T3825*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.302392829888612E-2},{"$f":"U3825*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9917764326206362E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1682159004023729},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.38975631293868856}]
["Multi-Family (5+ units)",13828,"Middle Atlantic","1970s","Brick","heater burning gas/oil/kerosene","window/wall unit",16.974093639710642,17008.10986,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1352.8494217489967},"Cold/Very Cold",47.333569738792299,"Metropolitan Area",0.59586354951646825,0.33556218380726444,1.134954572579772E-2,0,0.15015946550476217,1.0929347445542927,0,0,{"$f":"T3829*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3829*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59586354951646825},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.134954572579772E-2}]
["Single Family Attached",13834,"South Atlantic","1990s","Brick","central furnace","central AC",28.876627097581483,16425.840209999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16425.840209999998},"Mixed-Humid",116.35270197483048,"Metropolitan Area",0.48125755497730988,0.23211886997973802,0.10720792749502485,1.961925350858694E-2,0.31515301984442784,1.1357373722965005,903.48199999999997,290.93200000000002,{"$f":"T3835*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4840450964611217E-2},{"$f":"U3835*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7788025439757199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49609800594192111},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11198673003900057}]
["Single Family Detached",13835,"East South Central","Before 1950","Brick","central furnace","central AC",61.750780890254575,12252.139069999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12252.139069999999},"Mixed-Humid",707.27958714769284,"Metropolitan Area",1.4921835943130957,0.19910992859929835,0.26097548755090616,3.4557440046133606E-2,2.1920910451363214,4.1443600555996216,1596.308,1224.2149999999999,{"$f":"T3836*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9558187614553559E-2},{"$f":"U3836*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4999252431580049E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5117417819276493},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27597473998248623}]
["Single Family Detached",13839,"Pacific","1980s","Siding","central furnace","central AC",17.503523671830543,10627.51893,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10627.51893},"Cold/Very Cold",108.72815879026814,"Micropolitan Area",0.14424928052789204,0.12719540717611036,1.60732721801106E-2,3.6731787402569703E-3,8.3462507872986799E-2,0.37098046775709975,274.86700000000002,70.762,{"$f":"T3840*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9211542457323104E-3},{"$f":"U3840*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5202449452466005E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14717043477362435},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6825296674635261E-2}]
["Single Family Detached",13846,"Pacific","2000s","Shingle","central furnace","N/A",27.9552961266116,14226.613799999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14226.613799999999},"Marine",73.359064606666934,"Metropolitan Area",0.22926944994554158,0.24359102639265656,0,1.29579270611574E-2,0.23231310592852741,0.70517358226672555,910.82299999999998,0,{"$f":"T3847*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.29579270611574E-2},{"$f":"U3847*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24222737700669897},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13851,"Mountain North","1990s","Siding","central furnace","central AC",96.14543715409377,18216.263200000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18216.263200000001},"Cold/Very Cold",311.81019990711718,"Metropolitan Area",1.452494130250521,0.83355600219611137,0.21725229190942241,6.9119661572237617E-2,0.79187866751183034,3.2951810918678852,3006.4029999999998,787.99,{"$f":"T3852*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4765428333269604E-2},{"$f":"U3852*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4354233238968001E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5072595585837907},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23160652514839042}]
["Single Family Detached",13853,"South Atlantic","1950s","Siding","heat pump","central AC",37.676294147659902,31163.187880000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31163.187880000001},"Mixed-Humid",630.27528790625036,"Metropolitan Area",0.70497899628967542,0.55372665644919838,0.27573537663928255,2.3740646301177958E-2,0.61605823646157432,2.1504992658397306,372.21699999999998,389.6,{"$f":"T3854*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.159946830312996E-2},{"$f":"U3854*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2141177998048001E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.71657846459280539},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28787655463733053}]
["Multi-Family (5+ units)",13858,"Pacific","Before 1950","Wood","central furnace","N/A",9.6313699892768145,20535.970130000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1633.4604811533816},"Hot-Dry/Mixed-Dry",15.257548116893449,"Metropolitan Area",3.0721445504587615E-2,0.22327727363051461,0,3.8034670277773005E-4,8.0990046502275828E-2,0.33533885901858435,18.521000000000001,0,{"$f":"T3859*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0253321571441784E-5},{"$f":"U3859*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0751698826159055E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",13863,"East South Central","Before 1950","Siding","central furnace","central AC",22.992332464004441,20769.94803,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6923.3160099999996},"Mixed-Humid",316.12128826832475,"Metropolitan Area",0.97866060742866801,0.69549805573364953,0.18438239584670893,1.9720068696979561E-2,1.8367720141689399,3.7084597856426189,559.19899999999996,390.25299999999999,{"$f":"T3864*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8715113894759894E-3},{"$f":"U3864*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7018448428505295E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.98253211881814395},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18708424068955945}]
["Single Family Detached",13869,"South Atlantic","1950s","Concrete","portable electric heaters","window/wall unit",34.780552184118207,20665.806410000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20665.806410000001},"Hot-Humid",314.34235281813392,"Metropolitan Area",6.7443541190646536E-2,0.11196285464938904,0.37548278175747196,0,0.70017027197335502,1.2550594495708625,0,0,{"$f":"T3870*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3870*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.7443541190646536E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37548278175747196}]
["Single Family Detached",13873,"West North Central","1960s","Shingle","central furnace","central AC",50.557588519333251,13166.03868,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13166.03868},"Mixed-Humid",250.92327603697154,"Metropolitan Area",0.75579435702524977,0.3544365417755202,0.17048164995749987,3.5083306281899755E-2,0.33482256731237697,1.6155351160706468,1917.453,747.22900000000004,{"$f":"T3874*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.524526036508204E-2},{"$f":"U3874*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8380459168177208E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78103961739033179},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18031969587431759}]
["Multi-Family (5+ units)",13876,"Middle Atlantic","2000s","Siding","central furnace","central AC",47.260475424147394,37868.970690000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3012.1521745742189},"Mixed-Humid",134.46389145863267,"Metropolitan Area",0.98642231317729889,0.63549059570906774,0.10404926851815192,1.3115312094950459E-2,0.58832414894217111,2.326358427730411,219.84899999999999,126.485,{"$f":"T3877*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6221864342796749E-4},{"$f":"U3877*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8099206780102003E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.98708453182072686},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10443026058595295}]
["Single Family Detached",13882,"South Atlantic","1960s","Brick","central furnace","central AC",172.46272874787286,65080.275000000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":65080.275000000001},"Cold/Very Cold",667.17486461297108,"Micropolitan Area",4.4492245846639502,0.63165379020509993,0.52796939292142497,0.22457653991954998,1.6995189269233493,7.3083666947138255,3035.982,414.78,{"$f":"T3883*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.19758254345505},{"$f":"U3883*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.69939964645E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.6468071281190007},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.55496338938592493}]
["Single Family Detached",13887,"Middle Atlantic","1970s","Siding","central furnace","central AC",65.341825651780951,24807.071240000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24807.071240000001},"Cold/Very Cold",218.43826890947108,"Metropolitan Area",1.423186315961122,0.57767966322339992,0.20701912747162585,6.783563090377473E-2,0.50547307598127988,2.7133581826374273,2354.2440000000001,380.28399999999999,{"$f":"T3888*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8401898624342571E-2},{"$f":"U3888*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4337322794321599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4815882145854646},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21645285975105802}]
["Multi-Family (2-4 units)",13888,"Mountain North","2000s","Stucco","central furnace","N/A",75.288560695432167,70428.962299999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23476.320766666668},"Cold/Very Cold",264.91248478919391,"Rural",1.0253745343597562,2.748490324186462,0,1.85063367077218E-2,1.5346180717845326,5.3208204881358983,262.76600000000002,0,{"$f":"T3889*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1687789025739338E-3},{"$f":"U3889*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0315433132623302},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13892,"South Atlantic","1950s","Other","N/A","window/wall unit",28.050955787103927,30656.782279999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30656.782279999999},"Hot-Humid",441.9026480410343,"Rural",0,0.56238527391274362,0.35653810200535946,0,0.58884842297431561,1.5077717988924186,0,0,{"$f":"T3893*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3893*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35653810200535946}]
["Single Family Attached",13899,"Pacific","1950s","Stucco","N/A","N/A",11.942048810786545,9366.3127929999991,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9366.3127929999991},"Marine",20.611236308706946,"Metropolitan Area",0,0.11031209547313084,0,0,7.9984761419671438E-2,0.19029685689280226,0,0,{"$f":"T3900*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3900*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",13901,"Middle Atlantic","1970s","Brick","central furnace","central AC",21.773673543629805,22082.833210000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1756.5001863603934},"Cold/Very Cold",68.611362778963297,"Metropolitan Area",0.37903384724986672,0.21921065415320146,3.6320185430199228E-2,8.0485302200486997E-3,0.21650016303933967,0.85847318846973297,292.00599999999997,72.463999999999999,{"$f":"T3902*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1290859341835305E-4},{"$f":"U3902*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2728302950441956E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37954675584328507},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6447468459703647E-2}]
["Single Family Detached",13906,"Mountain North","2000s","Siding","radiator","N/A",46.566843331802097,15522.28111,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15522.28111},"Cold/Very Cold",61.680034723732916,"Rural",0.9980321037811436,0.28463849493844956,5.249120131669148E-2,1.6264867038302401E-3,0.21322946695210243,1.5483912669883868,104.78400000000001,0,{"$f":"T3907*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6264867038302401E-3},{"$f":"U3907*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.99965859048497385},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.249120131669148E-2}]
["Single Family Detached",13911,"South Atlantic","1990s","Wood","fireplace","central AC",33.669373838177357,20161.3017,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20161.3017},"Hot-Humid",328.6837741843695,"Metropolitan Area",0,0.36239141418202681,0.39862262414414068,1.9177248725324701E-2,0.36045498163764705,1.1214690199638144,0,951.19100000000003,{"$f":"T3912*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3912*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9177248725324701E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.41779987286946541}]
["Multi-Family (5+ units)",13917,"South Atlantic","2000s","Brick","central furnace","central AC",23.440909017318774,29411.42913,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2339.4272037781921},"Mixed-Humid",194.38013512604741,"Metropolitan Area",0.11365134969097726,0.21766763412243792,3.8010498148605382E-2,3.2286396327457501E-3,0.29092368064511942,0.66322499161859094,53.430999999999997,56.344000000000001,{"$f":"T3918*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2499793492507259E-4},{"$f":"U3918*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3181268636967844E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11377634762590233},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.814231083497506E-2}]
["Single Family Detached",13922,"Middle Atlantic","1990s","Siding","radiator","central AC",27.509646970899151,22962.977439999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22962.977439999999},"Mixed-Humid",179.19761073866266,"Metropolitan Area",1.5503470292700208,0.68732919554974892,7.8756169651922878E-2,6.7888894652487989E-3,0.57561228956213428,2.8920446840338268,144.774,150.87100000000001,{"$f":"T3923*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3244420958985599E-3},{"$f":"U3923*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4644473693502399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5536714713659194},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.2220617021273118E-2}]
["Single Family Detached",13925,"Middle Atlantic","1950s","Siding","heat pump","both central and individual units",39.425359290866005,15082.38687,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15082.38687},"Mixed-Humid",136.19745259367846,"Metropolitan Area",0.15877507682206096,0.20750684192973201,6.1792584253550616E-2,6.644937677637121E-3,0.24413803821637595,0.67221254122171947,245.66499999999999,194.911,{"$f":"T3926*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7052145704185501E-3},{"$f":"U3926*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9397231072185699E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16248029139247952},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4732307360769181E-2}]
["Multi-Family (5+ units)",13929,"Pacific","1980s","Wood","N/A","N/A",14.384080641591682,21565.33829,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1715.3378991313734},"Hot-Dry/Mixed-Dry",64.390067425356492,"Metropolitan Area",0,0.45951194235746129,0,0,0.27383554420882888,0.73334748656629012,0,0,{"$f":"T3930*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3930*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",13935,"Pacific","Before 1950","Concrete","N/A","N/A",7.5081587072490432,15417.16367,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1226.3032828251698},"Hot-Humid",51.622229562963277,"Metropolitan Area",0,4.8642245997470565E-2,0,0,0.12749282082128446,0.17613506681875504,0,0,{"$f":"T3936*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3936*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13940,"East North Central","1990s","Brick","heat pump","N/A",115.79319463465268,21741.118030000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21741.118030000001},"Cold/Very Cold",864.55729963229408,"Metropolitan Area",1.7711705526558379,0.27015358902139991,0,4.7308238010919407E-2,1.1203535977833186,3.1616777394605564,2175.98,0,{"$f":"T3941*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7308238010919407E-2},{"$f":"U3941*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8184787906667572},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13945,"East South Central","1990s","Wood","central furnace","central AC",29.243080617137519,28697.822,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28697.822},"Mixed-Humid",454.1981616526661,"Micropolitan Area",0.50298755843083809,0.33780476035726797,0.20483139327272798,1.6350957156186001E-2,1.56598246391778,2.611606175978614,261.05900000000003,308.70400000000001,{"$f":"T3946*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4918247134980014E-3},{"$f":"U3946*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8591324426879996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.51047938314433605},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21369052571541597}]
["Single Family Detached",13947,"East South Central","1960s","Wood","central furnace","N/A",60.559460578606796,25233.10857,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25233.10857},"Mixed-Humid",178.04481410110398,"Micropolitan Area",0.94946333467721755,0.38270707551220734,0,8.2645495837149613E-3,0.27055302365517403,1.602723433844599,327.52800000000002,0,{"$f":"T3948*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2645495837149613E-3},{"$f":"U3948*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95772788426093247},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13950,"Middle Atlantic","1970s","Siding","central furnace","central AC",94.096697441007422,27385.534759999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27385.534759999999},"Mixed-Humid",175.38296204567843,"Metropolitan Area",2.1980912662968812,0.58486163780006839,0.10075603792294918,2.9028310833648114E-2,0.60453808975405887,3.4882470317739571,840.65599999999995,219.33099999999999,{"$f":"T3951*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3021814109202555E-2},{"$f":"U3951*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0064967244455592E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2211130804060839},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10676253464739474}]
["Single Family Attached",13958,"West North Central","1980s","Brick","central furnace","central AC",13.636040526360297,12815.82756,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12815.82756},"Cold/Very Cold",46.093866780607513,"Micropolitan Area",0.57931252034861369,0.15095791477744633,6.7735621561143605E-3,4.1477913264837598E-3,0.14661957772680032,0.88366357500897474,302.685,20.960999999999999,{"$f":"T3959*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8791587649985998E-3},{"$f":"U3959*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6863256148515995E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58319167911361225},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0421947175995205E-3}]
["Single Family Detached",13959,"West North Central","1960s","Siding","central furnace","central AC",18.499295781713855,14811.28565,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14811.28565},"Cold/Very Cold",45.214574639785013,"Metropolitan Area",1.0857703839382666,0.2556253722470756,1.0746180190501E-2,6.3572111589791005E-3,0.13766627899562717,1.4898082153714705,395.62,33.594000000000001,{"$f":"T3960*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8596408288530003E-3},{"$f":"U3960*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9757033012609998E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0916300247671196},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1243750520627099E-2}]
["Single Family Attached",13964,"Pacific","1950s","Concrete","built-in furnace","N/A",25.189897597128713,15359.693660000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15359.693660000001},"Hot-Dry/Mixed-Dry",56.943176610125875,"Metropolitan Area",4.7744378966617207E-2,0.1234877899091118,0,0,0.19429011027873369,0.36552227915446267,0,0,{"$f":"T3965*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3965*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.7744378966617207E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",13970,"East North Central","2000s","Siding","central furnace","central AC",47.758630110429117,18981.96745,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18981.96745},"Cold/Very Cold",124.15562026395281,"Metropolitan Area",1.2799494904993447,0.41880336184612393,6.7317402599103154E-2,3.2563792944084395E-2,0.38007299204639527,2.1461432469909671,1532.606,182.90600000000001,{"$f":"T3971*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9091877205674702E-2},{"$f":"U3971*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4719157384097005E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3090413677050194},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0789318337512855E-2}]
["Single Family Detached",13973,"Pacific","2000s","Stucco","central furnace","central AC",29.481698838047983,14304.56033,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14304.56033},"Hot-Dry/Mixed-Dry",96.478065544413766,"Metropolitan Area",0.42768162128218939,0.20616587760303737,4.1251548297895325E-2,6.0070427604198701E-3,0.34523858953522457,1.0203376367183465,266.38499999999999,153.554,{"$f":"T3974*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8105203035070502E-3},{"$f":"U3974*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1965224569128203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43149214158569643},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.3448070754808145E-2}]
["Multi-Family (2-4 units)",13977,"East North Central","1990s","Siding","central furnace","both central and individual units",22.089344724162217,28950.648389999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9650.2161299999989},"Cold/Very Cold",143.32111129226243,"Metropolitan Area",0.11932866673130843,0.15749656465441983,1.4789226425276639E-2,2.7916531229509197E-3,0.19553609540257008,0.48901165529554225,81.831000000000003,14.597,{"$f":"T3978*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8968683613402991E-4},{"$f":"U3978*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4086420484961E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12011835356744247},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.493009063012625E-2}]
["Single Family Detached",13983,"South Atlantic","1990s","Siding","wood-burning stove","window/wall unit",27.332065887363417,20336.358550000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20336.358550000001},"Mixed-Humid",89.770543498361363,"Metropolitan Area",0,0.12583754313563406,3.6337005457139998E-2,0,0.18499304104923583,0.34716758964200983,0,0,{"$f":"T3984*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U3984*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6337005457139998E-2}]
["Single Family Detached",13988,"Middle Atlantic","2010s","Siding","heat pump","central AC",38.499788377698941,18580.978950000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18580.978950000001},"Cold/Very Cold",209.19365417650073,"Metropolitan Area",0.19319580295654082,0.23873133476329514,3.480902995458255E-2,4.9860198914430014E-3,0.24703257291899711,0.71376874059341566,184.74700000000001,83.593000000000004,{"$f":"T3989*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4327801180756502E-3},{"$f":"U3989*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5532397733673503E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19662858307461648},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6362269727949897E-2}]
["Single Family Detached",13993,"East North Central","Before 1950","Siding","central furnace","window/wall unit",30.989846082578655,14898.964459999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14898.964459999999},"Cold/Very Cold",192.64256757620973,"Micropolitan Area",0.3391686385688979,0.39829292928477444,6.6050074345107526E-2,2.6686280192528999E-2,0.56063983819934682,1.3641514803981265,1791.15,0,{"$f":"T3994*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6686280192528999E-2},{"$f":"U3994*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36585491876142689},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6050074345107526E-2}]
["Single Family Detached",13997,"West South Central","2000s","Siding","central furnace","central AC",69.349231602560081,26848.328150000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26848.328150000001},"Hot-Humid",326.53250817283515,"Metropolitan Area",6.1174023083087607E-2,0.16601397913103816,0.82018141476259243,4.7069039102859901E-2,0.38222316299806597,1.4295925799747842,89.26,1663.886,{"$f":"T3998*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3964817706690002E-3},{"$f":"U3998*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4672557332190901E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.3570504853756607E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.86485397209478332}]
["Single Family Detached",14000,"South Atlantic","1990s","Siding","heat pump","central AC",22.686544225466594,19160.93262,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19160.93262},"Hot-Humid",213.03109561349982,"Metropolitan Area",0.10868558089286237,0.37647961827101767,0.23962227381401524,1.2960895525618259E-2,0.48511950033958151,1.2099069733174768,110.66,565.76300000000003,{"$f":"T4001*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1203488037291997E-3},{"$f":"U4001*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.084054672188906E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11080592969659157},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2504628205359043}]
["Single Family Detached",14007,"West North Central","Before 1950","Siding","central furnace","window/wall unit",31.282209254254877,14329.9172,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14329.9172},"Cold/Very Cold",187.47830676748353,"Micropolitan Area",0.97187646504988279,0.40337398565617605,4.5680179224382798E-2,2.7292359061438398E-2,0.27915355077691839,1.7000841807073601,1904.5719999999999,0,{"$f":"T4008*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7292359061438398E-2},{"$f":"U4008*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.99916882411132124},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.5680179224382798E-2}]
["Multi-Family (2-4 units)",14011,"Middle Atlantic","Before 1950","Brick","portable electric heaters","window/wall unit",40.673655941575724,58105.22277,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19368.407589999999},"Mixed-Humid",293.3168496129951,"Metropolitan Area",0.62298252529184683,1.219485396568172,0.16075222426402166,0,0.29185236555972505,2.2950725116837654,0,0,{"$f":"T4012*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4012*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62298252529184683},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16075222426402166}]
["Single Family Detached",14012,"Middle Atlantic","1950s","Siding","central furnace","central AC",85.837924498272272,30932.5854,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30932.5854},"Mixed-Humid",292.90065119788829,"Metropolitan Area",2.4238901671017703,0.65971910754562679,0.42476245800479584,9.1222235895236384E-2,0.5599432075400701,4.0683149401922627,2296.9409999999998,652.125,{"$f":"T4013*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1050323641261404E-2},{"$f":"U4013*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0171912253975001E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4949404907430317},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.44493437025877086}]
["Single Family Detached",14018,"East South Central","Before 1950","Brick","central furnace","central AC",37.547426773275596,15644.76116,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15644.76116},"Hot-Humid",434.07918319187041,"Metropolitan Area",0.11962325438729289,0.25073353385346531,0.67479933472314424,4.0771029821018004E-2,0.80123563227943839,1.8463917552433406,322.35599999999999,2283.694,{"$f":"T4019*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0431826284929602E-3},{"$f":"U4019*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5727847192525038E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12466643701578585},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.71052718191566933}]
["Mobile Home",14022,"Pacific","1980s","Stucco","heat pump","central AC",9.4187817247487029,18688.058980000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18688.058980000002},"Hot-Dry/Mixed-Dry",51.261345775765264,"Metropolitan Area",4.3304904671404999E-2,0.18057047324510811,3.8822106523577503E-2,1.6469412617894402E-3,0.1720836276444028,0.43478111208449338,21.84,66.287999999999997,{"$f":"T4023*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0814720812320002E-4},{"$f":"U4023*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2387940536662402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.3713051879528196E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.0060900577243742E-2}]
["Single Family Detached",14029,"Pacific","1970s","Stucco","central furnace","central AC",20.8098533239646,14864.18095,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14864.18095},"Hot-Dry/Mixed-Dry",81.394872489765021,"Metropolitan Area",0.32569620360230606,0.18420109230306603,4.9670786222300853E-2,6.7349752526259495E-3,0.28477175414206124,0.84433983626973419,290.13900000000001,162.96199999999999,{"$f":"T4030*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3126785966520502E-3},{"$f":"U4030*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4222966559738998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33000888219895813},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.209308287827475E-2}]
["Single Family Detached",14030,"East North Central","1980s","Siding","central furnace","central AC",56.682457204408486,18069.001339999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18069.001339999999},"Mixed-Humid",199.59523005593121,"Micropolitan Area",1.6788420859111948,0.10739684974756739,0.16159980631126722,3.0086694131234E-2,0.34980907199789646,2.2976478139679255,1157.9580000000001,507.142,{"$f":"T4031*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0923144653663722E-2},{"$f":"U4031*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1635494775702785E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6997652305648585},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1707633557888375}]
["Single Family Attached",14036,"South Atlantic","2000s","Shingle","built-in electric unit","central AC",12.870348003494618,12280.86642,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12280.86642},"Mixed-Humid",173.31986772263315,"Metropolitan Area",0.18657207705408346,0.1653043918904544,5.934738522158136E-2,2.6136631149700799E-3,0.18016126828898085,0.59138512245510011,0,212.82400000000001,{"$f":"T4037*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4037*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6136631149700799E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18657207705408346},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1961048336551437E-2}]
["Single Family Detached",14041,"East South Central","1960s","Brick","built-in electric unit","N/A",69.944321688422377,20180.12743,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20180.12743},"Mixed-Humid",920.98065586157543,"Micropolitan Area",1.6665791131673211,0.52690958483807759,0,0,0.94889729907356124,3.1423859970789598,0,0,{"$f":"T4042*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4042*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6665791131673211},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14046,"Pacific","1990s","Stucco","central furnace","central AC",41.615498216896235,16123.78854,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16123.78854},"Hot-Dry/Mixed-Dry",60.949000967938133,"Metropolitan Area",0.11571227171457876,0.24145595846931853,3.7338115102694636E-2,7.0687333910901592E-3,0.239334261382917,0.63384060666950892,291.971,146.43299999999999,{"$f":"T4047*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.70767866381234E-3},{"$f":"U4047*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.36105472727782E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12041995037839111},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9699169829972458E-2}]
["Single Family Detached",14048,"Mountain South","2000s","Stucco","central furnace","central AC",16.572197651336971,11099.93145,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11099.93145},"Hot-Dry/Mixed-Dry",174.63327897782693,"Metropolitan Area",3.4425094300469548E-2,6.2863440573381599E-2,0.27228523674430188,1.5794714056366201E-2,0.32032825974434098,0.68990203136249395,291.46600000000001,1131.49,{"$f":"T4049*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2352526200057001E-3},{"$f":"U4049*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2559461436360501E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.7660346920475249E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28484469818066238}]
["Single Family Attached",14055,"Mountain South","1960s","Stucco","central furnace","central AC",12.919542743514373,10624.623970000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10624.623970000001},"Hot-Dry/Mixed-Dry",100.25550294493603,"Metropolitan Area",9.7036422531717112E-2,7.0757870715405999E-2,0.16314784769557095,9.0397169385231894E-3,0.17733324001674866,0.50827538095944269,149.71600000000001,701.11099999999999,{"$f":"T4056*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.59067620229252E-3},{"$f":"U4056*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4490407362306707E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.8627098734009627E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17059688843180162}]
["Single Family Detached",14059,"West South Central","1980s","Brick","built-in electric unit","window/wall unit",11.032668020404065,10507.302879999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10507.302879999999},"Hot-Humid",161.85449351076593,"Metropolitan Area",0.19313516503669809,0.10269495296838112,7.6558341766164648E-2,0,0.17986487229867607,0.55225333206991989,0,0,{"$f":"T4060*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4060*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19313516503669809},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.6558341766164648E-2}]
["Single Family Detached",14064,"South Atlantic","1990s","Stucco","heat pump","central AC",48.879660650976952,34325.60439,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34325.60439},"Hot-Humid",343.4238617771714,"Metropolitan Area",3.5238699792378397E-2,0.29906042089809504,0.42356048643996552,2.1066893461505427E-2,0.41390260006319068,1.1717622071936296,17.309999999999999,596.42700000000002,{"$f":"T4065*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9417621199089996E-4},{"$f":"U4065*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0472717249514532E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.5832876004369296E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.44403320368948007}]
["Single Family Attached",14069,"South Atlantic","1990s","Wood","central furnace","central AC",18.047254782935635,11216.44175,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11216.44175},"Mixed-Humid",97.496441117067107,"Metropolitan Area",0.33912983416352199,0.3135651182309705,4.8269474764129752E-2,8.6670791375260004E-3,0.27784079612298762,0.97880522328160979,583.75,188.96199999999999,{"$f":"T4070*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5475978715624997E-3},{"$f":"U4070*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1194812659634998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3456774320350845},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0388956030093253E-2}]
["Single Family Detached",14071,"South Atlantic","1970s","Wood","heat pump","central AC",113.87263314625609,26243.980899999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26243.980899999999},"Mixed-Humid",542.0571434071461,"Micropolitan Area",0.7721522168744821,0.22959021810746996,0.43669939602832464,4.3509895934109998E-2,0.41105718961036181,1.8494990206206383,548.82000000000005,1109.08,{"$f":"T4072*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4403221597538001E-2},{"$f":"U4072*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9106674336571995E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78655543847202014},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46580607036489663}]
["Multi-Family (5+ units)",14074,"South Atlantic","2000s","Brick","central furnace","central AC",6.8003089350923451,7606.609547,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":605.04061955355621},"Hot-Humid",48.464166359350514,"Metropolitan Area",1.6096456063790091E-3,3.1186947010509055E-2,6.7497976976092749E-2,3.0681259607824498E-3,6.224107501171796E-2,0.16535972743158431,3.4,399.95,{"$f":"T4075*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.057138106482091E-6},{"$f":"U4075*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4198599579044482E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6117027444854913E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.77399629718832E-2}]
["Mobile Home",14082,"East South Central","1970s","Siding","heat pump","N/A",65.945011696256955,39252.98315,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39252.98315},"Mixed-Humid",343.22808468575647,"Metropolitan Area",0.44653914935259631,0.35364676846320564,0,6.4361938881560511E-3,0.37096608744759813,1.1711520052634001,163.96700000000001,0,{"$f":"T4083*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4361938881560511E-3},{"$f":"U4083*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45297534324075234},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14084,"South Atlantic","2000s","Concrete","N/A","central AC",22.763075585960181,19589.565910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19589.565910000001},"Hot-Humid",169.64946073507264,"Metropolitan Area",0,0.12339340234530587,0.20718009141549412,9.5432529287156013E-3,0.2482704988230692,0.5788439925838692,0,487.16,{"$f":"T4085*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4085*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5432529287156013E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21672334434420973}]
["Single Family Detached",14089,"West South Central","1980s","Brick","central furnace","central AC",60.49490240276463,23045.677110000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23045.677110000001},"Hot-Humid",169.37784510617081,"Micropolitan Area",0.3153845390660322,8.737567978865643E-2,0.17850739012405487,2.0173425234749371E-2,0.43516327051572468,1.0164308794944681,425.82100000000003,449.54599999999999,{"$f":"T4090*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8133332726573104E-3},{"$f":"U4090*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0360091962092061E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.32519787233868952},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18886748208614693}]
["Single Family Detached",14094,"East North Central","1980s","Wood","central furnace","central AC",91.24240545931238,20774.682479999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20774.682479999999},"Cold/Very Cold",243.38884649184351,"Metropolitan Area",3.3178016981832963,0.55449966768367243,9.0921478157208968E-2,4.7720214319811757E-2,0.50258568898630529,4.4658085330104829,2022.2349999999999,274.80200000000002,{"$f":"T4095*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2011290024942798E-2},{"$f":"U4095*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7089242948689597E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.359812988208239},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.6630402452077935E-2}]
["Single Family Detached",14100,"South Atlantic","2000s","Stucco","central furnace","central AC",55.210158514883844,12434.72039,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12434.72039},"Hot-Humid",173.66602811792399,"Metropolitan Area",5.368227956783992E-2,7.8296982665930381E-2,0.25198209813223449,1.9337258547929781E-2,0.2085871124819231,0.59254847284792778,93.373999999999995,1461.7280000000001,{"$f":"T4101*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1610795816958601E-3},{"$f":"U4101*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.817617896623392E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.4843359149535781E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2701582770984684}]
["Single Family Detached",14101,"East North Central","1960s","Siding","central furnace","central AC",157.75116537115244,29585.739939999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29585.739939999999},"Cold/Very Cold",133.44790012425372,"Metropolitan Area",1.8437039049348007,0.44400686789143229,2.4312318481614519E-2,1.4036658457133601E-2,0.49171487945984027,2.8037379707676884,400.44,74,{"$f":"T4102*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.18473137015736E-2},{"$f":"U4102*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1893447555600002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8555512186363743},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6501663237174518E-2}]
["Multi-Family (5+ units)",14108,"East North Central","1970s","Brick","built-in electric unit","window/wall unit",14.557157241365889,16085.25662,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1279.4443530864648},"Cold/Very Cold",232.96951135423899,"Metropolitan Area",0.24819234085104586,0.33017093164115902,1.2855690966349639E-2,0,0.20367298308079232,0.79489194653934681,0,0,{"$f":"T4109*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4109*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24819234085104586},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2855690966349639E-2}]
["Single Family Detached",14112,"West South Central","2000s","Stone","built-in electric unit","central AC",56.716744592252546,19019.69973,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19019.69973},"Mixed-Humid",847.63990738239818,"Metropolitan Area",1.3191958173394498,0.44639457796796839,0.28848867529827027,1.6409930651247778E-2,0.838068319611043,2.8921473902167314,0,862.78599999999994,{"$f":"T4113*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4113*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6409930651247778E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3191958173394498},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30489860594951806}]
["Multi-Family (5+ units)",14118,"South Atlantic","2000s","Concrete","N/A","central AC",9.3559423460217843,8567.7127710000004,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":681.48814673512732},"Hot-Humid",145.45585036663201,"Metropolitan Area",0,0.18375862424070488,0.11147000546294798,5.1682328331481616E-3,0.19630959519463431,0.49629536908858551,0,603.22199999999998,{"$f":"T4119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1108864284985694E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11188109410579784}]
["Single Family Detached",14119,"Mountain South","1970s","Stucco","central furnace","both central and individual units",36.610817034941412,14016.39243,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14016.39243},"Hot-Dry/Mixed-Dry",196.87611229381804,"Metropolitan Area",0.52366160192184175,0.19241004109921744,0.359483210258421,1.9239208610051458E-2,0.30860978885183599,1.3841646421313158,458.399,914.22299999999996,{"$f":"T4120*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.4251002735195703E-3},{"$f":"U4120*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2814108336531889E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53008670219536136},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37229731859495291}]
["Single Family Detached",14127,"Pacific","2000s","Siding","central furnace","central AC",34.201958417748493,14948.4084,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14948.4084},"Marine",181.26227757671458,"Metropolitan Area",0.34510043621483161,0.60685138738885913,1.9841605457247599E-2,8.7415302641519997E-3,0.64340387839010049,1.6151973074510388,520.25199999999995,64.528000000000006,{"$f":"T4128*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7769393669167991E-3},{"$f":"U4128*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6459089723520018E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35287737558174842},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.08061963544828E-2}]
["Single Family Detached",14130,"Pacific","Before 1950","Wood","central furnace","central AC",34.243131217540807,13599.33726,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13599.33726},"Hot-Dry/Mixed-Dry",153.03846912289745,"Metropolitan Area",0.21032783963930138,0.29001220436066316,8.7992771025660721E-2,1.3746876469933741E-2,0.47892859464963211,1.0672614096752573,656.97,353.87900000000002,{"$f":"T4131*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9343565997022003E-3},{"$f":"U4131*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.81251987023154E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21926219623900359},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.2805290895892262E-2}]
["Single Family Detached",14135,"Pacific","1980s","Wood","central furnace","N/A",20.365250806599704,9588.1595130000005,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9588.1595130000005},"Marine",44.069098755787927,"Metropolitan Area",0.21118629892370511,0.14175151323890373,0,4.6227585223217156E-3,0.16571571807035834,0.51865353023296723,482.13200000000001,0,{"$f":"T4136*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6227585223217156E-3},{"$f":"U4136*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21580905744602683},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14137,"Middle Atlantic","1970s","Siding","central furnace","central AC",55.212849820297976,21875.138599999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21875.138599999998},"Cold/Very Cold",354.48679597493162,"Metropolitan Area",1.0406084151281432,0.29040499936941777,0.10007114654676719,5.73469445979388E-2,1.0566475292513262,2.4877320902956548,2413.252,208.30600000000001,{"$f":"T4138*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2790221976727197E-2},{"$f":"U4138*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5567226212115996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0933986371048703},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10462786916797878}]
["Single Family Detached",14142,"Pacific","1990s","Wood","central furnace","central AC",53.034967604001864,14998.57681,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14998.57681},"Hot-Dry/Mixed-Dry",124.02227174195835,"Metropolitan Area",0.2230827120526015,0.29570490605343608,0.19004354708399734,2.0026009765251141E-2,0.31427156929365097,1.023102734483686,691.14,644.05399999999997,{"$f":"T4143*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.03661163764634E-2},{"$f":"U4143*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6598933887877408E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23344882842906489},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1997034404727851}]
["Single Family Detached",14146,"West South Central","1990s","Brick","heat pump","central AC",62.56739577574794,14896.99899,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14896.99899},"Hot-Humid",234.75540144043529,"Metropolitan Area",0.15244015643272657,0.11423371884408062,0.14883846429591732,1.0424592159224219E-2,0.53296668531945013,0.94847902489217462,181.547,518.23099999999999,{"$f":"T4147*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7045054756375301E-3},{"$f":"U4147*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.72008668358669E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1551446619083641},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15655855097950402}]
["Single Family Detached",14153,"East South Central","1970s","Siding","central furnace","both central and individual units",38.493232371995127,17433.529149999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17433.529149999998},"Mixed-Humid",378.45095598519998,"Metropolitan Area",2.7522245698688352,0.73085763136322035,0.37948647266318125,4.4244518762726705E-2,0.40171512887294769,4.2642838027681842,1625.0730000000001,912.82500000000005,{"$f":"T4154*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8330757516377949E-2},{"$f":"U4154*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5913761246348749E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.7805553273852133},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.39540023390953}]
["Single Family Attached",14156,"South Atlantic","2000s","Stucco","heat pump","N/A",12.406035090144833,11917.420840000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11917.420840000001},"Hot-Humid",53.46724639689031,"Metropolitan Area",6.2062590856884802E-3,4.247455784548132E-2,0,1.0096438935647999E-4,0.13374940476605343,0.18243022169722325,8.4719999999999995,0,{"$f":"T4157*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0096438935647999E-4},{"$f":"U4157*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.3072234750449598E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14160,"Pacific","1960s","Stucco","central furnace","central AC",32.279011652192821,19864.007170000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19864.007170000001},"Hot-Dry/Mixed-Dry",69.666390436422247,"Metropolitan Area",0.34056973381813038,0.14885475161777165,3.1070783415134751E-2,6.7342162547447204E-3,0.2016774174443432,0.72217268629538001,249.37100000000001,89.644999999999996,{"$f":"T4161*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9535073319900711E-3},{"$f":"U4161*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.78070892275465E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34552324115012045},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.28514923378894E-2}]
["Single Family Detached",14166,"New England","1970s","Wood","central furnace","window/wall unit",46.785539753294593,15779.271419999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15779.271419999999},"Cold/Very Cold",126.64064537281673,"Metropolitan Area",1.2595173818085341,0.35243457159586894,6.2457811940800981E-2,4.1133846557255757E-2,0.32850625324372412,2.0029160185889281,2606.828,0,{"$f":"T4167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1133846557255757E-2},{"$f":"U4167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3006512283657898},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2457811940800981E-2}]
["Multi-Family (5+ units)",14171,"Middle Atlantic","1990s","Brick","central furnace","window/wall unit",20.672698502381557,20247.500980000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1610.5152317410564},"Mixed-Humid",45.415083959594824,"Metropolitan Area",0.25244025425590849,0.48489978790965149,2.2548811693885822E-2,2.7738671392580402E-3,0.15396319205447792,0.91640527568746377,136.99799999999999,0,{"$f":"T4172*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2063736571806123E-4},{"$f":"U4172*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25266089162162653},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.2548811693885822E-2}]
["Single Family Detached",14172,"South Atlantic","1950s","Brick","heat pump","central AC",100.70547482559741,22887.607909999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22887.607909999999},"Mixed-Humid",423.05925954639918,"Metropolitan Area",1.0272718985218849,0.62355816077606385,0.2574212061464492,3.1842796481729878E-2,1.2368144261309733,3.1450656915753714,744.12,647.14800000000002,{"$f":"T4173*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.70311267979892E-2},{"$f":"U4173*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.481166968374068E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0443030253198742},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2722328758301899}]
["Single Family Detached",14180,"East North Central","Before 1950","Wood","central furnace","central AC",32.11702691958638,17922.448059999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17922.448059999999},"Mixed-Humid",239.26878581230065,"Rural",1.2024388340422409,0.14339166420999244,9.7595956090359523E-2,1.7385509438570458E-2,0.56222183683022997,2.0056482911728231,735.14700000000005,234.89400000000001,{"$f":"T4181*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.317563392396482E-2},{"$f":"U4181*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2098755146056394E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2156144679662058},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10180583160496516}]
["Single Family Detached",14183,"West South Central","1970s","Brick","central furnace","central AC",37.885509620453433,21924.48473,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21924.48473},"Hot-Humid",244.98314004310467,"Metropolitan Area",6.0123821417865216E-2,0.18974255906380066,0.13598440216486729,8.9435235090005189E-3,0.45003168611471533,0.8358824687612485,83.171999999999997,324.75200000000001,{"$f":"T4184*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8235032439635598E-3},{"$f":"U4184*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.1200202650369597E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.1947324661828777E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14310442242990426}]
["Single Family Detached",14185,"Pacific","1980s","Stucco","N/A","N/A",31.93258397600453,10089.28404,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10089.28404},"Marine",57.248615480772479,"Metropolitan Area",0,0.12814810293064427,0,0,0.1953322720494948,0.3234803749801391,0,0,{"$f":"T4186*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4186*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14190,"East North Central","2010s","Siding","central furnace","central AC",34.842875786187832,12587.744140000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12587.744140000001},"Cold/Very Cold",166.68777648812446,"Metropolitan Area",6.7375472526049238E-2,0.17948948707111737,1.119265704470794E-2,1.77501038892554E-3,0.31068108382695708,0.56873870046883168,93.606999999999999,47.404000000000003,{"$f":"T4191*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.17830096571298E-3},{"$f":"U4191*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9670942321256011E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.8553773491762213E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.17893664679205E-2}]
["Single Family Detached",14195,"East South Central","2000s","Siding","central furnace","central AC",75.042135435819063,42492.71542,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":42492.71542},"Mixed-Humid",587.97170329865708,"Rural",0.99683784332652725,0.21237251521085496,0.31315746002017314,3.5554419860791567E-2,0.48375576913606477,2.0061235876936201,474.63,362.08800000000002,{"$f":"T4196*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0168317519794598E-2},{"$f":"U4196*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5386102340996962E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0170061608463219},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32854356236117011}]
["Single Family Detached",14201,"Pacific","1970s","Wood","heat pump","central AC",13.462991519813279,9414.6793839999991,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9414.6793839999991},"Marine",146.9887437050543,"Micropolitan Area",0.3220263686580192,7.2100580346677948E-2,1.0828171102675605E-2,6.5286564922317179E-3,0.1581051546241812,0.56306027473155407,640.64,52.814999999999998,{"$f":"T4202*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0314202005657593E-3},{"$f":"U4202*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9723629166595991E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.32805778885858494},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1325407394341565E-2}]
["Single Family Detached",14206,"East South Central","1990s","Siding","heat pump","central AC",49.321440941257507,24035.789929999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24035.789929999999},"Mixed-Humid",422.06835103376073,"Micropolitan Area",0.52548637517838359,0.28173399740972943,0.16728967477175832,1.7753964124424707E-2,0.46558714363067949,1.4400971909905507,394.10899999999998,344.53800000000001,{"$f":"T4207*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4727211335223684E-3},{"$f":"U4207*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2812429909023405E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53495909631190597},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17557091776266065}]
["Single Family Detached",14209,"Pacific","1970s","Concrete","central furnace","N/A",55.226824798342612,13642.990320000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13642.990320000001},"Marine",119.74041946165731,"Metropolitan Area",0.73117601100462981,0.31235929212025104,0,1.4277143796054241E-2,0.5347506895116908,1.5782859926365715,1046.482,0,{"$f":"T4210*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4277143796054241E-2},{"$f":"U4210*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.74545315480068408},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",14213,"East North Central","1970s","Brick","heater burning gas/oil/kerosene","window/wall unit",18.026616769410431,21956.902279999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1746.4834597968211},"Cold/Very Cold",62.542479583829561,"Metropolitan Area",0.63789445008232226,5.084002155661687E-2,1.5380788090237719E-2,0,0.18436817815965176,0.88848343788882866,0,0,{"$f":"T4214*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4214*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63789445008232226},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5380788090237719E-2}]
["Multi-Family (5+ units)",14218,"Pacific","1950s","Stucco","central furnace","N/A",15.345803565664275,20461.07142,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1627.502930470366},"Hot-Dry/Mixed-Dry",40.714708499706461,"Metropolitan Area",2.5313578086827878E-2,0.15728527905911099,0,3.1614401451042002E-4,0.18933797712104083,0.37222783173371143,15.451000000000001,0,{"$f":"T4219*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5146547778697625E-5},{"$f":"U4219*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5338724634606576E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14224,"New England","2000s","Siding","central furnace","window/wall unit",17.816493100917612,10031.80918,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10031.80918},"Cold/Very Cold",27.984173102875065,"Metropolitan Area",0.6841682123543259,6.4912215720666022E-2,3.8059279575634805E-3,1.7534599265722E-3,0.17710354556193769,0.92998990159449313,174.79,0,{"$f":"T4225*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7534599265722E-3},{"$f":"U4225*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.68592167228089806},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8059279575634805E-3}]
["Single Family Attached",14228,"West North Central","2000s","Siding","central furnace","central AC",59.579180953332973,16085.092049999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16085.092049999999},"Cold/Very Cold",127.71654772753189,"Metropolitan Area",1.1812180318749548,0.16242288437586239,5.7287344867731897E-2,1.9459068788223899E-2,0.36241290336180093,1.7633411644803501,998.97500000000002,210.78299999999999,{"$f":"T4229*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6068604830648751E-2},{"$f":"U4229*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3904639575751496E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1972866367056034},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0677808825307045E-2}]
["Single Family Detached",14231,"South Atlantic","2010s","Brick","built-in electric unit","central AC",49.454569603505661,8846.9713069999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8846.9713069999998},"Hot-Humid",137.5309374775513,"Metropolitan Area",5.8604151566685928E-2,0.15956535462057589,0.24695503828038864,1.9122383448199526E-2,0.1922158365276779,0.65734038099532832,0,2161.4609999999998,{"$f":"T4232*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4232*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9122383448199526E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.8604151566685928E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26607742172858817}]
["Single Family Detached",14238,"South Atlantic","1980s","Stucco","heat pump","central AC",30.454247158797113,18857.118979999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18857.118979999999},"Hot-Humid",312.11782885460923,"Metropolitan Area",1.9904349082554298E-2,0.1333937699521206,0.37300435455390984,1.860633815468498E-2,0.53864357167640253,1.0649460452649873,27.523,959.178,{"$f":"T4239*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1900448568653992E-4},{"$f":"U4239*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8087333668998441E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0423353568240838E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3910916882229083}]
["Multi-Family (5+ units)",14242,"Mountain North","1970s","Brick","central furnace","central AC",21.872987078897122,27792.86795,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2210.6845289923194},"Cold/Very Cold",168.8694656815488,"Metropolitan Area",0.17255240552545373,0.15976655100314036,1.2187603794940665E-2,3.5442298995878503E-3,0.22846065410741806,0.57622953120734999,108.583,18.940000000000001,{"$f":"T4243*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.40042758211573E-4},{"$f":"U4243*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1870364979114535E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1727924482836653},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2229474159919779E-2}]
["Single Family Attached",14243,"East North Central","1990s","Brick","central furnace","window/wall unit",59.318609547233493,18618.521519999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18618.521519999998},"Cold/Very Cold",61.470817541776,"Metropolitan Area",2.0227269022011951,0.33904465464979244,3.2566140072191517E-2,1.17486594495504E-2,0.20309712580043363,2.5974348227236135,631.02,0,{"$f":"T4244*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.17486594495504E-2},{"$f":"U4244*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0344755616507455},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2566140072191517E-2}]
["Single Family Detached",14247,"South Atlantic","1980s","Stucco","N/A","central AC",34.131170536570295,18330.381600000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18330.381600000001},"Hot-Humid",439.8747537935202,"Metropolitan Area",0,0.21773708955834961,0.66499510112966165,3.2702573918822406E-2,0.61812048432870714,1.5008526750167184,0,1784.0640000000001,{"$f":"T4248*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4248*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2702573918822406E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.69769767504848401}]
["Multi-Family (5+ units)",14254,"Pacific","1980s","Stucco","central furnace","central AC",12.706071558421172,11314.400320000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":899.96360891031225},"Hot-Dry/Mixed-Dry",64.300280105024328,"Metropolitan Area",1.5036136088622988E-2,5.6657968413631361E-2,1.8875717007188722E-2,1.0949171477670401E-3,0.15057489068744062,0.24215253806628928,18.228999999999999,78.543000000000006,{"$f":"T4255*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6405436626826081E-5},{"$f":"U4255*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0685841734642658E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5052541525249813E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8946402848923363E-2}]
["Single Family Detached",14257,"West South Central","1980s","Brick","central furnace","central AC",26.339103628176652,14973.90769,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14973.90769},"Mixed-Humid",142.03236599365044,"Metropolitan Area",0.7022993454527503,0.62233354233781257,0.17937875920755517,2.023747582555804E-2,0.32074975763844488,1.8247614046365628,795.72699999999998,555.78899999999999,{"$f":"T4258*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1915142644440631E-2},{"$f":"U4258*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3223331811174105E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.7142144880971909},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18770109238867258}]
["Single Family Detached",14261,"East North Central","1990s","Siding","central furnace","central AC",83.468443475914043,24349.020850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24349.020850000001},"Cold/Very Cold",270.20386016767048,"Metropolitan Area",1.8562754110815607,0.4118623728306241,4.4434795988394352E-2,5.309871328528306E-2,1.0998438595512909,3.4124164394518699,2093.165,87.567999999999998,{"$f":"T4262*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0966518227490251E-2},{"$f":"U4262*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1321950577928E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.907241929309051},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.6566991046187153E-2}]
["Single Family Detached",14267,"South Atlantic","1950s","Brick","central furnace","N/A",76.890797910622538,33300.475489999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33300.475489999997},"Hot-Humid",497.37590194588921,"Metropolitan Area",0.65541629554187608,0.67535012667256744,0,1.4281142017214929E-2,0.76463979051959585,2.0954062127340394,428.85700000000003,0,{"$f":"T4268*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4281142017214929E-2},{"$f":"U4268*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.66969743755909106},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",14272,"South Atlantic","2000s","Brick","N/A","central AC",10.525314484171064,10839.66476,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10839.66476},"Hot-Humid",100.58432779396169,"Metropolitan Area",0,6.4187768614884649E-2,9.2467836112833324E-2,4.0497529526598002E-3,0.20521841933798826,0.36187402406570618,0,373.60500000000002,{"$f":"T4273*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4273*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0497529526598002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.6517589065493126E-2}]
["Single Family Detached",14277,"Pacific","1960s","Stucco","built-in electric unit","central AC",19.194355981105712,10905.88408,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10905.88408},"Hot-Dry/Mixed-Dry",81.194983141706174,"Metropolitan Area",4.0091425831242242E-2,0.19586200033440765,7.0632525350092151E-2,3.5238547345091999E-3,0.24001433025579463,0.54660028177153674,0,323.11500000000001,{"$f":"T4278*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4278*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5238547345091999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.0091425831242242E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4156380084601348E-2}]
["Single Family Detached",14281,"South Atlantic","1980s","Siding","heat pump","central AC",61.139942793521378,24833.445489999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24833.445489999998},"Mixed-Humid",566.04315125893402,"Metropolitan Area",0.98368356933130752,0.30578628337287811,0.48941809005272074,3.9890931994961104E-2,2.0052594749645412,3.7841474177214476,605.35400000000004,1000.985,{"$f":"T4282*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5033025561153461E-2},{"$f":"U4282*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4857906433807649E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.99871659489246101},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.51427599648652844}]
["Multi-Family (2-4 units)",14284,"Middle Atlantic","Before 1950","Brick","central furnace","both central and individual units",37.365297951400962,46706.622439999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15568.874146666667},"Mixed-Humid",146.09831498997775,"Metropolitan Area",1.8881396241316621,0.50639959930175427,0.21904010953236455,2.9635632177914643E-2,0.34202671109369231,2.9753631321780829,501.48200000000003,133.024,{"$f":"T4285*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8075101448186945E-3},{"$f":"U4285*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0710339144861868E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8959471342764809},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22111114344685073}]
["Multi-Family (5+ units)",14291,"East North Central","1990s","Brick","central furnace","central AC",8.0176316759290529,11569.45408,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":920.25095033573416},"Cold/Very Cold",27.41960616443269,"Metropolitan Area",0.13063913109069797,0.11732871461934592,1.9168620118640213E-2,3.5425321309337596E-3,6.7442223599436815E-2,0.33783944347881473,237.04900000000001,69.147999999999996,{"$f":"T4292*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1814456752613544E-4},{"$f":"U4292*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3633512713815338E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13085727565822411},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9232253631354029E-2}]
["Single Family Detached",14295,"Pacific","2010s","Stucco","central furnace","central AC",12.560836306780592,10626.76506,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10626.76506},"Hot-Dry/Mixed-Dry",113.38757261633893,"Metropolitan Area",0.14025274662837395,0.35819551973621516,8.3684882199234978E-2,6.6118563259163392E-3,0.35372844214882848,0.93586159071265251,278.89999999999998,343.28899999999999,{"$f":"T4296*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9638047752339998E-3},{"$f":"U4296*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6480515506823398E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14321655140360795},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.7332933749917324E-2}]
["Single Family Detached",14300,"Mountain South","2000s","Stucco","built-in furnace","central AC",96.851499181619715,13267.328659999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13267.328659999999},"Hot-Dry/Mixed-Dry",62.928240008950972,"Metropolitan Area",0.91357896439753794,0.21926217541627346,4.0520624104197558E-2,8.8941517870907982E-4,0.18200758287563706,1.3553693467936458,0,67.037999999999997,{"$f":"T4301*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4301*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8941517870907982E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.91357896439753794},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1410039282906638E-2}]
["Single Family Attached",14302,"West South Central","Before 1950","Wood","portable electric heaters","window/wall unit",5.1599593164356294,10177.43455,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10177.43455},"Hot-Humid",62.316431744645676,"Metropolitan Area",2.3407560060968849E-2,7.4221221201214188E-2,5.8847443005847953E-2,0,5.6160915785118996E-2,0.21263714005314999,0,0,{"$f":"T4303*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4303*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3407560060968849E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8847443005847953E-2}]
["Multi-Family (5+ units)",14305,"West South Central","2000s","Brick","built-in electric unit","central AC",18.546145449405699,27847.06524,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2214.995459074521},"Hot-Humid",423.55294333732866,"Metropolitan Area",0.13878311770756765,0.17321467721769609,0.1554364341164122,6.6324469164717598E-3,0.97162348197384951,1.4451626036035274,0,238.17400000000001,{"$f":"T4306*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4306*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2755432846961496E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13878311770756765},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15596398844488182}]
["Single Family Detached",14313,"Mountain North","1990s","Wood","central furnace","N/A",25.67750520052201,22289.501039999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22289.501039999999},"Cold/Very Cold",138.57543282293383,"Metropolitan Area",0.76334671437779467,0.21625619396274121,0,1.41684327835812E-2,0.46900096981299355,1.4486038781535293,635.65499999999997,0,{"$f":"T4314*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.41684327835812E-2},{"$f":"U4314*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.77751514716137582},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14314,"East North Central","1960s","Brick","central furnace","central AC",43.076597243777456,15579.239509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15579.239509999999},"Cold/Very Cold",154.25005038359515,"Metropolitan Area",1.4907842212603264,0.36381663659787805,4.2513921851767333E-2,1.9729424281547919E-2,0.5000894909310083,2.3972042706409802,1118.211,148.18100000000001,{"$f":"T4315*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.742087699171661E-2},{"$f":"U4315*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3085472898313102E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.508205098252043},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.4822469141598646E-2}]
["Single Family Detached",14319,"South Atlantic","1960s","Stucco","heat pump","central AC",66.950699252211081,35348.838040000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35348.838040000002},"Hot-Humid",693.54077355361881,"Metropolitan Area",7.3274252884735604E-3,0.4085640616942785,0.56920339198093062,3.2447723553219163E-2,1.381266274320222,2.3663611532839046,3.5710000000000002,914.35799999999995,{"$f":"T4320*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2623070064084001E-4},{"$f":"U4320*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2321492852578321E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.4536559891144006E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.60152488483350897}]
["Single Family Detached",14325,"East South Central","1990s","Brick","heat pump","central AC",58.017985042744058,15689.01705,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15689.01705},"Hot-Humid",231.88964948189789,"Metropolitan Area",0.1736293475952588,7.4131719481460551E-2,0.29733158329935377,1.6944938553869551E-2,0.33537948921782018,0.88047213959389325,132.316,947.73500000000001,{"$f":"T4326*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0759079799878002E-3},{"$f":"U4326*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4869030573881751E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1757052555752466},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3122006138732355}]
["Mobile Home",14329,"East South Central","1980s","Siding","built-in furnace","central AC",43.891282962993238,24050.018059999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24050.018059999999},"Mixed-Humid",523.42302984832452,"Micropolitan Area",0.71166492616409205,0.4309189643421269,0.30676570041109724,1.232652410641822E-2,0.33656982959206083,1.7859194205093767,0,512.53700000000003,{"$f":"T4330*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4330*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.232652410641822E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.71166492616409205},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31909222451751545}]
["Single Family Detached",14332,"West North Central","Before 1950","Wood","central furnace","central AC",26.852444661739025,9708.0421769999994,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9708.0421769999994},"Cold/Very Cold",122.66042363611771,"Rural",0.49623059500681621,0.1385445572086908,4.8006093820505809E-2,2.2176740891789136E-2,0.21235422910593343,0.89513547514194625,2020.231,264.137,{"$f":"T4333*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9612487755282886E-2},{"$f":"U4333*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5642531365062489E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.51584308276209911},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0570346957012055E-2}]
["Multi-Family (5+ units)",14339,"West North Central","1970s","Brick","central furnace","central AC",10.496291967755612,11237.999970000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":893.8866156306533},"Cold/Very Cold",89.18558810002375,"Metropolitan Area",0.23115490608209222,0.17185612559722765,1.8220882707674788E-2,6.2402141473416606E-3,0.27990328069479431,0.70687905365697645,484.61700000000002,70.661000000000001,{"$f":"T4340*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3319265000708033E-4},{"$f":"U4340*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.31629221470776E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23158809873209929},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8284045629821864E-2}]
["Multi-Family (2-4 units)",14343,"Pacific","1980s","Shingle","central furnace","N/A",23.394347696938325,25595.566409999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8531.8554700000004},"Marine",116.43935070340461,"Metropolitan Area",0.13012550483633029,0.31789317226393771,0,3.19217666038956E-3,0.52311161531865269,0.97325841019251369,124.71599999999999,0,{"$f":"T4344*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.06405888679652E-3},{"$f":"U4344*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13118956372312682},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",14348,"Pacific","1950s","Siding","heater burning gas/oil/kerosene","window/wall unit",10.411899254263515,13031.16302,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1036.5173732670087},"Marine",30.625669928260081,"Metropolitan Area",0.1456014065192785,0.1822084323945953,3.8285166017869403E-3,0,0.10066629466950983,0.43230465018517056,0,0,{"$f":"T4349*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4349*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1456014065192785},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8285166017869403E-3}]
["Mobile Home",14353,"Pacific","1980s","Concrete","central furnace","window/wall unit",12.193208277296597,9841.1689079999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9841.1689079999996},"Hot-Dry/Mixed-Dry",27.52574943631847,"Metropolitan Area",0.20617271496948489,0.34545169823854066,2.9525199405052174E-2,2.2813600939147441E-3,0.13577950297004651,0.71692911558312433,231.81800000000001,0,{"$f":"T4354*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2813600939147441E-3},{"$f":"U4354*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20845407506339964},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.9525199405052174E-2}]
["Single Family Detached",14355,"Pacific","1970s","Stucco","central furnace","central AC",14.594644747585788,10079.17455,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10079.17455},"Hot-Dry/Mixed-Dry",45.705266812069375,"Metropolitan Area",1.8799615895612697E-2,0.3518311657481652,4.4044682490808496E-3,7.3256448546855002E-4,0.13274229541899429,0.50777754531185304,40.192,32.488999999999997,{"$f":"T4356*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.051021835136E-4},{"$f":"U4356*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2746230195494997E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9204718079126298E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7319305510358E-3}]
["Single Family Attached",14358,"Mountain North","1980s","Wood","central furnace","both central and individual units",9.5895995687265803,6050.2205480000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6050.2205480000002},"Cold/Very Cold",33.205189475494585,"Metropolitan Area",0.24256651914967356,6.0334795877436842E-2,8.0262467798589924E-3,2.9274657645758278E-3,0.10025946314678204,0.41118702495375142,433.988,49.872999999999998,{"$f":"T4359*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6257231151854241E-3},{"$f":"U4359*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.01742649390404E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24519224226485897},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.3279894292493956E-3}]
["Single Family Detached",14366,"East South Central","Before 1950","Wood","central furnace","central AC",31.953765987579271,17518.512050000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17518.512050000001},"Mixed-Humid",126.16832381718525,"Metropolitan Area",0.82722159881675283,0.25824974101448472,0.1812423562634321,2.3011056096012401E-2,0.25015583807714364,1.5168695341718132,857.22,456.30799999999999,{"$f":"T4367*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5017218899501002E-2},{"$f":"U4367*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.9938371965114011E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84223881771625386},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1892361934599435}]
["Single Family Detached",14367,"East South Central","1960s","Shingle","heat pump","central AC",74.990567894364915,26706.042700000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26706.042700000002},"Mixed-Humid",393.4845096781217,"Metropolitan Area",0.74610225782675144,0.83492562113545687,0.51388029082558473,3.4521592802197694E-2,0.98101042542685457,3.0759185952146479,429.38,863.27099999999996,{"$f":"T4368*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1467040614525999E-2},{"$f":"U4368*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.30545521876717E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.75756929844127741},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.53693484301325645}]
["Single Family Detached",14373,"West North Central","1970s","Wood","central furnace","central AC",65.282618126034265,15192.603709999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15192.603709999999},"Cold/Very Cold",173.94288488747156,"Metropolitan Area",0.81405314570256571,0.25552728839319488,9.3762566708410017E-2,0.11729378289068061,0.38698136795698856,1.5503243687611592,7421.32,299.13299999999998,{"$f":"T4374*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.11274917376509719},{"$f":"U4374*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5446091255834297E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.92680231946766289},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.830717583399344E-2}]
["Single Family Detached",14378,"West South Central","1990s","Brick","central furnace","central AC",38.844659830373466,18648.420470000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18648.420470000001},"Hot-Humid",215.02632082150495,"Metropolitan Area",0.38387007087413683,0.113240985485176,0.4185323935090785,3.0025579369280891E-2,0.34347158734472572,1.259115037213117,453.92599999999999,1156.1610000000001,{"$f":"T4379*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4650029102652201E-3},{"$f":"U4379*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1560576459015671E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39233507378440202},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.44009296996809416}]
["Single Family Detached",14382,"Pacific","1980s","Stucco","central furnace","central AC",15.582469257148295,10614.76107,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10614.76107},"Hot-Dry/Mixed-Dry",94.22711729464821,"Metropolitan Area",0.28473428901803699,0.28499927591338842,0.15055028142048343,6.1414141565531112E-3,0.20707251481405545,0.92735636116596432,272.33600000000001,306.23700000000002,{"$f":"T4383*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8907815707595202E-3},{"$f":"U4383*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2506325857935901E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28762507058879649},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15380091400627702}]
["Single Family Detached",14385,"East North Central","2000s","Siding","central furnace","central AC",75.177997671398515,27730.72581,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27730.72581},"Cold/Very Cold",191.53487528825318,"Micropolitan Area",2.1926229004834679,0.26905254202523404,6.7280730651834958E-2,2.7740265179678637E-2,0.52494463619555853,3.053900809356096,871.42899999999997,128.91499999999999,{"$f":"T4386*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4165358661882491E-2},{"$f":"U4386*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5749065177961498E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2167882591453503},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0855637169631114E-2}]
["Multi-Family (5+ units)",14391,"Pacific","2000s","Siding","built-in electric unit","window/wall unit",7.9535402875066454,14102.021790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1121.695013798156},"Marine",57.832391345859492,"Metropolitan Area",2.9066988599395473E-2,8.1566023523251055E-2,4.3885773850915804E-3,0,8.2293899377941904E-2,0.19731548888568001,0,0,{"$f":"T4392*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4392*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9066988599395473E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.3885773850915804E-3}]
["Single Family Detached",14396,"South Atlantic","1970s","Brick","built-in electric unit","central AC",26.355201553877858,19097.972140000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19097.972140000002},"Mixed-Humid",394.04784803964651,"Metropolitan Area",0.52685388582491033,0.36269308383964172,0.15657579407622985,7.163878525379681E-3,0.29836847815196632,1.3444912418927482,0,375.11200000000002,{"$f":"T4397*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4397*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.163878525379681E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52685388582491033},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16373967260160951}]
["Single Family Detached",14401,"East North Central","1960s","Siding","central furnace","N/A",59.415356539184472,18631.344160000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18631.344160000001},"Cold/Very Cold",79.783458712184668,"Metropolitan Area",1.2582462527490625,0.29472701613708496,0,3.7616497545598405E-2,0.29420286053183176,1.8471761294179794,2018.99,0,{"$f":"T4402*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7616497545598405E-2},{"$f":"U4402*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2958627502946609},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",14403,"Mountain North","2000s","Other","heater burning gas/oil/kerosene","central AC",3.7935144550175708,9032.1772739999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9032.1772739999997},"Cold/Very Cold",73.408858214035988,"Metropolitan Area",0.12555829239705155,0.22268404040626485,6.3030416854199817E-3,1.9046152217683799E-4,0.29065097568521492,0.64519635017395127,0,21.087,{"$f":"T4404*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4404*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9046152217683799E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12555829239705155},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4935032075968194E-3}]
["Mobile Home",14411,"South Atlantic","1980s","Siding","heat pump","central AC",18.503379599960638,20025.302599999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20025.302599999999},"Mixed-Humid",318.24947818860096,"Metropolitan Area",0.1718759506723414,0.4046009460274636,7.0847117562487988E-2,4.5368524558455992E-3,0.43854321315008282,1.085867227412376,107.59699999999999,118.959,{"$f":"T4412*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1546624838522E-3},{"$f":"U4412*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3821899719933997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17403061315619361},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.3229307534481383E-2}]
["Single Family Detached",14414,"Pacific","1950s","Stucco","N/A","N/A",12.492282126820497,11234.06666,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11234.06666},"Hot-Dry/Mixed-Dry",36.095056181181889,"Metropolitan Area",0,0.43024862095827621,0,0,0.12314783872692006,0.55339645968519624,0,0,{"$f":"T4415*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4415*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14419,"South Atlantic","1990s","Siding","central furnace","central AC",61.997451247419683,16634.679700000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16634.679700000001},"Mixed-Humid",236.19162514204396,"Metropolitan Area",1.0578566551332853,0.44297385182365834,0.14441237488629882,2.8866625454441599E-2,0.34442788004185676,1.9896707618850993,1209.942,525.38599999999997,{"$f":"T4420*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0126997625577403E-2},{"$f":"U4420*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7396278288641993E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0779836527588627},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15315200271516302}]
["Single Family Detached",14420,"East South Central","2000s","Wood","built-in electric unit","central AC",51.653157446270804,24364.696909999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24364.696909999999},"Mixed-Humid",409.7394023834504,"Metropolitan Area",0.40415530625127716,0.37237053581491203,0.13399586784396383,6.7806707853560891E-3,0.48750917593250298,1.398030885842656,0,278.29899999999998,{"$f":"T4421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7806707853560891E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.40415530625127716},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14077653862931994}]
["Single Family Detached",14426,"West North Central","2000s","Wood","central furnace","central AC",56.885781796596135,14852.68454,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14852.68454},"Mixed-Humid",187.58841063802316,"Metropolitan Area",0.99148745123414861,0.47035037306004257,0.12776871863421146,2.8090095078221376E-2,0.4920077556113055,2.0816142985397081,1365.086,526.16099999999994,{"$f":"T4427*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0275191727970439E-2},{"$f":"U4427*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8149033502509391E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0117626429621192},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13558362198446242}]
["Multi-Family (5+ units)",14430,"West South Central","1980s","Brick","central furnace","central AC",29.521544098053731,26311.536629999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2092.8573138475158},"Hot-Humid",431.52111984630807,"Metropolitan Area",0.29937062680726817,0.35171315113273377,0.27648135005386565,1.7519668222768649E-2,0.52865881382328961,1.4723500705332138,182.86799999999999,482.98700000000002,{"$f":"T4431*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8271663126866751E-4},{"$f":"U4431*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0108228754432702E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29975334343853682},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27749217292930894}]
["Single Family Detached",14437,"South Atlantic","1990s","Concrete","N/A","both central and individual units",102.97681316919299,34325.60439,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34325.60439},"Hot-Humid",563.18825773934816,"Metropolitan Area",0,0.212111639767566,0.72772272191854626,3.7628722974845312E-2,0.98176401423981574,1.9215983759259279,0,1096.229,{"$f":"T4438*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4438*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7628722974845312E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.76535144489339157}]
["Single Family Detached",14440,"Pacific","1970s","Stucco","central furnace","central AC",27.731682119256295,9569.2484879999993,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9569.2484879999993},"Hot-Dry/Mixed-Dry",113.69702591440432,"Metropolitan Area",0.10238968611155108,0.16353195914019661,0.10030047993540848,7.385536413789911E-3,0.50786436142631342,0.87408648661346977,185.85599999999999,585.94299999999998,{"$f":"T4441*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7785022469857278E-3},{"$f":"U4441*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6070341668041836E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10416818835853681},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10590751410221266}]
["Multi-Family (2-4 units)",14444,"South Atlantic","1960s","Brick","central furnace","central AC",37.272207859817392,31321.183079999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10440.39436},"Mixed-Humid",501.87027883244122,"Metropolitan Area",0.43512435750329737,0.57985983684701958,0.15578608343288097,1.4759762993436121E-2,0.53177129690170477,1.7123814166805267,242.648,228.59100000000001,{"$f":"T4445*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5333408106652799E-3},{"$f":"U4445*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.38658018714676E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43765769831396262},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15817266362002774}]
["Multi-Family (5+ units)",14449,"South Atlantic","1980s","Stucco","heat pump","central AC",34.552611460343485,31993.158759999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2544.781676780035},"Mixed-Humid",251.47483400998394,"Metropolitan Area",7.8005332637887934E-2,0.24246277710167832,8.524873348070755E-2,5.2853658066282791E-3,0.44745030370351313,0.8580321071630661,41.298000000000002,123.905,{"$f":"T4450*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0509439368766189E-4},{"$f":"U4450*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1531117366143026E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.8110427031575599E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5564044654368981E-2}]
["Single Family Detached",14454,"Pacific","Before 1950","Siding","wood-burning stove","N/A",35.469061660325103,19926.439139999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19926.439139999999},"Marine",192.17737393382106,"Micropolitan Area",7.4472455922222652E-2,0.27621691186402619,0,0,0.3050198224362089,0.65570919022245777,0,0,{"$f":"T4455*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4455*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.4472455922222652E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14456,"South Atlantic","1990s","Shingle","heat pump","central AC",24.444872012405504,14996.853999999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14996.853999999999},"Hot-Humid",229.8954880667504,"Metropolitan Area",7.3182517966732002E-2,0.21910007777054399,0.20066756449397596,1.1095722368979998E-2,0.29145322472051405,0.78440338495176598,83.516999999999996,656.35299999999995,{"$f":"T4457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2524922555179998E-3},{"$f":"U4457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8432301134619999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.4435010222250006E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21051079460743796}]
["Single Family Detached",14463,"South Atlantic","1950s","Shingle","heat pump","central AC",49.175004352500004,17512.465939999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17512.465939999998},"Mixed-Humid",175.33198945923405,"Metropolitan Area",0.26843263653778859,9.08685957071423E-2,0.13677304197757165,1.0961542780892317E-2,0.10215846219947773,0.59823273642198027,260.52199999999999,365.40600000000001,{"$f":"T4464*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5623826516206795E-3},{"$f":"U4464*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3991601292716395E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27299501918940927},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14317220210684328}]
["Single Family Detached",14467,"East North Central","1960s","Brick","central furnace","central AC",63.105790353447205,20020.87257,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20020.87257},"Cold/Very Cold",125.85590990561617,"Metropolitan Area",1.3191815201286694,0.32346296323134754,6.374641822113486E-2,3.9118903039758422E-2,0.34784710468576313,2.0542380062669148,1800.9280000000001,152.97800000000001,{"$f":"T4468*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6056149995744961E-2},{"$f":"U4468*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0627530440134601E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3552376701244144},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.680917126514832E-2}]
["Multi-Family (5+ units)",14473,"Pacific","1960s","Concrete","N/A","window/wall unit",14.668954913702965,17463.041560000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1389.0353408397316},"Hot-Humid",37.781080867068326,"Metropolitan Area",0,2.266809319041516E-2,1.8822399641113523E-2,0,8.7418554079952096E-2,0.12890904691148078,0,0,{"$f":"T4474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8822399641113523E-2}]
["Single Family Detached",14474,"Pacific","1970s","Stucco","heat pump","central AC",49.135027000899299,11928.87278,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11928.87278},"Marine",177.59701030572489,"Metropolitan Area",0.24363420020242424,0.12653006651898954,4.3296690704977381E-2,8.8758209384323609E-3,0.19250002536127686,0.60596098278766797,515.32000000000005,228.74199999999999,{"$f":"T4475*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1471867209896012E-3},{"$f":"U4475*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7286342174427597E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24978138692341384},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.602532492242014E-2}]
["Single Family Detached",14478,"Pacific","1970s","Siding","heater burning gas/oil/kerosene","window/wall unit",2.6766639170621338,1416.224295,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1416.224295},"Marine",12.915792788681896,"Micropolitan Area",8.7465341168884173E-2,1.6341118190100451E-2,7.9442676960736502E-4,0,2.2651846221779241E-2,0.12725273235037124,0,0,{"$f":"T4479*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4479*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.7465341168884173E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9442676960736502E-4}]
["Single Family Detached",14485,"Pacific","1950s","Wood","heat pump","central AC",12.08068185227329,9430.6649899999993,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9430.6649899999993},"Marine",119.76725745954808,"Metropolitan Area",0.14966272010497703,0.13405377185207332,1.8663965023089278E-2,3.3120872671479596E-3,0.10626543097652924,0.40864588795666884,262.5,88.703999999999994,{"$f":"T4486*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4755495598749997E-3},{"$f":"U4486*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3653770727295986E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15213826966485203},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9500502730362239E-2}]
["Single Family Detached",14490,"East North Central","1970s","Siding","central furnace","central AC",39.256234422357174,15168.560439999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15168.560439999999},"Mixed-Humid",396.23313585039188,"Rural",1.1203931196642143,0.19875071991315507,0.19138973607139231,4.8859070819272994E-2,1.0458264484540314,2.5563600241027933,2562.8589999999999,658.21600000000001,{"$f":"T4491*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8874881640697953E-2},{"$f":"U4491*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9841891785750394E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1592680013049121},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20137392524996736}]
["Multi-Family (5+ units)",14492,"New England","1960s","Concrete","radiator","central AC",23.089873286693678,33463.584470000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2661.7414440835587},"Cold/Very Cold",222.38509502311916,"Metropolitan Area",0.56992055911009332,0.34963271739815288,3.3081488998468453E-2,5.0665874702648201E-3,0.79361494037476776,1.7509132897266644,109.783,41.622999999999998,{"$f":"T4493*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9221396095582532E-4},{"$f":"U4493*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1078966412708995E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.57021277307104912},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.319227866259554E-2}]
["Mobile Home",14497,"South Atlantic","1990s","Siding","heat pump","both central and individual units",26.693743530122269,23171.65237,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23171.65237},"Cold/Very Cold",345.93077998447512,"Micropolitan Area",0.35393565901374108,0.5109347030419763,4.7611002669510329E-2,6.0720851602537604E-3,0.78232584578815212,1.6948072105133798,200.38900000000001,61.658999999999999,{"$f":"T4498*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.6433442467719299E-3},{"$f":"U4498*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4287409134818298E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35857900326051301},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.9039743582992158E-2}]
["Single Family Attached",14502,"Pacific","1980s","Stucco","central furnace","central AC",17.304509013349193,7484.6492269999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7484.6492269999999},"Hot-Dry/Mixed-Dry",31.603871484772863,"Metropolitan Area",6.1052485830168125E-2,4.6341594890730302E-2,1.283686949668311E-2,1.5728017346140989E-3,0.10296866211104706,0.22319961232862859,115.88,94.257000000000005,{"$f":"T4503*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6732115242475988E-4},{"$f":"U4503*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0548058218933903E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.1919806982592883E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.354235007887245E-2}]
["Single Family Detached",14508,"South Atlantic","2000s","Brick","heat pump","central AC",32.734961268432528,19485.095990000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19485.095990000002},"Hot-Humid",282.91492295230705,"Rural",0.12501571337857634,0.19447468321133712,0.24466051592827712,1.4374759349798691E-2,0.40115481106571427,0.96530572358390487,111.166,626.56500000000005,{"$f":"T4509*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1660801808243402E-3},{"$f":"U4509*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2208679168974354E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12718179355940068},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25686919509725148}]
["Single Family Detached",14512,"East North Central","2000s","Siding","central furnace","central AC",84.661946945907829,19219.51122,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19219.51122},"Cold/Very Cold",184.36452601063658,"Metropolitan Area",1.443404877303933,0.32030583935870521,2.576210191244508E-2,2.459786080078236E-2,0.57999870257316088,2.3694715211482444,1211.8409999999999,67.997,{"$f":"T4513*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3290991696356018E-2},{"$f":"U4513*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.30686910442634E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4666958690002889},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7068971016871422E-2}]
["Single Family Detached",14515,"East North Central","1970s","Siding","central furnace","central AC",77.995374146185796,30550.479490000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30550.479490000002},"Cold/Very Cold",406.495698295789,"Metropolitan Area",2.0710938390830176,0.48732102440705766,0.24769742201285794,0.10674847726813483,1.2105883816435419,4.0167006671464751,3078.5839999999998,415.58300000000003,{"$f":"T4516*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4052217350242148E-2},{"$f":"U4516*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2696259917892671E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1651460564332599},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26039368193075063}]
["Single Family Attached",14520,"Middle Atlantic","1990s","Siding","central furnace","central AC",21.74172532838115,19240.464889999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19240.464889999999},"Cold/Very Cold",100.31978394883126,"Metropolitan Area",0.63327356165791548,0.18317634472480931,4.2902446333116663E-2,1.2927168107503859E-2,0.30470727892716265,1.1640596316430041,575.96299999999997,95.911000000000001,{"$f":"T4521*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1081795879439069E-2},{"$f":"U4521*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.84537222806479E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.64435535753735451},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.474781856118145E-2}]
["Single Family Detached",14526,"Middle Atlantic","2000s","Siding","central furnace","central AC",45.241853879045841,14804.271559999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14804.271559999999},"Cold/Very Cold",186.7635246992032,"Metropolitan Area",0.72959949265807089,0.17267871116279784,2.1545737113091875E-2,2.2433371627286359E-2,0.50923477198190015,1.4330587129158607,1443.73,71.600999999999999,{"$f":"T4527*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1373370979318799E-2},{"$f":"U4527*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.06000064796756E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.75097286363738969},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.2605737761059435E-2}]
["Single Family Detached",14527,"East North Central","1950s","Siding","central furnace","central AC",39.306535346141317,18248.1594,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18248.1594},"Cold/Very Cold",97.627014100798007,"Metropolitan Area",0.64445396817161527,0.22602783370995841,4.1396679525276002E-2,2.6572841981164202E-2,0.40398921264130305,1.3158676940481526,1341.412,114.78100000000001,{"$f":"T4528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4478299997072801E-2},{"$f":"U4528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0945419840914001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.66893226816868812},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.3491221509367399E-2}]
["Single Family Detached",14531,"East North Central","1990s","Siding","central furnace","central AC",92.763076311845253,25269.15726,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25269.15726},"Cold/Very Cold",154.24462896584484,"Metropolitan Area",1.2694078398450683,0.51195110455501913,4.7785366182309302E-2,3.2803762956843237E-2,0.4473185890742104,2.276462899656607,1205.2539999999999,92.92,{"$f":"T4532*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0455752864244037E-2},{"$f":"U4532*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3480100925992002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2998635927093123},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0133376274908506E-2}]
["Single Family Detached",14538,"Middle Atlantic","1990s","Brick","central furnace","central AC",66.134913923006721,21451.480350000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21451.480350000002},"Cold/Very Cold",126.39602639918573,"Metropolitan Area",0.99149724655500038,0.33724249804289164,6.5759169789239402E-2,2.6326908449506952E-2,0.37385959581037237,1.7683585101975039,1055.463,171.81399999999999,{"$f":"T4539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2641243804652052E-2},{"$f":"U4539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6856646448548999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0141384903596524},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9444834434094299E-2}]
["Single Family Detached",14540,"West North Central","2000s","Siding","central furnace","central AC",35.498053859312087,15918.409799999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15918.409799999999},"Cold/Very Cold",143.64741168850003,"Metropolitan Area",0.78312267750196252,0.37498635026116561,3.20937745709916E-2,3.0564588451964397E-2,0.42902409845693157,1.6192269007910514,1822.2380000000001,97.84,{"$f":"T4541*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9007131237132399E-2},{"$f":"U4541*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.557457214832E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.8121298087390949},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3651231785823597E-2}]
["Single Family Detached",14545,"Pacific","1960s","Siding","fireplace","N/A",47.351272230428435,14843.659009999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14843.659009999999},"Marine",374.93179693091633,"Micropolitan Area",0.41502585593707009,0.49885617722265452,0,0,0.36538527585337577,1.2792673090131004,0,0,{"$f":"T4546*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4546*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.41502585593707009},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",14550,"South Atlantic","1980s","Wood","heat pump","both central and individual units",18.83790795897557,34756.287750000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2764.5649147241129},"Mixed-Humid",111.22665497309616,"Metropolitan Area",7.128721273935365E-2,0.21176279719661026,6.1796875892152853E-2,3.1116261733942501E-3,0.3146987915676856,0.66240980036607611,52.645000000000003,36.881999999999998,{"$f":"T4551*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4554051993565092E-4},{"$f":"U4551*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0196268318485473E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.14327532592893E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1898838575337706E-2}]
["Single Family Detached",14556,"South Atlantic","1990s","Siding","central furnace","central AC",69.230227910785558,16554.334750000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16554.334750000002},"Mixed-Humid",141.13798703217518,"Metropolitan Area",1.749334313470065,0.15862966135234902,0.1226295124189055,3.3140586257397998E-2,0.38785218758547474,2.4184456748267942,1529.9079999999999,472.02,{"$f":"T4557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5326609168702999E-2},{"$f":"U4557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8139770886950007E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.774660922638768},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13044348950760051}]
["Single Family Detached",14561,"Pacific","2000s","Stucco","central furnace","central AC",11.041801524380926,12187.418900000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12187.418900000001},"Hot-Dry/Mixed-Dry",38.177491892465291,"Metropolitan Area",7.0176913014521614E-2,8.2830305688744207E-2,4.9672190086216601E-2,3.6196390384622E-3,0.10340521596249434,0.30608462475197673,119.48699999999999,177.511,{"$f":"T4562*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4562381221042999E-3},{"$f":"U4562*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1634009163578999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.1633151136625911E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.1835591002574503E-2}]
["Single Family Detached",14564,"West South Central","1980s","Brick","central furnace","central AC",57.422830891114323,17100.307000000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17100.307000000001},"Hot-Humid",595.96334631233287,"Metropolitan Area",1.0749441425583142,0.42574148689181202,0.65864706972106712,5.2733789924144008E-2,1.361682637544138,3.521015336715331,765.90499999999997,2317.8870000000002,{"$f":"T4565*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3097210632835001E-2},{"$f":"U4565*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.963657929130901E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0880413531911493},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.69828364901237616}]
["Single Family Detached",14568,"South Atlantic","1970s","Siding","central furnace","central AC",23.689165995896214,16292.41128,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16292.41128},"Mixed-Humid",155.62511251224254,"Metropolitan Area",0.85443063106757544,0.14132057095165534,0.31342187317745374,2.5738588416031199E-2,0.20610639944672107,1.5152794746434057,704.25400000000002,875.53599999999994,{"$f":"T4569*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1473995813585122E-2},{"$f":"U4569*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4264592602446079E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.86590462688116054},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32768646577989979}]
["Multi-Family (2-4 units)",14574,"East North Central","1980s","Wood","built-in electric unit","central AC",22.655241714757302,24841.273809999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8280.4246033333329},"Cold/Very Cold",98.447632474537357,"Metropolitan Area",6.5638967232746342E-2,0.12472341532308134,2.5467762455063596E-2,1.1181305754619101E-3,0.11932771676263267,0.33590328215716525,0,45.011000000000003,{"$f":"T4575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7271019182063669E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.5638967232746342E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5840472646884233E-2}]
["Single Family Detached",14579,"South Atlantic","2000s","Concrete","heat pump","central AC",46.614292261704719,25896.829030000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25896.829030000001},"Hot-Humid",261.24267935273969,"Metropolitan Area",1.5809962329156942E-2,0.13786386698435643,0.18562714974875952,1.025182950176416E-2,0.55205904533162786,0.89136002439390072,10.679,385.19299999999998,{"$f":"T4580*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7655223721137002E-4},{"$f":"U4580*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9752772645527905E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6086514566368313E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19560242701331232}]
["Single Family Detached",14584,"Mountain North","1990s","Wood","central furnace","central AC",95.64679801812153,44445.538110000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":44445.538110000001},"Cold/Very Cold",473.50258477637851,"Metropolitan Area",0.16713731272604065,0.64705965544582522,4.6379407918704214E-2,7.9244172173224513E-3,0.7550144896541191,1.6155908657446891,126.22,52.075000000000003,{"$f":"T4585*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6099158202442007E-3},{"$f":"U4585*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3145013970782501E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17274722854628485},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.8693909315782463E-2}]
["Single Family Detached",14586,"Middle Atlantic","1950s","Brick","central furnace","window/wall unit",23.328528521679164,22871.106390000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22871.106390000001},"Mixed-Humid",349.29343759161054,"Metropolitan Area",1.1742516148435937,0.68034419447720162,0.11833910690547825,1.9642826851945114E-2,0.74492648114596416,2.7178613973722379,858.84900000000005,0,{"$f":"T4587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9642826851945114E-2},{"$f":"U4587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1938944416955388},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11833910690547825}]
["Single Family Attached",14591,"Pacific","1970s","Siding","built-in electric unit","window/wall unit",8.6415073246749436,8038.611465,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8038.611465},"Marine",115.91195415573755,"Metropolitan Area",0.10344848901251176,0.13813685793989761,6.7651024822688397E-3,0,0.14714113976157658,0.39549158919625477,0,0,{"$f":"T4592*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4592*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10344848901251176},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7651024822688397E-3}]
["Single Family Attached",14593,"South Atlantic","1980s","Wood","central furnace","central AC",38.386412658490102,13724.13753,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13724.13753},"Mixed-Humid",187.90822851483398,"Metropolitan Area",0.59082801832155862,0.39925931522975278,6.7690232297878586E-2,9.0579307698000003E-3,0.37022713745741548,1.4280047033066054,400.49400000000003,259.50599999999997,{"$f":"T4594*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4964347359398201E-3},{"$f":"U4594*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5614960338601798E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59632445305749848},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.1251728331738762E-2}]
["Single Family Detached",14598,"East North Central","1950s","Siding","central furnace","central AC",93.811418172606409,48506.420980000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":48506.420980000003},"Cold/Very Cold",424.07068384200988,"Metropolitan Area",2.0974141022064687,0.71678869605428819,0.27100144499516066,9.6214814322037059E-2,1.0926796496738649,4.1778838929297821,1716.2260000000001,267.322,{"$f":"T4599*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3247980852821479E-2},{"$f":"U4599*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2966833469215561E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.18066208305929},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28396827846437622}]
["Mobile Home",14603,"West North Central","1980s","Siding","portable electric heaters","N/A",46.18769990471403,45105.175689999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":45105.175689999996},"Mixed-Humid",519.38609804959185,"Micropolitan Area",0.68916757240929549,0.32207003391591688,0,0,0.76090776029082174,1.7721453666160341,0,0,{"$f":"T4604*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4604*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.68916757240929549},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14609,"West South Central","Before 1950","Brick","central furnace","central AC",16.494279805552949,13930.97957,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13930.97957},"Hot-Humid",276.64520930011588,"Metropolitan Area",0.15217603050146492,0.29949175119565036,0.53153584287535094,2.6428349894410438E-2,0.41465013202607903,1.3978537565985454,148.96100000000001,1748.1310000000001,{"$f":"T4610*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0751726477267699E-3},{"$f":"U4610*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4353177246683674E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15425120314919169},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.55588902012203456}]
["Single Family Attached",14612,"South Atlantic","1980s","Wood","heat pump","central AC",15.51388450832439,10219.950269999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10219.950269999999},"Mixed-Humid",135.82380337162331,"Metropolitan Area",0.11969592470288649,0.12833390843069264,4.7288905633471594E-2,5.01837372072999E-3,0.16811206019128816,0.46343079895833894,274.64400000000001,216.393,{"$f":"T4613*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8068480219538799E-3},{"$f":"U4613*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2115256987761101E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12250277272484038},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.9500431332247706E-2}]
["Mobile Home",14616,"Pacific","1970s","Siding","central furnace","central AC",12.476408325344927,13444.40552,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13444.40552},"Cold/Very Cold",334.86419123758645,"Micropolitan Area",0.77308472353129465,9.30686955461172E-2,5.8441795576214955E-2,1.1512834334536081E-2,0.21796141484373271,1.1425566294973595,710.99400000000003,145.33500000000001,{"$f":"T4617*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5588916582868815E-3},{"$f":"U4617*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9539426762492E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78264361518958148},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0395738252464158E-2}]
["Single Family Detached",14622,"Mountain North","1970s","Wood","built-in electric unit","N/A",28.571176052175002,13637.792869999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13637.792869999999},"Cold/Very Cold",135.27767243503041,"Rural",0.16491199632825074,0.15155710583354598,5.1824703929429592E-3,0,0.13991583128854257,0.46156740384328221,0,0,{"$f":"T4623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16491199632825074},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.1824703929429592E-3}]
["Single Family Detached",14627,"South Atlantic","1950s","Shingle","central furnace","window/wall unit",46.036751992347007,30447.587299999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":30447.587299999999},"Mixed-Humid",174.02303295535671,"Metropolitan Area",1.9097011439501255,0.1391674875666179,0.1305549003374161,1.7588809993527497E-2,0.30645542288830946,2.4858789547424687,577.67499999999995,0,{"$f":"T4628*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7588809993527497E-2},{"$f":"U4628*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.927289953943653},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1305549003374161}]
["Single Family Detached",14632,"West South Central","1950s","Wood","central furnace","central AC",64.413130067823261,29093.554680000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29093.554680000001},"Hot-Humid",391.54524839362927,"Metropolitan Area",1.4547201814962782,0.42968302909802153,0.71197939030356894,5.477743203216804E-2,0.60683563281270503,3.2032182337105737,589.04200000000003,1293.761,{"$f":"T4633*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7137325635816564E-2},{"$f":"U4633*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7640106396351479E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4718575071320947},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.74961949669992045}]
["Single Family Attached",14636,"South Atlantic","2000s","Concrete","N/A","central AC",20.231427305200899,13327.68597,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13327.68597},"Hot-Humid",288.0878214235691,"Metropolitan Area",0,0.22072986975207737,0.50141724027574119,2.3811763533754828E-2,0.26080855380891205,0.98295566383673061,0,1786.6389999999999,{"$f":"T4637*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4637*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3811763533754828E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.525229003809496}]
["Single Family Detached",14639,"Middle Atlantic","1980s","Siding","wood-burning stove","central AC",28.909590079682559,17269.767070000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17269.767070000002},"Cold/Very Cold",249.27490921550918,"Metropolitan Area",8.8163939678358227E-2,0.1776816736671008,6.4562644256319468E-2,3.0250587488165502E-3,0.52011771959128683,0.85052597719306533,0,175.16499999999999,{"$f":"T4640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0250587488165502E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.8163939678358227E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7587703005136016E-2}]
["Single Family Detached",14646,"South Atlantic","1970s","Concrete","radiator","central AC",30.664398807545446,27208.872060000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27208.872060000002},"Hot-Humid",163.11365082465832,"Metropolitan Area",1.2511673310326281E-2,6.8260992420070624E-2,0.24525413378405739,1.133339310576798E-2,0.24295811311527432,0.5689849126297285,2.593,413.94,{"$f":"T4647*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.055260525158E-5},{"$f":"U4647*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1262840500516401E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2582225915577861E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25651697428457376}]
["Multi-Family (5+ units)",14650,"South Atlantic","2010s","Stone","built-in electric unit","N/A",17.143801436603802,16741.993589999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1331.6821524315405},"Mixed-Humid",171.38238072133703,"Metropolitan Area",6.2592270173323999E-2,0.24823303669912225,0,0,0.27393139414800305,0.5847567010204493,0,0,{"$f":"T4651*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4651*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.2592270173323999E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14651,"East South Central","1990s","Brick","heater burning gas/oil/kerosene","central AC",37.127426122039381,21585.71286,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21585.71286},"Mixed-Humid",286.86849006028223,"Rural",0.74930905972318773,0.63842174176146749,0.25605458273071352,1.2073817388250979E-2,0.80121596440907528,2.445001348624444,0,559.34299999999996,{"$f":"T4652*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4652*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2073817388250979E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.74930905972318773},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26812840011896449}]
["Multi-Family (5+ units)",14657,"Middle Atlantic","1980s","Brick","radiator","window/wall unit",31.407366756014486,28218.658360000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2244.5525081326405},"Cold/Very Cold",183.67908501058145,"Metropolitan Area",0.33422116810689634,0.24414769103742823,2.8406114907485482E-2,1.21010072645188E-3,0.35294913045511245,0.96083795208816813,42.883000000000003,0,{"$f":"T4658*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6253145206252026E-5},{"$f":"U4658*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33431742125210256},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8406114907485482E-2}]
["Single Family Attached",14662,"South Atlantic","1980s","Brick","heat pump","central AC",20.709263927295279,9587.6221889999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9587.6221889999997},"Mixed-Humid",81.821947034722669,"Metropolitan Area",0.10074674354963419,5.3033730798387538E-2,4.6916041656786034E-2,3.9163998498736646E-3,7.8479960809168969E-2,0.27917647681397673,174.30799999999999,234.17699999999999,{"$f":"T4663*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6711992485202117E-3},{"$f":"U4663*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2452006013534529E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1024179427981544},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.916124225813949E-2}]
["Multi-Family (5+ units)",14665,"Pacific","1980s","Brick","heat pump","central AC",13.415420030597472,17959.062959999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1428.4895935279328},"Hot-Dry/Mixed-Dry",95.699662048442846,"Metropolitan Area",1.4580923282759379E-2,0.12278810691350855,3.0205607341676238E-2,1.5658506994823999E-3,0.15751129066133901,0.32652722889110591,13.223000000000001,73.966999999999999,{"$f":"T4666*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8888917895219857E-5},{"$f":"U4666*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0566108976448062E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4599812200654599E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0311268431440719E-2}]
["Multi-Family (5+ units)",14669,"Middle Atlantic","1960s","Brick","central furnace","window/wall unit",34.776920899290637,35092.755700000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2791.3280574449332},"Mixed-Humid",96.996376756447333,"Metropolitan Area",0.76415869896088384,1.0149935634157905,7.1855645829274395E-2,7.3852002515536006E-3,0.4056954171107619,2.2635010961612312,210.44800000000001,0,{"$f":"T4670*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8742940703317126E-4},{"$f":"U4670*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.764746128367917},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.1855645829274395E-2}]
["Single Family Detached",14675,"West South Central","1960s","Siding","central furnace","N/A",160.36430303167694,33775.127009999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33775.127009999997},"Hot-Humid",535.77159730800349,"Metropolitan Area",0.79172390059572828,0.78307449586999145,0,3.6438329549865506E-2,1.8555381303261418,3.4303365267918617,1078.8510000000001,0,{"$f":"T4676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6438329549865506E-2},{"$f":"U4676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.82816223014559376},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14680,"East North Central","2000s","Brick","radiator","central AC",181.11254709077906,24310.409009999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24310.409009999999},"Cold/Very Cold",215.3539769686698,"Metropolitan Area",2.2258707001879765,0.70670239871065854,0.10433069716977006,0.16639013911763498,0.52630591468354748,3.5632097107519529,6572.8519999999999,271.54700000000003,{"$f":"T4681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.1597887204821965},{"$f":"U4681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6014186354384705E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3856594206701729},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11093211580520854}]
["Single Family Detached",14685,"Middle Atlantic","1980s","Siding","central furnace","central AC",96.129183222041803,19820.450150000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19820.450150000001},"Mixed-Humid",297.69971247777056,"Metropolitan Area",3.0268132299197945,0.34954507479498659,0.20382631451919556,7.2234480985566299E-2,2.0379115898676448,5.6180962091016218,3045.4830000000002,598.95899999999995,{"$f":"T4686*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0362843984172458E-2},{"$f":"U4686*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1871637001393849E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0871760739039669},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2156979515205894}]
["Single Family Detached",14687,"Pacific","2000s","Wood","central furnace","central AC",24.181335098938817,12225.144130000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12225.144130000001},"Hot-Dry/Mixed-Dry",143.52319214435877,"Metropolitan Area",0.20096531788295732,0.14700503538586529,0.1971124292338024,1.3375310140038661E-2,0.28399017149076472,0.82907295399338976,704.46900000000005,389.613,{"$f":"T4688*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6122350601169715E-3},{"$f":"U4688*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7630750799216902E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20957755294307429},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20187550431372409}]
["Single Family Detached",14694,"West North Central","Before 1950","Stucco","heat pump","central AC",33.059864395555287,18006.462090000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18006.462090000001},"Mixed-Humid",196.08862552328469,"Micropolitan Area",0.20867274767472929,9.3254638866853867E-2,0.10212242530401287,8.8105619006369987E-3,0.26500459583217545,0.66905440767777147,210.83500000000001,278.46499999999997,{"$f":"T4695*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.79639243474515E-3},{"$f":"U4695*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.01416946589185E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21246914010947443},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10713659476990472}]
["Single Family Detached",14698,"Mountain South","2000s","Stucco","N/A","central AC",29.682913933100874,10051.782569999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10051.782569999999},"Hot-Dry/Mixed-Dry",279.7939411289637,"Metropolitan Area",0,0.19709574465208024,0.44355304936878881,2.5167130506072357E-2,0.76601830518632952,1.4066670992071986,0,2503.748,{"$f":"T4699*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4699*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5167130506072357E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46872017987486114}]
["Single Family Detached",14703,"West North Central","1950s","Siding","central furnace","central AC",32.345805165321693,15402.764359999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15402.764359999999},"Cold/Very Cold",119.75789458506962,"Metropolitan Area",1.5474391527048021,0.16031936478577277,5.4580496453406721E-2,5.6691722558703202E-2,0.31596728677985836,2.07830630072384,3515.674,164.946,{"$f":"T4704*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4151098188578634E-2},{"$f":"U4704*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5406243701245599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6015902508933808},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7121120823531282E-2}]
["Single Family Detached",14708,"Mountain North","1990s","Stucco","central furnace","central AC",91.919307481398434,18472.529640000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18472.529640000001},"Cold/Very Cold",337.56748690053649,"Metropolitan Area",0.94834690145001876,0.6673713760422213,0.22328106790195978,6.4546971683502971E-2,1.0064426746622848,2.8454420200564847,2714.0520000000001,780.16200000000003,{"$f":"T4709*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0135406014501283E-2},{"$f":"U4709*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4411565669001682E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.99848230746452005},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23769263357096146}]
["Single Family Detached",14710,"East North Central","1950s","Siding","central furnace","window/wall unit",60.688329417762851,24168.988219999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24168.988219999999},"Cold/Very Cold",233.98582384272453,"Metropolitan Area",1.8649516138508717,0.71109322826112664,4.585797238975757E-2,4.7038144084540177E-2,0.70546354583504156,3.3273663603367978,1946.2190000000001,0,{"$f":"T4711*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7038144084540177E-2},{"$f":"U4711*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9119897579354119},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.585797238975757E-2}]
["Single Family Detached",14713,"Middle Atlantic","1970s","Siding","built-in electric unit","window/wall unit",21.749845780836399,15783.63264,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15783.63264},"Cold/Very Cold",187.0173747716637,"Metropolitan Area",0.13085774193563138,0.20584211880549888,1.5721097887480322E-2,0,0.28568231447342973,0.63810327310204029,0,0,{"$f":"T4714*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4714*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13085774193563138},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5721097887480322E-2}]
["Single Family Detached",14721,"Pacific","1950s","Stucco","central furnace","N/A",37.317368723780007,17340.78472,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17340.78472},"Marine",88.30232778735278,"Metropolitan Area",0.3796823773112048,0.23510171190345505,0,8.9509489159848802E-3,0.29233661924636339,0.90712070846102322,516.17899999999997,0,{"$f":"T4722*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9509489159848802E-3},{"$f":"U4722*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38863332622718966},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14723,"East North Central","2000s","Siding","central furnace","central AC",59.5373186840541,13568.213009999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13568.213009999999},"Cold/Very Cold",211.33065697127304,"Metropolitan Area",0.80849300270400382,0.37939085801845046,7.2037618356501923E-2,2.9380418496871858E-2,0.62414996914706988,1.8840714482260261,1833.154,332.23200000000003,{"$f":"T4724*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4872623952133539E-2},{"$f":"U4724*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5077945447383203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83336562665613734},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.6545412901240242E-2}]
["Single Family Detached",14728,"Pacific","2000s","Wood","heater burning gas/oil/kerosene","central AC",66.948845751802182,15789.822109999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15789.822109999999},"Hot-Dry/Mixed-Dry",47.065622786935052,"Metropolitan Area",3.2414878440152665E-2,9.1415933017306272E-2,2.6781180440059438E-2,2.7129124960075398E-3,0.21932852401895497,0.36994051591647331,0,171.81399999999999,{"$f":"T4729*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4729*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7129124960075398E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2414878440152665E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.9494092936066977E-2}]
["Single Family Detached",14733,"East North Central","Before 1950","Siding","central furnace","central AC",32.604385666324752,22641.93449,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22641.93449},"Cold/Very Cold",185.93158105554278,"Micropolitan Area",2.7095411000578524,0.34968151549906679,6.1729724887139049E-2,2.7909671116836458E-2,0.6815882973138413,3.8025406377578999,1122.431,110.223,{"$f":"T4734*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5414009171545189E-2},{"$f":"U4734*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4956619452912699E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.7349551092293978},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4225386832430315E-2}]
["Single Family Detached",14737,"Pacific","1960s","Siding","central furnace","N/A",23.80203228040898,9855.9139880000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9855.9139880000002},"Marine",307.05678195707071,"Metropolitan Area",0.60617205281902131,0.19573479525759047,0,1.273073625958978E-2,0.24577088544348144,1.0476777335200933,1291.6849999999999,0,{"$f":"T4738*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.273073625958978E-2},{"$f":"U4738*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.61890278907861107},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14740,"West South Central","1990s","Stucco","central furnace","central AC",98.658682429044589,18003.409199999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18003.409199999998},"Hot-Humid",569.50911667621699,"Metropolitan Area",1.5965637339095384,0.37044297261286557,0.87551218060626601,6.9513341333713188E-2,1.3285321283365492,4.1710510154652187,898.38199999999995,2962.739,{"$f":"T4741*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6173938763914396E-2},{"$f":"U4741*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3339402569798799E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6127376726734528},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.92885158317606487}]
["Multi-Family (5+ units)",14747,"West North Central","1990s","Siding","central furnace","central AC",5.7243259058777989,8793.1273519999995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":699.41794540586807},"Cold/Very Cold",35.515247924225037,"Metropolitan Area",9.2375603445147669E-2,0.14155697843701573,2.9708037363824027E-3,1.5206306854907679E-3,0.11669653878605488,0.35499960194712066,158.69999999999999,14.234,{"$f":"T4748*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1099762793591126E-4},{"$f":"U4748*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9555150349071265E-6},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.2486601073083582E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.9807592514173096E-3}]
["Single Family Attached",14751,"East North Central","1960s","Brick","central furnace","window/wall unit",10.322147863889253,16384.361690000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16384.361690000002},"Cold/Very Cold",114.68504305982597,"Metropolitan Area",0.7204136659210072,0.39554483725019757,5.695489211337406E-2,1.5230181715109642E-2,0.31912027706570317,1.4920336723502821,929.55600000000004,0,{"$f":"T4752*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5230181715109642E-2},{"$f":"U4752*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.73564384763611679},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.695489211337406E-2}]
["Single Family Detached",14757,"Pacific","Before 1950","Wood","central furnace","N/A",21.246158380556018,14754.27665,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14754.27665},"Marine",44.899226174372622,"Metropolitan Area",0.56379787025950823,0.14511996673130351,0,4.5120200966131492E-3,0.15854171088565863,0.86745954787647039,305.81099999999998,0,{"$f":"T4758*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5120200966131492E-3},{"$f":"U4758*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.56830989035612134},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14758,"Mountain South","1980s","Stucco","heat pump","central AC",30.51902444403305,14395.766250000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14395.766250000001},"Hot-Dry/Mixed-Dry",129.73278836578893,"Metropolitan Area",3.834725499178876E-2,8.713534176748125E-2,0.13220647048895626,8.4887514846375012E-3,0.18495920887296374,0.44264827612119001,48.883000000000003,540.78700000000003,{"$f":"T4759*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0370824159875017E-4},{"$f":"U4759*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7850432430387508E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.9050963233387512E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.139991513731995}]
["Single Family Attached",14766,"Pacific","2000s","Stucco","central furnace","central AC",17.042297427921575,6163.5795399999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6163.5795399999997},"Marine",39.160931292093082,"Metropolitan Area",5.9009296923460706E-2,6.3283992041211864E-2,1.6244329602953897E-2,3.6616963146004398E-3,0.12470192955879102,0.26323954812641748,447.22,146.86600000000001,{"$f":"T4767*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7564760418787998E-3},{"$f":"U4767*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0522027272164007E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.1765772965339506E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7149549875675536E-2}]
["Mobile Home",14769,"South Atlantic","2000s","Siding","portable electric heaters","window/wall unit",32.011973330097142,18546.913860000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18546.913860000001},"Hot-Humid",146.99165550082961,"Metropolitan Area",6.0904170264329408E-3,0.15251832049804678,0.20640096301942967,0,0.1365258545370707,0.50153555508098013,0,0,{"$f":"T4770*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4770*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.0904170264329408E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20640096301942967}]
["Single Family Detached",14774,"West North Central","1950s","Brick","central furnace","central AC",54.724866111740774,15320.51123,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15320.51123},"Mixed-Humid",181.77254952051052,"Metropolitan Area",0.92522171375495776,0.31862767352394211,0.22376239388528799,3.6617431326733167E-2,0.49731197567879676,1.9649237568429847,1695.4090000000001,694.68299999999999,{"$f":"T4775*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5974532623943072E-2},{"$f":"U4775*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0642898702790091E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95119624637890088},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23440529258807807}]
["Multi-Family (5+ units)",14776,"Pacific","1960s","Stucco","built-in furnace","N/A",16.065532043737228,15227.992459999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1211.2563338010495},"Marine",55.164133624621996,"Metropolitan Area",4.7237339206867221E-2,0.27319373285464316,0,0,0.1409826576937375,0.46141372975524791,0,0,{"$f":"T4777*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4777*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.7237339206867221E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14781,"East North Central","1990s","Brick","central furnace","N/A",38.327924611091127,18321.187669999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18321.187669999999},"Cold/Very Cold",81.703556280237194,"Metropolitan Area",0.99491610202251413,0.45758772973983658,0,1.2371766719108569E-2,0.26595796351060297,1.7184617952729535,675.27099999999996,0,{"$f":"T4782*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2371766719108569E-2},{"$f":"U4782*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0072878687416227},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14785,"East North Central","1990s","Siding","central furnace","central AC",53.138837560526014,12749.241260000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12749.241260000001},"Cold/Very Cold",157.84764204941678,"Metropolitan Area",1.3512841893670604,0.3042625805545715,8.1717638774026075E-2,5.0190422539409883E-2,0.5650975353483767,2.3023619440440344,3546.5169999999998,390.221,{"$f":"T4786*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5215400865691424E-2},{"$f":"U4786*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.97502167371846E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3964995902327519},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.6692660447744541E-2}]
["Multi-Family (5+ units)",14792,"Pacific","1980s","Stucco","heat pump","central AC",6.5079534414306659,10956.15057,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":871.46791061587373},"Hot-Dry/Mixed-Dry",42.210060125891701,"Metropolitan Area",3.1977453173022245E-3,6.6302876246145059E-2,1.2716495521319432E-2,5.9055842802413993E-4,0.14113088663691509,0.22389158828638792,4.6340000000000003,49.268000000000001,{"$f":"T4793*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0383822977939593E-6},{"$f":"U4793*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2935481020222868E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2017836996000187E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2759431002339654E-2}]
["Multi-Family (5+ units)",14795,"Middle Atlantic","1980s","Brick","built-in electric unit","window/wall unit",31.110907937874604,23730.669669999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1887.5714588532153},"Mixed-Humid",195.06610469056389,"Metropolitan Area",0.23186788824900237,0.23372808798309433,5.2971244877328946E-2,0,0.14695940978572433,0.66552663089514996,0,0,{"$f":"T4796*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4796*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23186788824900237},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2971244877328946E-2}]
["Multi-Family (5+ units)",14799,"New England","Before 1950","Brick","radiator","N/A",18.131002061332719,28463.111560000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2263.9966658307549},"Cold/Very Cold",37.402207908497338,"Rural",0.58220215684836529,0.33997903072088648,0,3.0569951077671202E-3,0.12455930106307889,1.0495543259701943,107.402,0,{"$f":"T4800*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4315776990355473E-4},{"$f":"U4800*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58244531461826887},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14804,"East South Central","1970s","Brick","central furnace","central AC",27.014442699994081,17428.672709999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17428.672709999999},"Mixed-Humid",246.4697188505925,"Metropolitan Area",0.40054946852850726,0.25842981435766432,0.28736625622727768,2.1119211585015209E-2,0.54444662074302497,1.4907921598564742,524.52599999999995,687.22500000000002,{"$f":"T4805*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1417919818854599E-3},{"$f":"U4805*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1977419603129751E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.40969126051039273},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.29934367583040744}]
["Single Family Detached",14809,"Mountain North","2010s","Wood","central furnace","N/A",116.99038633788395,44432.353340000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":44432.353340000001},"Cold/Very Cold",137.85275363283762,"Rural",3.3112403546451281,0.55585549400110768,0,7.4943517190337927E-2,0.3954100439286008,4.2625058925748371,1686.6880000000001,0,{"$f":"T4810*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4943517190337927E-2},{"$f":"U4810*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.386183871835466},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",14811,"West South Central","2000s","Concrete","central furnace","central AC",18.557271894088355,29409.305700000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9803.1018999999997},"Hot-Humid",284.22614666973249,"Metropolitan Area",8.7085385179758806E-2,0.16981294845640107,0.29052881580189227,1.3336120218556201E-2,0.41346169385447612,0.969779590104899,45.866,407.6,{"$f":"T4812*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4962907174539999E-4},{"$f":"U4812*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9957443344399999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.7535014251504201E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.29452456013633227}]
["Multi-Family (5+ units)",14819,"South Atlantic","1960s","Concrete","built-in electric unit","window/wall unit",28.940144480076771,42559.036,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3385.2066876756835},"Hot-Humid",352.04149378813793,"Metropolitan Area",8.4099208678159992E-3,0.170015815870628,0.51635346253504,0,0.50638634909902003,1.2011655483725039,0,0,{"$f":"T4820*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4820*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.4099208678159992E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.51635346253504}]
["Single Family Detached",14822,"South Atlantic","1980s","Stucco","central furnace","central AC",25.854242308964089,11058.273010000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11058.273010000001},"Hot-Humid",163.09418914591009,"Metropolitan Area",1.130366714636491E-2,6.4298980854752594E-2,0.18323705452601033,1.0766124495348811E-2,0.29763766444098577,0.55647736696811367,18.696000000000002,954.88499999999999,{"$f":"T4823*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0674547219496001E-4},{"$f":"U4823*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0559379023153851E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1510412618559869E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19379643354916418}]
["Single Family Detached",14824,"Pacific","1950s","Siding","central furnace","N/A",10.174859670130481,9464.9857400000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9464.9857400000001},"Marine",24.382125074869677,"Metropolitan Area",0.34607478552180915,9.8218582948338296E-2,0,3.1566106042329603E-3,0.10727675413624733,0.55157012260639482,333.50400000000002,0,{"$f":"T4825*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1566106042329603E-3},{"$f":"U4825*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34923139612604209},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",14829,"West South Central","1980s","Brick","central furnace","central AC",15.70864668624016,19489.63609,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6496.5453633333336},"Mixed-Humid",119.91353313993731,"Metropolitan Area",0.27004745566396232,0.31507062640910538,7.676569417620227E-2,8.193326074419461E-3,0.32525922346787478,0.99260521710009098,255.185,165.209,{"$f":"T4830*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6578209285422168E-3},{"$f":"U4830*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0732877629309366E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27170527659250454},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.7838981939133203E-2}]
["Multi-Family (5+ units)",14834,"West South Central","1990s","Brick","central furnace","central AC",33.31009354829952,37511.366609999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2983.7078337964781},"Hot-Humid",232.15784793966859,"Metropolitan Area",0.30946631328840352,0.19516905218753389,0.13649405077784058,1.1046084659746529E-2,0.335999701374321,0.98729658089090389,132.703,161.77000000000001,{"$f":"T4835*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9594698066829407E-4},{"$f":"U4835*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8267441627325631E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.30986226026907182},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13697672519411383}]
["Single Family Detached",14840,"Middle Atlantic","1980s","Siding","central furnace","central AC",49.224825240378465,20613.410899999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20613.410899999999},"Cold/Very Cold",303.99060862878571,"Metropolitan Area",0.76882302435475247,0.33657552581426919,8.1682186697067491E-2,2.6256991763023801E-2,1.041299417448956,2.2283801543150452,1079.8530000000001,193.929,{"$f":"T4841*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2259453600597702E-2},{"$f":"U4841*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9975381624260996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.79108247795535014},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5679724859493586E-2}]
["Single Family Detached",14845,"East South Central","1970s","Brick","heat pump","both central and individual units",42.697459704708855,18491.75388,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18491.75388},"Mixed-Humid",489.95982222539141,"Metropolitan Area",0.48887661231493235,0.59681527268997348,0.17153418740461165,1.482186191322132E-2,0.41451685043427516,1.6717429228437923,433.31400000000002,368.22500000000002,{"$f":"T4846*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0127358407583206E-3},{"$f":"U4846*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.8091260724630004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49688934815569069},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17834331347707466}]
["Single Family Detached",14848,"West South Central","1970s","Brick","central furnace","central AC",63.015197358631013,34680.901129999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34680.901129999998},"Hot-Humid",628.46280561572712,"Metropolitan Area",0.60615754123359478,0.35928116504977736,0.37981260532774869,3.0511147025337842E-2,0.79906374184521389,2.1443150534563347,331.221,548.54700000000003,{"$f":"T4849*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.148704275317973E-2},{"$f":"U4849*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9024104272158109E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.61764458398677446},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.3988367095999068}]
["Single Family Detached",14852,"Pacific","1990s","Wood","central furnace","N/A",47.492126626450343,16746.165949999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16746.165949999999},null,101.93273988940037,"Metropolitan Area",1.4915984004329219,0.33825161948256249,0,2.6502934378950647E-2,0.36912774811469173,2.1989777680301761,1582.627,0,{"$f":"T4853*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6502934378950647E-2},{"$f":"U4853*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5181013348118726},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14857,"West South Central","2000s","Wood","central furnace","central AC",29.914368530110501,25329.693930000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25329.693930000001},"Hot-Humid",257.47446439060286,"Metropolitan Area",0.27819721892880472,1.3790692335407766,0.22920285316959932,1.50075903565857E-2,0.48981255109627198,2.3762818567354524,179.54499999999999,412.94499999999999,{"$f":"T4858*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5478198966618496E-3},{"$f":"U4858*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0459770459923851E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28274503882546659},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23966262362952317}]
["Single Family Detached",14863,"Pacific","1970s","Stucco","central furnace","central AC",16.122193648758909,10171.73101,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10171.73101},"Hot-Dry/Mixed-Dry",92.9211327776232,"Metropolitan Area",0.17097732839652971,0.12028794112226708,0.11759730466377089,9.4018733767771388E-3,0.26407612064002567,0.67293869482259339,384.17399999999998,540.14,{"$f":"T4864*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.90771458903574E-3},{"$f":"U4864*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4941587877413997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17488504298556545},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12309146345151228}]
["Single Family Detached",14867,"West North Central","1950s","Siding","built-in furnace","window/wall unit",35.971429757245879,19808.05603,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19808.05603},"Mixed-Humid",326.88593091442033,"Metropolitan Area",1.5303538889590709,0.38388333476647685,0.150650170136165,0,0.54022550826731086,2.6051129021290236,0,0,{"$f":"T4868*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4868*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5303538889590709},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.150650170136165}]
["Single Family Detached",14870,"Pacific","1960s","Wood","built-in electric unit","window/wall unit",18.827688443121904,16961.88148,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16961.88148},"Marine",186.23565769011796,"Metropolitan Area",0.11030706738282484,0.13394461959502696,1.211651649266024E-2,0,0.37906787589084706,0.63543607936135915,0,0,{"$f":"T4871*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4871*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11030706738282484},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.211651649266024E-2}]
["Single Family Detached",14875,"Pacific","Before 1950","Siding","central furnace","N/A",42.752546179656036,23400.40842,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23400.40842},"Marine",125.185843525531,"Metropolitan Area",0.72794870368292586,0.347492999583497,0,1.6320123443952179E-2,0.56061294468130829,1.6360546479477309,697.42899999999997,0,{"$f":"T4876*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6320123443952179E-2},{"$f":"U4876*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.74426882712687803},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14881,"South Atlantic","2000s","Siding","heat pump","central AC",22.67564877900379,13894.39263,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13894.39263},"Mixed-Humid",181.49258596169943,"Metropolitan Area",0.25158037632706959,0.10190890904847705,3.7830109975382074E-2,5.8024095174290394E-3,0.22793330109418319,0.61925269644511183,296.947,120.661,{"$f":"T4882*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1258982083006105E-3},{"$f":"U4882*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.67651130912843E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2557062745353702},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9506621284510504E-2}]
["Single Family Detached",14882,"West North Central","1960s","Siding","central furnace","central AC",33.974846164660761,17881.49798,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17881.49798},"Mixed-Humid",303.43149687634303,"Metropolitan Area",0.71777005236044045,0.24983308353287403,0.18668149779885151,3.1501960161851854E-2,0.91708726036588761,2.0713718940580534,1285.1969999999999,476.51,{"$f":"T4883*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2981247559402059E-2},{"$f":"U4883*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.5207126024497981E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.74075129991984245},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19520221040130131}]
["Single Family Detached",14886,"Pacific","2000s","Stucco","central furnace","central AC",29.925458797913198,10537.133379999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10537.133379999999},"Hot-Dry/Mixed-Dry",159.97520152788297,"Metropolitan Area",2.6255912636748379E-2,7.3940276697798693E-2,0.17778672924071198,1.420493037831054E-2,0.51224969429757561,0.79023261287283464,418.28800000000001,929.79499999999996,{"$f":"T4887*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.40755644725344E-3},{"$f":"U4887*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7973739310570993E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0663469084001818E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18758410317176907}]
["Single Family Detached",14893,"Pacific","1950s","Stucco","central furnace","central AC",22.997758701979073,13066.90835,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13066.90835},"Hot-Dry/Mixed-Dry",99.187386312291082,"Metropolitan Area",0.14540450537721153,5.5722602369190098E-2,6.226289053725715E-2,4.0880084111141997E-3,1.0478786320531386,1.3112686303367973,60.454000000000001,252.398,{"$f":"T4894*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8994687739090009E-4},{"$f":"U4894*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2980615337233001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14619445225460242},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5560952070980449E-2}]
["Single Family Detached",14896,"South Atlantic","1950s","Brick","central furnace","central AC",123.01543580012742,31381.488720000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31381.488720000001},"Mixed-Humid",1045.6555249548446,"Metropolitan Area",1.939078788816333,0.45412224504136056,0.50640647267542183,6.9170889147691678E-2,3.1853375931661292,6.0849450996992447,1299.979,904.21500000000003,{"$f":"T4897*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0795276324736889E-2},{"$f":"U4897*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8375612822954803E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9798740651410698},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.53478208549837658}]
["Single Family Detached",14900,"East North Central","Before 1950","Siding","central furnace","window/wall unit",105.26770940287614,32988.940580000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32988.940580000002},"Cold/Very Cold",764.55264364921027,"Metropolitan Area",2.8988230563197717,1.6030871429798768,0.23938820599163962,8.5870113362918263E-2,0.68030815921234034,5.4216065645036275,2602.9969999999998,0,{"$f":"T4901*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.5870113362918263E-2},{"$f":"U4901*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9846931696826897},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23938820599163962}]
["Single Family Detached",14905,"South Atlantic","Before 1950","Siding","central furnace","central AC",30.6353123660157,16365.01729,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16365.01729},"Mixed-Humid",253.20671538130938,"Metropolitan Area",0.82536481934104933,0.23698060436521054,0.28942642625537263,2.5831263351296759E-2,0.32871321956773231,1.6804850695293647,734.21699999999998,844.22699999999998,{"$f":"T4906*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2015473899611929E-2},{"$f":"U4906*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3815789451684829E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83738029324066121},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30324221570705745}]
["Single Family Detached",14910,"Middle Atlantic","Before 1950","Siding","other","window/wall unit",43.213507166500527,18887.022359999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18887.022359999999},"Cold/Very Cold",314.55361175190927,"Metropolitan Area",0.62301836847504055,0.29717260273120394,3.0375865852431475E-2,0,0.49702768851898099,1.447594525577657,0,0,{"$f":"T4911*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4911*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62301836847504055},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0375865852431475E-2}]
["Single Family Detached",14916,"West South Central","Before 1950","Wood","central furnace","central AC",29.963160460032515,29375.647509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29375.647509999999},"Hot-Humid",263.47018251571728,"Metropolitan Area",0.61047404319277387,0.20730785143918881,0.57739180585560945,3.5048936937958783E-2,0.34042016117999507,1.7355938616675672,333.738,859.39099999999996,{"$f":"T4917*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8037698486923806E-3},{"$f":"U4917*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5245167089266409E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62027781304146623},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.60263697294487584}]
["Single Family Detached",14920,"West North Central","1960s","Siding","central furnace","central AC",44.400352567382996,22200.17628,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22200.17628},"Cold/Very Cold",428.05565163744342,"Rural",1.2767431269500586,0.53783820949219507,6.7170318564402476E-2,3.0999926554218959E-2,0.72618361704466394,2.60793527205132,1251.0070000000001,145.375,{"$f":"T4921*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7772575927513962E-2},{"$f":"U4921*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2273506267050003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3045157028775727},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.0397669191107473E-2}]
["Single Family Detached",14923,"West South Central","2010s","Siding","built-in electric unit","N/A",17.417581327325344,15278.580110000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15278.580110000001},"Hot-Humid",251.97943096915051,"Metropolitan Area",0.39580897421655492,0.33459436517671293,0,0,0.12935046070525444,0.85975380009852231,0,0,{"$f":"T4924*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4924*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39580897421655492},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14930,"East South Central","Before 1950","Stucco","central furnace","central AC",23.581041917113833,20068.971839999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20068.971839999998},"Mixed-Humid",208.51872470486302,"Metropolitan Area",1.0985875599047039,0.23955723595561246,0.17076702186936285,2.0718524182573438E-2,0.28786260896739363,1.7967744266970727,661.66899999999998,370.697,{"$f":"T4931*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.327901652840096E-2},{"$f":"U4931*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4395076541724789E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1118665764331048},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17820652952353533}]
["Single Family Detached",14934,"Pacific","1980s","Stucco","central furnace","central AC",24.299975834691327,15779.205089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15779.205089999999},"Hot-Dry/Mixed-Dry",178.91461551846336,"Metropolitan Area",0.18382434676940565,0.65747471049545969,0.11381278696612505,8.8210332422576105E-3,0.62599806815623604,1.5811099123872263,224.47300000000001,334.55599999999998,{"$f":"T4935*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5420055041675701E-3},{"$f":"U4935*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2790277380900391E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18736635227357323},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11909181470421509}]
["Single Family Detached",14939,"East North Central","Before 1950","Brick","central furnace","central AC",34.155704778641436,18216.37588,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18216.37588},"Cold/Very Cold",117.68957419254157,"Metropolitan Area",1.9792441783709376,0.30924635217325402,7.8511669224005987E-2,3.2576290337076361E-2,0.32514680732212636,2.692149007090324,1593.4839999999999,194.81299999999999,{"$f":"T4940*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9027503502765915E-2},{"$f":"U4940*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5487868343104397E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0082716818737034},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.2060456058316425E-2}]
["Multi-Family (5+ units)",14941,"Pacific","1990s","Brick","central furnace","N/A",17.419652191343552,18650.591209999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1483.494741121423},"Hot-Dry/Mixed-Dry",94.614449214867065,"Metropolitan Area",3.3996877865609988E-2,0.11827733085424387,0,1.6533189589928701E-3,0.40613518093600393,0.55993120125653451,88.647000000000006,0,{"$f":"T4942*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3150735831619079E-4},{"$f":"U4942*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.412838522392618E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",14946,"Pacific","2000s","Stucco","central furnace","central AC",59.668844609154895,17929.340329999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17929.340329999999},"Hot-Dry/Mixed-Dry",307.75820247801096,"Metropolitan Area",0.11075308522779534,0.89687628955171284,0.13941914207431089,1.0547866774819659E-2,1.0270898987030304,2.1741384155568495,124.94,463.36200000000002,{"$f":"T4947*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2400917808302E-3},{"$f":"U4947*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3077749939894606E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11299317700862554},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14772691706830035}]
["Single Family Detached",14948,"East North Central","1990s","Siding","central furnace","window/wall unit",22.737306767368882,12688.229219999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12688.229219999999},"Cold/Very Cold",360.5545328058335,"Metropolitan Area",0.41453057703211321,0.33833834422455733,1.0848664371225961E-2,8.0075668372004399E-3,0.4664944711970993,1.2302120568249957,631.10199999999998,0,{"$f":"T4949*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0075668372004399E-3},{"$f":"U4949*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42253814386931365},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0848664371225961E-2}]
["Multi-Family (2-4 units)",14953,"Pacific","1980s","Concrete","central furnace","central AC",31.67961701599021,26224.84852,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8741.6161733333338},"Hot-Dry/Mixed-Dry",142.8664447669517,"Metropolitan Area",0.1126497896538229,0.66172239778332953,5.8829083758045818E-2,4.0088352441612803E-3,0.42553800278190196,1.261411830806541,48.118000000000002,104.746,{"$f":"T4954*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2062908702845335E-4},{"$f":"U4954*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1564932769197332E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11307041874085136},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9744733085737793E-2}]
["Single Family Detached",14958,"Middle Atlantic","1950s","Siding","central furnace","central AC",47.554836486195569,21784.166969999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21784.166969999998},"Mixed-Humid",250.70905438688911,"Metropolitan Area",2.1835176993218623,0.68149799255367616,0.15913458141336731,3.5614760305917238E-2,0.78273568241835834,3.8068859557072638,1278.855,356.03699999999998,{"$f":"T4959*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7858790850419351E-2},{"$f":"U4959*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7559694554978891E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2113764901722819},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1668905508688652}]
["Single Family Detached",14964,"Pacific","1980s","Siding","central furnace","window/wall unit",20.687976759102082,14406.66905,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14406.66905},"Marine",184.50612411278539,"Metropolitan Area",0.30438885788918651,0.288054129913556,6.1993625722436005E-3,1.02031775946053E-2,0.61313237641210927,1.2117747267870953,708.226,0,{"$f":"T4965*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.02031775946053E-2},{"$f":"U4965*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31459203548379183},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1993625722436005E-3}]
["Single Family Detached",14968,"East North Central","1980s","Brick","built-in electric unit","window/wall unit",13.591928411200513,21237.388139999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21237.388139999999},"Cold/Very Cold",184.99544765244536,"Metropolitan Area",0.39258163596054418,0.1291161628913968,1.9165128754851359E-2,0,9.034153427225268E-2,0.631204461879045,0,0,{"$f":"T4969*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4969*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39258163596054418},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9165128754851359E-2}]
["Single Family Detached",14971,"South Atlantic","1970s","Concrete","heat pump","central AC",31.908272776996014,25324.026010000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25324.026010000001},"Hot-Humid",295.71602105107979,"Metropolitan Area",3.5487494636775377E-2,0.16893561519972164,0.38271514227808134,1.8533717647756631E-2,0.4218447889836669,1.0089830410982452,23.268999999999998,708.59400000000005,{"$f":"T4972*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8926476122669001E-4},{"$f":"U4972*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7944452886529943E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.6076759398002069E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4006595951646113}]
["Single Family Detached",14976,"Mountain South","1980s","Wood","central furnace","N/A",9.9738946123042656,10261.20845,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10261.20845},"Cold/Very Cold",18.969567700760596,"Metropolitan Area",0.23331542769326369,9.3700266006008809E-2,1.7093746969725453E-2,7.940123098609999E-4,7.2326199588284193E-2,0.41643564025728208,77.38,0,{"$f":"T4977*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.940123098609999E-4},{"$f":"U4977*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2341094400031247},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7093746969725453E-2}]
["Single Family Detached",14982,"Pacific","1990s","Wood","wood-burning stove","central AC",54.556466355472146,12547.485360000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12547.485360000001},"Marine",512.43970371766454,"Micropolitan Area",0.37983316048295618,0.4175229331302488,2.27709254816208E-2,1.46525769788472E-3,1.39210864377767,2.2122356628724957,0,116.777,{"$f":"T4983*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4983*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.46525769788472E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37983316048295618},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.423618317950552E-2}]
["Single Family Detached",14987,"West North Central","1970s","Siding","central furnace","central AC",77.218620427685252,24702.053879999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24702.053879999999},"Cold/Very Cold",142.27723489821267,"Metropolitan Area",1.5827248668357956,0.23823189385825033,5.5338529184131194E-2,2.493788438839236E-2,0.40831516862306333,2.2846104585012408,882.36400000000003,127.18300000000001,{"$f":"T4988*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1796203069772323E-2},{"$f":"U4988*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.14168131862004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6045210699055679},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8480210502751234E-2}]
["Single Family Detached",14992,"South Atlantic","1990s","Siding","central furnace","central AC",16.839719029851906,15946.70363,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15946.70363},"Hot-Humid",259.35203700025073,"Rural",0.23765072621760758,0.13503338537118859,0.16509322470110757,1.0937206151671802E-2,0.34713183129374753,0.88490916758365123,226.733,459.12700000000001,{"$f":"T4993*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6156439541407902E-3},{"$f":"U4993*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.32156219753101E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24126637017174837},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17241478689863859}]
["Multi-Family (2-4 units)",14994,"South Atlantic","1990s","Brick","built-in electric unit","central AC",77.040562078234231,44947.819179999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14982.606393333333},"Mixed-Humid",231.42360073614933,"Metropolitan Area",0.17901673589989026,0.22312587372181064,9.1965335607175056E-2,4.58665526040392E-3,0.29245163706009447,0.78961735246257303,0,102.044,{"$f":"T4995*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U4995*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5288850868013066E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17901673589989026},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.3494220693976365E-2}]
["Single Family Detached",14997,"South Atlantic","Before 1950","Siding","central furnace","central AC",112.41770703230121,35688.160960000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35688.160960000001},"Cold/Very Cold",354.90395018660854,"Micropolitan Area",3.4782690575926338,0.35575404215446882,0.19550409969451712,5.0562736631001283E-2,0.69347878227355431,4.7230059817151746,1111.23,305.56299999999999,{"$f":"T4998*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.96577551035808E-2},{"$f":"U4998*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.090498152742048E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.5179268126962144},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2064090812219376}]
["Multi-Family (5+ units)",15005,"South Atlantic","2000s","Brick","built-in electric unit","central AC",36.991078830649322,27854.728040000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2215.604969163197},"Mixed-Humid",227.76811114323755,"Metropolitan Area",0.13868362135065676,0.28749538894502569,4.1788960080162939E-2,1.9847329370341199E-3,0.43060537727379083,0.90040021208580256,0,71.253,{"$f":"T5006*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5006*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5786850086778526E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13868362135065676},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.1946828581030722E-2}]
["Single Family Detached",15006,"East North Central","1950s","Brick","radiator","window/wall unit",23.183696260440875,20336.575669999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20336.575669999998},"Cold/Very Cold",113.23236537837296,"Metropolitan Area",1.6785566942670256,0.66260034986326866,4.7801771882756444E-2,5.4993761195300597E-3,0.46786517150213336,2.8568239875151837,270.41800000000001,0,{"$f":"T5007*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.4993761195300597E-3},{"$f":"U5007*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6840560703865557},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7801771882756444E-2}]
["Multi-Family (5+ units)",15012,"Mountain South","1980s","Stucco","central furnace","central AC",11.411608752812313,12024.87751,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":956.47598233505391},"Hot-Dry/Mixed-Dry",91.069700320872116,"Metropolitan Area",3.0902675323823191E-2,6.4439226247403267E-2,5.8204284029153272E-2,3.6808150058110002E-3,0.3278551949166299,0.48478941822462784,93.186999999999998,212.91300000000001,{"$f":"T5013*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9131127365856669E-5},{"$f":"U5013*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0364617082690333E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0991806451189048E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8407930199980175E-2}]
["Single Family Detached",15017,"Mountain North","2000s","Brick","central furnace","central AC",48.249029352782095,11061.21718,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11061.21718},"Cold/Very Cold",414.1052142517554,"Metropolitan Area",1.2674967909064414,0.68586239658515624,4.5794158104316696E-2,1.9341699667033901E-2,2.1676158712880063,4.166769216883921,1491.028,257.577,{"$f":"T5018*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6492584529461039E-2},{"$f":"U5018*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8491151375728599E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2839893754359024},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.8643273241889558E-2}]
["Mobile Home",15021,"South Atlantic","1970s","Siding","portable electric heaters","window/wall unit",32.550962144235498,32813.469899999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32813.469899999996},"Hot-Humid",147.04260567342257,"Metropolitan Area",4.1846493147951594E-2,9.2567586111177588E-2,0.10428540746634719,0,0.2630098709164097,0.50170935764188607,0,0,{"$f":"T5022*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5022*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.1846493147951594E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10428540746634719}]
["Single Family Detached",15024,"Pacific","1990s","Wood","central furnace","central AC",82.314849322698961,23667.29423,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23667.29423},"Hot-Dry/Mixed-Dry",120.37701791040807,"Metropolitan Area",0.54873894972684578,0.73273585559937116,0.1736306073324913,1.03241470890106E-2,0.27854623161454489,1.7336516442732532,259.93400000000003,176.286,{"$f":"T5025*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1519344583808198E-3},{"$f":"U5025*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.17221263062978E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55489088418522658},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.17780281996312108}]
["Single Family Detached",15030,"Pacific","1980s","Stucco","central furnace","central AC",27.924064719863992,17441.639429999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17441.639429999999},"Hot-Dry/Mixed-Dry",128.88356431863082,"Metropolitan Area",0.25459686655774894,0.77189475278455977,0.22916509001338997,9.2309179017697803E-3,0.31222132233871769,1.5678780316944165,194.83699999999999,334.40899999999999,{"$f":"T5031*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3982767016229099E-3},{"$f":"U5031*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.83264120014687E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.25799514325937184},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23499773121353684}]
["Single Family Attached",15035,"South Atlantic","1990s","Siding","central furnace","central AC",26.327091375554868,16833.178629999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16833.178629999999},"Mixed-Humid",185.55633632070666,"Metropolitan Area",0.27063472243032255,0.20221194176177962,0.10935926994658948,1.0910374229498608E-2,0.31567803596508742,0.89788397010377907,348.654,299.49299999999999,{"$f":"T5036*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8689550620640192E-3},{"$f":"U5036*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0414191674345897E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27650367749238658},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11440068911402407}]
["Single Family Detached",15040,"South Atlantic","1970s","Concrete","heat pump","central AC",69.758179647461517,24545.45378,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24545.45378},"Hot-Humid",725.29172379416184,"Metropolitan Area",0.16010727046157042,0.5406396622309606,1.3520849960167958,7.9902545690042404E-2,0.42186342593501996,2.4746953546443469,177.50200000000001,3077.7869999999998,{"$f":"T5041*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3568671368575595E-3},{"$f":"U5041*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.554567855318485E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16446413759842798},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4276306745699807}]
["Single Family Detached",15042,"Middle Atlantic","1970s","Brick","central furnace","N/A",102.51925287749846,45767.523609999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":45767.523609999997},"Cold/Very Cold",328.38198187323724,"Metropolitan Area",3.6035547138459942,2.0006104043558501,0,2.9330987088417089E-2,4.7797626789640226,10.383927797165867,640.86900000000003,0,{"$f":"T5043*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9330987088417089E-2},{"$f":"U5043*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.6328857009344113},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",15047,"East South Central","1970s","Siding","heat pump","central AC",16.800523214941855,6661.5873179999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6661.5873179999999},"Mixed-Humid",74.074965742301174,"Metropolitan Area",7.6816955026085612E-2,3.7199236205936521E-2,4.3371836368446048E-2,3.092555311746366E-3,9.5355759498427839E-2,0.252743787098896,187.65899999999999,276.57799999999997,{"$f":"T5048*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2501068145085619E-3},{"$f":"U5048*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8424484972378039E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.8067061840594171E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.5214284865683851E-2}]
["Single Family Detached",15054,"Pacific","1950s","Stucco","N/A","window/wall unit",14.377283267454931,11613.31443,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11613.31443},"Marine",51.637836145430292,"Metropolitan Area",0,0.18311979874385315,5.3705540315246393E-3,0,0.20976800036779186,0.39825835314316965,0,0,{"$f":"T5055*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5055*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.3705540315246393E-3}]
["Single Family Detached",15058,"West South Central","1970s","Brick","central furnace","central AC",35.830565321509674,25056.339390000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25056.339390000001},"Hot-Humid",541.91853328963396,"Metropolitan Area",0.33675802826079992,0.25003277580073796,0.59568239688283076,3.6943417585367462E-2,1.3898697087376526,2.5723429096820212,377.70699999999999,1096.7070000000001,{"$f":"T5059*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.4639547819787301E-3},{"$f":"U5059*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7479462803388734E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.34622198304277868},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.62316185968621951}]
["Single Family Detached",15059,"New England","Before 1950","Wood","central furnace","window/wall unit",16.08078564392731,9231.2202319999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9231.2202319999997},"Cold/Very Cold",96.646638697651198,"Metropolitan Area",1.0978072007098663,0.11453581115532609,1.2016076289149297E-2,7.753486497261439E-3,0.22331214400204444,1.447671232156386,839.92,0,{"$f":"T5060*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.753486497261439E-3},{"$f":"U5060*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1055606872071277},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2016076289149297E-2}]
["Multi-Family (2-4 units)",15065,"East North Central","Before 1950","Wood","central furnace","central AC",27.221028664708424,26351.431430000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8783.8104766666675},"Cold/Very Cold",99.386584446561784,"Metropolitan Area",1.1628069268656043,0.27870420167635201,7.3566951263311087E-2,2.0804639574005006E-2,0.24581416321419453,1.7747620027354654,666.69899999999996,122.80800000000001,{"$f":"T5066*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8561576609831899E-3},{"$f":"U5066*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0787221970184801E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1686630845265875},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4645673460329562E-2}]
["Single Family Detached",15069,"East North Central","1990s","Siding","radiator","window/wall unit",38.179362889707797,13548.389950000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13548.389950000001},"Cold/Very Cold",148.14091381956922,"Metropolitan Area",0.73552655038222736,0.35096589326656902,2.00796893899764E-2,2.2854101587157501E-3,0.48309167528517222,1.5896638083239449,168.685,0,{"$f":"T5070*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2854101587157501E-3},{"$f":"U5070*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.73781196054094311},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.00796893899764E-2}]
["Multi-Family (2-4 units)",15076,"East South Central","1960s","Brick","built-in electric unit","window/wall unit",11.323251854995059,13609.67771,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4536.5592366666669},"Mixed-Humid",120.46927413693095,"Metropolitan Area",0.21396756946621662,8.1255451164305076E-2,5.2896625478035322E-2,0,6.2921527688898984E-2,0.41104117379745603,0,0,{"$f":"T5077*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5077*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21396756946621662},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2896625478035322E-2}]
["Single Family Detached",15079,"East North Central","Before 1950","Siding","central furnace","central AC",49.813748559927078,22238.280610000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22238.280610000002},"Cold/Very Cold",195.03632569369765,"Metropolitan Area",0.98023625634817524,0.41425711517566649,7.1596433521542935E-2,4.0090416182167264E-2,0.55685155008753751,2.0229413551329221,1664.5139999999999,138.25200000000001,{"$f":"T5080*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7015929411273539E-2},{"$f":"U5080*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0744867708937204E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0172521857594488},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.467092029243666E-2}]
["Single Family Detached",15083,"Middle Atlantic","Before 1950","Siding","wood-burning stove","N/A",99.545551082721047,39643.787770000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":39643.787770000003},"Cold/Very Cold",225.4539038801378,"Micropolitan Area",0.3422033524164026,1.0455462692716382,0,0,0.42704537941706966,1.8147950011051104,0,0,{"$f":"T5084*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5084*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3422033524164026},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15088,"East North Central","Before 1950","Siding","central furnace","window/wall unit",133.03928554802036,57742.745459999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":57742.745459999998},"Cold/Very Cold",142.0719254781381,"Metropolitan Area",6.9953852713659126,1.1315205460749049,2.9594196417668278E-2,6.3589775865279608E-3,0.48260820776562502,8.6391082216241113,110.126,0,{"$f":"T5089*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3589775865279608E-3},{"$f":"U5089*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.0017442489524404},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.9594196417668278E-2}]
["Single Family Detached",15093,"Pacific","1970s","Stucco","central furnace","central AC",16.245509072515109,10096.649520000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10096.649520000001},"Hot-Dry/Mixed-Dry",96.329417040973368,"Metropolitan Area",0.2406997729008569,0.13114057461010847,6.2886860375525766E-2,7.9356030433372794E-3,0.28622274862132091,0.72094995650781202,488.988,296.976,{"$f":"T5094*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9371404554857598E-3},{"$f":"U5094*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.99846258785152E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24563691335634266},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5885322963377291E-2}]
["Single Family Detached",15095,"East South Central","Before 1950","Brick","central furnace","central AC",28.840401436621701,22889.207490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22889.207490000001},"Hot-Humid",370.63607875226921,"Metropolitan Area",0.41708395728293896,0.26678449411267779,0.64081051028263325,3.946680757146246E-2,0.34595201406694315,1.6706309757451929,483.34,1240.914,{"$f":"T5096*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1063269548216599E-2},{"$f":"U5096*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8403538023245859E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42814722683115558},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.66921404830587916}]
["Multi-Family (2-4 units)",15102,"South Atlantic","Before 1950","Wood","heater burning gas/oil/kerosene","window/wall unit",13.923817537502396,24513.763269999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8171.2544233333329},"Hot-Humid",276.39268087207665,"Metropolitan Area",0.15934164297993103,0.50109904792047255,0.2175191032568014,0,0.77956745620837298,1.657527250365578,0,0,{"$f":"T5103*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5103*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15934164297993103},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2175191032568014}]
["Single Family Detached",15106,"East North Central","1960s","Brick","central furnace","central AC",32.517272568871228,15484.415510000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15484.415510000001},"Cold/Very Cold",71.704224852005666,"Metropolitan Area",1.1481926676585961,0.36237852445327295,7.2454831898547109E-2,3.3030968055544251E-2,0.17503498128218697,1.7580610052926031,1901.3030000000001,231.87200000000001,{"$f":"T5107*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9440565662409532E-2},{"$f":"U5107*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.59040239313472E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1776332333210056},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.6045234291681835E-2}]
["Single Family Detached",15112,"New England","Before 1950","Shingle","radiator","window/wall unit",34.391602085349362,14413.91538,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14413.91538},"Cold/Very Cold",50.273704466808276,"Metropolitan Area",1.6786091269229653,0.14673223159077736,2.1896596857304017E-2,3.0267348489000602E-3,0.14661052048930859,1.9938484758603554,209.98699999999999,0,{"$f":"T5113*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0267348489000602E-3},{"$f":"U5113*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6816358617718654},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1896596857304017E-2}]
["Single Family Detached",15113,"Pacific","1980s","Stucco","portable electric heaters","N/A",20.632882793112056,15847.0682,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15847.0682},"Hot-Dry/Mixed-Dry",81.159745561002026,"Metropolitan Area",1.6267110589709203E-2,7.2115966375808999E-2,6.5380170037398988E-2,0,0.13156023668926123,0.28532348369217841,0,0,{"$f":"T5114*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5114*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6267110589709203E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.5380170037398988E-2}]
["Single Family Detached",15118,"East North Central","1960s","Brick","radiator","central AC",66.478546897427989,20800.546590000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20800.546590000002},"Cold/Very Cold",145.75024116821245,"Metropolitan Area",0.96380222888159051,0.31126701297335857,9.1571473485405827E-2,6.7531678575491706E-3,0.46074720816532444,1.8273879235056794,115.023,209.64,{"$f":"T5119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3925412704215703E-3},{"$f":"U5119*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3606265871276003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.96619477015201205},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.593210007253343E-2}]
["Multi-Family (5+ units)",15121,"Mountain North","1990s","Concrete","built-in electric unit","window/wall unit",8.3604104129675303,20694.085179999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1646.0371787243078},"Cold/Very Cold",180.57658728602641,"Metropolitan Area",0.13058249188138449,0.23498061292591868,7.6561906940446007E-3,0,0.24288500847761219,0.61610430397895988,0,0,{"$f":"T5122*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5122*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13058249188138449},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.6561906940446007E-3}]
["Single Family Detached",15129,"East North Central","1980s","Other","fireplace","window/wall unit",49.882393442745787,22923.894049999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22923.894049999999},"Cold/Very Cold",211.40415088648976,"Metropolitan Area",0.58372516654220263,0.53410683342496457,3.8940635431582597E-2,0.12964381333426403,0.63083003222022249,1.7876026676189722,5655.4009999999998,0,{"$f":"T5130*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.12964381333426403},{"$f":"U5130*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.71336897987646664},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8940635431582597E-2}]
["Single Family Detached",15131,"East North Central","1950s","Brick","central furnace","central AC",102.84228433729419,26369.816500000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26369.816500000001},"Cold/Very Cold",112.37539491793039,"Metropolitan Area",0.95791216924358602,0.41090204884033554,5.5590552971264501E-2,1.3209643137877E-2,0.43813194327529953,1.8625367143304856,348.00799999999998,152.93,{"$f":"T5132*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1769071005319992E-3},{"$f":"U5132*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0327360373449998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.967089076344118},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9623289008609498E-2}]
["Single Family Detached",15136,"East North Central","1960s","Siding","central furnace","both central and individual units",62.878006121779649,16011.715340000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16011.715340000001},"Cold/Very Cold",183.9771230420701,"Metropolitan Area",2.4806737140096522,0.27845229603030691,8.4560254456125666E-2,6.0365992167348767E-2,0.50385025363298419,3.3475365181290684,3509.9650000000001,260.149,{"$f":"T5137*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6200560433363099E-2},{"$f":"U5137*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1654317339856603E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5368742744430155},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.8725686190111328E-2}]
["Single Family Detached",15141,"Pacific","Before 1950","Wood","heater burning gas/oil/kerosene","N/A",54.261417089732845,15022.540720000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15022.540720000001},"Marine",114.44135468316021,"Metropolitan Area",0.51769700359609061,0.18597053633301178,0,0,0.20696087148927617,0.91062841141837847,0,0,{"$f":"T5142*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5142*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.51769700359609061},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15147,"Pacific","1970s","Wood","heat pump","central AC",26.068382825409163,14129.20478,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14129.20478},"Marine",297.50179485395518,"Micropolitan Area",0.44381608255020849,0.19989614608373982,1.8287302583910977E-2,1.1393960285049359E-2,0.35307661981927002,1.0150761510371293,743.52599999999995,62.886000000000003,{"$f":"T5148*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0505431113254278E-2},{"$f":"U5148*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.885291717950801E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45432151366346279},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9175831755706058E-2}]
["Multi-Family (5+ units)",15151,"Pacific","1980s","Concrete","N/A","central AC",13.165024504462709,10642.70372,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":846.53589916592273},"Hot-Humid",153.31878982319304,"Metropolitan Area",0,8.4393149692779834E-2,0.20030193739217941,9.60523167596696E-3,0.22959515377859713,0.52313145865287991,0,902.51800000000003,{"$f":"T5152*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5152*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6401388664343024E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20106595127882285}]
["Single Family Detached",15154,"East North Central","1980s","Siding","central furnace","central AC",57.06396602145329,19027.664560000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19027.664560000001},"Cold/Very Cold",177.83850865550755,"Metropolitan Area",1.8792651401423046,0.12531798739262864,9.3760967245495278E-2,2.8006838493528561E-2,0.36479867035928848,2.4631427651397173,1203.896,268.005,{"$f":"T5155*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2907329253125761E-2},{"$f":"U5155*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0995092404028004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9021724693954303},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.8860476485898074E-2}]
["Multi-Family (5+ units)",15159,"East North Central","1960s","Brick","central furnace","window/wall unit",9.9693113356232921,21485.584780000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1708.9941907020377},"Cold/Very Cold",33.189943023597898,"Metropolitan Area",0.29596968479605607,0.53046574567005167,6.1886004121073012E-3,2.0695989539335001E-3,0.19331397078787638,1.0278429817546055,96.325000000000003,0,{"$f":"T5160*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6461886541937378E-4},{"$f":"U5160*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29613430366147542},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1886004121073012E-3}]
["Single Family Detached",15165,"South Atlantic","1950s","Brick","heat pump","central AC",446.34108076857359,139307.4534,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":139307.4534},"Mixed-Humid",2126.8275089181543,"Micropolitan Area",1.5457334923487629,1.1001814490712205,1.5203803716746833,0.1158817906511628,3.0904401494585145,7.2567354625531806,308.49400000000003,523.34799999999996,{"$f":"T5166*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2975513529179603E-2},{"$f":"U5166*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.2906277121983207E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5887090058779425},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.5932866487966666}]
["Single Family Detached",15166,"Middle Atlantic","1990s","Siding","heat pump","central AC",54.064064043298607,14564.672430000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14564.672430000001},"Mixed-Humid",343.46741131778168,"Metropolitan Area",0.26223557258761399,0.19207030685010629,5.9336650255889155E-2,1.3116346838888369E-2,0.65826829958561139,1.1719108292792209,654.17399999999998,246.38499999999999,{"$f":"T5167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5278300222228201E-3},{"$f":"U5167*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5885168166655502E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27176340260983678},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2925167072554702E-2}]
["Single Family Detached",15170,"Pacific","1970s","Wood","heat pump","central AC",17.2523523796993,12991.2292,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12991.2292},"Marine",119.68059476508098,"Metropolitan Area",7.1452605029897989E-2,0.1300384888004488,1.6625759410825596E-2,2.0545888804383997E-3,0.19023333630741959,0.40835018954859198,99.924999999999997,58.226999999999997,{"$f":"T5171*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.29814857781E-3},{"$f":"U5171*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5644030262839992E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.2750753607707982E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7382199713453995E-2}]
["Single Family Detached",15177,"East North Central","1950s","Brick","central furnace","central AC",61.52981095051679,25940.055209999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25940.055209999999},"Cold/Very Cold",205.73190078790356,"Metropolitan Area",1.8824656561808666,0.42887868363194015,0.15169417442112354,4.7801036738227491E-2,0.58808989695209313,3.0511284111860233,1541.3689999999999,301.38099999999997,{"$f":"T5178*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9983196958982482E-2},{"$f":"U5178*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8178397792450088E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9224488531398491},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15951201420036853}]
["Multi-Family (5+ units)",15179,"Mountain North","1950s","Stucco","central furnace","central AC",24.889288312133623,29144.365709999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2318.1845967929789},"Cold/Very Cold",161.77856707819484,"Metropolitan Area",0.23699499721393591,0.48035067413937527,4.7525508220909347E-2,8.5614780153353085E-3,0.49606455837669872,1.268816223740916,223.435,70.325999999999993,{"$f":"T5180*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1796357538443929E-4},{"$f":"U5180*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6302864995406302E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23751296078932035},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7688536870863413E-2}]
["Multi-Family (5+ units)",15184,"Pacific","1960s","Stucco","N/A","window/wall unit",15.880184071350472,14622.637269999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1163.1055148396617},"Hot-Dry/Mixed-Dry",76.311508045648651,"Metropolitan Area",0,1.9001722321158706E-2,5.2584641358294243E-2,0,0.21067633373147668,0.28226269741092963,0,0,{"$f":"T5185*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5185*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.2584641358294243E-2}]
["Multi-Family (5+ units)",15189,"Middle Atlantic","1990s","Stone","built-in electric unit","window/wall unit",25.726297116237046,25421.24221,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2022.0420203670822},"Cold/Very Cold",283.72849258082397,"Metropolitan Area",0.52064447943295611,0.23671904848561059,6.9759447598149407E-2,0,0.14095865267010427,0.96808162818682042,0,0,{"$f":"T5190*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5190*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52064447943295611},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9759447598149407E-2}]
["Multi-Family (5+ units)",15193,"West North Central","1970s","Siding","central furnace","central AC",17.671823979383024,18162.20347,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1444.6476806845558},"Mixed-Humid",185.17641427568702,"Metropolitan Area",0.13136774422592337,9.2299791330639369E-2,3.9849330276481278E-2,4.1495912756047797E-3,0.3644855649803953,0.63182195765484739,129.55500000000001,98.918999999999997,{"$f":"T5194*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8716133027108764E-4},{"$f":"U5194*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4290310392563556E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13155490555619445},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9992233380406916E-2}]
["Single Family Detached",15200,"West North Central","1990s","Brick","central furnace","central AC",122.06662457193407,21377.692569999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21377.692569999999},"Mixed-Humid",556.89876792984842,"Metropolitan Area",2.8783316701798953,0.51695303155924976,0.26839464280324499,7.8764825612610792E-2,1.570717025705255,5.2343963702476453,2854.7,829.74,{"$f":"T5201*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1026898979578997E-2},{"$f":"U5201*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7737926633031802E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9393585691594741},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2861325694362768}]
["Single Family Detached",15203,"South Atlantic","2000s","Siding","heat pump","central AC",75.216340571908901,17048.127960000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17048.127960000002},"Mixed-Humid",474.80962814880081,"Micropolitan Area",0.56871613817896616,0.35746761904383428,0.30672633814944839,2.968196709918924E-2,0.52506582153200698,1.7579759169042557,665.23800000000006,1075.8309999999999,{"$f":"T5204*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1341062547854481E-2},{"$f":"U5204*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8340904551334761E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.58005720072682065},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32506724270078313}]
["Multi-Family (2-4 units)",15207,"West North Central","1990s","Siding","central furnace","central AC",14.609242325832321,19147.106589999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6382.3688633333331},"Mixed-Humid",211.80726521666668,"Metropolitan Area",0.34865646750251827,0.1287165963752343,5.4735316636955064E-2,7.8389786147987205E-3,0.18535201442886115,0.72268638068676794,287.44600000000003,121.962,{"$f":"T5208*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8345864002897133E-3},{"$f":"U5208*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7840647130986E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35049105390280799},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5513723108264926E-2}]
["Single Family Detached",15213,"West North Central","2000s","Siding","central furnace","central AC",48.739601563267989,14424.268,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14424.268},"Cold/Very Cold",130.64059525259489,"Metropolitan Area",0.67185054023198798,0.40542284297892794,2.0582723646867997E-2,1.4851702333644001E-2,0.39576804573873614,1.4936241525965199,949.36699999999996,80.266000000000005,{"$f":"T5214*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3693924038355999E-2},{"$f":"U5214*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1577782952879999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.68554446427034399},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1740501942155998E-2}]
["Single Family Detached",15218,"Pacific","1990s","Stucco","central furnace","central AC",29.700993373296392,22000.735830000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22000.735830000001},"Hot-Dry/Mixed-Dry",159.44498676413028,"Metropolitan Area",0.31151658088996298,0.65524360308066742,0.12461579786253196,1.261442989843212E-2,0.43415094848217345,1.5255269303153358,320.73899999999998,252.625,{"$f":"T5219*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0564940093783696E-3},{"$f":"U5219*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5579358890537507E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31857307489934134},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13017373375158572}]
["Single Family Detached",15223,"South Atlantic","1990s","Wood","central furnace","central AC",26.8080868977198,15658.929260000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15658.929260000001},"Mixed-Humid",130.71679543473519,"Metropolitan Area",0.52305106445552618,0.32562857706353598,0.17883729572652765,1.9328254835637278E-2,0.2463575965241748,1.2738745337697646,692.30399999999997,542.024,{"$f":"T5224*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0840739362415039E-2},{"$f":"U5224*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.4875154732222402E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53389180381794121},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18732481119974989}]
["Multi-Family (2-4 units)",15225,"East South Central","1970s","Wood","central furnace","central AC",9.3251133217576463,11789.018110000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3929.6727033333336},"Mixed-Humid",66.558544523387127,"Micropolitan Area",8.0095123474827654E-2,0.15157441203988806,3.1636364533672662E-2,5.1675392532468502E-3,0.29924523261417485,0.56599615883139442,325.05099999999999,113.28400000000001,{"$f":"T5226*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2773440418912035E-3},{"$f":"U5226*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4516904252441339E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.1372467516718852E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2081533576197079E-2}]
["Single Family Detached",15230,"West North Central","1990s","Concrete","heat pump","central AC",47.802776489133755,17704.732029999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17704.732029999999},"Cold/Very Cold",795.14732973661535,"Metropolitan Area",0.65341087570864398,0.54907016205768266,0.1014600475212882,2.175141410643695E-2,1.4091015988504934,2.7130426841381081,926.94,301.625,{"$f":"T5231*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.64112243078882E-2},{"$f":"U5231*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3401897985487492E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6698221000165322},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10680023731983695}]
["Single Family Detached",15232,"Pacific","Before 1950","Siding","heat pump","central AC",44.418276895551749,26097.695,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26097.695},"Marine",498.64975453051528,"Metropolitan Area",0.49753363434612502,0.96972387537083504,3.8097545649474998E-2,8.3463038379500004E-3,0.71121028680188492,2.21656534216832,259.649,60.161000000000001,{"$f":"T5233*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7762404090550002E-3},{"$f":"U5233*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5700634288949998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.50430987475517997},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9667609078369997E-2}]
["Single Family Detached",15237,"West South Central","1970s","Siding","central furnace","central AC",43.871674279566058,22429.281330000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22429.281330000002},"Hot-Humid",622.82467249548608,"Metropolitan Area",1.0183163099488775,0.33753323057615209,0.33575319795124059,3.5105638259276109E-2,0.43347504219726013,2.1250777806735304,811.28800000000001,753.88199999999995,{"$f":"T5238*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8196606791653042E-2},{"$f":"U5238*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.690903146762306E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0365129167405305},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35266222941886366}]
["Multi-Family (2-4 units)",15242,"West North Central","1960s","Siding","radiator","N/A",12.001791154614912,15627.33223,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5209.1107433333336},"Cold/Very Cold",83.931635383336371,"Metropolitan Area",3.6951707397550625E-2,0.10620102136257772,0,7.0891829928171996E-4,0.14274941336082578,0.28637475432047527,45.363999999999997,0,{"$f":"T5243*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3630609976057332E-4},{"$f":"U5243*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.7188013497311198E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15248,"East North Central","1960s","Siding","central furnace","window/wall unit",25.522874600977307,16747.29305,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16747.29305},"Cold/Very Cold",124.21552662864393,"Metropolitan Area",1.02156104465199,0.47962016555765741,3.79999093817249E-2,3.139824369246625E-2,0.35442524044900486,1.8936063600403772,1874.825,0,{"$f":"T5249*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.139824369246625E-2},{"$f":"U5249*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0529592883444563},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.79999093817249E-2}]
["Single Family Detached",15251,"East South Central","1960s","Brick","central furnace","central AC",53.208994714058946,28108.290919999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28108.290919999999},"Mixed-Humid",601.76025324151931,"Metropolitan Area",0.52947019818527419,0.39178893083612965,0.20832440139554353,1.8551668765236441E-2,0.92362244601366639,2.0532059764306139,296.90600000000001,363.101,{"$f":"T5252*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3455202238935204E-3},{"$f":"U5252*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.020614854134292E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53781571840916775},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21853054993688645}]
["Single Family Detached",15255,"West South Central","1970s","Brick","central furnace","central AC",62.779308182098603,17794.588489999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17794.588489999998},"Hot-Humid",225.55945250595161,"Metropolitan Area",0.42406109443551793,0.17403500803625627,0.39734636344889684,3.940732624312232E-2,0.38266022264927246,1.3781026885699434,763.61900000000003,1450.9490000000001,{"$f":"T5256*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3588285868145309E-2},{"$f":"U5256*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5819040374977009E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43764938030366324},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.42316540382387385}]
["Single Family Attached",15260,"Pacific","1970s","Wood","central furnace","central AC",8.6938593792336736,8359.4801719999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8359.4801719999996},"Hot-Dry/Mixed-Dry",42.397628257034711,"Metropolitan Area",3.8218347940719405E-2,0.10787874052149278,6.3554435995100605E-2,7.0233342992282073E-3,7.6844162023462559E-2,0.28649568648077534,509.85500000000002,330.30900000000003,{"$f":"T5261*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2621227630950604E-3},{"$f":"U5261*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7612115361331483E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.2480470703814464E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6315647531233757E-2}]
["Single Family Detached",15266,"South Atlantic","2000s","Stucco","heat pump","both central and individual units",29.637225067364966,10532.06292,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10532.06292},"Hot-Humid",194.27593877604789,"Metropolitan Area",0.18410150251582905,4.9506309313536369E-2,0.24252623632526638,1.163673940349004E-2,0.20070286680267455,0.67683691495730636,235.477,869.41,{"$f":"T5267*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4800585802128403E-3},{"$f":"U5267*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1566808232772003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18658156109604188},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25168291714854357}]
["Single Family Detached",15271,"Pacific","Before 1950","Stucco","central furnace","N/A",26.547856468295816,23535.333750000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23535.333750000002},"Hot-Dry/Mixed-Dry",88.682337866328481,"Metropolitan Area",0.10210072598557875,0.28563716644021875,0,2.3067215961712502E-3,0.32203592513395124,0.70977381755974878,98.010999999999996,0,{"$f":"T5272*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3067215961712502E-3},{"$f":"U5272*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10440744758175},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15275,"Mountain South","Before 1950","Stucco","central furnace","central AC",35.772835200295418,18279.42524,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18279.42524},"Hot-Dry/Mixed-Dry",111.13557862125177,"Metropolitan Area",0.35944477169741074,0.29236293695165877,0.22835879075414034,2.0591041355850402E-2,0.24617225516534733,1.1263387545685573,480.78,645.67999999999995,{"$f":"T5276*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7883820668871997E-3},{"$f":"U5276*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1802659288963199E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36823315376429794},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24016145004310355}]
["Single Family Detached",15278,"West South Central","1970s","Siding","central furnace","central AC",31.612896488793577,15390.8941,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15390.8941},"Hot-Humid",246.06824513877518,"Metropolitan Area",0.234343754382833,0.10868089021628159,0.30664791240320027,2.0974587352327202E-2,0.18991230549594235,0.83958486249825726,311.28500000000003,1051.5070000000001,{"$f":"T5279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7909544699185009E-3},{"$f":"U5279*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6183632882408702E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23913470885275151},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.32283154528560898}]
["Multi-Family (2-4 units)",15285,"Middle Atlantic","Before 1950","Wood","central furnace","N/A",49.733664730468568,41583.331709999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13861.110569999999},"Cold/Very Cold",180.50783713925509,"Metropolitan Area",1.0740764307645654,0.38953007171016146,0,2.5081028104218209E-2,0.62195677763666934,2.1022839655142085,603.15099999999995,0,{"$f":"T5286*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3603427014060684E-3},{"$f":"U5286*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0824367734659714},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15289,"Pacific","Before 1950","Concrete","central furnace","central AC",43.478124817965515,15417.77476,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15417.77476},"Marine",43.961549145507114,"Metropolitan Area",0.17128181063882544,0.17417048491785908,2.8640012140851722E-2,6.6260508052809197E-3,0.1555724240870148,0.52966473178455109,341.33199999999999,88.435000000000002,{"$f":"T5290*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2625798943803197E-3},{"$f":"U5290*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3634709109006E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17654439053320575},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0003483051752322E-2}]
["Single Family Detached",15290,"Mountain South","1990s","Brick","central furnace","central AC",35.941391049910052,26623.252629999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26623.252629999999},"Hot-Dry/Mixed-Dry",494.13901680332003,"Metropolitan Area",0.54497012747657414,0.48522195769180176,0.70892378466887163,4.0910275051605313E-2,0.55334247484739352,2.2924583446846407,328.22800000000001,1208.4090000000001,{"$f":"T5291*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7384969642396396E-3},{"$f":"U5291*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2171778087365675E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55370862444081381},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.74109556275623734}]
["Single Family Detached",15296,"Pacific","1970s","Siding","heat pump","central AC",27.8435949873274,13921.797490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13921.797490000001},"Marine",358.49032278311347,"Metropolitan Area",0.33087717522262411,0.18238249409594751,3.5060237144891301E-2,1.0078337247948252E-2,0.70069702886516316,1.2490169353286262,599.17600000000004,124.749,{"$f":"T5297*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3416069328682407E-3},{"$f":"U5297*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7367303150800102E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33921878215549234},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6796967459971311E-2}]
["Single Family Detached",15301,"Middle Atlantic","1990s","Siding","central furnace","window/wall unit",42.861075040571542,15302.06178,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15302.06178},"Mixed-Humid",92.941754640440436,"Metropolitan Area",1.13456595374823,0.27050556356954164,6.7362843482348472E-2,1.6615804992060119E-2,0.23313864789968514,1.7055730086998053,1085.854,0,{"$f":"T5302*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6615804992060119E-2},{"$f":"U5302*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1511817587402902},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7362843482348472E-2}]
["Single Family Detached",15304,"South Atlantic","2000s","Concrete","heat pump","central AC",56.455087294731271,25896.829030000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25896.829030000001},"Hot-Humid",143.270218520485,"Metropolitan Area",1.9766479868360342E-2,8.5328238875817891E-2,8.1443973489608204E-2,6.5993666322019902E-3,0.30229927898226061,0.488837971216047,13.881,240.952,{"$f":"T5305*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5947388376543E-4},{"$f":"U5305*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2398927484365596E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0125953752125773E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.7683866238044764E-2}]
["Single Family Detached",15308,"South Atlantic","2010s","Stucco","heat pump","central AC",24.209862734585201,8874.5831139999991,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8874.5831139999991},"Hot-Humid",181.96445216639844,"Metropolitan Area",2.1939132028195935E-2,0.14432117734771777,0.28451997772023585,1.6266871234217918E-2,0.17008242370603435,0.62086271080218391,46.286999999999999,1786.6859999999999,{"$f":"T5309*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1077782859771797E-4},{"$f":"U5309*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5856093405620202E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2349909856793655E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30037607112585607}]
["Mobile Home",15314,"West North Central","1980s","Siding","wood-burning stove","N/A",26.22983561978447,21290.450990000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21290.450990000001},"Mixed-Humid",141.51762773109365,"Rural",0,0.23771657180735392,0,0,0.24514157400921446,0.48285814581656838,0,0,{"$f":"T5315*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5315*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",15319,"West South Central","2010s","Wood","central furnace","central AC",31.066733808646518,31317.271980000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10439.09066},"Mixed-Humid",309.7051149047407,"Metropolitan Area",0.4237723173263977,0.31228888375018049,9.7106665723811908E-2,1.1214088750598402E-2,0.21606991653973209,1.0567138425071878,219.011,139.06899999999999,{"$f":"T5320*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2862756845372597E-3},{"$f":"U5320*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.45175389899554E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42605859301093496},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.8558419622807453E-2}]
["Single Family Attached",15324,"South Atlantic","Before 1950","Brick","central furnace","central AC",21.962431442396625,10926.58281,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10926.58281},"Mixed-Humid",75.796940072489775,"Metropolitan Area",0.10477373508148403,7.8373898161832128E-2,6.5426432934539827E-2,1.1005199573317951E-2,0.12612956635830413,0.37470363253616012,714.87800000000004,292.31700000000001,{"$f":"T5325*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8111736660471803E-3},{"$f":"U5325*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1940259072707699E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11258490874753121},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.8620458841810603E-2}]
["Single Family Attached",15326,"South Atlantic","2000s","Concrete","central furnace","central AC",8.1165712904038649,8231.8167250000006,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8231.8167250000006},"Hot-Humid",139.50917492100584,"Metropolitan Area",6.1063616466050007E-3,0.13369106680832843,0.1438481902198718,6.3072509019619005E-3,0.19235969382095672,0.476005312495762,11.959,754.245,{"$f":"T5327*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8444296214275E-5},{"$f":"U5327*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2088066057476255E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.2048059428192756E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15005699682561943}]
["Single Family Detached",15331,"West North Central","1950s","Siding","heat pump","central AC",34.142185853247902,8033.4554950000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8033.4554950000002},"Cold/Very Cold",132.05032636989532,"Rural",0.13314970475632801,0.15394869860529128,3.0399318604074549E-2,6.0319200584207497E-3,0.13305799482839703,0.4505557167940909,515.03,235.82,{"$f":"T5332*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1374705835898499E-3},{"$f":"U5332*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8944494748309002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13728717533991786},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.2293768078905452E-2}]
["Single Family Detached",15338,"New England","1980s","Siding","N/A","central AC",25.063350800073554,12107.898939999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12107.898939999999},"Cold/Very Cold",42.335595547308586,"Rural",0,2.7097623122507283E-2,1.2615788976836179E-2,6.3786833195707997E-4,0.10473562633179859,0.14444903843114204,0,52.682000000000002,{"$f":"T5339*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5339*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3786833195707997E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3253657308793259E-2}]
["Single Family Detached",15342,"New England","1970s","Siding","central furnace","central AC",88.889782672636969,40700.449939999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":40700.449939999999},"Cold/Very Cold",300.12511786997487,"Metropolitan Area",2.9692779633144344,0.65288332496942914,8.4391243337991681E-2,6.9553405906965404E-2,0.93238357122079374,4.6389361028426483,1606.2190000000001,102.691,{"$f":"T5343*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5373836002176861E-2},{"$f":"U5343*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1795699047885394E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0346517993166113},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.8570813242780225E-2}]
["Single Family Detached",15347,"Middle Atlantic","Before 1950","Brick","central furnace","both central and individual units",48.377835554543346,22501.318859999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22501.318859999999},"Cold/Very Cold",169.41242971635202,"Metropolitan Area",2.1380902364516046,0.53877850919004888,0.11538723564177605,4.0806591778987197E-2,0.48810398652632714,3.2803599678097566,1599.4,214.12,{"$f":"T5348*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5988609384684005E-2},{"$f":"U5348*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8179823943031996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1740788458362887},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12020521803607925}]
["Single Family Detached",15349,"South Atlantic","1960s","Brick","wood-burning stove","central AC",38.641896152840644,22207.986290000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22207.986290000001},"Mixed-Humid",245.06746060097271,"Metropolitan Area",0.54388320030016357,0.17717073977644426,0.20483409569059649,2.4387255984637705E-2,0.4399609506640948,1.3658489864312993,639.60599999999999,458.524,{"$f":"T5350*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4204361279001741E-2},{"$f":"U5350*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0182894705635961E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55808756157916528},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21501699039623245}]
["Single Family Detached",15352,"South Atlantic","1990s","Concrete","central furnace","central AC",51.042840430933801,23851.794590000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23851.794590000001},"Hot-Humid",525.01587566142871,"Metropolitan Area",9.792836075175218E-2,0.22008902377259865,0.87763341273794615,4.7365346880919208E-2,0.98446500441169138,2.1801158016739883,94.233999999999995,1891.585,{"$f":"T5353*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2476500113940601E-3},{"$f":"U5353*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5117696869525159E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10017601076314624},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.92275110960747131}]
["Multi-Family (5+ units)",15360,"Mountain North","1980s","Stucco","central furnace","central AC",22.539567163420543,33541.022559999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2667.9009806893409},"Cold/Very Cold",214.9644136166105,"Metropolitan Area",0.18253665633681923,0.23544224763161933,2.5775733646809695E-2,4.055713365910079E-3,0.2859873276117047,0.73347508134207995,88.370999999999995,32.546999999999997,{"$f":"T5361*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3576507756449774E-4},{"$f":"U5361*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6832173218495969E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18277242141438374},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5862565820028192E-2}]
["Multi-Family (5+ units)",15362,"Pacific","1970s","Wood","built-in electric unit","window/wall unit",13.835302643420066,16975.831460000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1350.2819515753897},"Marine",43.466412754411479,"Metropolitan Area",1.9099321241499941E-2,3.1337232092676866E-2,3.6652347946971404E-3,0,9.4205594224966702E-2,0.14830738235384064,0,0,{"$f":"T5363*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5363*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9099321241499941E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6652347946971404E-3}]
["Multi-Family (5+ units)",15367,"Mountain South","1990s","Stucco","central furnace","central AC",20.34322343159528,23518.177380000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1870.6695177193155},"Hot-Dry/Mixed-Dry",60.343692097036978,"Metropolitan Area",0.48219218293708549,0.34873063859005415,6.0944056148538185E-2,8.0516832078168007E-3,0.29274735768209026,1.1920254761494986,232.49700000000001,109.863,{"$f":"T5368*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3492505086118773E-4},{"$f":"U5368*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0551736522519718E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.48262710798794667},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1149573513763385E-2}]
["Multi-Family (2-4 units)",15372,"East South Central","2000s","Siding","built-in electric unit","central AC",9.81340001986832,20027.346979999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6675.7823266666664},"Mixed-Humid",103.63118650695573,"Micropolitan Area",7.3585259340448211E-2,9.4836096974803386E-2,1.4138031893455607E-2,5.8095328119583999E-4,0.17064290980635513,0.35358960020252622,0,29.007999999999999,{"$f":"T5373*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5373*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9365109373194666E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.3585259340448211E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4331682987187554E-2}]
["Single Family Attached",15376,"West North Central","2000s","Siding","radiator","window/wall unit",15.439442817458314,9619.5905399999992,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9619.5905399999992},null,75.888949773787317,"Metropolitan Area",0.28756887650713697,0.16107489711136108,4.5553186218548402E-3,6.0579371425650006E-4,0.25377198427933328,0.70697107651968627,62.975000000000001,0,{"$f":"T5377*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0579371425650006E-4},{"$f":"U5377*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28817467022139348},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.5553186218548402E-3}]
["Single Family Detached",15379,"Pacific","2000s","Wood","central furnace","central AC",18.285379368284101,12558.63968,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12558.63968},"Cold/Very Cold",295.53368900662861,"Micropolitan Area",0.73570392529664064,8.6298676826189441E-2,3.499859288117952E-2,1.3999417058648321E-2,0.15135975205552279,1.0083609470595325,988.24900000000002,126.47499999999999,{"$f":"T5380*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.241106310512032E-2},{"$f":"U5380*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5883539535280001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.74811498840176094},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6586946834707521E-2}]
["Single Family Detached",15386,"Mountain South","1980s","Stucco","central furnace","central AC",12.692396063698608,9190.7285040000006,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9190.7285040000006},"Hot-Dry/Mixed-Dry",88.509537044901634,"Metropolitan Area",4.6306768690580695E-2,5.4039820081660785E-2,9.8975874332426411E-2,5.6539431703622163E-3,0.10267207285196611,0.301994535956634,87.081000000000003,528.09799999999996,{"$f":"T5387*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.0033782885682414E-4},{"$f":"U5387*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8536053415053912E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.7107106519437517E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1038294796739318}]
["Single Family Attached",15390,"Pacific","1970s","Stucco","central furnace","central AC",16.525021929452663,6914.2351170000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6914.2351170000002},"Hot-Dry/Mixed-Dry",26.761180565600114,"Metropolitan Area",0.12515913324799421,7.6495840729747897E-2,5.7402470852027314E-2,4.2588369487863847E-3,3.5953905066403058E-2,0.29501134989617245,173.91300000000001,442.03899999999999,{"$f":"T5391*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2024753719028212E-3},{"$f":"U5391*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0563615768835627E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12636160861989704},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.0458832428910876E-2}]
["Single Family Detached",15396,"West South Central","1960s","Brick","central furnace","both central and individual units",52.697400714449287,36595.417159999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":36595.417159999997},"Hot-Humid",712.22644961606773,"Metropolitan Area",0.41613183145726529,0.58670742569466738,1.2873759080589475,6.1673414845153318E-2,1.2570783060242634,3.5472934712351436,387.8,1297.4770000000001,{"$f":"T5397*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4191702774647999E-2},{"$f":"U5397*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.7481712070505319E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43032353423191327},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.3348576201294529}]
["Single Family Detached",15397,"East North Central","Before 1950","Wood","central furnace","central AC",60.647928872601035,22868.751459999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22868.751459999999},"Cold/Very Cold",163.14567291747201,"Micropolitan Area",1.9533650043453532,0.13976260323530459,5.3312067909829737E-2,3.89030622024217E-2,0.28051777889022778,2.4269574543807155,1591.79,109.355,{"$f":"T5398*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6402249886513395E-2},{"$f":"U5398*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5008123159083002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9897672542318665},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5812880225738035E-2}]
["Single Family Detached",15402,"New England","Before 1950","Siding","central furnace","window/wall unit",62.056433328195723,21057.493490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21057.493490000001},"Cold/Very Cold",249.82302842431224,"Rural",2.8339410372194158,0.27824561184186636,3.0800164003018302E-2,1.7645716279763218E-2,0.34850019063740922,3.4914870037017098,837.97799999999995,0,{"$f":"T5403*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7645716279763218E-2},{"$f":"U5403*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8515867534991792},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.0800164003018302E-2}]
["Multi-Family (5+ units)",15405,"East North Central","2010s","Concrete","central furnace","central AC",9.793440478165536,11957.80278,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":951.14076222879862},"Cold/Very Cold",125.03078588485816,"Metropolitan Area",7.6443043761528157E-3,1.4108927795502539E-2,6.5913075743231726E-3,2.3482613521336199E-3,0.41768791652263365,0.44819393354900011,172.78200000000001,23.597000000000001,{"$f":"T5406*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.643400031794163E-4},{"$f":"U5406*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2444068566312964E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.8086443793322323E-3},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6137516428894857E-3}]
["Single Family Detached",15413,"East North Central","1980s","Brick","central furnace","central AC",54.962234524100865,16348.0769,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16348.0769},"Cold/Very Cold",110.02688974995471,"Metropolitan Area",1.7653659170310889,0.29412479073866005,4.7897315017003603E-2,2.1948993438247601E-2,0.39890229667537142,2.5062903194621238,1174.29,168.31399999999999,{"$f":"T5414*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9197383222900998E-2},{"$f":"U5414*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7516102153465997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.78456330025399},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.0648925232350206E-2}]
["Single Family Detached",15415,"New England","1970s","Wood","central furnace","central AC",63.060709156448183,24729.689869999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24729.689869999998},"Cold/Very Cold",119.45221663126988,"Metropolitan Area",1.7353474514513278,0.39007776937420391,0.11450204990313115,5.6622334410845493E-2,0.3540828154995837,2.5940100862282462,2049.31,240.34,{"$f":"T5416*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0678800747489698E-2},{"$f":"U5416*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9435336633557991E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7860262521988175},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12044558356648695}]
["Multi-Family (5+ units)",15420,"Pacific","1980s","Stucco","central furnace","central AC",16.088593361564509,16953.206910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1348.4823624595635},"Hot-Dry/Mixed-Dry",101.74455262305149,"Metropolitan Area",3.2519817965331425E-2,6.0569553034495592E-2,3.5785784836114734E-2,2.1183201566114104E-3,0.28059290053796199,0.41141788231084347,31.033000000000001,93.918000000000006,{"$f":"T5421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1847453154207634E-5},{"$f":"U5421*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2664676651747729E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2561665418485632E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.591243160263221E-2}]
["Multi-Family (2-4 units)",15424,"Mountain South","Before 1950","Stucco","portable electric heaters","both central and individual units",14.102164317151347,19344.532670000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6448.1775566666665},"Hot-Dry/Mixed-Dry",154.83493558228892,"Metropolitan Area",3.9172814068478688E-2,0.13163151683829197,0.18117946793998002,2.3579824652769804E-3,0.38468061792058333,0.73823640507751853,0,121.89400000000001,{"$f":"T5425*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5425*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8599415509232671E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.9172814068478688E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18196546209507236}]
["Single Family Detached",15431,"South Atlantic","1980s","Siding","built-in electric unit","window/wall unit",71.584514425635604,22148.674019999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22148.674019999999},"Mixed-Humid",456.24443425996498,"Metropolitan Area",0.631665808560961,0.37781478357139037,4.468382025297498E-2,0,0.5025416304192214,1.5567060428045478,0,0,{"$f":"T5432*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5432*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.631665808560961},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.468382025297498E-2}]
["Single Family Detached",15434,"East South Central","Before 1950","Wood","heater burning gas/oil/kerosene","N/A",12.789190237323448,12297.29831,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12297.29831},"Mixed-Humid",140.38063272106893,"Rural",0.50388452825247487,0.10039176164580477,0,0,0.19663436565262221,0.80091065555090191,0,0,{"$f":"T5435*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5435*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.50388452825247487},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15437,"South Atlantic","1970s","Siding","central furnace","central AC",68.841437073572408,17530.28701,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17530.28701},"Mixed-Humid",305.90690913486901,"Metropolitan Area",1.3515721911191865,0.27858409868467188,0.13575408681797776,3.1108213041012411E-2,0.6059431005835807,2.3718534772054172,1339,435.541,{"$f":"T5438*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.347305430639E-2},{"$f":"U5438*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.6351587346224093E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3750452454255764},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14338924555260019}]
["Single Family Detached",15438,"East South Central","Before 1950","Brick","central furnace","central AC",32.527588623676046,28990.720700000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28990.720700000002},"Mixed-Humid",274.08282502642356,"Metropolitan Area",0.94521099349154059,0.72030617163994581,0.24177501506917662,1.9820607853941605E-2,0.63217009008528235,2.5394622702859455,312.40300000000002,371.28500000000003,{"$f":"T5439*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0567881188421007E-3},{"$f":"U5439*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0763819735099501E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95426778161038273},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25253883480427614}]
["Single Family Detached",15439,"West South Central","1990s","Brick","central furnace","central AC",40.04585409272476,21716.840609999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21716.840609999999},"Hot-Humid",191.15134876792848,"Metropolitan Area",0.41029375049121924,0.38615598164053822,0.24707408094933453,1.868308484414544E-2,0.39899675859010014,1.4425205716711922,282.61799999999999,577.68600000000004,{"$f":"T5440*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1375700595169792E-3},{"$f":"U5440*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.254551478462846E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.41643132055073623},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25961959573396298}]
["Single Family Attached",15440,"Pacific","1990s","Siding","heat pump","N/A",13.943529329980121,15305.74021,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15305.74021},"Marine",184.75559005728874,"Micropolitan Area",0.14623332252163129,0.24158848197917673,0,2.3251868297423598E-3,0.24256041178825194,0.63038221628905999,151.916,0,{"$f":"T5441*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3251868297423598E-3},{"$f":"U5441*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14855850935137366},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15441,"East North Central","1960s","Brick","central furnace","central AC",43.588902240637815,14984.153399999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14984.153399999999},"Cold/Very Cold",188.04406763391177,"Metropolitan Area",1.1866937634119854,0.24963323855977437,7.5561369526156816E-2,3.4140209773781398E-2,0.56902079793214921,2.0809091694300657,2016.376,262.04500000000002,{"$f":"T5442*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0213687296078397E-2},{"$f":"U5442*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9265224777029996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2169074507080637},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.948789200385982E-2}]
["Single Family Detached",15442,"East South Central","1980s","Brick","central furnace","central AC",26.461124073626362,15438.22875,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15438.22875},"Hot-Humid",358.75034848840261,"Rural",0.26350126300433246,0.31639620093267373,0.15237077892324749,1.2551048400318751E-2,0.49178792622991502,1.2240561690901688,335.89100000000002,477.09399999999999,{"$f":"T5443*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1855620930662503E-3},{"$f":"U5443*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3654863072525004E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26868682509739872},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1597362652305}]
["Single Family Detached",15443,"Pacific","Before 1950","Siding","portable electric heaters","window/wall unit",70.513502360530964,23781.95695,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23781.95695},"Cold/Very Cold",562.1477673005819,"Micropolitan Area",0.98263749938166733,0.26088124231985532,0.1114716923304041,0,0.56305773628921696,1.9180481703211438,0,0,{"$f":"T5444*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5444*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.98263749938166733},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1114716923304041}]
["Mobile Home",15444,"South Atlantic","1990s","Siding","central furnace","both central and individual units",15.271690509821291,15150.48662,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15150.48662},"Mixed-Humid",210.20224496379805,"Micropolitan Area",0.18071023200007469,0.14495170501835844,6.9300643824332847E-2,4.1467942413003396E-3,0.32224750214985703,0.71721008299262301,154.31200000000001,119.395,{"$f":"T5445*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3379018913054399E-3},{"$f":"U5445*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8088923499948999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18304813389138014},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.1109536174327748E-2}]
["Single Family Detached",15445,"South Atlantic","Before 1950","Siding","portable electric heaters","window/wall unit",49.0836359266915,22109.745910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22109.745910000001},"Mixed-Humid",413.12836290380221,"Metropolitan Area",0.76332725937741785,0.32920768266384026,0.14707334439119679,0,0.54926025728187944,1.7888685437143343,0,0,{"$f":"T5446*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5446*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.76332725937741785},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14707334439119679}]
["Multi-Family (5+ units)",15446,"Mountain North","1960s","Brick","central furnace","central AC",33.632949714435519,33835.965510000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2691.361165427144},"Cold/Very Cold",173.55857366969059,"Metropolitan Area",0.31804260729411465,0.82044166785555173,5.5587934412341534E-2,9.6334039043865904E-3,0.52715483473949198,1.7300941934598388,212.49100000000001,72.218000000000004,{"$f":"T5447*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.718900254027793E-4},{"$f":"U5447*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9436472064481749E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31861449731951741},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5782299132986352E-2}]
["Single Family Detached",15447,"Pacific","Before 1950","Stucco","central furnace","N/A",39.262060793163648,23651.843850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23651.843850000001},"Hot-Dry/Mixed-Dry",114.1716839502909,"Metropolitan Area",7.8941363759357855E-2,0.26766652139166286,0,9.3599806851989999E-4,0.48519593514562731,0.83180382029664801,39.573999999999998,0,{"$f":"T5448*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.3599806851989999E-4},{"$f":"U5448*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.987736182787776E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15448,"South Atlantic","1960s","Brick","central furnace","both central and individual units",39.720349939640364,25203.26773,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25203.26773},"Mixed-Humid",518.02718358408629,"Metropolitan Area",0.58365709766846585,0.21498899000024918,0.21920839506726714,1.9665000865938882E-2,0.74965423682966781,1.76750871956565,419.31,360.94600000000003,{"$f":"T5449*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0567982191866299E-2},{"$f":"U5449*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0970186740725809E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59422507986033213},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22830541374133972}]
["Single Family Detached",15449,"East North Central","1990s","Brick","central furnace","central AC",64.99778103678662,15468.2963,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15468.2963},"Cold/Very Cold",154.09606486429522,"Metropolitan Area",1.9733320758982693,0.39529401345909304,0.1526814118636689,5.7304515609720899E-2,0.3667742184095979,2.888081719630629,3179.5360000000001,525.10699999999997,{"$f":"T5450*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9182004944516799E-2},{"$f":"U5450*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1225106652040996E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.0225140808427859},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16080392252887299}]
["Multi-Family (2-4 units)",15450,"West North Central","1950s","Stone","built-in furnace","N/A",7.6417352779688636,13266.901519999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4422.3005066666665},"Cold/Very Cold",34.650758739070554,"Metropolitan Area",0.16751904278879678,0.24338223706750636,0,0,0.15218722764861792,0.56308850750492112,0,0,{"$f":"T5451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5451*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16751904278879678},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15451,"South Atlantic","2000s","Siding","heat pump","central AC",28.030166830358606,23108.134239999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1838.0540989921728},"Mixed-Humid",500.16084569401579,"Metropolitan Area",0.10095396978263392,0.67512648738740999,6.5787253464565862E-2,4.7600907883660797E-3,0.8602996620612321,1.7065488390442483,73.048000000000002,132.94399999999999,{"$f":"T5452*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3426617582318023E-4},{"$f":"U5452*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.443582641364154E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1010882359584571},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6031611728702283E-2}]
["Multi-Family (5+ units)",15452,"Middle Atlantic","1960s","Brick","radiator","N/A",14.268198230041429,24600.341779999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1956.746424255557},"Mixed-Humid",108.74226837129829,"Metropolitan Area",0.37205990732038469,0.16433065209552669,0,2.3846341304443E-3,0.25351279513005387,0.79209831146177434,96.935000000000002,0,{"$f":"T5453*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.896772146352124E-4},{"$f":"U5453*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.37224958453501988},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15453,"East North Central","1960s","Siding","central furnace","central AC",53.669177635553979,20252.51986,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20252.51986},"Cold/Very Cold",230.17912338606521,"Metropolitan Area",2.1781333573133339,0.32323280928814208,0.19894894788556161,0.10751378258502731,0.65691063291636087,3.3572257474033984,4820.0649999999996,488.59699999999998,{"$f":"T5454*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7618462138990891E-2},{"$f":"U5454*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.8953204460364187E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2757518194523247},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20884426833159803}]
["Multi-Family (5+ units)",15454,"Pacific","1980s","Wood","N/A","central AC",11.025187606360619,12250.20845,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":974.39912808084216},"Hot-Dry/Mixed-Dry",92.069406167782205,"Metropolitan Area",0,0.33586835064827508,2.1115872379591054E-2,9.3304937680269997E-4,0.30967292140588248,0.6675159777265619,0,76.165999999999997,{"$f":"T5455*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5455*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4216083989405419E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1190088463580458E-2}]
["Multi-Family (5+ units)",15455,"Pacific","1970s","Stucco","N/A","N/A",13.824575115012497,18681.858260000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1485.981767067309},"Hot-Dry/Mixed-Dry",79.896385644049985,"Metropolitan Area",0,0.23829960026947594,0,0,0.27260644168610865,0.51090604195558453,0,0,{"$f":"T5456*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5456*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15456,"Pacific","1970s","Wood","N/A","window/wall unit",9.5904206184921357,15443.51146,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1228.3990237839987},"Hot-Dry/Mixed-Dry",74.603928321784721,"Metropolitan Area",0,0.25462359794178735,2.2298191239078297E-2,0,0.23225041301105934,0.50917220219192494,0,0,{"$f":"T5457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5457*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.2298191239078297E-2}]
["Single Family Detached",15457,"Middle Atlantic","1970s","Siding","built-in electric unit","window/wall unit",34.538677207308979,17470.246439999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17470.246439999999},"Cold/Very Cold",156.11412216717909,"Metropolitan Area",0.17928487510071914,0.13146971904725399,1.013953886106516E-2,0,0.21176725189587181,0.53266138490491011,0,0,{"$f":"T5458*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5458*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17928487510071914},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.013953886106516E-2}]
["Multi-Family (5+ units)",15458,"Middle Atlantic","2010s","Wood","heat pump","N/A",26.138650536201673,19998.967509999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1590.7465235223069},"Mixed-Humid",167.49135290029764,"Metropolitan Area",9.997226022210158E-2,0.29767447191085489,0,1.7725884862813397E-3,0.21157477699403035,0.61085310338590226,88.634,0,{"$f":"T5459*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4099422736587615E-4},{"$f":"U5459*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10011325444946746},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15459,"Pacific","2000s","Stucco","central furnace","central AC",37.871193004865646,18233.602790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18233.602790000001},"Hot-Dry/Mixed-Dry",278.40109532589338,"Metropolitan Area",0.35292299680542727,1.1933482222984142,0.22843343842875805,1.757826887212461E-2,0.78036971852444148,2.5550743760570414,324.39600000000002,639.66300000000001,{"$f":"T5460*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9149078106648413E-3},{"$f":"U5460*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.166336106145977E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.35883790461609211},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24009679949021781}]
["Multi-Family (5+ units)",15460,"Middle Atlantic","1980s","Wood","radiator","window/wall unit",23.602858121417395,32964.88564,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2622.0742247778385},"Mixed-Humid",73.169783193191975,"Metropolitan Area",2.7188132897408894E-2,6.7373237692404317E-2,6.2879530411730812E-3,1.9703112147028003E-4,0.39895119920005717,0.49998188181487219,5.9770000000000003,0,{"$f":"T5461*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5672137641497143E-5},{"$f":"U5461*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.7203805035050391E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2879530411730812E-3}]
["Single Family Detached",15461,"Pacific","1990s","Siding","central furnace","central AC",43.034534606423676,13448.29206,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13448.29206},"Hot-Dry/Mixed-Dry",183.42515547251514,"Metropolitan Area",0.10695243778545985,0.37868022196728235,0.1796502198297954,1.320526797418374E-2,0.49987253173168589,1.1651554113142235,218.60900000000001,763.32,{"$f":"T5462*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9399176789445401E-3},{"$f":"U5462*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0265350295239201E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10989235546440439},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1899155701250346}]
["Single Family Attached",15462,"New England","Before 1950","Wood","heat pump","window/wall unit",15.454404232614321,11015.25605,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11015.25605},"Cold/Very Cold",86.359805675675318,"Metropolitan Area",0.82443432758387059,0.13285961861133494,3.3421046908367454E-2,6.6147053190491996E-3,0.14860360291578328,1.1393185960193561,600.50400000000002,0,{"$f":"T5463*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6147053190491996E-3},{"$f":"U5463*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83104903290291976},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3421046908367454E-2}]
["Single Family Attached",15463,"Pacific","1950s","Stucco","built-in furnace","N/A",37.835533691235845,20040.007249999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20040.007249999999},"Hot-Dry/Mixed-Dry",74.794156745151199,"Metropolitan Area",0.1509449017282905,0.54362002618885052,0,0,0.32482402863364052,1.0193889565507814,0,0,{"$f":"T5464*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5464*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1509449017282905},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15464,"East North Central","Before 1950","Siding","central furnace","both central and individual units",101.21871644750071,28400.313259999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":28400.313259999999},"Cold/Very Cold",159.02201602078367,"Metropolitan Area",2.2891648202542894,0.28207918177851449,0.10250172901047377,4.9656385717880697E-2,0.51426347200839095,3.1880092030516685,1559.1579999999999,189.28700000000001,{"$f":"T5465*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4280575621835072E-2},{"$f":"U5465*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3758100960456202E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.3334453958761245},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1078775391065194}]
["Single Family Detached",15465,"Pacific","1960s","Wood","central furnace","central AC",25.488620628394443,11238.36888,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11238.36888},"Hot-Dry/Mixed-Dry",139.4439504010324,"Metropolitan Area",0.10819698057255143,0.23409784231034905,0.13972076261811575,8.5492294976558404E-3,0.3394915016727354,0.82150708717375176,163.065,597.65300000000002,{"$f":"T5466*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8325846214172E-3},{"$f":"U5466*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7166448762386406E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11002956519396863},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14643740749435438}]
["Single Family Detached",15466,"Pacific","1970s","Wood","built-in furnace","N/A",41.169887956507026,22472.646260000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22472.646260000001},"Hot-Dry/Mixed-Dry",128.75615033907027,"Metropolitan Area",0.28069593646930563,0.37189173280408638,0,0,0.78840047771160693,1.440988146984999,0,0,{"$f":"T5467*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5467*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28069593646930563},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15467,"Pacific","2000s","Stucco","central furnace","window/wall unit",67.355828557542026,20712.124400000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20712.124400000001},"Hot-Dry/Mixed-Dry",127.92704866086869,"Metropolitan Area",0.18130875896650001,0.31535280215831485,0.19592627862542683,5.7284350938056E-3,0.30206804556815492,0.99465588531839644,276.57400000000001,0,{"$f":"T5468*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7284350938056E-3},{"$f":"U5468*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18703719406030561},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19592627862542683}]
["Single Family Attached",15468,"South Atlantic","1980s","Siding","central furnace","central AC",24.823464641440747,12697.424370000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12697.424370000001},"Mixed-Humid",118.01339196967807,"Metropolitan Area",0.30453436582401278,0.16711916973622984,8.6497813308318225E-2,1.17423241088886E-2,0.30866758061523769,0.86681892948379857,590.38,334.4,{"$f":"T5469*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4963053995606007E-3},{"$f":"U5469*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2460187093279998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31203067122357336},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0743832017646228E-2}]
["Multi-Family (5+ units)",15469,"West North Central","1980s","Stucco","central furnace","central AC",7.9439980870352347,11981.897569999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":953.05729634028887},"Mixed-Humid",177.92502017715913,"Metropolitan Area",0.11407770925054361,0.30800229752370445,1.9841121976502646E-2,2.5661270568741899E-3,0.16279703580419416,0.60708017818983373,143.803,70.364000000000004,{"$f":"T5470*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3705249838562254E-4},{"$f":"U5470*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7060923599688088E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11421476174892924},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.9908182900102333E-2}]
["Single Family Detached",15470,"South Atlantic","1970s","Stucco","central furnace","central AC",86.691523971119807,20188.99021,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20188.99021},"Mixed-Humid",363.72093099861303,"Metropolitan Area",1.140659877718762,0.33363267317958994,0.69058106604997327,5.326009053723596E-2,0.55189727975820491,2.7167708967065303,996.24300000000005,1641.8330000000001,{"$f":"T5471*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0113140173781029E-2},{"$f":"U5471*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3146950363454927E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1607730178925431},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.72372801641342821}]
["Single Family Detached",15471,"South Atlantic","2000s","Wood","heat pump","N/A",14.828287699432115,11768.4823,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11768.4823},"Mixed-Humid",137.50826656048014,"Rural",0.14507083449496719,0.15006017671391061,0,2.3209212367945003E-3,0.17404717984554494,0.46917819105442271,197.215,0,{"$f":"T5472*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3209212367945003E-3},{"$f":"U5472*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.14739175573176169},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15472,"West North Central","2000s","Siding","central furnace","central AC",20.456854308091394,20518.409540000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1632.0636866698896},"Cold/Very Cold",125.9830345553472,"Metropolitan Area",0.12064178050427686,0.1410510363974421,2.203285936981831E-2,3.0932117933836199E-3,0.28433886669247782,0.57091171626044213,102.86199999999999,47.890999999999998,{"$f":"T5473*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6787733493823817E-4},{"$f":"U5473*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8161162018307691E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1208096578392151},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.2111020531836618E-2}]
["Single Family Detached",15473,"East North Central","Before 1950","Siding","central furnace","both central and individual units",175.34304519727158,35124.808729999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35124.808729999997},"Mixed-Humid",549.53247985808321,"Micropolitan Area",0.91625690907897994,0.68112409835533549,0.80135853150107539,0.12119745002669038,1.2158334171284075,3.6145729560637982,2338.5839999999998,1111.896,{"$f":"T5474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2142315699038307E-2},{"$f":"U5474*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9055134327652077E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.99839922477801823},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.84041366582872745}]
["Single Family Detached",15474,"East North Central","1980s","Siding","built-in electric unit","window/wall unit",12.470390440867051,16195.312260000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16195.312260000001},"Cold/Very Cold",354.62253357628123,"Metropolitan Area",0.62239119460484593,0.22272935189466331,4.2569248712911928E-2,0,0.32228230884906528,1.2099721040614866,0,0,{"$f":"T5475*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5475*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62239119460484593},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.2569248712911928E-2}]
["Multi-Family (5+ units)",15475,"Middle Atlantic","1960s","Stone","heater burning gas/oil/kerosene","window/wall unit",22.101936197802832,22235.348290000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1768.6314542957712},"Cold/Very Cold",112.08839071742864,"Metropolitan Area",0.32318473938041514,0.28559234767579206,8.6201909309278846E-2,0,0.29622384593043111,0.99120284229591715,0,0,{"$f":"T5476*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5476*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.32318473938041514},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.6201909309278846E-2}]
["Multi-Family (5+ units)",15476,"East North Central","1950s","Brick","central furnace","N/A",19.541566986637044,18010.660820000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1432.5937612243476},"Cold/Very Cold",45.584982528274985,"Metropolitan Area",0.52945202411871994,0.19909949841847954,0,1.0308888008169139E-2,0.21466980475067365,0.95271023157677404,572.37699999999995,0,{"$f":"T5477*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.1998371926830836E-4},{"$f":"U5477*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53027200783798822},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15477,"Pacific","1980s","Stucco","central furnace","central AC",13.166847876469516,23596.50157,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1876.8995359884038},"Hot-Dry/Mixed-Dry",62.47414475167821,"Metropolitan Area",7.6763103341699362E-2,0.29061028956233897,1.4267738890557794E-2,1.8033626324872501E-3,0.19713867131467802,0.58043972369472352,50.868000000000002,25.556999999999999,{"$f":"T5478*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5474125596658143E-5},{"$f":"U5478*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.796792144125563E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":7.6858577467296019E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.4315706811999051E-2}]
["Single Family Detached",15478,"West North Central","Before 1950","Wood","heater burning gas/oil/kerosene","N/A",15.04378769607858,16351.943149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16351.943149999999},"Cold/Very Cold",106.05870325735398,"Rural",1.1406679598635621,0.59489162248942773,0,0,0.4663952406825061,2.2019548230354959,0,0,{"$f":"T5479*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5479*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1406679598635621},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15479,"Mountain South","1980s","Stucco","central furnace","N/A",30.204957633591693,14542.58914,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14542.58914},"Cold/Very Cold",177.62972786115748,"Metropolitan Area",0.81487951258370572,0.38762382800473549,6.914429612316797E-2,1.232901801923318E-2,0.52459931170726393,1.7962469484188732,847.78700000000003,0,{"$f":"T5480*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.232901801923318E-2},{"$f":"U5480*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.82720853060293886},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.914429612316797E-2}]
["Single Family Attached",15480,"East South Central","1980s","Brick","central furnace","central AC",17.603245278707973,6770.4789529999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6770.4789529999998},"Mixed-Humid",54.132321817744874,"Metropolitan Area",0.12735469285626322,5.3742768767433981E-2,3.2477026129529671E-2,3.6971419009068042E-3,0.14999923676246707,0.36357372451569392,328.36900000000003,217.69900000000001,{"$f":"T5481*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2232154033176572E-3},{"$f":"U5481*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4739264975891469E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12957790825958088},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3950952627118815E-2}]
["Single Family Detached",15481,"South Atlantic","2000s","Siding","heat pump","central AC",27.153550361319869,11262.36017,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11262.36017},"Mixed-Humid",159.80933185616541,"Micropolitan Area",0.21707407483755051,0.10583477487548587,0.10847932345408408,8.9922062305331004E-3,0.17264336570056987,0.60403153886769034,285.74200000000002,512.68799999999999,{"$f":"T5482*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2181293196961399E-3},{"$f":"U5482*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7740769108369601E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22029220415724665},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11425340036492104}]
["Single Family Detached",15482,"East South Central","1970s","Brick","central furnace","central AC",24.47373617481588,10436.56127,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10436.56127},"Hot-Humid",260.91167305160832,"Metropolitan Area",0.28674954087922089,0.1249213594117793,0.20481041806208639,1.6222256868127359E-2,0.27374932182573558,0.89023064017882203,492.56,1061.808,{"$f":"T5483*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1406326191511999E-3},{"$f":"U5483*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1081624248976159E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2918901734983721},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21589204231106254}]
["Multi-Family (5+ units)",15483,"New England","1990s","Brick","built-in electric unit","central AC",72.059798065455823,55133.739909999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4385.4166494725996},"Cold/Very Cold",432.94491518174334,"Metropolitan Area",0.29101175776207405,0.54263067889341265,4.2931227411744273E-2,2.0054897892262499E-3,0.59878836262102131,1.4772079969468541,0,36.375,{"$f":"T5484*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5484*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5951953062456583E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.29101175776207405},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.3090746942368842E-2}]
["Single Family Detached",15484,"West North Central","1990s","Siding","central furnace","central AC",44.674981632821158,14031.0872,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14031.0872},"Cold/Very Cold",200.37071620847877,"Rural",0.60708558950918312,0.26250215233187918,2.3960480709911199E-2,2.2871752529714399E-2,0.37563761464291956,1.2691858371938929,1536.9179999999999,93.159000000000006,{"$f":"T5485*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1564630477249599E-2},{"$f":"U5485*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3071220524648003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62865021998643267},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5267602762375999E-2}]
["Multi-Family (5+ units)",15485,"Middle Atlantic","2000s","Wood","built-in electric unit","central AC",9.4358892931880831,12665.62321,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1007.4418131574305},"Mixed-Humid",58.996472923047108,"Metropolitan Area",0.11507077123421842,8.4314369765316644E-2,1.2271286545271152E-2,5.2938505330836993E-4,7.3452749265986592E-2,0.28559645381863663,0,41.796999999999997,{"$f":"T5486*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5486*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2108045464541112E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11507077123421842},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2313394590735693E-2}]
["Single Family Detached",15486,"Pacific","Before 1950","Siding","heat pump","central AC",11.84001427277186,14527.62487,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14527.62487},"Hot-Dry/Mixed-Dry",68.881120776396926,"Metropolitan Area",1.203542535117637E-2,0.13925354578526897,3.3885583315900906E-2,1.7375765725763498E-3,0.18910138598233217,0.37427594043467838,20.405999999999999,99.198999999999998,{"$f":"T5487*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.9645071309722002E-4},{"$f":"U5487*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4411258594791299E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.233187606427359E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.5326709175380035E-2}]
["Single Family Detached",15487,"West South Central","1960s","Brick","central furnace","central AC",61.780958942616827,33073.318489999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33073.318489999998},"Hot-Humid",260.65082303359918,"Metropolitan Area",0.84072620344136806,0.75379328345026952,0.34289907281327253,3.3563167410155387E-2,0.66261933875588008,2.6000378984607901,499.58199999999999,515.22900000000004,{"$f":"T5488*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.652283459787118E-2},{"$f":"U5488*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.704033281228421E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.85724903803923924},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.35993940562555676}]
["Single Family Detached",15488,"Pacific","1950s","Stucco","central furnace","N/A",21.190438931440134,17340.78472,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17340.78472},"Marine",81.087226102183536,"Metropolitan Area",0.10898147366272153,0.18144854364446264,0,5.0151110080864803E-3,0.33156934699926632,0.62199936430645053,289.209,0,{"$f":"T5489*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0151110080864803E-3},{"$f":"U5489*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.113996584670808},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15489,"South Atlantic","1980s","Brick","radiator","central AC",33.001776312482271,26678.881420000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2122.0764446518606},"Mixed-Humid",262.30676208918811,"Metropolitan Area",0.61419006835459944,0.19790973169082815,4.1988643573973077E-2,3.19063414454348E-3,0.65206427674572542,1.5090895668993478,45.68,73.914000000000001,{"$f":"T5490*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6936451991696981E-5},{"$f":"U5490*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5685115832999761E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.61428700480659115},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.2145494732303071E-2}]
["Single Family Detached",15490,"East North Central","1960s","Siding","central furnace","central AC",60.684254178577525,27483.81077,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27483.81077},"Cold/Very Cold",151.038876143621,"Metropolitan Area",2.4596536957216513,0.44896159844665962,0.12075669124876905,4.9309254578672398E-2,0.39159491506454658,3.4209669004816265,1569.671,224.44900000000001,{"$f":"T5491*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.314054073515667E-2},{"$f":"U5491*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1687138435157305E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5027942364568081},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12692540509228478}]
["Single Family Detached",15491,"Pacific","1960s","Stucco","central furnace","N/A",29.435216067974984,18808.444769999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18808.444769999998},"Hot-Dry/Mixed-Dry",81.179109671419027,"Metropolitan Area",0.19542267527768409,0.23252626355146602,0,1.80421887300702E-3,0.47109137327368078,0.89904031210283086,95.926000000000002,0,{"$f":"T5492*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.80421887300702E-3},{"$f":"U5492*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19722689415069111},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15492,"Middle Atlantic","1990s","Brick","central furnace","central AC",91.073987840971043,16510.875240000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16510.875240000001},"Cold/Very Cold",251.57206184951553,"Metropolitan Area",1.8379433280592374,0.24870985204671509,6.9971950016728443E-2,3.3831988660652519E-2,0.4788129053287139,2.6354380354513949,1755.297,293.77600000000001,{"$f":"T5493*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8981489776146282E-2},{"$f":"U5493*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8504988845062408E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8669248178353837},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4822448901234684E-2}]
["Single Family Detached",15493,"West South Central","1950s","Brick","central furnace","central AC",49.185219603911705,23669.499329999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23669.499329999999},"Hot-Humid",182.4568326305895,"Metropolitan Area",0.8086880192853958,0.1281095082586719,0.39689314712235552,3.2409296271107182E-2,0.2286709856881311,1.5623616603545545,466.94299999999998,902.3,{"$f":"T5494*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1052307025648189E-2},{"$f":"U5494*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1356989245458997E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.81974032631104399},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4182501363678145}]
["Single Family Detached",15494,"East North Central","1990s","Siding","central furnace","central AC",72.924690336640893,14053.707909999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14053.707909999999},"Cold/Very Cold",133.24319062574716,"Metropolitan Area",0.7391842522056451,0.41036848177761864,6.3652250617882725E-2,4.9337579405701951E-2,0.34507686613203453,1.558281850733181,3265.8040000000001,244.84100000000001,{"$f":"T5495*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.589665550730964E-2},{"$f":"U5495*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.44092389839231E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.78508090771295469},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.7093174516275028E-2}]
["Single Family Detached",15495,"Pacific","Before 1950","Siding","heat pump","central AC",65.155090908980611,24158.357769999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24158.357769999999},"Marine",482.09416196399326,"Metropolitan Area",0.86712997144447435,0.28408916938693091,6.6316600588913824E-2,2.047411157664392E-2,0.42736953863458421,1.6449052800549033,699.12400000000002,148.37200000000001,{"$f":"T5496*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6889687717593482E-2},{"$f":"U5496*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5844238590504399E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88401965916206782},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9901024447964269E-2}]
["Multi-Family (5+ units)",15496,"Middle Atlantic","1980s","Brick","radiator","window/wall unit",17.422837517938003,25360.7533,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2017.230645817569},"Mixed-Humid",52.237775320812936,"Metropolitan Area",0.28252967020977121,0.69600540819058687,2.8574214350643001E-2,1.3301715105850001E-3,0.19049729841295004,1.1988309589271631,52.45,0,{"$f":"T5497*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.058037473731315E-4},{"$f":"U5497*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.28263547395714433},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8574214350643001E-2}]
["Single Family Attached",15497,"West South Central","1990s","Siding","central furnace","central AC",20.09606031952071,19139.105070000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19139.105070000001},"Hot-Humid",329.1747120755785,"Metropolitan Area",0.22186950135082292,0.27222125228123606,0.12409129686531564,9.1708849763919003E-3,0.50496203325929001,1.1231440837566644,192.357,286.81299999999999,{"$f":"T5498*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6815408339499903E-3},{"$f":"U5498*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.48934414244191E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22555104218477293},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12958064100775754}]
["Multi-Family (5+ units)",15498,"South Atlantic","1980s","Shingle","N/A","central AC",19.665646048800728,25673.167170000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2042.0804925586147},"Hot-Humid",190.75394262497886,"Metropolitan Area",0,0.13208022967615562,0.30603710055234645,1.301914547674587E-2,0.20075153607115245,0.65085245029573846,0,507.11099999999999,{"$f":"T5499*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5499*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0355614806618915E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30707266203300837}]
["Single Family Detached",15499,"Mountain North","2000s","Siding","central furnace","central AC",61.807347106721544,8939.4485260000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8939.4485260000001},"Cold/Very Cold",54.646732624801331,"Metropolitan Area",0.47681720429758023,0.14062396171691871,2.5994226757836587E-2,1.3919096811820091E-2,0.18421915807208192,0.82765455084441752,1325.8219999999999,231.22,{"$f":"T5500*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1852117523638371E-2},{"$f":"U5500*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0669792881817203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.48866932182121858},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8061206046018309E-2}]
["Single Family Detached",15500,"Pacific","2000s","Stucco","N/A","central AC",87.839264523228394,14615.51822,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14615.51822},"Hot-Dry/Mixed-Dry",212.94031044516586,"Metropolitan Area",0,0.74697155674131888,0.15423205372529106,9.6362450107375201E-3,0.61346442477613361,1.5146680352427435,0,659.31600000000003,{"$f":"T5501*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5501*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6362450107375201E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16386829873602857}]
["Mobile Home",15501,"Mountain North","1960s","Brick","central furnace","central AC",20.779688905647081,17102.624609999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17102.624609999999},"Cold/Very Cold",94.834053482973715,"Metropolitan Area",0.40376849318628305,0.2714259895866577,0.11054832121185941,1.4751646523235568E-2,0.20989225127084338,0.99563505525564344,642.73599999999999,219.80099999999999,{"$f":"T5502*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0992472531332958E-2},{"$f":"U5502*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7591739919026093E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.414760965717616},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11430749520376202}]
["Single Family Detached",15502,"West North Central","1980s","Wood","central furnace","central AC",42.356425143191466,11386.13579,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11386.13579},"Mixed-Humid",127.17509817561762,"Metropolitan Area",1.0563061637693953,0.11080859826107153,9.7484280278490348E-2,1.9935518323143608E-2,0.33065400957906793,1.5952530518880255,1295.229,455.63,{"$f":"T5503*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.474765327314591E-2},{"$f":"U5503*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1878650499977003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0710538170425412},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10267214532848805}]
["Single Family Detached",15503,"Pacific","1960s","Siding","central furnace","central AC",51.932998285236245,20907.004140000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20907.004140000001},"Cold/Very Cold",149.53642720741857,"Metropolitan Area",1.2889777073340598,0.34892169616839147,0.11472484363378634,5.4026395701294055E-2,0.34729651110857296,2.0999207582448105,2305.3009999999999,278.82799999999997,{"$f":"T5504*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8196937550946138E-2},{"$f":"U5504*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8294581503479199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3371746448850059},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12055430178413426}]
["Single Family Detached",15504,"East North Central","Before 1950","Brick","central furnace","central AC",151.68079244174126,31859.019629999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31859.019629999999},"Cold/Very Cold",422.26320549387668,"Metropolitan Area",4.9878810236400781,0.27242102896377324,0.13855184976400514,7.1789267011103469E-2,1.0587055202325668,6.4575594226004238,1961.653,291.68900000000002,{"$f":"T5505*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2496341434248391E-2},{"$f":"U5505*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.2929255768550711E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.0503773650743264},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14784477534086021}]
["Multi-Family (2-4 units)",15505,"Pacific","1970s","Wood","N/A","N/A",16.763851366334162,19357.796040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6452.5986800000001},"Hot-Dry/Mixed-Dry",55.196567962930096,"Metropolitan Area",0,0.2538654738732592,0,0,0.18833064262743723,0.4421961165006964,0,0,{"$f":"T5506*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5506*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",15506,"South Atlantic","1990s","Siding","portable electric heaters","window/wall unit",47.51598471943668,45688.44685,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":45688.44685},"Mixed-Humid",566.03416797028945,"Metropolitan Area",0.290184687554153,0.88974384997771494,0.16230176536361915,0,0.58902034545401283,1.9312506483495,0,0,{"$f":"T5507*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5507*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.290184687554153},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.16230176536361915}]
["Single Family Detached",15507,"Mountain South","2000s","Stucco","central furnace","central AC",43.558537556976411,10001.9604,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10001.9604},"Cold/Very Cold",88.161249774190637,"Metropolitan Area",1.205119405302528,0.19053376491817681,9.0988903968562795E-2,2.4468325830421203E-2,0.19085887864097859,1.6775009528302463,1895.4690000000001,550.88400000000001,{"$f":"T5508*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.89584058774276E-2},{"$f":"U5508*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.5099199529936001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.2240778111799557},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.6498823921556398E-2}]
["Multi-Family (5+ units)",15508,"Middle Atlantic","1960s","Brick","radiator","N/A",18.952471958038103,35491.520519999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2823.0463824435014},"Mixed-Humid",196.16163391774643,"Metropolitan Area",0.43876499292329491,0.88523060504697604,0,3.8851502767628401E-3,0.81786801852370072,2.1454397363523876,109.467,0,{"$f":"T5509*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0903041834694277E-4},{"$f":"U5509*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43907402334164186},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15509,"East North Central","1970s","Siding","central furnace","central AC",61.097018300996091,18237.91591,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18237.91591},"Cold/Very Cold",110.74055245838061,"Metropolitan Area",1.4611535034762011,0.38656544896733475,6.1290048400491438E-2,2.3249786391647553E-2,0.36920061856777836,2.2782096194118058,1072.02,202.785,{"$f":"T5510*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9551410613838201E-2},{"$f":"U5510*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6983757778093498E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4807049140900392},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.4988424178300794E-2}]
["Single Family Attached",15510,"Mountain North","2000s","Wood","radiator","N/A",26.022281368464832,14424.76794,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14424.76794},"Cold/Very Cold",109.4357378356267,"Rural",0.66026856680867674,0.29706495476070666,0,1.4712686308082398E-3,0.40691077430431366,1.3642442958736971,101.996,0,{"$f":"T5511*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4712686308082398E-3},{"$f":"U5511*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.661739835439485},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",15511,"South Atlantic","1970s","Brick","central furnace","central AC",13.743651443701829,31306.723109999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10435.57437},"Mixed-Humid",161.73053156757095,"Metropolitan Area",0.26853765431921922,0.27020503995648348,9.5774967447375056E-2,8.8741724260374896E-3,0.44849228859308243,1.088926065266852,162.09399999999999,121.36499999999999,{"$f":"T5512*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6915439919307799E-3},{"$f":"U5512*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2665134834150499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27022919831115},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.7041480930790111E-2}]
["Single Family Detached",15512,"South Atlantic","2000s","Stucco","heat pump","central AC",29.797386192821708,15917.407149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15917.407149999999},"Hot-Humid",200.54552975198948,"Metropolitan Area",3.0342191279323052E-2,9.9728763583538507E-2,0.25304374893347353,1.3886123153959899E-2,0.30114666269780238,0.68426136649413738,48.802999999999997,823.58299999999997,{"$f":"T5513*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7681722114144984E-4},{"$f":"U5513*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3109305932818447E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.1119008500464503E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26615305486629198}]
["Single Family Detached",15513,"Middle Atlantic","Before 1950","Shingle","central furnace","N/A",94.396499454009401,45492.288890000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":45492.288890000003},"Cold/Very Cold",285.66382395494554,"Metropolitan Area",1.5819475800767713,0.21366677219759644,0,7.3804278403824836E-2,0.68721393121542884,2.4828282834897966,1622.347,0,{"$f":"T5514*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3804278403824836E-2},{"$f":"U5514*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6557518584805961},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15514,"Pacific","1970s","Stucco","central furnace","central AC",22.691419907676195,22601.01584,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1797.7171750279319},"Hot-Dry/Mixed-Dry",139.16860278926748,"Metropolitan Area",0.3059530903509371,0.60130990306712206,8.5366699829051013E-2,7.3716829324694394E-3,0.3824058882644874,1.3818209102239569,158.74600000000001,167.42,{"$f":"T5515*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.853804106669841E-4},{"$f":"U5515*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0097380944317634E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.3062384707616041},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.5667673638494188E-2}]
["Multi-Family (5+ units)",15515,"Pacific","1970s","Stucco","built-in electric unit","N/A",7.3139316487724582,12169.60341,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":967.98768773552115},"Hot-Dry/Mixed-Dry",35.937629890819032,"Metropolitan Area",1.040350188472716E-2,0.10612593925716075,0,0,0.11221566965154178,0.22874511079342971,0,0,{"$f":"T5516*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5516*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.040350188472716E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15516,"Pacific","1990s","Siding","built-in electric unit","window/wall unit",16.356521534611399,29000.924709999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2306.7750941790832},"Cold/Very Cold",204.60274184501398,"Micropolitan Area",9.2735589923898673E-2,0.14299436645187694,8.4000308394773689E-3,0,0.45397461722354854,0.69810460443880151,0,0,{"$f":"T5517*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5517*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.2735589923898673E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.4000308394773689E-3}]
["Multi-Family (5+ units)",15517,"Mountain North","1960s","Siding","radiator","N/A",6.7031071861193707,12459.30704,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":991.03112945539283},"Cold/Very Cold",89.09650462442309,"Metropolitan Area",8.6949882430565811E-2,0.11877786326937854,0,7.7212817588287995E-4,9.7568634081327349E-2,0.30400709177599994,61.972000000000001,0,{"$f":"T5518*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1416181154609606E-5},{"$f":"U5518*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.7011298611720425E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15518,"Middle Atlantic","1970s","Brick","heat pump","central AC",36.477771331572619,14338.746590000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14338.746590000001},"Cold/Very Cold",311.6401107868773,"Metropolitan Area",0.53576630563932848,0.15292409456327605,6.3039281331927113E-2,1.3240642359898028E-2,0.56936019655637493,1.3210898780909064,694.41099999999994,229.006,{"$f":"T5519*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9569833583084896E-3},{"$f":"U5519*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2836590015895401E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.545723288997637},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6322940333516656E-2}]
["Single Family Detached",15519,"West South Central","1990s","Brick","central furnace","central AC",103.7568097197215,33191.557809999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":33191.557809999998},"Hot-Humid",697.71688228810933,"Metropolitan Area",1.4208293887863372,0.44338703521272266,1.0551287214395788,8.6769503193133229E-2,1.3007388143246292,4.2200839597632687,745.44500000000005,1868.759,{"$f":"T5520*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4742480811675453E-2},{"$f":"U5520*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.202702238145779E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4455718695980126},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.1171557438210367}]
["Single Family Detached",15520,"West South Central","1950s","Siding","central furnace","central AC",38.151852000105386,22389.584510000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22389.584510000001},"Hot-Humid",195.23717690194778,"Metropolitan Area",0.15221124671184005,0.1798796683409318,0.47778636727009621,2.8632114125571144E-2,0.23654757239823485,1.0464248547211028,290.95499999999998,987.85900000000004,{"$f":"T5521*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5143615611070495E-3},{"$f":"U5521*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2117752564464091E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1587256082729471},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.49990411983456029}]
["Single Family Detached",15521,"East North Central","1960s","Siding","radiator","central AC",43.098234643203767,19697.54783,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19697.54783},"Mixed-Humid",280.24727534237167,"Rural",1.802543560114191,0.44751774850951093,0.28984360554184008,1.8609514380514287E-2,0.66197259438327938,3.2018775085488209,222.74299999999999,722.02,{"$f":"T5522*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.3874908962976897E-3},{"$f":"U5522*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4222023484216599E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.8069310510104888},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.30406562902605666}]
["Single Family Detached",15522,"South Atlantic","1970s","Siding","central furnace","central AC",125.9098329690547,27223.747670000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27223.747670000001},"Mixed-Humid",313.9486683658551,"Metropolitan Area",0.48875578235883899,0.16080044135756608,0.2271138426994983,2.0189349062053361E-2,1.437829665274164,2.3144997316900673,272.822,468.786,{"$f":"T5523*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.4272372868247408E-3},{"$f":"U5523*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2762111775228619E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.49618301964566375},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.23987595447472693}]
["Multi-Family (5+ units)",15523,"Pacific","Before 1950","Wood","radiator","central AC",11.791382906743285,40942.301760000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3256.6093303144348},"Hot-Dry/Mixed-Dry",74.433104598816996,"Metropolitan Area",0.11286480431612522,0.3295478622503808,6.9196004252314453E-2,5.6369770486185593E-3,0.17930767034625708,0.69610494498448905,71.201999999999998,66.478999999999999,{"$f":"T5524*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3187709753704839E-4},{"$f":"U5524*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1649613166997331E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11309668141366228},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.941250038398443E-2}]
["Single Family Attached",15524,"South Atlantic","1980s","Brick","central furnace","N/A",25.812772039411659,11203.46009,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11203.46009},"Mixed-Humid",73.776039457462758,"Metropolitan Area",0.39422007139786153,0.28472206830375857,7.1860169380569439E-2,9.0445197202767297E-3,0.1898075643949684,0.94060987347715785,807.29700000000003,0,{"$f":"T5525*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.0445197202767297E-3},{"$f":"U5525*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.40326459111813828},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.1860169380569439E-2}]
["Multi-Family (5+ units)",15525,"West North Central","1990s","Brick","radiator","central AC",17.981672935348108,15136.08833,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1203.9461476516026},"Cold/Very Cold",83.399846695090986,"Micropolitan Area",0.19554049719714869,0.43447239440400531,1.0654738877937818E-2,1.3194582279910901E-3,0.27260733825257527,0.91448947536212899,55.435000000000002,31.738,{"$f":"T5526*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.6740754695066587E-5},{"$f":"U5526*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8210842834166563E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.19560723795184376},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0692949720771986E-2}]
["Multi-Family (5+ units)",15526,"Middle Atlantic","1960s","Brick","radiator","N/A",16.468065521591157,35491.520519999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2823.0463824435014},"Mixed-Humid",91.426156861247463,"Metropolitan Area",0.52535993503949963,0.39802427076920754,0,5.1072652943485201E-3,0.3947176322769208,1.3228028641824965,143.90100000000001,0,{"$f":"T5527*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0623919748000232E-4},{"$f":"U5527*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52576617423697958},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15527,"West South Central","1980s","Brick","built-in electric unit","central AC",19.183992525430831,28462.896919999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2263.9795930576911},"Hot-Humid",302.80659909900152,"Metropolitan Area",0.31480368166656264,0.21205208299032113,0.18442666982943304,7.7474297642424802E-3,0.31476249585471949,1.0331761184439261,0,272.19400000000002,{"$f":"T5528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5528*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1624166135274526E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.31480368166656264},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18504291149078578}]
["Single Family Detached",15528,"South Atlantic","2000s","Brick","central furnace","central AC",62.799763281221061,20076.650669999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20076.650669999999},"Mixed-Humid",198.51031272839842,"Metropolitan Area",1.1349466141143021,0.25199822433961,0.13000010757522662,1.6634850215689889E-2,0.59883254352574944,2.1157774895548886,444.58199999999999,383.98500000000001,{"$f":"T5529*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9257175081699398E-3},{"$f":"U5529*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.7091327075199502E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1438723316224719},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13770924028274656}]
["Single Family Detached",15529,"South Atlantic","Before 1950","Siding","central furnace","central AC",105.92721307794848,48881.962659999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":48881.962659999997},"Cold/Very Cold",582.75071719332709,"Micropolitan Area",3.0966249190072195,1.4222845923178966,0.39627013576479275,0.15699111991147441,1.660843283569458,6.5760229306593665,2818.5949999999998,393.04199999999997,{"$f":"T5530*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.13777845554366269},{"$f":"U5530*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9212664367811716E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2344033745508822},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.41548280013260447}]
["Multi-Family (2-4 units)",15530,"East South Central","1970s","Siding","central furnace","central AC",9.8896256547212609,14128.03665,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4709.34555},"Mixed-Humid",145.44422384149857,"Metropolitan Area",0.33377543568706158,0.10996404743731679,4.4144741167977453E-2,5.0841011408323498E-3,0.65013822632074669,1.1414118513736575,229.77099999999999,130.08799999999999,{"$f":"T5531*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0820710363690499E-3},{"$f":"U5531*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1262934390839997E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.33485750672343062},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.4757370511885851E-2}]
["Single Family Detached",15531,"Mountain South","2000s","Stucco","central furnace","central AC",26.136702441631815,10118.73885,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10118.73885},"Hot-Dry/Mixed-Dry",205.55728220587244,"Metropolitan Area",0.26852307756013083,0.14953090796075352,0.29469646043801201,2.1935493147679654E-2,0.43673834811353673,1.149488794072433,630.99099999999999,1536.818,{"$f":"T5532*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.3848331457003497E-3},{"$f":"U5532*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.55506600019793E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2749079107058312},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31024712043999131}]
["Single Family Detached",15532,"East North Central","2000s","Siding","central furnace","central AC",79.859779827960054,21867.409589999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21867.409589999999},"Cold/Very Cold",268.35685050622288,"Metropolitan Area",1.7352646274772736,0.38936278554389581,8.6473949599138525E-2,5.4938455278978962E-2,0.77881105079187962,2.9899124134121871,2302.4479999999999,209.89599999999999,{"$f":"T5533*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0348573475676311E-2},{"$f":"U5533*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5898818033026393E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.78561320095295},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.1063831402441162E-2}]
["Multi-Family (2-4 units)",15533,"East South Central","Before 1950","Siding","heater burning gas/oil/kerosene","central AC",5.1964902224735177,9396.9081779999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3132.3027259999999},"Mixed-Humid",22.890257522750506,"Micropolitan Area",0.10977844009866719,1.0991178222571302E-2,8.4929256112764012E-3,3.8376033308134199E-4,5.8361621940717263E-2,0.18788000609528638,0,40.838999999999999,{"$f":"T5534*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5534*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.27920111027114E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.10977844009866719},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.6208457223035159E-3}]
["Single Family Detached",15534,"West South Central","2000s","Brick","central furnace","central AC",52.061385825745262,16870.183349999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16870.183349999999},"Hot-Humid",345.1844149240942,"Metropolitan Area",0.35398427365279728,0.27461795623685503,0.42737051595556486,3.5314253585454897E-2,0.4657091885312743,1.5216819343764916,597.005,1496.289,{"$f":"T5535*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0071583810866749E-2},{"$f":"U5535*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5242669774588149E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36405585746366403},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.45261318573015302}]
["Single Family Detached",15535,"East North Central","1970s","Siding","built-in electric unit","window/wall unit",37.867853163063614,32588.513910000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":32588.513910000001},"Cold/Very Cold",148.48822750044721,"Metropolitan Area",3.7214192751413216E-2,0.15348303644031649,2.0475591409250371E-2,0,0.29546900811575455,0.50664182871673469,0,0,{"$f":"T5536*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5536*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.7214192751413216E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.0475591409250371E-2}]
["Single Family Detached",15536,"West South Central","1990s","Wood","heat pump","central AC",42.127532553165999,18244.925319999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18244.925319999998},"Hot-Humid",157.17995861212424,"Rural",0.26663790679959515,0.10664990818134591,0.1736235624952551,1.2381115791703919E-2,0.34115970565749226,0.88807108313368843,134.01599999999999,544.59,{"$f":"T5537*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.44511191168512E-3},{"$f":"U5537*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9360038800187997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26908301871128026},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1835595663752739}]
["Single Family Detached",15537,"East South Central","1960s","Brick","central furnace","central AC",14.411307885839628,13356.17042,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13356.17042},"Mixed-Humid",67.475105850884219,"Rural",0.28299012481767705,0.10065722905456129,8.828220291361448E-2,7.4897129740825602E-3,0.13838611322974889,0.61031567001560172,266.30200000000002,294.46600000000001,{"$f":"T5538*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5567748951868404E-3},{"$f":"U5538*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9329380788957202E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.2865468997128639},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.22151409925102E-2}]
["Single Family Detached",15538,"Pacific","2000s","Stucco","central furnace","central AC",22.020935128624917,15062.199130000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15062.199130000001},"Hot-Dry/Mixed-Dry",123.1284621785984,"Metropolitan Area",0.26144046455707076,0.3384234396214964,0.10447181984505652,8.9529259762746102E-3,0.42339290477941821,1.1277286288030419,274.40199999999999,319.995,{"$f":"T5539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1330975656702603E-3},{"$f":"U5539*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.81982841060435E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26557356212274102},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10929164825566087}]
["Multi-Family (5+ units)",15539,"East North Central","1980s","Brick","central furnace","central AC",19.16459794986315,15670.153679999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1246.4264706193469},"Cold/Very Cold",72.176727847154254,"Metropolitan Area",0.56357353445206793,0.11460659925741816,1.6407138281380476E-2,5.2110155853619198E-3,0.11012289818495966,0.80950669411694254,284.52999999999997,48.014000000000003,{"$f":"T5540*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.5464572368532272E-4},{"$f":"U5540*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.9845920560317326E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5639281801757533},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6466984201940794E-2}]
["Single Family Detached",15540,"South Atlantic","1970s","Siding","built-in electric unit","window/wall unit",33.8904321129016,26664.384040000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26664.384040000001},"Mixed-Humid",514.0626598777576,"Metropolitan Area",0.55798172684574832,0.23846158629852304,0.13565033420752493,0,0.82188814825143375,1.75398179560323,0,0,{"$f":"T5541*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5541*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55798172684574832},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13565033420752493}]
["Multi-Family (5+ units)",15541,"Pacific","1950s","Stucco","N/A","N/A",9.7435679377386553,22044.271349999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1753.4329207775634},"Hot-Dry/Mixed-Dry",78.319063614799546,"Metropolitan Area",0,0.37479081567224953,0,0,0.30284664672041989,0.67763746239266942,0,0,{"$f":"T5542*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5542*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15542,"Pacific","1980s","Wood","built-in electric unit","window/wall unit",10.016518972580588,15017.26982,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1194.4951531631075},"Cold/Very Cold",173.8284873398122,"Metropolitan Area",0.17160387399466165,0.31934557655620005,7.1882564756601203E-3,0,9.4965099609749262E-2,0.59310280663627113,0,0,{"$f":"T5543*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5543*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.17160387399466165},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.1882564756601203E-3}]
["Single Family Detached",15543,"Middle Atlantic","1960s","Siding","central furnace","window/wall unit",77.839992636657129,29596.955379999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29596.955379999999},"Mixed-Humid",244.06916152042706,"Metropolitan Area",2.8158496881312054,0.39845777250204245,0.19284192247392801,5.2168925415780096E-2,0.71684397151598833,4.1239933546231642,1762.645,0,{"$f":"T5544*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2168925415780096E-2},{"$f":"U5544*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8680186135469854},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19284192247392801}]
["Single Family Detached",15544,"Mountain South","2000s","Stucco","N/A","central AC",27.729018909535402,13864.50945,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13864.50945},"Hot-Dry/Mixed-Dry",223.00786167804748,"Metropolitan Area",0,0.1503304080836679,0.37625231228122885,1.878273620974575E-2,0.23432010896474731,0.76090282932964404,0,1354.7349999999999,{"$f":"T5545*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5545*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.878273620974575E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.39503504849097459}]
["Single Family Detached",15545,"Pacific","1970s","Concrete","heat pump","central AC",13.939588933296198,12991.2292,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12991.2292},"Marine",226.69470208493311,"Metropolitan Area",0.1726004448440932,0.21556744143173517,1.6844661622845598E-2,3.5143873231839999E-3,0.36846976611534882,0.77348231401402279,214.12799999999999,56.392000000000003,{"$f":"T5546*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7817859261375995E-3},{"$f":"U5546*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.3260139704640003E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1753822307702308},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7577263019891997E-2}]
["Single Family Detached",15546,"East North Central","1960s","Wood","heater burning gas/oil/kerosene","window/wall unit",52.974810385139399,16806.729179999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16806.729179999998},"Cold/Very Cold",61.241553075161264,"Metropolitan Area",0.96445412038084144,0.27989951986465766,2.1475638546203997E-2,0,0.18748054299506783,1.453309821786771,0,0,{"$f":"T5547*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5547*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.96445412038084144},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1475638546203997E-2}]
["Single Family Detached",15547,"South Atlantic","1970s","Wood","central furnace","both central and individual units",45.755146227586501,20950.158530000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20950.158530000001},"Mixed-Humid",397.01342328664754,"Metropolitan Area",1.9678829584844744,0.43506400208242713,0.35194793534255336,4.03160660719614E-2,0.54305796307350496,3.2979528589829603,1171.348,753.03200000000004,{"$f":"T5548*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4539926293798441E-2},{"$f":"U5548*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5776139778162963E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9924228847782728},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36772407512071631}]
["Single Family Detached",15548,"West South Central","1980s","Brick","central furnace","central AC",39.697849921731404,15065.597690000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15065.597690000001},"Hot-Humid",469.0769658996802,"Metropolitan Area",0.49032191423360427,0.41271019209216797,0.55929145211294207,4.1783154617411354E-2,1.0300296712373043,2.4923532296760187,741.39,2032.0250000000001,{"$f":"T5549*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1169483471389101E-2},{"$f":"U5549*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0613671146022252E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.5014913977049934},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.58990512325896427}]
["Single Family Detached",15549,"South Atlantic","1990s","Siding","fireplace","N/A",49.072806132730683,22164.772420000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22164.772420000001},"Mixed-Humid",201.22805078582857,"Metropolitan Area",0.36254745362169127,0.19812019507730114,0,0,0.12592248290773153,0.686590131606724,0,0,{"$f":"T5550*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5550*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.36254745362169127},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (5+ units)",15550,"West South Central","Before 1950","Brick","central furnace","central AC",10.827051287914053,23486.011470000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1868.1109951614462},"Hot-Humid",122.32320344045151,"Metropolitan Area",1.3873982758772828E-2,7.3188071869284277E-2,0.11634687762330553,5.2119686933994602E-3,0.2091604527049066,0.41736678619384449,9.2390000000000008,212.679,{"$f":"T5551*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7259477484296604E-5},{"$f":"U5551*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9730797833994124E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3891242236257125E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.11674418560164547}]
["Single Family Detached",15551,"East North Central","2000s","Siding","heat pump","central AC",54.369895040435871,16066.753849999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16066.753849999999},"Cold/Very Cold",388.83661923765112,"Micropolitan Area",0.44026514141914708,0.22726522934698867,4.5820550370261094E-2,1.2856150494908349E-2,0.61335962315170656,1.3267105442881033,637.47900000000004,162.69200000000001,{"$f":"T5552*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.024221817754415E-2},{"$f":"U5552*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6139323173641998E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.45050735959669125},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.8434482687625291E-2}]
["Multi-Family (5+ units)",15552,"Middle Atlantic","Before 1950","Concrete","radiator","window/wall unit",23.773688281047928,65855.092189999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":5238.2083677620585},"Mixed-Humid",142.06471223795452,"Metropolitan Area",0.91483120160656617,7.8758475533339825E-2,7.7517699741388058E-2,4.4367234159324899E-3,0.32401199270671438,1.3992031896679964,67.370999999999995,0,{"$f":"T5553*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.529033359444976E-4},{"$f":"U5553*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.91518410494251068},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.7517699741388058E-2}]
["Single Family Detached",15553,"Pacific","1950s","Siding","central furnace","central AC",48.007305556380942,9172.2020549999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9172.2020549999997},"Marine",75.872299472332571,"Metropolitan Area",0.4570288976655365,0.16476473237636577,2.6011557874199162E-2,5.4529750159201043E-3,0.22867182088952684,0.87647700880562829,457.13299999999998,137.37799999999999,{"$f":"T5554*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.192916242008315E-3},{"$f":"U5554*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2600587739117898E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4612218139075448},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7271616648110952E-2}]
["Single Family Detached",15554,"Middle Atlantic","1960s","Siding","heater burning gas/oil/kerosene","window/wall unit",56.248950575430825,20476.501850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20476.501850000001},"Mixed-Humid",309.54129220989512,"Metropolitan Area",2.758962271493743,0.43038488317468243,0.19783648695152475,0,1.0689495282038783,4.4561331698238291,0,0,{"$f":"T5555*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5555*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.758962271493743},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19783648695152475}]
["Single Family Detached",15555,"Pacific","2000s","Stucco","central furnace","both central and individual units",107.161471309201,18224.740020000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18224.740020000001},"Hot-Dry/Mixed-Dry",262.2667115110383,"Metropolitan Area",0.57597911220390496,0.4810107938482458,0.44108439790723014,4.4001520708447678E-2,0.48822638759118414,1.986300691550565,1286.5619999999999,1127.8219999999999,{"$f":"T5556*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3447257969611238E-2},{"$f":"U5556*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0554262738836437E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.59942637017351619},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.46163866064606657}]
["Single Family Detached",15556,"Middle Atlantic","Before 1950","Siding","central furnace","window/wall unit",15.638967910613514,2833.1463610000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2833.1463610000001},"Cold/Very Cold",11.83971014158517,"Metropolitan Area",0.52220769045075432,4.7951818106076974E-2,1.443012102340852E-3,8.3910995661553602E-4,5.2224392639271137E-2,0.62382691329844331,296.17599999999999,0,{"$f":"T5557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3910995661553602E-4},{"$f":"U5557*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.52304680040736984},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.443012102340852E-3}]
["Multi-Family (5+ units)",15557,"Middle Atlantic","1990s","Siding","built-in electric unit","window/wall unit",21.698726470399137,28702.01914,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2282.9997169701746},"Cold/Very Cold",78.650937566564807,"Metropolitan Area",2.62316363526202E-2,7.8706016739267776E-2,8.3389124288207606E-3,0,0.15508045365571679,0.26835701917642557,0,0,{"$f":"T5558*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5558*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.62316363526202E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.3389124288207606E-3}]
["Multi-Family (2-4 units)",15558,"West North Central","1990s","Brick","central furnace","central AC",15.872819112268324,20803.170529999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6934.3901766666668},"Mixed-Humid",54.956422086382631,"Metropolitan Area",0.42464132059243848,0.23448990569102252,3.8778968284487347E-2,5.6394482862955802E-3,0.14365375610811032,0.84532358286692222,190.202,80.884,{"$f":"T5559*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3189348803823535E-3},{"$f":"U5559*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6088121504950668E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42596025547282085},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9339849499536853E-2}]
["Single Family Detached",15559,"South Atlantic","1990s","Siding","heat pump","window/wall unit",61.148868866065762,48530.848310000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":48530.848310000001},"Cold/Very Cold",685.18205385120359,"Micropolitan Area",0.74515070107255954,0.514286252625901,6.1712506142872339E-2,1.6064729938424512E-2,1.0166916682770304,2.3378411281183635,331.02100000000002,0,{"$f":"T5560*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6064729938424512E-2},{"$f":"U5560*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.7612154310109841},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1712506142872339E-2}]
["Single Family Detached",15560,"East South Central","1990s","Brick","wood-burning stove","central AC",59.547335384816002,14506.05003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14506.05003},"Hot-Humid",348.38898946505753,"Rural",1.357513877537478E-2,0.24285853437020638,0.20544615481043371,1.042633950746274E-2,0.72682343183354547,1.1887032597895604,0,718.75800000000004,{"$f":"T5561*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5561*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.042633950746274E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.357513877537478E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21587249431789646}]
["Single Family Detached",15561,"East North Central","2010s","Brick","central furnace","central AC",40.122495933113434,8975.9498729999996,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8975.9498729999996},"Cold/Very Cold",279.16722836307531,"Metropolitan Area",0.9016256555423704,0.35720646132436418,6.2615705708955374E-2,2.5607038595188047E-2,0.97979630539134022,2.3012441279670299,2416.7269999999999,436.12299999999999,{"$f":"T5562*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1692420408725668E-2},{"$f":"U5562*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9146181864623784E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.92331807595109605},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6530323895417756E-2}]
["Multi-Family (2-4 units)",15562,"New England","Before 1950","Wood","radiator","window/wall unit",59.751701042820983,45892.243499999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15297.414499999999},"Cold/Very Cold",326.71798743125578,"Rural",2.8413076865904938,0.31621839279354896,3.8931766928355004E-2,5.4441050619179997E-3,0.75416747591488309,3.954254725601893,118.628,0,{"$f":"T5563*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8147016873059998E-3},{"$f":"U5563*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8431223882777998},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8931766928355004E-2}]
["Mobile Home",15563,"South Atlantic","1990s","Siding","central furnace","central AC",14.68542453808085,15893.3166,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15893.3166},"Mixed-Humid",227.44973065715499,"Metropolitan Area",0.161146866602631,0.378077208340104,9.7363109117580615E-2,5.3203354117998007E-3,0.13947127534385217,0.77605845940416773,125.67400000000001,209.07900000000001,{"$f":"T5564*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9973766703884001E-3},{"$f":"U5564*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3229587414114001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16314424327301941},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10068606785899202}]
["Multi-Family (5+ units)",15564,"East North Central","1970s","Brick","central furnace","central AC",16.770808872473321,14309.56388,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1138.2032089330783},"Cold/Very Cold",233.51300794414468,"Metropolitan Area",0.38806823989503958,0.15938653351395254,3.6838813048213841E-2,8.3158313340954398E-3,0.20479840670274055,0.79674637135760906,463.803,117.33499999999999,{"$f":"T5565*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2790206291278849E-4},{"$f":"U5565*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3355107352016273E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38859614195795239},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.6972364121734005E-2}]
["Single Family Detached",15565,"East South Central","1950s","Brick","central furnace","central AC",39.210027930430499,10053.85332,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10053.85332},"Mixed-Humid",137.19752650666675,"Metropolitan Area",0.41827111317242582,0.13746154075632636,5.5888857859360687E-2,1.2476158361947562E-2,0.40253333398567043,1.0141548457737832,964.38300000000004,276.55,{"$f":"T5566*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.6957652263015594E-3},{"$f":"U5566*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.780393135646E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.42796687839872738},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.8669250995006687E-2}]
["Single Family Detached",15566,"Middle Atlantic","2000s","Siding","central furnace","central AC",60.771534742631943,14804.271559999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14804.271559999999},"Cold/Very Cold",106.02274492130198,"Metropolitan Area",0.8525435051876652,0.2509354378176698,2.9783810890998838E-2,3.7995607086886804E-2,0.29574074334526851,1.4290034972416021,2446.933,119.59699999999999,{"$f":"T5567*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6225060621125474E-2},{"$f":"U5567*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7705464657613197E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88876856580879071},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.1554357356760154E-2}]
["Multi-Family (5+ units)",15567,"East North Central","2010s","Concrete","central furnace","both central and individual units",14.903755885291062,15412.363890000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1225.9215014484637},"Cold/Very Cold",32.26880463496417,"Metropolitan Area",1.1668141152695179E-2,1.908825891485667E-2,3.7047047759480628E-3,3.8190296483031004E-4,7.5288534510272162E-2,0.11010116520971799,16.541,8.2379999999999995,{"$f":"T5568*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0277967555459041E-5},{"$f":"U5568*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0099141328932443E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1688419120250638E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7148039172769953E-3}]
["Single Family Detached",15568,"East North Central","Before 1950","Siding","central furnace","central AC",29.245816284797399,24371.513569999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24371.513569999999},"Cold/Very Cold",178.97208804860691,"Metropolitan Area",1.3991423946766122,0.52930482109964827,0.18077380092741652,5.0094793140160056E-2,0.44611063669282697,2.5553316533965038,1731.508,323.95699999999999,{"$f":"T5569*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2199470718563559E-2},{"$f":"U5569*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8953224215964901E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4413418653951757},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18866912334901301}]
["Single Family Detached",15569,"East South Central","1950s","Siding","central furnace","central AC",37.641292813845048,17873.358410000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17873.358410000001},"Mixed-Humid",241.96453950291507,"Metropolitan Area",1.5852775241749502,0.31852115597132685,0.24884320871182258,3.2575732811048259E-2,0.56984363184827613,2.7224855207063756,1235.877,586.70899999999995,{"$f":"T5570*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2089272571675568E-2},{"$f":"U5570*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.048646023937269E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6073667967466256},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25932966895119525}]
["Single Family Detached",15570,"West South Central","1970s","Brick","central furnace","central AC",72.005239797752978,23078.602500000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23078.602500000001},"Hot-Humid",399.7297958988359,"Micropolitan Area",0.80573297910438757,0.46955062290608252,0.75388207516021499,7.4552794415565005E-2,0.60622570717307234,2.6353913843437575,1383.9390000000001,1846.4469999999999,{"$f":"T5571*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1939378065247499E-2},{"$f":"U5571*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2613416350317498E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83767235716963506},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.79649549151053245}]
["Single Family Detached",15571,"Pacific","1980s","Wood","central furnace","N/A",17.377221436806852,11454.99106,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11454.99106},null,54.560488974684922,"Metropolitan Area",0.94592990810294819,0.14692307847949615,0,1.3062435590476621E-2,0.18374275314873481,1.2765957397311789,1140.327,0,{"$f":"T5572*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3062435590476621E-2},{"$f":"U5572*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.95899234369342479},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",15572,"New England","Before 1950","Wood","radiator","window/wall unit",33.371155291126549,27308.637719999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9102.8792400000002},"Cold/Very Cold",57.075599002913513,"Micropolitan Area",0.86168792482401724,0.24487715522526984,1.8936300950526959E-2,1.82397122195652E-3,0.15780902558259391,1.2845263873970456,66.790999999999997,0,{"$f":"T5573*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0799040731883999E-4},{"$f":"U5573*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.86229591523133609},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.8936300950526959E-2}]
["Multi-Family (5+ units)",15573,"East North Central","1990s","Concrete","central furnace","central AC",20.269950913449573,16560.417409999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1317.2393229732181},"Cold/Very Cold",141.78265953724195,"Metropolitan Area",0.55753223449177214,0.32078432721960581,1.6132424180509801E-2,5.4950942654036087E-3,0.14140952018691194,1.040916512674815,287.09399999999999,44.726999999999997,{"$f":"T5574*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.7817150618967309E-4},{"$f":"U5574*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.8916163198623123E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55791040599796182},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.6191340343708425E-2}]
["Single Family Detached",15574,"Middle Atlantic","1960s","Siding","radiator","window/wall unit",41.27935111498936,25994.553599999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25994.553599999999},"Cold/Very Cold",88.233547231592212,"Metropolitan Area",1.6600779851111616,0.40953964292112,1.7089105476729597E-2,1.0988937588864E-3,0.41218700624340465,2.4988937397524156,42.274000000000001,0,{"$f":"T5575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0988937588864E-3},{"$f":"U5575*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6611768788700481},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.7089105476729597E-2}]
["Single Family Attached",15575,"New England","1980s","Wood","central furnace","central AC",28.542591945341172,9866.0877789999995,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9866.0877789999995},"Cold/Very Cold",33.980246760518156,"Metropolitan Area",1.3045301373597733,1.3825171215132676E-2,1.1450522279780724E-2,5.0294257010130511E-3,7.9814163877989772E-2,1.4096199947326764,446.39699999999999,63.372,{"$f":"T5576*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4041919862822633E-3},{"$f":"U5576*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.25233714730788E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3089343293460556},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2075755994511512E-2}]
["Single Family Detached",15576,"New England","1970s","Wood","central furnace","central AC",53.142244256103879,20685.965069999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20685.965069999998},"Cold/Very Cold",196.80869190157659,"Metropolitan Area",1.0788751636381204,0.44499271574019716,8.7372758683713886E-2,3.6111799512175052E-2,0.41453031534653451,2.0257709534085659,1525.1410000000001,220.57400000000001,{"$f":"T5577*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1549013452824869E-2},{"$f":"U5577*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5627860593501794E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1104241770909453},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.1935544743064063E-2}]
["Single Family Detached",15577,"East North Central","Before 1950","Siding","central furnace","N/A",159.80479457555563,36736.734389999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":36736.734389999998},"Cold/Very Cold",545.98762841420228,"Metropolitan Area",2.790207583924146,0.20076750249031922,0,0.12997151712286562,0.27880213073871279,3.269777217153178,3537.9169999999999,0,{"$f":"T5578*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.12997151712286562},{"$f":"U5578*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.9201791010470117},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15578,"East South Central","1990s","Brick","heat pump","central AC",56.831317042646539,21592.445680000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21592.445680000001},"Mixed-Humid",1098.7216877433686,"Metropolitan Area",0.4330432133630065,0.52213118269987902,0.21750709669856125,1.988834827448872E-2,2.5761568857084152,3.7488383784698613,386.22500000000002,534.85400000000004,{"$f":"T5579*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3395423327580018E-3},{"$f":"U5579*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1548805941730722E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44138275569576452},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22905590264029196}]
["Single Family Detached",15579,"Pacific","2000s","Stucco","fireplace","central AC",63.890024846371858,22858.685099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22858.685099999999},"Hot-Dry/Mixed-Dry",146.82133437862129,"Metropolitan Area",0,0.48265455258519119,0.15691705554119581,8.6894548365437987E-3,0.56032475288274541,1.1998963610091324,0,380.13799999999998,{"$f":"T5580*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5580*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6894548365437987E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1656065103777396}]
["Single Family Detached",15580,"New England","1990s","Wood","central furnace","central AC",77.779927495641218,25468.214639999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":25468.214639999998},"Cold/Very Cold",155.19874117597112,"Metropolitan Area",2.649894639515983,0.66641355448148176,5.7387604452955904E-2,2.6742771441658798E-2,0.37516468033387707,3.7488604787842985,946.44200000000001,103.60299999999999,{"$f":"T5581*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4104188000310878E-2},{"$f":"U5581*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6385834413479199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.6739988275162938},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.002618789430382E-2}]
["Single Family Attached",15581,"South Atlantic","1980s","Siding","heat pump","central AC",30.230612895667687,10219.950269999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10219.950269999999},"Mixed-Humid",79.260333753526623,"Metropolitan Area",6.2798906562228987E-2,5.264881987227471E-2,4.574391487135461E-2,4.1820854100861598E-3,0.10924460497872394,0.27043624628458224,156.07499999999999,253.13300000000001,{"$f":"T5582*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.59507873839025E-3},{"$f":"U5582*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.58700667169591E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.4393985300619239E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.833092154305052E-2}]
["Multi-Family (5+ units)",15582,"West South Central","1970s","Stucco","central furnace","central AC",42.379785335750157,45766.506840000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3640.33351287193},"Hot-Humid",760.51440115140497,"Metropolitan Area",0.70381281842452181,0.98816995806072261,0.27702869355016807,2.338581543161004E-2,0.60433802718590002,2.5948751713941816,243.636,267.34500000000003,{"$f":"T5583*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.8691629574206557E-4},{"$f":"U5583*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7322496299874625E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.70469973472026393},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2780019185131668}]
["Single Family Detached",15583,"South Atlantic","1980s","Shingle","central furnace","central AC",46.012168025903271,26292.667440000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26292.667440000001},"Mixed-Humid",312.42530274796246,"Metropolitan Area",0.94417586654724861,0.44162815411739237,0.25828780649822597,3.0987170626077122E-2,0.86103090610641286,2.50512273326928,709.27800000000002,469.27,{"$f":"T5584*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.8648810576508322E-2},{"$f":"U5584*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.23383600495688E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.96282467712375697},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27062616654779476}]
["Single Family Detached",15584,"East South Central","1970s","Brick","central furnace","central AC",60.094821165746197,18177.50187,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18177.50187},"Hot-Humid",174.33009556631873,"Micropolitan Area",0.21517914131892982,0.17765421538107473,0.35859764972552594,3.2796703216441889E-2,0.33782241924078632,1.0892534256663167,697.53399999999999,1106.713,{"$f":"T5585*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2679425589388579E-2},{"$f":"U5585*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0117277627053308E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.22785856690831841},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.37871492735257922}]
["Single Family Detached",15585,"Mountain North","Before 1950","Siding","central furnace","central AC",47.071823312820548,14068.08826,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14068.08826},"Cold/Very Cold",220.72267753999677,"Rural",0.81421152729474267,0.21190643174096618,0.14092423239072149,4.9972438027759837E-2,0.35814152219880868,1.5251837136252389,2994.9769999999999,557.20699999999999,{"$f":"T5586*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2133600772670018E-2},{"$f":"U5586*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8388372550898203E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.8563451280674127},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.14876306964581132}]
["Single Family Detached",15586,"Mountain South","2000s","Stucco","radiator","central AC",12.004049021783484,6187.6541349999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6187.6541349999998},"Hot-Dry/Mixed-Dry",42.936484738633936,"Metropolitan Area",0.38442895215846784,0.12369666985725121,2.0343602198391358E-2,1.4646857979499852E-3,0.14289366880615634,0.67136289302026675,73.150999999999996,163.56,{"$f":"T5587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5263308762938495E-4},{"$f":"U5587*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0120527103205999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.38488158524609722},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.1355654908711958E-2}]
["Single Family Detached",15587,"Mountain North","1970s","Siding","central furnace","N/A",22.733516981849011,24550.23432,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24550.23432},"Cold/Very Cold",157.7704360023919,"Metropolitan Area",0.24851750477824514,0.55372889022190053,8.9209610362174549E-2,2.7432088125887516E-2,0.42167104394423482,1.313127049306555,1117.386,0,{"$f":"T5588*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7432088125887516E-2},{"$f":"U5588*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.27594959290413268},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.9209610362174549E-2}]
["Single Family Detached",15588,"Middle Atlantic","1990s","Siding","other","central AC",62.259058810373872,23024.799859999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":23024.799859999999},"Cold/Very Cold",248.41456564538601,"Metropolitan Area",9.5839025582060366E-2,0.24427926558508425,4.578380143041616E-2,2.02498509808728E-3,0.91388053169044059,1.2997826242880013,0,87.947999999999993,{"$f":"T5589*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5589*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.02498509808728E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.5839025582060366E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7808786528503441E-2}]
["Single Family Attached",15589,"Pacific","2000s","Stucco","central furnace","central AC",14.108668909616076,12872.873089999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12872.873089999999},"Hot-Dry/Mixed-Dry",45.326557590902361,"Metropolitan Area",2.4227442290526858E-2,6.5814919408400466E-2,2.4528783376690667E-2,1.57450685338408E-3,0.16540993127846262,0.27998107635408059,37.731000000000002,84.581000000000003,{"$f":"T5590*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8570637455878999E-4},{"$f":"U5590*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.08880047882529E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4713148665085647E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5617583855515956E-2}]
["Multi-Family (5+ units)",15590,"South Atlantic","1950s","Stucco","built-in electric unit","window/wall unit",33.5406038437823,58230.21501,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":4631.7147145119779},"Hot-Humid",494.65065308531069,"Metropolitan Area",1.296082302671079E-2,0.39983293825831923,0.99839016933879066,0,0.67639699506702422,2.0875809256908449,0,0,{"$f":"T5591*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5591*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.296082302671079E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.99839016933879066}]
["Single Family Detached",15591,"West South Central","1960s","Brick","central furnace","central AC",154.10726657967697,48891.899299999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":48891.899299999997},"Hot-Humid",533.13990686840873,"Metropolitan Area",2.0839698803039779,0.21712687133152939,0.92936978389933389,7.039279650376519E-2,0.64692338399490401,3.8773899195297448,524.69399999999996,915.07,{"$f":"T5592*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5653286211314196E-2},{"$f":"U5592*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.4739510292451004E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1096231665152922},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.97410929419178494}]
["Single Family Detached",15592,"Pacific","1970s","Siding","central furnace","N/A",20.612354959348806,11671.775180000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11671.775180000001},null,86.545150792338674,"Metropolitan Area",1.0887205222030005,0.35164513003173242,0,1.1119758572861901E-2,0.2635256318084197,1.7038912840431526,952.70500000000004,0,{"$f":"T5593*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1119758572861901E-2},{"$f":"U5593*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0998402807758625},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Mobile Home",15593,"Mountain South","2000s","Wood","central furnace","central AC",186.49125622643672,137937.31969999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":137937.31969999999},"Cold/Very Cold",816.93267238980889,"Metropolitan Area",2.3513361059072766,1.8694587005266725,2.1814511235915598E-2,5.0586167065540096E-2,2.7538897589106828,6.9964990765805473,361.02300000000002,5.71,{"$f":"T5594*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.97985449700531E-2},{"$f":"U5594*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.8762209548700001E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.4011346508773297},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.2602133331402596E-2}]
["Single Family Detached",15594,"Pacific","1960s","Siding","N/A","N/A",15.515029187687809,10774.32582,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10774.32582},"Marine",53.884482894624973,"Metropolitan Area",0,8.3931534841789737E-2,0,0,0.13108359402925943,0.21501512887104918,0,0,{"$f":"T5595*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5595*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Multi-Family (2-4 units)",15595,"East North Central","1950s","Brick","central furnace","central AC",38.61688834600222,47675.1708,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15891.723599999999},"Cold/Very Cold",169.19918116044676,"Metropolitan Area",1.4972734147148952,1.5324191056603944,7.879553583278999E-2,3.0981852769892397E-2,0.57162172225418995,3.7007643469755309,579.60699999999997,70.245999999999995,{"$f":"T5596*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.2109542406251989E-3},{"$f":"U5596*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1163300160055999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5064843689555203},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9911865848795588E-2}]
["Single Family Detached",15596,"East South Central","1950s","Brick","wood-burning stove","window/wall unit",36.730986609890145,19747.842260000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19747.842260000001},"Mixed-Humid",313.02727375510932,"Rural",8.0493192443872999E-2,0.37534352524147518,0.20629202283553386,0,0.40592031403101086,1.0680490545518928,0,0,{"$f":"T5597*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5597*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.0493192443872999E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20629202283553386}]
["Single Family Detached",15597,"Pacific","1950s","Wood","central furnace","central AC",32.983940996765185,9747.0274809999992,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9747.0274809999992},"Marine",92.363573187016144,"Metropolitan Area",0.66075974576766794,0.10008762460541797,8.5269852282839911E-2,2.1450546547178685E-2,0.21323803999437738,1.0593552626503031,1706.8409999999999,493.88600000000002,{"$f":"T5598*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6636626132697518E-2},{"$f":"U5598*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.8139204144811657E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.6773963719003655},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.0083772697321082E-2}]
["Single Family Detached",15598,"West North Central","Before 1950","Siding","central furnace","central AC",34.918291382100414,10777.25043,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10777.25043},"Cold/Very Cold",402.24027684631687,"Rural",0.94623370729964562,0.1183957478213553,6.4582533097519421E-2,2.4321883225415397E-2,0.24323184039542295,1.3724438286139433,1920.549,336.23099999999999,{"$f":"T5599*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0698237536086073E-2},{"$f":"U5599*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6236456893293297E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.96693194483573164},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.8206178786848745E-2}]
["Single Family Detached",15599,"Pacific","2010s","Shingle","central furnace","N/A",51.216628043668806,14179.575870000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14179.575870000001},"Hot-Dry/Mixed-Dry",95.088235786501386,"Metropolitan Area",0.17677317075901905,0.14985527364917345,0,4.5189457523137806E-3,0.36329360884428996,0.68992205325248246,318.69400000000002,0,{"$f":"T5600*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5189457523137806E-3},{"$f":"U5600*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.18129211651133284},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",15600,"Pacific","2000s","Stucco","N/A","central AC",23.424871680457187,10457.531999999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10457.531999999999},"Hot-Dry/Mixed-Dry",116.85870571688474,"Metropolitan Area",0,0.35566291168937991,0.17877792000711595,8.962931069027999E-3,0.29944389939696003,0.83388473109345596,0,857.07899999999995,{"$f":"T5601*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5601*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.962931069027999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.18774085107614397}]
["Multi-Family (2-4 units)",15601,"East South Central","1950s","Siding","central furnace","both central and individual units",25.63874656646389,19248.308229999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":6416.1027433333329},"Mixed-Humid",200.10541239111006,"Micropolitan Area",0.70250839271654453,0.27375852484854452,6.2466823423442439E-2,7.8523858390449584E-3,0.26284200082236575,1.3068106657035941,331.45499999999998,76.497,{"$f":"T5602*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1266493347915499E-3},{"$f":"U5602*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.9081261155676994E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.70463504205133609},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.2957636034999209E-2}]
["Multi-Family (5+ units)",15602,"Pacific","1960s","Concrete","N/A","window/wall unit",8.4114612068778172,17820.892390000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1417.499308465932},"Hot-Humid",63.544312403788908,"Metropolitan Area",0,5.4273171355897203E-2,4.7626459658521733E-2,0,0.11491355153292512,0.21681318254734405,0,0,{"$f":"T5603*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5603*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.7626459658521733E-2}]
["Single Family Detached",15603,"Mountain South","2000s","Stucco","central furnace","central AC",91.346797881912025,18943.75734,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18943.75734},"Cold/Very Cold",357.9801824086461,"Metropolitan Area",1.3790984493867549,0.31793665980735725,0.15511089784344248,4.3788722416498081E-2,1.2299773402891316,3.0821233473266862,1787.1690000000001,524.34299999999996,{"$f":"T5604*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.3855695861570466E-2},{"$f":"U5604*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.9330265549276188E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4129541452483254},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.1650439243983701}]
["Multi-Family (2-4 units)",15604,"East South Central","2000s","Siding","central furnace","central AC",27.536379739709801,23820.397700000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7940.1325666666671},"Mixed-Humid",83.276110354693301,"Metropolitan Area",0.62633867438957069,0.12439087904212642,5.6555595119490133E-2,8.4257987152394007E-3,9.6571775000625137E-2,0.90947412269530536,245.21,108.512,{"$f":"T5605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9469999066723336E-3},{"$f":"U5605*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6159966507413346E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62828567429624305},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.7417194784564266E-2}]
["Single Family Detached",15605,"Mountain North","2000s","Shingle","central furnace","central AC",32.593720152075619,7101.0283559999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7101.0283559999998},"Cold/Very Cold",158.45253135297153,"Metropolitan Area",0.4692210771100741,0.30408027886680217,6.2439420445619911E-2,1.9314967553000544E-2,0.47867504541389133,1.3144158218363877,2167.39,552.63400000000001,{"$f":"T5606*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.539069784851084E-2},{"$f":"U5606*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9242697044897046E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.48461177495858493},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.6363690150109622E-2}]
["Single Family Detached",15606,"East North Central","1970s","Brick","central furnace","both central and individual units",62.342007500579328,16234.897790000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16234.897790000001},"Cold/Very Cold",123.19782375307909,"Metropolitan Area",0.86167400262642413,0.16216318572969127,6.9341147944131432E-2,2.734104525405889E-2,0.41906107502337792,1.5122394113236246,1434.683,249.40799999999999,{"$f":"T5607*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.329193186605057E-2},{"$f":"U5607*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0491133880083199E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.88496593449247474},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.3390261332139745E-2}]
["Single Family Detached",15607,"Middle Atlantic","1950s","Siding","central furnace","central AC",71.596793438864097,26517.330900000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26517.330900000001},"Mixed-Humid",310.51794487744394,"Metropolitan Area",3.2149177364106554,0.88570377835104608,0.18790379555721751,4.6236440194497908E-2,0.83488551461966087,5.1234108249385795,1382.403,361.22800000000001,{"$f":"T5608*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6657637788152703E-2},{"$f":"U5608*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.5788024063451997E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.2515753741988083},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19748259796356271}]
["Single Family Detached",15608,"Pacific","1950s","Stucco","N/A","N/A",49.597725018714293,17390.506669999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17390.506669999999},"Hot-Dry/Mixed-Dry",82.49529431209676,"Metropolitan Area",0,0.32991876274739729,0,0,0.28147394136424492,0.61139270411164226,0,0,{"$f":"T5609*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5609*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15609,"West South Central","1980s","Brick","central furnace","central AC",35.076027062097275,14246.964690000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14246.964690000001},"Hot-Humid",338.45230357996019,"Metropolitan Area",0.38705442746253965,0.33144785467012927,0.67838697543235371,4.4734229640671974E-2,0.53889612665063313,1.9357853842156558,611.95600000000002,2527.9569999999999,{"$f":"T5610*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7185155238336393E-3},{"$f":"U5610*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.6015714116838328E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.39577294298637328},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.71440268954919206}]
["Single Family Attached",15610,"Middle Atlantic","2010s","Siding","central furnace","central AC",25.351894712028031,35162.12859,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":35162.12859},"Cold/Very Cold",265.62227921223695,"Metropolitan Area",1.1455174159834658,0.27310597570283091,2.6771776627982791E-2,1.5321123966263518E-2,0.86528361970777035,2.3106787880220501,405.20299999999997,30.524999999999999,{"$f":"T5611*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4247799991053769E-2},{"$f":"U5611*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0733239752097499E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1597652159745195},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.7845100603192542E-2}]
["Multi-Family (5+ units)",15611,"Pacific","1960s","Concrete","central furnace","window/wall unit",12.420679428339096,13046.93217,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1037.7716740467295},"Hot-Humid",99.939500442308258,"Metropolitan Area",5.2020339059753039E-5,8.511222302907831E-2,0.15391412388527104,8.4805059104999993E-7,0.10192851827844868,0.34100766612729,6.5000000000000002E-2,0,{"$f":"T5612*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.745515881303742E-8},{"$f":"U5612*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.2087794218566074E-5},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.15391412388527104}]
["Single Family Detached",15612,"West North Central","1970s","Wood","radiator","central AC",29.343946122769683,11784.71732,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11784.71732},"Cold/Very Cold",175.24995379050117,"Metropolitan Area",1.4780848177762764,0.36714488985097438,3.2501225098153161E-2,4.4586063814141593E-3,0.44908929714557622,2.3268202298709801,258.51299999999998,119.825,{"$f":"T5613*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.0465026285451595E-3},{"$f":"U5613*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4121037528690001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4811313204048215},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.3913328851022162E-2}]
["Single Family Detached",15613,"Middle Atlantic","Before 1950","Wood","radiator","window/wall unit",354.91467261160437,55559.591829999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":55559.591829999998},"Cold/Very Cold",383.77565818374342,"Metropolitan Area",14.453608687544321,1.0274339740093366,0.2326222883542515,2.23932934870815E-3,1.6987216303769455,17.412386580284856,40.305,0,{"$f":"T5614*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.23932934870815E-3},{"$f":"U5614*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":14.455848016893029},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.2326222883542515}]
["Single Family Attached",15614,"South Atlantic","2000s","Siding","heat pump","central AC",21.425996687843856,14796.95904,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14796.95904},"Hot-Humid",175.19599501662378,"Metropolitan Area",5.3055414049380474E-2,0.16111463172973345,0.12125961443385505,6.66598565664288E-3,0.26232309412591098,0.59775275433887998,60.29,390.20699999999999,{"$f":"T5615*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.9210866052159994E-4},{"$f":"U5615*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7738769961212799E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.3947522709902072E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12703349142997633}]
["Mobile Home",15615,"Pacific","1960s","Siding","portable electric heaters","window/wall unit",15.973202350200346,11884.823179999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11884.823179999999},"Marine",78.998419659063757,"Metropolitan Area",0.12664872853078438,6.5439571613264275E-2,5.4354169179643801E-3,0,7.2000303014026934E-2,0.26952402007603998,0,0,{"$f":"T5616*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5616*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.12664872853078438},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.4354169179643801E-3}]
["Single Family Attached",15616,"West North Central","1970s","Wood","central furnace","central AC",9.652777647159219,7835.0467920000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":7835.0467920000001},"Cold/Very Cold",75.347364995482863,"Metropolitan Area",0.68215619430761221,8.2677920964157436E-2,1.0387532665804175E-2,1.148210437274016E-2,0.23563616464227413,1.010857812579848,1411.797,53.683,{"$f":"T5617*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1061495555805224E-2},{"$f":"U5617*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2060881693493598E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.69321768986341747},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.0808141482739111E-2}]
["Single Family Detached",15617,"South Atlantic","2000s","Siding","central furnace","central AC",37.581907090477834,12460.84453,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12460.84453},"Mixed-Humid",143.3752870712861,"Rural",0.21120230559290482,0.12863161586917846,0.11718775070464987,1.2571895576451362E-2,0.2373148277212587,0.69433649988799195,486.505,522.40700000000004,{"$f":"T5618*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.0622631680676501E-3},{"$f":"U5618*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.5096324083837101E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.21726456876097247},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12369738311303358}]
["Single Family Detached",15618,"East North Central","1960s","Brick","built-in electric unit","both central and individual units",13.352332647186479,14055.087,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14055.087},"Cold/Very Cold",346.97586659809838,"Metropolitan Area",0.62044333317559497,0.21265759850557797,4.3919588849165997E-2,1.608112779105E-3,0.30686113042381524,1.1838816509541541,0,114.41500000000001,{"$f":"T5619*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5619*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.608112779105E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.62044333317559497},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.5527701628270995E-2}]
["Single Family Detached",15619,"Mountain North","1980s","Wood","central furnace","N/A",16.745899929664446,8945.4593640000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8945.4593640000003},"Cold/Very Cold",73.782148835401898,"Metropolitan Area",0.39448189438183462,0.29462740808530113,3.4428863563573095E-2,7.0772985758816038E-3,0.3208464421356727,1.0443846081663817,791.16099999999994,0,{"$f":"T5620*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.0772985758816038E-3},{"$f":"U5620*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.40155919295771625},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.4428863563573095E-2}]
["Single Family Detached",15620,"West North Central","1960s","Brick","central furnace","central AC",104.3278284224557,29371.57332,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":29371.57332},"Mixed-Humid",216.4572754062616,"Metropolitan Area",1.5362353802248603,0.42180178671758817,0.26625384083411974,5.4856670686724285E-2,0.50039662170468335,2.7246876294812514,1312.623,555.05600000000004,{"$f":"T5621*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8553802686018365E-2},{"$f":"U5621*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.630286800070592E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.5747891829108787},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.28255670883482564}]
["Single Family Detached",15621,"New England","2000s","Siding","central furnace","both central and individual units",141.10931075550408,22537.82315,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22537.82315},"Cold/Very Cold",366.75666642309272,"Metropolitan Area",2.8240437596891996,0.40213298019319643,9.3830028783658745E-2,5.6285035484060844E-2,0.70433253132895279,4.0243392999950078,2266.3330000000001,231.02600000000001,{"$f":"T5622*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.1078212353008953E-2},{"$f":"U5622*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2068231310518995E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8751219720422085},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.903685191471065E-2}]
["Single Family Attached",15622,"Pacific","1960s","Brick","central furnace","window/wall unit",21.236513697567659,8167.8898840000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8167.8898840000002},"Marine",39.275077972647793,"Metropolitan Area",0.11268491127819402,0.13093655946527497,7.2965965664040676E-3,2.7315792460162361E-3,0.1418005962889744,0.39271866359884744,334.42899999999997,0,{"$f":"T5623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7315792460162361E-3},{"$f":"U5623*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11541649052421026},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.2965965664040676E-3}]
["Single Family Detached",15623,"Mountain South","2000s","Stucco","heater burning gas/oil/kerosene","central AC",34.287288119277882,11880.557210000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11880.557210000001},"Hot-Dry/Mixed-Dry",215.0108909758921,"Metropolitan Area",0.26991314367604019,0.15093867757474283,0.47323345936193167,2.7090806905903445E-2,0.29431154306534157,1.1883968236780562,0,2280.2640000000001,{"$f":"T5624*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5624*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7090806905903445E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.26991314367604019},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.5003242662678351}]
["Single Family Attached",15624,"Pacific","2000s","Wood","central furnace","N/A",17.46766658096525,13084.39444,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13084.39444},"Hot-Dry/Mixed-Dry",77.335025496726843,"Metropolitan Area",3.5096048771706523E-2,0.39817343155069479,0,6.388455585330001E-4,0.27413528258108305,0.70740476290348431,48.825000000000003,0,{"$f":"T5625*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.388455585330001E-4},{"$f":"U5625*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.5734894330239519E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15625,"Middle Atlantic","2000s","Siding","fireplace","both central and individual units",149.39465071424823,19953.873479999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19953.873479999998},"Cold/Very Cold",211.496851686887,"Micropolitan Area",2.2457392202330242,0.48552880373063528,5.2360081428434881E-2,3.31032765645852E-3,0.83026024273635679,3.6138883481284507,0,165.899,{"$f":"T5626*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5626*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.31032765645852E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2457392202330242},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5670409084893402E-2}]
["Single Family Detached",15626,"Pacific","1960s","Stucco","central furnace","central AC",22.728618689451622,17826.367600000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17826.367600000001},"Marine",90.437922472767184,"Metropolitan Area",8.4725266887485606E-2,0.19593520377102644,2.4826960420196002E-2,7.2495202173624004E-3,0.34521251082509002,0.6506999419037981,343.03,63.643999999999998,{"$f":"T5627*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.1149788778280005E-3},{"$f":"U5627*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1345413395343999E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.0840245765313604E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.5961501759730402E-2}]
["Single Family Detached",15627,"Middle Atlantic","2000s","Brick","central furnace","central AC",61.46312918497766,15027.659949999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15027.659949999999},"Cold/Very Cold",237.00316359900918,"Metropolitan Area",1.4238585327196407,0.54070632546936293,7.4834064774312245E-2,3.1287993762718645E-2,0.46546839233389475,2.5048673152972105,1778.8920000000001,303.13499999999999,{"$f":"T5628*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6732584063775398E-2},{"$f":"U5628*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.5554096989432495E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.450591116783416},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9389474473255492E-2}]
["Multi-Family (5+ units)",15628,"West South Central","1970s","Brick","central furnace","central AC",28.219556971637651,24474.897629999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1946.7684168704793},"Hot-Humid",103.01741400442748,"Metropolitan Area",5.9227145270795659E-2,0.1391100070761343,7.4262636716800418E-2,4.7298963414856496E-3,7.454197196680945E-2,0.35149543464162319,47.295000000000002,145.96,{"$f":"T5629*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.2072412275889326E-5},{"$f":"U5629*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8415031812641518E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":5.9319217683071551E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.4546787034926829E-2}]
["Single Family Detached",15629,"Pacific","1970s","Siding","central furnace","window/wall unit",22.152433086652586,15491.211950000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15491.211950000001},"Marine",214.56804861459432,"Metropolitan Area",0.62863003482921886,0.65885716919938453,1.70477069618882E-2,7.30675543166845E-3,0.70775172517929485,2.0122866361697866,471.67099999999999,0,{"$f":"T5630*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.30675543166845E-3},{"$f":"U5630*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63593679026088734},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.70477069618882E-2}]
["Single Family Detached",15630,"East South Central","1990s","Shingle","central furnace","window/wall unit",92.483896728907354,51695.861779999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":51695.861779999999},"Mixed-Humid",584.94234647526798,"Rural",2.1888459021139246,0.62682385225967696,0.31257582310933968,2.7411265446088979E-2,0.78299823970187754,3.9112438171848187,530.24099999999999,0,{"$f":"T5631*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7411265446088979E-2},{"$f":"U5631*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.2162571675600136},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.31257582310933968}]
["Single Family Attached",15631,"East North Central","1980s","Brick","central furnace","both central and individual units",51.960014394878407,18445.159530000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18445.159530000001},"Cold/Very Cold",120.40946649959132,"Metropolitan Area",0.85706464840562735,0.16875194243056191,8.3567510650501289E-2,2.3311103284971182E-2,0.95490063355247445,2.0642847350391649,1077.018,186.78800000000001,{"$f":"T5632*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9865768826681542E-2},{"$f":"U5632*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.4453344582896406E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.87693041723230891},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.7012845108790926E-2}]
["Single Family Detached",15632,"Mountain North","2010s","Wood","central furnace","central AC",62.446899626298986,26516.730200000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26516.730200000002},"Cold/Very Cold",136.26947650936327,"Metropolitan Area",0.64567182671138046,0.52442779021410846,3.6419827360873201E-2,1.39476409848188E-2,0.44384535634088301,1.6503648006272449,454.04199999999997,71.951999999999998,{"$f":"T5633*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.20397092134684E-2},{"$f":"U5633*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9079317713504001E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.65771153592484888},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.8327759132223603E-2}]
["Single Family Detached",15633,"South Atlantic","1990s","Siding","central furnace","central AC",60.990455941528886,16395.28386,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16395.28386},"Mixed-Humid",371.8991750643533,"Metropolitan Area",0.62190400552459224,0.27865691691582917,0.21045361814696392,2.6069435868580022E-2,0.15790547093880652,1.268920011526192,789.48599999999999,800.57100000000003,{"$f":"T5634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2943847073495961E-2},{"$f":"U5634*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.312558879508406E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.63484785259808818},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.22357920694204797}]
["Single Family Detached",15634,"East North Central","Before 1950","Brick","central furnace","both central and individual units",105.66692870999991,27149.776129999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":27149.776129999998},"Cold/Very Cold",204.48915450886173,"Metropolitan Area",2.4651789030252602,0.80810597326810396,0.27770411867398959,9.6128234951550304E-2,0.46240909554473925,4.0133980905120934,3041.0239999999999,499.64,{"$f":"T5635*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.256312080595711E-2},{"$f":"U5635*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3565114145593199E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5477420238312174},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.29126923281958278}]
["Single Family Detached",15635,"East North Central","1990s","Siding","central furnace","central AC",23.349878945355119,13481.45436,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13481.45436},"Cold/Very Cold",189.80876624791631,"Metropolitan Area",0.71196927494632101,0.21089734698392976,8.7156726142866597E-2,1.9715049671339881E-2,0.34127130173956122,1.3512946498126785,1160.364,302.01900000000001,{"$f":"T5636*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.5643394306987041E-2},{"$f":"U5636*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.07165536435284E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.72761266925330803},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.122838150721943E-2}]
["Single Family Detached",15636,"Mountain North","1990s","Wood","central furnace","N/A",45.678482748340166,19040.634740000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19040.634740000001},"Cold/Very Cold",125.87002003175388,"Metropolitan Area",0.82560858654855906,0.49206093537952955,0,1.475165560227604E-2,0.41471686791200829,1.7323863898400969,774.74599999999998,0,{"$f":"T5637*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.475165560227604E-2},{"$f":"U5637*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.84036024215083516},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Attached",15637,"Mountain North","2010s","Stucco","central furnace","central AC",84.529371019661639,26531.503769999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26531.503769999999},"Cold/Very Cold",274.07502392162303,"Metropolitan Area",1.421703868735831,0.50768125324158186,0.10115703586493177,2.6840569257416728E-2,0.87279937110612293,2.9033415289484679,799.72500000000002,211.92400000000001,{"$f":"T5638*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1217906852463247E-2},{"$f":"U5638*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.6226624049534801E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4429217755882942},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10677969826988525}]
["Single Family Detached",15638,"Mountain South","1990s","Stucco","heat pump","central AC",42.87053785101709,14172.07863,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14172.07863},"Hot-Dry/Mixed-Dry",191.75553663530323,"Metropolitan Area",0.151439997824454,0.10796377367221506,0.4196843828309102,2.6825250560751121E-2,0.24019543214431918,0.91928358647189845,156.22999999999999,1736.5940000000001,{"$f":"T5639*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2141038443648999E-3},{"$f":"U5639*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.4611146716386222E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.1536541016688189},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.4442955295472964}]
["Single Family Detached",15639,"South Atlantic","2000s","Siding","heat pump","central AC",21.448465781746389,11902.58922,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11902.58922},"Hot-Humid",290.3244926996756,"Metropolitan Area",0.11097427859882801,0.30562365229095306,0.24802897508000513,1.3779270462317401E-2,0.32596026149858537,0.99058716746837139,162.16,995.51,{"$f":"T5640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9301238679151997E-3},{"$f":"U5640*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1849146594402199E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11290440246674321},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.25987812167440733}]
["Multi-Family (5+ units)",15640,"South Atlantic","2010s","Concrete","N/A","central AC",13.309426040593385,17605.0609,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1400.3317625807524},"Hot-Humid",145.84907421298647,"Metropolitan Area",0,0.1055667583149683,0.12008789783723038,5.1350265582510999E-3,0.26725581002000159,0.49763704536227366,0,291.67899999999997,{"$f":"T5641*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5641*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.0844736817779125E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12049634520540817}]
["Multi-Family (5+ units)",15641,"Middle Atlantic","1950s","Brick","heat pump","window/wall unit",22.789429412586049,45127.582999999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3589.5125954036998},"Mixed-Humid",88.446768357072344,"Metropolitan Area",0.43518719488096058,0.99806125612660501,5.5546007576877998E-2,4.0784053136250003E-3,0.5542431202380188,2.046791581935278,90.375,0,{"$f":"T5642*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.2440220080960939E-4},{"$f":"U5642*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.43551159708177017},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.5546007576877998E-2}]
["Multi-Family (2-4 units)",15642,"Middle Atlantic","1970s","Brick","built-in electric unit","window/wall unit",18.959898819073768,37618.846859999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12539.615619999999},"Mixed-Humid",370.50802275606651,"Metropolitan Area",0.4041197476354596,0.51092153481334268,6.8772894887108998E-2,0,0.66309642889793685,1.6469106062338481,0,0,{"$f":"T5643*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5643*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.4041197476354596},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.8772894887108998E-2}]
["Single Family Detached",15643,"New England","Before 1950","Wood","central furnace","N/A",33.388314819416252,10191.79329,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10191.79329},"Cold/Very Cold",42.460947288615316,"Micropolitan Area",0.53215164497780443,0.19062930947943812,0,1.112747125657503E-2,0.16122146068156742,0.88400241513881006,1091.807,0,{"$f":"T5644*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.112747125657503E-2},{"$f":"U5644*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54327911623437941},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15644,"East South Central","1980s","Siding","heat pump","central AC",17.072055398938698,16060.25908,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16060.25908},"Mixed-Humid",156.15799437253779,"Metropolitan Area",0.24162937628342082,0.11740666101428671,4.1410960471043916E-2,5.69869384987456E-3,0.13236407816352225,0.53281107593227373,242.98500000000001,111.84699999999999,{"$f":"T5645*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.9024020525538004E-3},{"$f":"U5645*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7962917973207598E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.24553177833597462},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.3207252268364672E-2}]
["Single Family Detached",15645,"Pacific","1990s","Stucco","N/A","central AC",40.981609624483987,20739.680980000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":20739.680980000001},"Hot-Dry/Mixed-Dry",108.2241144061876,"Metropolitan Area",0,0.23355946108328843,7.8441496964470142E-2,4.1632835599252002E-3,0.35384857378323936,0.66584953183099793,0,200.74,{"$f":"T5646*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5646*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.1632835599252002E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.2604780524395349E-2}]
["Single Family Detached",15646,"West South Central","1980s","Brick","central furnace","central AC",46.901137450954771,22081.514810000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22081.514810000001},"Hot-Humid",174.32514634741952,"Metropolitan Area",0.50130194652408133,0.25348477134290981,0.13238868421215894,1.6036611804703262E-2,0.45373215871767986,1.3409075607968299,392.93200000000002,333.31400000000002,{"$f":"T5647*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.6765337773229197E-3},{"$f":"U5647*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.360078027380341E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.50997848030140425},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13974876223953928}]
["Single Family Detached",15647,"New England","Before 1950","Shingle","radiator","window/wall unit",58.632257546552353,14836.09756,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14836.09756},"Cold/Very Cold",82.230895551478909,"Metropolitan Area",1.7740032659330991,0.38084048796715136,4.428236858635632E-2,3.8477567382835601E-3,0.29588733169566489,2.4950134541822715,259.351,0,{"$f":"T5648*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.8477567382835601E-3},{"$f":"U5648*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.7778510226713826},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.428236858635632E-2}]
["Single Family Attached",15648,"South Atlantic","2000s","Brick","built-in electric unit","central AC",8.5733929986479414,13895.288490000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13895.288490000001},"Mixed-Humid",111.12483233106347,"Metropolitan Area",8.8408411740124274E-2,0.1029293633849635,2.7779627492669885E-2,1.1457360124429502E-3,0.16004052756059739,0.37915793017835503,0,82.454999999999998,{"$f":"T5649*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5649*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1457360124429502E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.8408411740124274E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8925363505112836E-2}]
["Multi-Family (5+ units)",15649,"West South Central","1990s","Brick","central furnace","central AC",21.377886395676416,25602.259160000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2036.4403678701283},"Mixed-Humid",286.56426897828982,"Metropolitan Area",0.20278576979009905,0.36443251616225325,3.9593583081208805E-2,5.0463332917318011E-3,0.36630048259282599,0.97775729233940978,129.381,67.724000000000004,{"$f":"T5650*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.6347669123540502E-4},{"$f":"U5650*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3791588747363658E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.20304924648133446},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.9731498968682444E-2}]
["Single Family Detached",15650,"West South Central","1970s","Wood","portable electric heaters","window/wall unit",9.0492863059516218,15656.204680000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15656.204680000001},"Hot-Humid",176.84672659977323,"Metropolitan Area",0.23021742887108934,0.3356182709236275,0.13234349509291737,0,0.32375941606394265,1.0219386109515769,0,0,{"$f":"T5651*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5651*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.23021742887108934},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.13234349509291737}]
["Multi-Family (5+ units)",15651,"Middle Atlantic","Before 1950","Brick","built-in electric unit","window/wall unit",47.499100436847449,38060.176630000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3027.3609689372138},"Mixed-Humid",175.81301050420529,"Metropolitan Area",6.1238253295020549E-2,0.23676478484008065,6.1862820793518847E-2,0,0.24000812085178275,0.5998739797804028,0,0,{"$f":"T5652*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5652*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.1238253295020549E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.1862820793518847E-2}]
["Single Family Detached",15652,"Mountain South","1960s","Stucco","central furnace","central AC",19.288647120189417,9601.1185270000005,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":9601.1185270000005},"Hot-Dry/Mixed-Dry",35.065742745940526,"Metropolitan Area",0.60120283992368606,0.1938556081115454,2.5260677260196381E-2,7.578143651124046E-3,9.8353618162624834E-2,0.91867274345805261,648.34500000000003,140.953,{"$f":"T5653*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.2248371913878157E-3},{"$f":"U5653*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3533064597362309E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.60742767711507384},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.6613983719932611E-2}]
["Single Family Detached",15653,"Pacific","1970s","Stucco","central furnace","central AC",26.981070189057267,11530.371880000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11530.371880000001},"Hot-Dry/Mixed-Dry",130.32702077573148,"Metropolitan Area",0.15693228161323922,0.14215096750316075,0.23644564538511603,1.822426009270272E-2,0.27860392501289422,0.8141328195144103,532.38199999999995,1048.162,{"$f":"T5654*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.138562442218159E-3},{"$f":"U5654*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2085697650484561E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16307084405545738},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.24853134303560059}]
["Single Family Attached",15654,"West North Central","Before 1950","Stucco","radiator","window/wall unit",11.877429824655492,13390.5635,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13390.5635},"Cold/Very Cold",34.371715216623471,"Metropolitan Area",0.52953829644363204,7.5283435208001001E-2,1.2047945260108999E-2,1.9258710142605001E-3,0.10330247963188553,0.72017215654362754,143.82300000000001,0,{"$f":"T5655*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.9258710142605001E-3},{"$f":"U5655*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.53146416745789249},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.2047945260108999E-2}]
["Single Family Detached",15655,"East North Central","1960s","Siding","central furnace","central AC",38.34364966187627,19114.481390000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19114.481390000001},"Cold/Very Cold",123.83290006150055,"Metropolitan Area",1.3793730769262034,0.30966975630174226,4.2097867614705728E-2,3.3633917911769562E-2,0.37528051950461938,2.1064212203472708,1651.915,107.68899999999999,{"$f":"T5656*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":3.1575498525361852E-2},{"$f":"U5656*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0584193864077098E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.4109485754515652},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":4.4156287001113438E-2}]
["Single Family Detached",15656,"Pacific","Before 1950","Stucco","central furnace","window/wall unit",27.153416168063128,21722.732929999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21722.732929999998},"Hot-Dry/Mixed-Dry",107.90589458778223,"Metropolitan Area",7.9316736092899326E-2,0.38561954375000473,6.8439121023667684E-2,1.6957851461804497E-3,0.48914133463301401,1.0225167354995857,78.064999999999998,0,{"$f":"T5657*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.6957851461804497E-3},{"$f":"U5657*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.1012521239079774E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.8439121023667684E-2}]
["Single Family Detached",15657,"Pacific","1950s","Shingle","central furnace","central AC",19.257124871118219,16774.499019999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":16774.499019999999},"Hot-Dry/Mixed-Dry",98.481104335888716,"Metropolitan Area",0.65707780957069151,0.30644612633630042,5.6621600138552136E-2,7.8101396457159189E-3,0.27415432667435241,1.2942998627198965,312.476,153.12,{"$f":"T5658*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2416283557735199E-3},{"$f":"U5658*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5685112899424003E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.66231943792646497},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.9190111428494535E-2}]
["Single Family Detached",15658,"Pacific","Before 1950","Wood","wood-burning stove","N/A",91.238378429538145,22511.319619999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":22511.319619999998},"Marine",94.246273423522752,"Metropolitan Area",0,0.24380502022007458,0,0,0.32156828029463991,0.56537330051471446,0,0,{"$f":"T5659*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5659*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15659,"West South Central","1960s","Brick","central furnace","central AC",20.610840267983672,24478.43262,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24478.43262},"Hot-Humid",379.44307253345193,"Metropolitan Area",0.10523197404510354,0.20264561014667695,0.69300401021829605,3.6895337872388578E-2,0.82559156289668889,1.8264731573067656,340.12799999999999,1167.1310000000001,{"$f":"T5660*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3258003301753605E-3},{"$f":"U5660*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8569537542213221E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.11355777437527889},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.7215735477605093}]
["Multi-Family (5+ units)",15660,"Pacific","1980s","Stucco","central furnace","central AC",11.757584143124873,11316.250379999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":900.11076533285427},"Marine",32.388240207928483,"Metropolitan Area",6.0646637208694301E-2,0.1454922842631349,3.7620337651034087E-3,1.8707232990689401E-3,0.10488962316469645,0.31651250168974854,150.08500000000001,15.228,{"$f":"T5661*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3509312421498146E-4},{"$f":"U5661*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3706886734488704E-5},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":6.0781730332909283E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.7757406518378975E-3}]
["Single Family Detached",15661,"Mountain North","Before 1950","Siding","central furnace","central AC",111.32376097664473,24738.613549999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24738.613549999998},"Cold/Very Cold",169.8783028087978,"Micropolitan Area",1.9545582500652063,0.67929516508532206,8.7824997258898904E-2,3.3586230254476199E-2,0.46381869926090147,3.1854971116703288,1131.069,226.57499999999999,{"$f":"T5662*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7981078889384947E-2},{"$f":"U5662*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.605151365091249E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.9825393289545912},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.3430148623990156E-2}]
["Single Family Detached",15662,"East North Central","2000s","Brick","central furnace","central AC",92.296229159895418,15651.387000000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15651.387000000001},"Cold/Very Cold",246.72837081553615,"Metropolitan Area",2.0355276604407933,0.64857646422233106,0.216518407902792,8.0419737563981991E-2,0.67792857455774735,3.5785511071236633,4297.8670000000002,840.31899999999996,{"$f":"T5663*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":6.7267579691529009E-2},{"$f":"U5663*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.3152157872453E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.1027952401323224},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.229670565775245}]
["Multi-Family (5+ units)",15663,"East South Central","1970s","Brick","heat pump","central AC",16.031747087991356,25406.889200000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":2020.9003613915293},"Mixed-Humid",139.73789062433033,"Micropolitan Area",9.5952449328842879E-2,0.1620073592733596,3.1885915666174797E-2,2.8759582298832002E-3,0.18426735117704762,0.47676027583800001,60.109000000000002,53.087000000000003,{"$f":"T5664*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2147429982288344E-4},{"$f":"U5664*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.0728353748519212E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":9.6073923628665764E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.1993199203659992E-2}]
["Single Family Detached",15664,"East North Central","Before 1950","Siding","central furnace","both central and individual units",71.226016154926569,19785.004489999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19785.004489999999},"Mixed-Humid",376.73121669722093,"Rural",1.6143621501926186,0.56769861256326726,0.48758089882138933,8.0292553826555965E-2,1.0255215390363956,3.695163200613671,2915.5529999999999,1142.7,{"$f":"T5665*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.7684229195832964E-2},{"$f":"U5665*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.2608324630723001E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.6720463793884517},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.51018922345211237}]
["Single Family Attached",15665,"East North Central","1980s","Brick","heat pump","central AC",16.50566311102757,11398.938609999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":11398.938609999999},"Cold/Very Cold",118.80160764632565,"Metropolitan Area",0.13304119592777985,0.10525412866650757,3.0797173581076382E-2,3.8902753645752397E-3,0.13625860334514542,0.40535110152050924,217.93100000000001,123.35299999999999,{"$f":"T5666*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.48418209021591E-3},{"$f":"U5666*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.4060932743593299E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.13552537801799577},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.220326685543571E-2}]
["Single Family Detached",15666,"Middle Atlantic","1960s","Siding","central furnace","central AC",83.428440614141294,19474.425910000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":19474.425910000002},"Cold/Very Cold",290.71423003919261,"Metropolitan Area",2.458992584853458,0.59562991242186492,0.19731533123191597,9.9677356293818534E-2,1.4249455354818836,4.6768833639891225,4499.2370000000001,619.13499999999999,{"$f":"T5667*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.7620057608030683E-2},{"$f":"U5667*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2057298685787851E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5466126424614886},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.20937262991770383}]
["Single Family Detached",15667,"South Atlantic","1980s","Brick","central furnace","both central and individual units",44.40475029475396,18855.5203,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":18855.5203},"Mixed-Humid",227.39868723354573,"Metropolitan Area",0.71783439055659537,0.28216358437351241,0.20201870443741049,1.7438452527373801E-2,0.56553991810168025,1.7675565974691985,441.55200000000002,483.29399999999998,{"$f":"T5668*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3256926995056001E-3},{"$f":"U5668*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.1127598278681991E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.72616008325610093},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.21113146426527868}]
["Single Family Detached",15668,"New England","1950s","Siding","central furnace","central AC",136.33713944874017,26519.575850000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":26519.575850000001},"Cold/Very Cold",273.9325797324471,"Rural",4.3703177145735017,0.2149742586949108,0.10420384673977032,0.11745620918353229,0.70796020567382045,5.3974560256820032,4229.8969999999999,199.14099999999999,{"$f":"T5669*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.11217507432918745},{"$f":"U5669*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2811348543448508E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.4824927889026895},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10948498159411517}]
["Multi-Family (5+ units)",15669,"East North Central","Before 1950","Brick","heater burning gas/oil/kerosene","window/wall unit",61.527137186204023,42786.604440000003,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":3403.3078073766078},"Cold/Very Cold",127.93194727868568,"Metropolitan Area",1.0673298181296649,1.515325205667903,9.5727197485887483E-2,0,0.30342167603890846,2.9818038973223637,0,0,{"$f":"T5670*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5670*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0673298181296649},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":9.5727197485887483E-2}]
["Single Family Detached",15670,"Middle Atlantic","1950s","Shingle","radiator","window/wall unit",294.4720319303712,42019.410949999998,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":42019.410949999998},"Cold/Very Cold",93.155731472123747,"Metropolitan Area",3.159382236873375,0.39384373689325491,2.8298014323688451E-2,1.1957043579931999E-3,0.38450282183907031,3.9660268099293887,28.456,0,{"$f":"T5671*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1957043579931999E-3},{"$f":"U5671*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.1605779412313684},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":2.8298014323688451E-2}]
["Single Family Detached",15671,"Middle Atlantic","1960s","Brick","central furnace","central AC",71.046016652618746,24754.709640000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24754.709640000001},"Cold/Very Cold",69.123887713585347,"Metropolitan Area",1.0920042835569332,0.42560428193588007,7.5322145210013607E-3,7.5469435732371613E-3,0.22119454451686693,1.7463353245306816,287.78100000000001,17.088000000000001,{"$f":"T5672*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.12393509490884E-3},{"$f":"U5672*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":4.2300847832832004E-4},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.0991282186518421},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":7.9552229993296811E-3}]
["Single Family Detached",15672,"Middle Atlantic","1950s","Siding","radiator","central AC",73.724484991499295,31425.611680000002,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":31425.611680000002},"Cold/Very Cold",339.14978934487175,"Metropolitan Area",2.9932945406178693,0.52660064047917909,0.18892593787596132,1.668913674367424E-2,1.017011106589107,4.725832225562117,263.82100000000003,267.24700000000001,{"$f":"T5673*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.2907362990292822E-3},{"$f":"U5673*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":8.3984004446449618E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":3.0015852769168987},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19732433832060628}]
["Multi-Family (2-4 units)",15673,"Middle Atlantic","1970s","Brick","built-in electric unit","N/A",57.396115553617435,43914.395989999997,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":14638.131996666665},"Cold/Very Cold",461.45247302020812,"Metropolitan Area",0.55789397595645873,0.58687673076512692,0,0,0.67059474005089903,1.8153654467724847,0,0,{"$f":"T5674*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5674*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.55789397595645873},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0}]
["Single Family Detached",15674,"Middle Atlantic","1960s","Siding","central furnace","central AC",142.80310369256551,24162.96171,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":24162.96171},"Cold/Very Cold",757.48311598248665,"Metropolitan Area",3.8941467407961419,0.41686212167263154,0.24514325001409792,0.1540818426471704,2.2261174248320312,6.7822695373149022,5661.3069999999998,715.471,{"$f":"T5675*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0.13679394426955496},{"$f":"U5675*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7287898377615411E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.0309406850656968},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.26243114839171333}]
["Single Family Detached",15675,"Mountain North","Before 1950","Siding","central furnace","central AC",23.459215542104026,17454.77347,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":17454.77347},"Cold/Very Cold",155.78385320928453,"Micropolitan Area",0.5231839690100043,0.33659146314838995,5.2546443516385988E-2,1.9895945723193791E-2,0.4614326983398932,1.3737545740146735,1005.763,134.09399999999999,{"$f":"T5676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7555365329507612E-2},{"$f":"U5676*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.3405803936861801E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.54073933433951193},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":5.488702391007217E-2}]
["Single Family Detached",15676,"South Atlantic","1950s","Brick","central furnace","both central and individual units",66.032293217786858,34553.790280000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":34553.790280000001},"Mixed-Humid",344.26051824290602,"Rural",1.1397193851847172,0.15353835040377853,0.25984115118794282,3.3214623583908316E-2,0.89324920323731305,2.4463480900137515,622.98699999999997,338.25700000000001,{"$f":"T5677*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.1526562145166361E-2},{"$f":"U5677*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.1688061438741959E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.1612459473298835},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.27152921262668478}]
["Single Family Detached",15677,"South Atlantic","1980s","Stucco","heat pump","central AC",27.488228949035157,12528.819030000001,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12528.819030000001},"Hot-Humid",285.56674106986281,"Metropolitan Area",2.8096490586907476E-2,0.11109049498874693,0.50244467037427853,2.6228205621972901E-2,0.3327220837229562,0.97435373967288907,40.085999999999999,2053.3440000000001,{"$f":"T5678*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.0223023963658E-4},{"$f":"U5678*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.5725975382336324E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.8598720826544057E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.52817064575661488}]
["Single Family Detached",15678,"New England","Before 1950","Shingle","central furnace","window/wall unit",23.116237864270275,12673.37602,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":12673.37602},"Cold/Very Cold",158.2595814983884,"Rural",0.81984971817752617,0.21633554253148163,1.293963097680418E-2,1.7247146732113919E-2,0.29345934695443965,1.3425842386402516,1360.896,0,{"$f":"T5679*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7247146732113919E-2},{"$f":"U5679*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.83709686490964008},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.293963097680418E-2}]
["Single Family Detached",15679,"East North Central","1960s","Brick","central furnace","central AC",51.961758819195104,21999.051149999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21999.051149999999},"Cold/Very Cold",120.32510821564689,"Metropolitan Area",1.3025219983952638,0.11297887706221874,0.10168482819042256,3.3318310934414098E-2,0.42145678797629593,1.9386424916242011,1275.2560000000001,239.27799999999999,{"$f":"T5680*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.8054421973344401E-2},{"$f":"U5680*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.2638889610696991E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":1.3305764203686081},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.10694871715149226}]
["Single Family Detached",15680,"Mountain South","1980s","Stucco","heat pump","central AC",8.9136198704095477,8307.1946599999992,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":8307.1946599999992},"Hot-Dry/Mixed-Dry",161.61686255261102,"Metropolitan Area",4.647571368945444E-2,9.0916754498029717E-2,0.12310422628739874,6.1328861440809205E-3,0.2909400458238009,0.55143674029868373,89.584999999999994,648.67700000000002,{"$f":"T5681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.442000336160999E-4},{"$f":"U5681*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":5.3886861104648198E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":4.7219913723070536E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.12849291239786356}]
["Single Family Detached",15681,"West South Central","1950s","Siding","heat pump","central AC",39.297030712273859,21264.62701,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":21264.62701},"Mixed-Humid",480.68376763389386,"Micropolitan Area",0.4360851251987744,0.36308083247805201,0.35120132733428849,2.4825495125959548E-2,0.53503417668812747,1.6854014616992425,353.60399999999998,813.851,{"$f":"T5682*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":7.5192571692440395E-3},{"$f":"U5682*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.7306237956715511E-2},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.44360438236801847},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.36850756529100398}]
["Multi-Family (5+ units)",15682,"East North Central","1960s","Brick","central furnace","window/wall unit",6.4709913663146921,14190.77054,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1128.7542165024383},"Cold/Very Cold",27.601048700618591,"Metropolitan Area",0.16643784983856372,0.14885235630532415,6.9399821418164595E-3,2.5832452967899798E-3,8.464672586483353E-2,0.40925468441601837,182.03700000000001,0,{"$f":"T5683*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.0547503130945437E-4},{"$f":"U5683*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.16664332486987318},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":6.9399821418164595E-3}]
["Single Family Detached",15683,"East South Central","Before 1950","Siding","heater burning gas/oil/kerosene","window/wall unit",13.345333359846615,13617.687099999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":13617.687099999999},"Mixed-Humid",63.850257223450463,"Micropolitan Area",8.7514311266517791E-2,4.8916652157081096E-2,3.96943459223481E-2,0,0.12924609467970663,0.3053714040256536,0,0,{"$f":"T5684*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5684*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":8.7514311266517791E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":3.96943459223481E-2}]
["Multi-Family (5+ units)",15684,"East North Central","2000s","Brick","built-in electric unit","window/wall unit",18.186103465770731,20365.177449999999,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":1619.8753867320215},"Cold/Very Cold",73.553501998123934,"Metropolitan Area",2.5137614229165349E-2,6.6688665415222892E-2,1.088948439946695E-2,0,0.14824877764635636,0.25096454169021154,0,0,{"$f":"T5685*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5685*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":2.5137614229165349E-2},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":1.088948439946695E-2}]
["Single Family Detached",15685,"West South Central","2000s","Brick","central furnace","central AC",66.907949436135965,15110.19635,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":15110.19635},"Hot-Humid",211.12603989980889,"Metropolitan Area",0.15082577933111468,9.5828109741882508E-2,0.18367898775333505,1.2569084409427798E-2,0.29002914316432543,0.72036201999065774,185.21299999999999,646.61500000000001,{"$f":"T5686*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":2.7986047965725498E-3},{"$f":"U5686*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":9.7704796128552495E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.15362438412768722},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":0.19344946736619029}]
["Multi-Family (2-4 units)",15686,"East North Central","1970s","Siding","built-in electric unit","central AC",39.32760364535833,31921.75621,{"$f":"IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (2-4 units)\",Table1343[[#This Row],[Number of Homes/ Units]]/3,IF(Table1343[[#This Row],[Housing Type]]=\"Multi-Family (5+ units)\",Table1343[[#This Row],[Number of Homes/ Units]]/12.5720642567977,IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Detached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Single Family Attached\",Table1343[[#This Row],[Number of Homes/ Units]],IF(Table1343[[#This Row],[Housing Type]]=\"Mobile Home\",Table1343[[#This Row],[Number of Homes/ Units]])))))","v":10640.585403333333},"Cold/Very Cold",347.79391821177609,"Metropolitan Area",0.76177517196634714,0.14070937759884464,8.0721736673792177E-2,3.6715765557617801E-3,0.20101883238883542,1.1866728363316605,0,115.018,{"$f":"T5687*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":0},{"$f":"U5687*Table1343[[#This Row],[Number of Buildings]]/1000000000","v":1.2238588519205933E-3},{"$f":"Table1343[[#This Row],[Wtd Air Handlers Heat (Tbtu)]]+Table1343[[#This Row],[Wtd Site Space Heating (TBtu)]]","v":0.76177517196634714},{"$f":"Table1343[[#This Row],[Wtd Site Total Cooling (TBtu)]]+Table1343[[#This Row],[Wtd Air Handlers Cool (Tbtu)]]","v":8.1945595525712775E-2}]